**3GPP TSG-RAN WG4 Meeting #112 R4-2413424**

**Maastricht, Netherlands, 19 August – 23 August 2024**

**Agenda item:** 5.28.3

**Source:** Moderator (Ericsson)

**Title:** Topic summary for [112][324] NR\_redcap\_enh\_demod

**Document for:** Information

# Introduction

This topic summary discusses the maintenance issues for CQI reporting in fading condition for eRedCap.

# Topic #1: Title

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2412549 | Ericsson | **Observation 1:** Throughput ratio of follow CQI and fixed median CQI is degraded due to the mismatch between CSI-RS BW and PDSCH BW.  **Observation 2:** Throughput ratio of follow CQI and fixed median CQI is high enough compared with the Rel-17 RedCap CQI fading test, i.e., γ=1.05, even if CSI-RS BW is 24RB.  **Proposal 1:** Apply the Rel-17 RedCap CQI reporting test in fading condition to Rel-18 eRedCap:   * A CQI index not in the set {median CQI - 1, median CQI, median CQI + 1} shall be reported at least α% of the time, where α = 20%. * Throughput ratio of follow CQI and fixed median CQI shall be ≥ γ, where γ = 1.05 * Average BLER with follow CQI shall be greater than or equal to 0.02.   **Proposal 2:** Set SNR=9/10dB and SNR=15/16dB for CQI reporting test in fading condition for FDD/HD-FDD/TDD with 1Rx, same as Rel-17 RedCap CQI reporting test in fading condition.  **Proposal 3:** Set SNR=6/7dB for CQI reporting test in fading condition for FDD/HD-FDD/TDD with 2Rx, same as Rel-17 RedCap CQI reporting test in fading condition. |
| R4-2412757 | Huawei, HiSilicon | **Proposal 1:** RAN4 to define CQI requirements for eRedCap UE under fading channel. The test SNR and metric can be:   * SNR=9/10dB and SNR=15/16dB for FDD/HD-FDD/TDD with 1Rx. * SNR=6/7dB for FDD/HD-FDD/TDD with 2Rx. * Requirements:   + A CQI index not in the set {median CQI - 1, median CQI, median CQI + 1} shall be reported at least α% of the time where α = 20%.   + Throughput ratio of follow CQI and fixed median CQI shall be ≥ γ, where γ = 1.05   + Average BLER with follow CQI shall be greater than or equal to 0.02. |
| R4-2413311 | Nokia, Nokia Shanghai Bell | **Observation 1:** Under static condition, the CQI metric > 90% is fulfilled in all cases. Thus, it is justified to specify CQI reporting requirements under static condition for eRedCap.  **Observation 2:** Under fading condition, the CQI metric > alpha=20% is not fulfilled in all cases. Especially, for 1Rx UE it is not fulfilled for SNR values > 9 dB. Thereagainst, for 2Rx UE, the CQI metric is fulfilled.  **Proposal 1:** RAN4 to remove CQI reporting requirements under fading condition for eRedCap, or to remove them at least for 1 Rx UE. |
| R4-2412550 | Ericsson | Simulation results summary |
| R4-2412551 | Ericsson, Huawei, HiSilicon | CR for 38.101-4: Correction of eRedCap demodulation and CSI reporting requirements |

## Open issues summary

|  |
| --- |
| RAN4#111 concluded that RAN4#112 discusses whether the following Rel-17 RedCap CQI fading test is applicable for Rel-18 eRedCap UE or not:   * SNR=9/10dB and SNR=15/16dB for FDD/HD-FDD/TDD with 1Rx. * SNR=6/7dB for FDD/HD-FDD/TDD with 2Rx. * Requirements:   + A CQI index not in the set {median CQI - 1, median CQI, median CQI + 1} shall be reported at least α% of the time where α = 20%.   + Throughput ratio of follow CQI and fixed median CQI shall be ≥ γ, where γ = 1.05   + Average BLER with follow CQI shall be greater than or equal to 0.02. |

### Sub-topic 1-1 CQI reporting tests in fading condition

**Issue 1-1-1: Whether to apply the CQI reporting tests in fading condition to eRedCap UEs.**

* Proposals
  + Option 1 (Ericsson, Huawei): Define the CQI reporting requirements under fading condition for eRedCap.
  + Option 2 (Nokia): RAN4 to remove CQI reporting requirements under fading condition for eRedCap, or to remove them at least for 1 Rx UE.
* Recommended WF
  + Two companies propose to apply Rel-17 CQI fading tests to Rel-18 eRedCap. One company proposes not to define CQI test or only limit to 2Rx UE.
  + Moderator recommends:
    - Define the CQI reporting requirements under fading condition for 2Rx eRedCap UE (FDD/HD-FDD/TDD).
    - Discuss further for 1Rx eRedCap UE.
    - Revise CR (R4-2412551) according to the conclusion.

# Recommendation for Tdocs

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Suggested status** | **Comments** |
| R4-2412549 | Noted |  |
| R4-2412757 | Noted |  |
| R4-2413311 | Noted |  |
| R4-2412550 | Withdrawn? | To be withdrawn if no new simulation results in this meeting. |
| R4-2412551 | Revised | Revise according to the online discussion. |