**3GPP TSG-SA5 Meeting #155 *S5-243041***

Jeju, South Korea, 27 - 31 May 2024 Revision of S5-25xxxx

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **32.291** | **CR** | **0565** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Rel-18 CR 32.291 Correction on session identifier | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI18 | | | | |  | ***Date:*** | | | 2024-05-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The session identifier IE in the charging data request and response is a special IE, which is coming from the HTTP header. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify the relationship between ChargingDataRef and session identifier. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The session identifier in the charging data request and response is not clearly defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.1.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Revision of S5-242739 | | | | | | | | |

|  |
| --- |
| **First change** |

#### 6.1.3.1 Overview



Figure 6.1.3.1-1: Resource URI structure of the Nchf\_ConvergedCharging API

Charging Data Ref is corresponding to the session identifier defined in TS 32.290 [58] and is a unique identifier for a charging data resource in a PLMN. It’s created in CHF when CHF receives a Nchf\_ ConvergedCharging\_Create request and provided to NF (CTF) in the Location header field in the Nchf\_ ConvergedCharging\_Create response. The NF (CTF) shall use the Charging Data Ref received in subsequent requests to the CHF for the same charging data resource.

Table 6.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.1.3.1-1: Resources and methods overview

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description | Corresponding service operation |
| Charging Data | {apiRoot}/ nchf-convergedcharging/{apiVersion}/chargingdata | POST | Create a new Charging Data resource | Nchf\_ ConvergedCharging\_Create |
| Individual Charging Data | {apiRoot}/ nchf-convergedcharging/{apiVersion}/ chargingdata/{ChargingDataRef}/update | update  (POST) | Update an existing Charging Data resource. | Nchf\_ ConvergedCharging\_Update |
| {apiRoot}/ nchf-convergedcharging/{apiVersion}/ chargingdata /{ChargingDataRef}/release | release  (POST) | Update and release an existing Charging Data resource. | Nchf\_ ConvergedCharging\_Release |

|  |
| --- |
| **End of change** |