**3GPP TSG-SA5 Meeting #155 *S5-243100***

**Jeju, South Korea, 27 - 31 May 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.541** | **CR** | **1261** | **rev** | **1** | **Current version:** | **18.7.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Rel-18 CR TS 28.541 updates to the terminology for ML entity | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Ericsson, Nokia | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | AIML\_MGT | | | | |  | ***Date:*** | | | 2024-04-29 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | During 3GPP SA5#154 meeting, S5-241931 was agreed to change the term “ML entity” to ML Model. This contribution propose to align the terminology with it.  The definitions of these attributes have been added to the attributes table of clause 6 which is incorrect. It should have been added to clause 4. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Correct the ML entity to ML model.  Moving the definitions of attributes mlModelRef and aIMLInferenceFunctionRef from Attributes Table of clause 6 to clause 5. And change the definition of mLModelRef   * DN to DN list * Change the name to mlModelRefList and aIMLInferenceFunctionRefList. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Inconsistent description | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.1.2, 4.3.58.1, 4.3.58.2, 4.3.58.3, 4.3.60.1, 4.3.60.2, 4.3.60.3, 4.3.69.1, 4.3.69.2, 4.3.69.3, 5.4.1 6.4.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Forge MR link: https://forge.3gpp.org/rep/sa5/MnS/-/merge\_requests/1153 | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **1st change** |

### 4.1.2 Associated information entities and local labels

|  |  |
| --- | --- |
| Label reference | Local label |
| TS 28.622 [30], IOC, ManagedElement | ManagedElement |
| TS 28.622 [30], IOC, SubNetwork | SubNetwork |
| TS 28.105 [105], IOC, MLModel | MLModel |
| TS 28.105 [105], IOC, AIMLInferenceFunction | AIMLInferenceFunction |

|  |
| --- |
| **Next change** |

### 4.3.58 DESManagementFunction

#### 4.3.58.1 Definition

This IOC represents the management capabilities of Distributed Energy Saving (ES) functions. This is provided for Energy Saving purposes.

This Function can be implemented as SON (See clause 6.2.3.0 in TS 28.310 [71]) and/or AI/ML feature (See TS 28.105 [105]) .Attribute mLModelRefList indicates that AI/ML is supported for this function. Attribute AIMLInferenceFunctionRefList indicates that AI/ML Inference Function is supported for this function.

NOTE: in the case where multiple DESManagementFunction MOIs exist at different levels of the containment tree, the DESManagementFunction MOI at the lower level overrides the DESManagementFunction MOIs at higher level(s) of the same containment tree.

#### 4.3.58.2 Attributes

The DESManagementFunction IOC includes attributes inherited from Top IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | S | isReadable | isWritable | isInvariant | isNotifyable |
| desSwitch | M | T | T | F | T |
| intraRatEsActivationOriginalCellLoadParameters | CM | T | T | F | T |
| intraRatEsActivationCandidateCellsLoadParameters | CM | T | T | F | T |
| intraRatEsDeactivationCandidateCellsLoadParameters | CM | T | T | F | T |
| esNotAllowedTimePeriod | O | T | T | F | T |
| interRatEsActivationOriginalCellParameters | CM | T | T | F | T |
| interRatEsActivationCandidateCellParameters | CM | T | T | F | T |
| interRatEsDeactivationCandidateCellParameters | CM | T | T | F | T |
| energySavingState | M | T | F | F | T |
| isProbingCapable | O | T | F | F | T |
| **Attribute related to role** |  |  |  |  |  |
| mLModelRefList | CM | T | F | F | T |
| aIMLInferenceFunctionRefList | CM | T | F | F | T |

#### 4.3.58.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| intraRatEsActivationOriginalCellLoadParameters S | The condition is " the cell acts as an original cell". |
| intraRatEsActivationCandidateCellsLoadParameters S | The condition is " the cell acts as a candidate cell". |
| intraRatEsDeactivationCandidateCellsLoadParameters S | The condition is " the cell acts as a candidate cell". |
| interRatEsActivationOriginalCellParameters CM S | The condition is "The cell acts as an original cell". |
| interRatEsActivationCandidateCellParameters CM S | The condition is "The cell acts as a candidate cell". |
| interRatEsDeactivationCandidateCellParameters CM S | The condition is "The cell acts as a candidate cell". |
| mLModelRefList | The condition is "MLModel is supported for this function". |
| aIMLInferenceFunctionRefList | The condition is "AIMLInferenceFunction is supported for this function ". |

#### 4.3.58.4 Notification

The common notifications defined in clause 4.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **Next change** |

### 4.3.60 DMROFunction

#### 4.3.60.1 Definition

This IOC contains attributes to support Distributed MRO function.

This Function can be implemented as SON (See clause 7.1.2 in TS 28.313 [57]) and/or AI/ML feature (See TS 28.105 [105]) .Attribute mLModelRefList indicates that AI/ML is supported for this function. Attribute AIMLInferenceFunctionRefList indicates that AI/ML Inference Function is supported for this function.

NOTE In the case where multiple DMROFunction MOIs exist at different levels of the containment tree, the DMROFunction MOI at the lower level overrides the DMROFunction MOIs at higher level(s) of the same containment tree.

#### 4.3.60.2 Attributes

The DMROFunction IOC includes attributes inherited from Top IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | S | isReadable | isWritable | isInvariant | isNotifyable |
| dmroControl | M | T | T | F | T |
| maximumDeviationHoTriggerLow | M | T | T | F | T |
| maximumDeviationHoTriggerHigh | M | T | T | F | T |
| minimumTimeBetweenHoTriggerChange | M | T | T | F | T |
| tstoreUEcntxt | M | T | T | F | T |
| **Attribute related to role** |  |  |  |  |  |
| mLModelRefList | CM | T | F | F | T |
| aIMLInferenceFunctionRef | CM | T | F | F | T |

#### 4.3.60.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| mLModelRefList | The condition is "MLModel is supported for this function". |
| aIMLInferenceFunctionRef | The condition is "AIMLInferenceFunction is supported for this function ". |

#### 4.3.60.4 Notifications

The common notifications defined in subclause 4.5 are valid for this IOC, without exceptions or additions

|  |
| --- |
| **Next change** |

### 4.3.69 DLBOFunction

#### 4.3.69.1 Definition

This IOC contains attributes to support the Distributed function of LBO.

This Function can be implemented as SON (See TS 28.313 [57]) and/or AI/ML feature (See TS 28.105 [105]) .Attribute mLModelRefList indicates that AI/ML is supported for this function. Attribute AIMLInferenceFunctionRefList indicates that AI/ML Inference Function is supported for this function.

NOTE In the case where multiple DLBOFunction MOIs exist at different levels of the containment tree, the DLBOFunction MOI at the lower level overrides the DLBOFunction MOIs at higher level(s) of the same containment tree.

#### 4.3.69.2 Attributes

The DLBOFunction IOC includes attributes inherited from Top IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | S | isReadable | isWritable | isInvariant | isNotifyable |
| dlboControl | M | T | T | F | T |
| maximumDeviationHoTriggerLow | M | T | T | F | T |
| maximumDeviationHoTriggerHigh | M | T | T | F | T |
| minimumTimeBetweenHoTriggerChange | M | T | T | F | T |
| **Attribute related to role** |  |  |  |  |  |
| mLModelRefList | CM | T | F | F | T |
| aIMLInferenceFunctionRefList | CM | T | F | F | T |

#### 4.3.69.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| mLModelRefList | The condition is "MLModel is supported for this function". |
| aIMLInferenceFunctionRefList | The condition is "AIMLInferenceFunction is supported for this function ". |

#### 4.3.69.4 Notifications

The common notifications defined in subclause 4.5 are valid for this IOC, without exceptions or additions

|  |
| --- |
| **Next change** |

## 5.4 Attribute definitions

### 5.4.1 Attribute properties

The following table defines the attributes that are present in several Information Object Classes (IOCs) of the present document.

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| aMFIdentifier | The AMFI is constructed from an AMF Region ID, an AMF Set ID and an AMF Pointer. The AMF Region ID identifies the region, the AMF Set ID uniquely identifies the AMF Set within the AMF Region, and the AMF Pointer uniquely identifies the AMF within the AMF Set. (Ref. 3GPP TS 23.003 [13]) | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| aMFSetId | It represents the AMF Set ID, which is uniquely identifies the AMF Set within the AMF Region.  allowedValues: defined in subclause 2.10.1 of 3GPP TS 23.003 [13]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| aMFSetMemberList | It is the list of DNs of AMFFunction instances of the AMFSet.  allowedValues: N/A | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| aMFRegionId | It represents the AMF Region ID, which identifies the region.  allowedValues: defined in subclause 2.10.1 of 3GPP TS 23.003 [13]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| gUAMIdList | List of supported Globally Unique AMF Ids (GUAMIs). | type: GUAMInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| backupInfoAmfFailure | List of GUAMIs for which the AMF acts as a backup for AMF failure. | type: GUAMInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| backupInfoAmfRemoval | List of GUAMIs for which the AMF acts as a backup for planned AMF removal. | type: GUAMInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| localAddress | This parameter specifies the localAddress including IP address and VLAN ID used for initialization of the underlying transport.  First string is IP address, IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).  Second string is VLAN Id (See IEEE 802.1Q [39]). | type: String  multiplicity: 2  isOrdered: True  isUnique: True  defaultValue: None  isNullable: False |
| remoteAddress | Remote address including IP address used for initialization of the underlying transport.  IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nfProfileList | It is a set of NFProfile(s) to be registered in the NRF instance. NFProfile is defined in 3GPP TS 29.510 [23]. | type: <<dataType>>  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| cNSIIdList | It is a set of NSI ID. NSI ID is an identifier for identifying the Core Network part of a Network Slice instance when multiple Network Slice instances of the same Network Slice are deployed, and there is a need to differentiate between them in the 5GC. See NSI ID definition in clause 3.1 of TS 23.501 [2] and subclause 6.1.6.2.7 of TS 29.531 [24]. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| energySavingControl | This attribute allows management system to initiate energy saving activation or deactivation for the edge UPF.  allowedValues:  TO\_BE\_ENERGYSAVING, TO\_BE\_NOT\_ENERGYSAVING. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: True |
| energySavingState | This attribute specifies the status regarding the energy saving in the edge UPF.  If the value of energySavingControl is TO\_BE\_ENERGYSAVING, then it shall be tried to achieve the value IS\_ENERGYSAVING for the energySavingState.  If the value of energySavingControl is TO\_BE\_NOT\_ENERGYSAVING, then it shall be tried to achieve the value IS\_NOT\_ENERGYSAVING for the energySavingState.  allowedValues:  IS\_NOT\_ENERGYSAVING, IS\_ENERGYSAVING. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sNSSAIList | See subclause 4.4.1. |  |
| pLMNInfoList | It defines the PLMN(s) of a Network Function. | type: PLMNInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| sBIFQDN | It is used to indicate the FQDN of the registered NF instance in service-based interface, for example, NF instance FQDN structure is:  nftype<nfnum>.slicetype<sliceid>.mnc<MNC>.mcc<MCC>.3gppnetwork.org | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| interPlmnFQDN | If the NF needs to be discoverable by other NFs in a different PLMN, then an FQDN that is used for inter-PLMN routing as specified in 3GPP TS 23.003 [13] shall be registered with the NRF. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| sBIServiceList | It is used to indicate the all supported NF services registered on service-based interface. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| nRTACList | It is the list of Tracking Area Codes (either legacy TAC or extended TAC).  allowedValues:  Legacy TAC and Extended TAC are defined in clause 9.3.3.10 of TS 38.413 [5]. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| taiList | The list of TAIs. | type: TAI  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| taiRangeList | The range of TAIs. | type: TAIRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| sNssaiSmfInfoList | List of parameters supported by the SMF per S-NSSAI | type: SnssaiSmfInfoItem  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dnnSmfInfoList | List of parameters supported by the SMF per DNN | type: DnnSmfInfoItem  multiplicity: 1..N  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| dnn | String representing a Data Network as defined in clause 9A of 3GPP TS 23.003 [13]; it shall contain either a DNN Network Identifier, or a full DNN with both the Network Identifier and Operator Identifier, as specified in 3GPP TS 23.003 [13] clause 9.1.1 and 9.1.2. It shall be coded as string in which the labels are separated by dots (e.g. "Label1.Label2.Label3").  Whether the dnn data type contains just the DNN Network Identifier, or the Network Identifier plus the Operator Identifier, shall be documented in each API where this data type is used. | type: string  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dnaiList | List of Data network access identifiers supported for this DNN.  allowedValues:  DNAI (Data network access identifier), see clause 5.6.7 of 3GPP TS 23.501 [2]. | type: string  multiplicity: 1..N  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| pgwFqdn | The FQDN of the PGW if the SMF is a combined SMF/PGW-C. | type: string  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| pgwIpAddrList | The PGW IP addresses of the combined SMF/PGW-C.  It allows the NF Service consumer to find the target combined SMF/PGW-C by PGW IP Address, e.g., when only PGW IP Address is available. | type: IpAddr  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| vsmfSupportInd | Used by an SMF to explicitly indicate the support of V-SMF capability and its preference to be selected as V-SMF.  When present it indicate whether the V-SMF capability is supported by the SMF:  - true: V-SMF capability supported by the SMF  - false: V-SMF capability not supported by the SMF.  When absence the V-SMF capability support of the SMF is not specified. | type: boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| pgwFqdnList | When present, this attribute provides additional FQDNs to the FQDN indicated in the pgwFqdn attribute.  The pgwFqdnList attribute may be present if the pgwFqdn attribute is present. | type: string  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| nRTACRangeList | The range of TACs. | type: nrTACRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| nRTACstart | First value identifying the start of a TAC range, to be used when the range of TAC's can be represented as a hexadecimal range (e.g., TAC ranges). 3-octet string identifying a tracking area code, each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the TAC shall appear first in the string, and the character representing the 4 least significant bit of the TAC shall appear last in the string.  Pattern: "^([A-Fa-f0-9]{4}|[A-Fa-f0-9]{6})$" | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| nRTACend | Last value identifying the end of a TAC range, to be used when the range of TAC's can be represented as a hexadecimal range (e.g. TAC ranges). 3-octet string identifying a tracking area code, each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the TAC shall appear first in the string, and the character representing the 4 least significant bit of the TAC shall appear last in the string.  Pattern: "^([A-Fa-f0-9]{4}|[A-Fa-f0-9]{6})$" | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| nRTACpattern | Pattern (regular expression according to the ECMA-262 dialect [x0]) representing the set of TAC's belonging to this range. A TAC value is considered part of the range if and only if the TAC string fully matches the regular expression. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| supportedBMOList | It is used to indicate the list of supported BMOs (Bridge Managed Objects) required for integration with TSN system. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| managedNFProfile | This parameter defines profile for managed NF (See TS 23.501 [2]).  allowedValues: N/A | type: ManagedNFProfile  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| nfInstanceID | This parameter defines unique identity of the NF Instance. The format of the NF Instance ID shall be a Universally Unique Identifier (UUID) version 4, as described in IETF RFC 4122 [44]  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nfType | This parameter defines type of Network Function  allowedValues: See TS 23.501[2] for NF types | type: ENUM  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| heartBeatTimer | Time between two consecutive heart-beat messages from an NF Instance to the NRF defined in seconds. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: 0  isNullable: False |
| fqdn | This parameter defines FQDN of the Network Function (See TS 23.003 [13])  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ipAddress | This parameter defines IP Address of the Network Function. It can be IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38]).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| authzInfo | This parameter defines NF Specific Service authorization information. It shall include the NF type (s) and NF realms/origins allowed to consume NF Service(s) of NF Service Producer (See TS 23.501[2]).  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| allowedPLMNs | PLMNs allowed to access the NF instance.  If not provided, any PLMN is allowed to access the NF. | type: PLMNId  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| allowedSNPNs | SNPNs allowed to access the NF instance.  The absence of this attribute in the NF profile indicates that no SNPN, other than the SNPN(s) registered in the snpnList attribute of the NF Profile, is allowed to access the service instance. | type: SNPNInfo  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mCC | This is the Mobile Country Code (MCC) of the PLMN identifier. See TS 23.003 [3] subclause 2.2 and 12.1.  allowedValues: a bounded string of 3 characters representing 3 digits. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mNC | This is the Mobile Network Code (MNC) of the PLMN identifier. See TS 23.003 [3] subclause 2.2 and 12.1.  allowedValues: A bounded string of 2 or 3 characters representing 2 or 3 digits. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nId | Network Identity; Shall be present if PlmnIdNid identifies an SNPN (see clauses 5.30.2.3, 5.30.2.9, 6.3.4, and 6.3.8 in 3GPP TS 23.501 [2]). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| allowedNfTypes | Type of the NFs allowed to access the NF instance.  If not provided, any NF type is allowed to access the NF.  allowedValues: See TS 23.501[2] for NF types | type: ENUM  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| allowedNfDomains | Pattern (regular expression according to the ECMA-262 dialect [72]) representing the NF domain names within the PLMN of the NRF allowed to access the NF instance.  If not provided, any NF domain is allowed to access the NF. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| allowedNSSAIs | S-NSSAI of the allowed slices to access the NF instance.  If not provided, any slice is allowed to access the NF. | type: S-NSSAI  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| locality | The parameter defines information about the location of the NF instance (e.g. geographic location, data center) defined by operator (See TS 29.510[23]).  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| capacity | This parameter defines static capacity information in the range of 0-65535, expressed as a weight relative to other NF instances of the same type; if capacity is also present in the nfServiceList parameters, those will have precedence over this value (See TS 29.510[23])  allowedValues: 0-65535 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| recoveryTime | Timestamp when the NF was (re)started. The NRF shall notify NFs subscribed to receiving notifications of changes of the NF profile, if the NF recoveryTime is changed. | type: DateTime  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| nfServicePersistence | This parameter indicates whether the different service instances of a same NF Service in the NF instance, supporting a same API version, are capable to persist their resource state in shared storage and therefore these resources are available after a new NF service instance supporting the same API version is selected by a NF Service Consumer (see TS 29.510 [23]). | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| nfSetIdList | A NF Set Identifier is a globally unique identifier of a set of equivalent and interchangeable CP NFs from a given network that provide distribution, redundancy and scalability (see clause 5.21.3 of 3GPP TS 23.501 [2]).  An NF Set Identifier shall be constructed from the MCC, MNC, NID (for SNPN), NF type and a Set ID. A NF Set Identifier shall be formatted as the following string:  set<Set ID>.<nftype>set.5gc.mnc<MNC>.mcc<MCC> for a NF Set in a PLMN, or  set<Set ID>.<nftype>set.5gc.nid<NID>.mnc<MNC>.mcc<MCC> for a NF Set in a SNPN.  At most one NF Set ID shall be indicated per PLMN-ID or SNPN of the NF. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| nfProfileChangesSupportInd | This parameter indicates if the NF Service Consumer supports or does not support receiving NF Profile Changes. It may be present in the NFRegister or NFUpdate (NF Profile Complete Replacement) request and shall be absent in the response (see Annex B 3GPP TS 29.510 [23]). | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| defaultNotificationSubscriptions | Notification endpoints for different notification types.  This attribute may contain multiple default subscriptions for a same notification type; in that case, those default subscriptions are used as alternative notification endpoints. | type: DefaultNotificationSubscription  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| notificationType | This parameter indicates the types of notifications used in Default Notification URIs in the NF Profile of an NF Instance.  allowedValues:  "N1\_MESSAGES",  "N2\_INFORMATION",  "LOCATION\_NOTIFICATION",  ”DATA\_REMOVAL\_NOTIFICATION”,  "DATA\_CHANGE\_NOTIFICATION",  "LOCATION\_UPDATE\_NOTIFICATION",  "NSSAA\_REAUTH\_NOTIFICATION",  "NSSAA\_REVOC\_NOTIFICATION" | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| callbackURI | This attribute contains a default notification endpoint to be used by a NF Service Producer towards an NF Service Consumer that has not registered explicitly a callback URI in the NF Service Producer (e.g. as a result of an implicit subscription). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| n1MessageClass | This attribute (if it is present) identifies that class of N1 messages shall be notified as per TS 29.518 [80]. | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| n2InformationClass | This attribute (if it is present) identifies that class of N2 messages shall be notified as per TS 29.518 [80]. | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| versions | This attribute identifies the API versions (e.g. "v1") supported for the default notification type. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| binding | This attribute shall contain the value of the Binding Indication for the default subscription notification (i.e. the value part of "3gpp-Sbi-Binding" header), as specified in clause 6.12.4 of 3GPP TS 29.500 [76]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| servingScope | This parameter indicates the served geographical areas of a NF instance. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| lcHSupportInd | This parameter indicates whether the NF supports or does not support Load Control based on LCI Header (see clause 6.3 of 3GPP TS 29.500 [76]). | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  allowedValues: N/A  isNullable: False |
| olcHSupportInd | This parameter indicates whether the NF supports or does not support Overload Control based on OCI Header (see clause 6.4 of 3GPP TS 29.500 [76]). | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  allowedValues: N/A  isNullable: False |
| nfSetRecoveryTimeList | This parameter contains the recovery time of NF Set(s) indicated by the NfSetId, where the NF instance belongs. | type: DateTime  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| serviceSetRecoveryTimeList | This parameter contains the recovery time of NF Service Set(s) configured in the NF instance, which are indicated by the NfServiceSetId. | type: DateTime  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| scpDomains | This parameter shall carry the list of SCP domains the SCP belongs to, or the SCP domain the NF (other than SCP) or the SEPP belongs to. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| vendorId | Vendor ID of the NF instance, according to the IANA-assigned "SMI Network Management Private Enterprise Codes" [77].  allowedValues: 6 decimal digits; if the SMI code has less than 6 digits, it shall be padded with leading digits "0" to complete a 6-digit string value. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| hostAddr | This parameter defines host address of a NF  allowedValues: N/A | type: HostAddr  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| priority | This parameter defines Priority (relative to other NFs of the same type) in the range of 0-65535, to be used for NF selection; lower values indicate a higher priority. If priority is also present in the nfServiceList parameters, those will have precedence over this value (See TS 29.510[23]).  allowedValues: 0-65535 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| supportedDataSets | This parameter defines list of supported data sets in the UDR instance (See TS 29.510[23]).  allowedValues: "SUBSCRIPTION", "POLICY", EXPOSURE", "APPLICATION", "A\_PFD", "A\_AFTI", "A\_IPTV", "A\_BDT", "A\_SPD", "A\_EASD", "A\_AMI", "P\_UE", "P\_SCD", "P\_BDT", "P\_PLMNUE", "P\_NSSCD". | type: ENUM  multiplicity: 1..\*  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| nFSrvGroupId | This parameter defines identity of the group that is served by the NF instance (See TS 29.510[23]).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| smfServingArea | This parameter defines the SMF service area(s) the UPF can serve (See TS 29.510[23]). If not provided, the UPF can serve any SMF service area.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| interfaceUpfInfoList | List of User Plane interfaces configured on the UPF. When this parameter is provided in the NF Discovery response, the NF Service Consumer (e.g., SMF) may use this information for UPF selection. | type: InterfaceUpfInfoItem  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| interfaceType | This parameter defines the type of User Plane (UP) interface.  allowedValues:  "N3"  "N6"  "N9"  "DATA\_FORWARDING"  "N6MB"  "N19MB"  "N3MB"  "NMB9" | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ipv4EndpointAddresses | Available endpoint IPv4 address(es) of the User Plane interface. | type: ipv4Addr  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ipv6EndpointAddresses | Available endpoint IPv6 address(es) of the User Plane interface. | type: ipv6Addr  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| networkInstance | Network Instance (See TS 29.244 [56]) associated to the User Plane interface | type: string  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| iwkEpsInd | Indicates whether interworking with EPS is supported by the UPF.  allowedValues:  True: Supported False: Not Supported | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| pduSessionTypes | Indicates the type of a PDU session.  allowedValues:  “IPv4” “IPv6” “IPv4v6” as per clause 5.8.2.2.1 TS 23.501 [2] “UNSTRUCTURED” “ETHERNET” | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| atsssCapability | Indicate the ATSSS capability of the UPF. | type: AtsssCapability  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| atsssLL | Indicates the ATSSS-LL capability to support procedures related to Access Traffic Steering, Switching, Splitting (see clauses 4.2.10, 5.32 of TS 23.501 [2]).  allowedValues:  True: Supported False: Not Supported | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| mptcp | Indicates the MPTCP capability to support procedures related to Access Traffic Steering, Switching, Splitting (see clauses 4.2.10, 5.32 of TS 23.501 [2]).  allowedValues:  True: Supported False: Not Supported | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| rttWithoutPmf | Indicates whether the UPF supports RTT measurement without PMF (see clauses 5.32.2, 6.3.3.3 of TS 23.501 [2]).  allowedValues:  True: Supported  False: Not Supported. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| ueIpAddrInd | Indicates whether the UPF supports allocating UE IP addresses/prefixes.  allowedValues:  True: supported False: not supported | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| wAgfInfo | Indicate that the UPF is collocated with W-AGF. If not present, the UPF is not collocated with Wireline Access Gateway Function (W-AGF). | type: IpInterface  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| tngfInfo | Indicate that the UPF is collocated with TNGF. If not present, the UPF is not collocated with Trusted Non-3GPP Gateway Function (TNGF). | type: IpInterface  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| twifInfo | Indicate that the UPF is collocated with TWIF. If not present, the UPF is not collocated with Trusted WLAN Interworking Function (TWIF). | type: IpInterface  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| redundantGtpu | Indicates whether the UPF supports redundant GTP-U path.  allowedValues:  True: supported False: not supported | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| ipups | Indicates whether the UPF is configured for Inter-PLMN User Plane Security (IPUPS). Any UPF can support the IPUPS functionality. In network deployments where specific UPFs are used to provide IPUPS, UPFs configured for providing IPUPS services shall be selected.  allowedValues:  True: The UPF is configured for IPUPS.  False: The UPF is not configured for IPUPS | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| dataForwarding | Indicates whether the UPF is configured for data forwarding.  Based on operator policies, if dedicated UPFs are preferred to be used for indirect data forwarding during handover scenarios, when setting up the indirect data forwarding tunnel, the SMF should preferably select a UPF configured for data forwarding and use the network instance indicated in the Network Instance ID associated to the DATA\_FORWARDING interface type in the interfaceUpfInfoList attribute.  allowedValues:  True: the UPF is configured for data forwarding  False: the UPF is not configured for data forwarding  If the UPF is configured for data forwarding, it shall support UP network interface with type "DATA\_FORWARDING". | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| supportedPfcpFeatures | Supported Packet Forwarding Control Protocol (PFCP) Features.  A string used to indicate the PFCP features supported by the UPF, which encodes the "UP Function Features" as specified in Table 8.2.25-1 of TS 29.244 [56] (starting from Octet 5), in hexadecimal representation.  Each character in the string shall take a value of "0" to "9", "a" to "f" or "A" to "F" and each two characters shall represent one octet of "UP Function Features" (starting from Octet 5, to higher octets). For each two characters representing one octet, the first character representing the 4 most significant bits of the octet and the second character the 4 least significant bits of the octet.  The supported PFCP features shall be provisioned in addition and be consistent with the existing UPF features (atsssCapability, ueIpAddrInd, redundantGtpu and ipups), e.g., if the ueIpAddrInd is set to "true", then the UEIP flag shall also be set to "1" in the supported PFCP features. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| isESCoveredBy | This indicates whether the adjacentCell provides no, partial or full coverage for the cell which name-contains the NRCellRelation instance.  Adjacent cells with this attribute equal to "FULL" are recommended to be considered as candidate cells to take over the coverage when the original cell state is about to be changed to energySaving.  All adjacent cells with this attribute value equal to "PARTIAL" are recommended to be considered as entirety of candidate cells to take over the coverage when the original cell state is about to be changed to energySaving.  allowedValues: NO, PARTIAL, FULL | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| commModelList | The attribute specifies a list of commModel which is defined as a datatype (see clause 5.3.69). It can be used by NF and NF services to interact with each other in 5G Core network (see TS 23.501 [2]).  allowedValues: Not applicable | type: commModel  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| groupId | This parameter identiies a list of target NF services on which the same communication model is applied to.  allowedValues: N/A | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| commModelType | This parameter defines communication model used by a NF to interact with NF service(s) (See TS 23.501 [2]).  allowedValues:”DIRECT\_COMMUNICATION\_WO\_NRF”, “DIRECT\_COMMUNICATION\_WITH\_NRF”, “INDIRECT\_COMMUNICATION\_WO\_DEDICATED\_DISCOVERY”, “INDIRECT\_COMMUNICATION\_WITH\_DEDICATED\_DISCOVERY” | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| targetNFServiceList | This parameter lists target NF services sharing same communication model and configuration.  allowedValues: N/A | type: DN  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| commModelConfiguration | This parameter defines configuration parameters for specific communication model for a group of NF Services.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| supportedFuncList | This parameter lists functionalities supported by a SCP. Refer to TS 23.501 [2]. | type: SupportedFunction  multiplicity: 1..\*  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| address | This parameter defines address of a SCP instance, it can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38])) or FQDN (See TS 23.003 [13]). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| function | This parameter defines name of a functionality supported by a SCP. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| policy | This parameter defines configuration policies of a functionality supported by a SCP. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| capabilityList | This parameter lists capabilities supported by a NEF. Refer to TS 23.501 [2].  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| isCAPIFSup | This parameter defines if the NEF support Common API Framework.  allowedValues: TRUE, FALSE | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sEPPType | This parameter defines the type of a SEPP entity. Refer to TS 33.501 [52].  allowedValues: “CSEPP”, “PSEPP” | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sEPPId | This parameter is identifier of a SEPP, it is unique inside a PLMN.  allowedValues: N/A | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| remotePlmnId | This parameter defines PLMNId of the remote SEPP.  allowedValues: N/A | Type: PLMNId  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| remoteSeppAddress | This parameter defines address of the remote SEPP. It can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38])) or FQDN(See TS 23.003 [13]).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| remoteSeppId | This parameter defines identifier of the remote SEPP. it is unique inside a PLMN.  allowedValues: N/A | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| n32cParas | This attribute is used to configure parameters to establish security link between two SEPPs.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n32fPolicy | This attribute is used to configure policies to protect the messages exchanged between SEPPs.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| withIPX | This attribute defines if there’s an IPX interconnected between two SEPPs.  allowedValues: TRUE, FALSE | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| FiveQiDscpMappingList | It provides the list of mapping between 5QIs and DSCP.  allowedValues: N/A | type: FiveQiDscpMapping  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| fiveQIValues | It indicates a list of 5QI value.  allowedValues: 0 - 255 | type: Integer  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| dscp | It indicates a DSCP.  allowedValues: 0 – 255 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| configurable5QISetRef | This is the DN of Configurable5QISet.  allowedValues: DN of the Configurable5QISet MOI. | type: DN  multiplicity: 0..1  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| dynamic5QISetRef | This is the DN of Dynamic5QISet MOI.  allowedValues: DN of the Dynamic5QISet MOI. | type: DN  multiplicity: 0..1  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| fiveQIValue | It identifies the 5QI value.  allowedValues: 0 – 255 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| resourceType | It indicates the Resource Type of a 5QI, as specified in TS 23.501 [2].  allowedValues: "GBR", NON\_GBR", "DELAY\_CRITICAL\_GBR" | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: False  defaultValue: None  isNullable: False |
| priorityLevel | It indicates the Priority Level of a 5QI, as specified in TS 23.501 [2].  allowedValues: 0 - 127 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| packetDelayBudget | It indicates the Packet Delay Budget (in unit of 0.5ms) of a 5QI, as specified in TS 23.501 [2].  allowedValues: 0 - 1023 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| packetErrorRate | It indicates the Packet Error Rate of a 5QI, as specified in TS 23.501 [2].  allowedValues: N/A | type: PacketErrorRate  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| averagingWindow | It indicates the Averaging Window (in unit of ms) of a 5QI, as specified in TS 23.501 [2].  allowedValues: 0 - 4095 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| maximumDataBurstVolume | It indicates the Maximum Data Burst Volume (in unit of Byte) of a 5QI, as specified in TS 23.501 [2].  allowedValues: 0 - 4095 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| scalar | The Packet Error Rate of a 5QI expressed as *Scalar* x 10-k where k is the *Exponent*.  This attriutes indicates the *Scalar* of this expression.  allowedValues: 0 - 9 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| exponent | The Packet Error Rate of a 5QI expressed as *Scalar* x 10-k where k is the *Exponent*.  This attriutes indicates the *Exponent* of this expression.  allowedValues: 0 - 9 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gtpUPathQoSMonitoringState | It indicates the state of GTP-U path QoS monitoring for URLLC service.  allowedValues: "Enabled", "Disabled". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Enabled  isNullable: False |
| gtpUPathMonitoredSNSSAIs | It specifies the S-NSSAIs for which the GTP-U path QoS monitoring is to be performed.  allowedValues: See 3GPP TS 23.003 [13] | type: S-NSSAI  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| monitoredDSCPs | It specifies the DSCPs for which the GTP-U path QoS monitoring is to be performed.  allowedValues: See 3GPP TS 29.244 [56] | type: Integer  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| isEventTriggeredGtpUPathMonitoringSupported | It indicates whether the event triggered GTP-U path QoS monitoring reporting based on thresholds is supported, see 3GPP TS 29.244 [56].  allowedValues: “Yes”, “No”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Yes  isNullable: False |
| isPeriodicGtpUMonitoringSupported | It indicates whether the periodic GTP-U path QoS monitoring reporting is supported, see 3GPP TS 29.244 [56].  allowedValues: “Yes”, “No”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Yes  isNullable: False |
| isImmediateGtpUMonitoringSupported | It indicates whether the immediate GTP-U path QoS monitoring reporting is supported, see 3GPP TS 29.244 [56].  allowedValues: “Yes”, “No”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Yes  isNullable: False |
| gtpUPathDelayThresholds | It specifies the thresholds for reporting the packet delay for the GTO-U path QoS monitoring, if the isEventTriggeredGtpUPathMonitoringSupported attribute of the same MOI is set to “yes”.  The packet delay will be reported to SMF when it exceeds the threshold (in milliseconds).  allowedValues: N/A. | type: GtpUPathDelayThresholdsType  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gtpUPathMinimumWaitTime | It specifies the minimum waiting time (in seconds) between two consecutive reports for event triggered GTP-U path QoS monitoring reporting, if the isEventTriggeredGtpUPathMonitoringSupported attribute of the same MOI is set to “yes”.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gtpUPathMeasurementPeriod | It specifies the period (in seconds) for reporting the packet delay for GTP-U path QoS monitoring, if the isPeriodicGtpUMonitoringSupported attribute of the same MOI is set to “yes”.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n3AveragePacketDelayThreshold | It specifies the threshold for reporting the average packet delay of a GTP-U path on N3 interface.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n3MinPacketDelayThreshold | It specifies the threshold for reporting the minimum packet delay of a GTP-U path on N3 interface.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n3MaxPacketDelayThreshold | It specifies the threshold for reporting the maxinum packet delay of a GTP-U path on N3 interface.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n9AveragePacketDelayThreshold | It specifies the threshold for reporting the average packet delay of a GTP-U path on N9 interface.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n9MinPacketDelayThreshold | It specifies the threshold for reporting the minimum packet delay of a GTP-U path on N9 interface.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| n9MaxPacketDelayThreshold | It specifies the threshold for reporting the maxinum packet delay of a GTP-U path on N9 interface.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qFQoSMonitoringState | It indicates the state of QoS monitoring per QoS flow per UE for URLLC service.  allowedValues: "Enabled", "Disabled". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Enabled  isNullable: False |
| qFMonitoredSNSSAIs | It specifies the S-NSSAIs for which the QoS monitoring per QoS flow per UE is to be performed.  allowedValues: See 3GPP TS 23.003 [13] | type: S-NSSAI  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| qFMonitored5QIs | It specifies the 5QIs for which the QoS monitoring per QoS flow per UE is to be performed.  allowedValues: See 3GPP TS 23.501[2] | type: Integer  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| isEventTriggeredQFMonitoringSupported | It indicates whether the event based QoS monitoring reporting per QoS flow per UE is supported, see 3GPP TS 29.244 [56].  allowedValues: “Yes”, “No”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Yes  isNullable: False |
| isPeriodicQFMonitoringSupported | It indicates whether the periodic QoS monitoring reporting per QoS flow per UE is supported, see 3GPP TS 29.244 [56].  allowedValues: “Yes”, “No”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Yes  isNullable: False |
| isSessionReleasedQFMonitoringSupported | It indicates whether the session release based QoS monitoring reporting per QoS flow per UE is supported, see 3GPP TS 29.244 [56].  allowedValues: “Yes”, “No”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Yes  isNullable: False |
| qFPacketDelayThresholds | It specifies the thresholds for reporting the packet delay between PSA and UE for QoS monitoring per QoS flow per UE, if the isEventTriggeredQFMonitoringSupported attribute of the same MOI is set to “yes”.”.  The packet delay will be reported by PSA UPF to SMF when it exceeds the threshold (in milliseconds).  allowedValues: see 3GPP TS 29.244 [56]. | type: QFPacketDelayThresholdsType  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qFMinimumWaitTime | It specifies the minimum waiting time (in seconds) between two consecutive reports for event triggered QoS monitoring reporting per QoS flow per UE, if the isEventTriggeredQFMonitoringSupported attribute of the same MOI is set to “yes”.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qFMeasurementPeriod | It specifies the period (in seconds) for reporting the packet delay for QoS monitoring per QoS flow per UE, if the isPeriodicQFMonitoringSupported attribute of the same MOI is set to “yes”.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| thresholdDl | It specifies the threshold for reporting the DL packet delay between PSA UPF and UE.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| thresholdUl | It specifies the threshold for reporting the UL packet delay between PSA UPF and UE.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| thresholdRtt | It specifies the threshold for reporting the round-trip packet delay between PSA UPF and UE.  allowedValues: see 3GPP TS 29.244 [56]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| predefinedPccRules | It specifies the predefined PCC Rules, see TS 25.503 [59].  allowedValues: N/A | type: PccRule  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| pccRuleId | It identifies the PCC rule.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| flowInfoList | It is a list of IP flow packet filter information.  allowedValues: N/A | type: FlowInformation  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| applicationId | A reference to the application detection filter configured at the UPF.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| appDescriptor | It is the ATSSS rule application descriptor.  allowedValues: see TS 29.571 [61]. | type: BitString  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| contentVersion | Indicates the content version of the PCC rule.  allowedValues: N/A | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| precedence | It indicates the order in which this PCC rule is applied relative to other PCC rules within the same PDU session.  allowedValues: 0..255. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| afSigProtocol | Indicates the protocol used for signalling between the UE and the AF. The default value is "NO\_INFORMATION".  allowedValues: “NO\_INFORMATION”, “SIP”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “NO\_INFORMATION”  isNullable: False |
| isAppRelocatable | It indicates the application relocation possibility. The default value is "FALSE.  allowedValues: “TRUE”, “FALSE”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| isUeAddrPreserved | It Indicates whether UE IP address should be preserved.  The default value is "FALSE".  allowedValues: “TRUE”, “FALSE”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| qosData | It contains the QoS control policy data for a PCC rule.  allowedValues: N/A | type: QoSData  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| altQosParams | It contains the QoS control policy data for the Alternative QoS parameter sets of the service data flow. Only the "qosId" attribute, "5qi" attribute, "maxbrUl" attribute, "maxbrDl" attribute, "gbrUl" attribute and "gbrDl" attribute are applicable within the QosData data type. This data type represents an ordered list, where the lower the index of the array for a given entry, the higher the priority.  allowedValues: N/A | type: QoSData  multiplicity: \*  isOrdered: True  isUnique: True  defaultValue: None  isNullable: False |
| trafficControlData | It contains the traffic control policy data for a PCC rule.  allowedValues: N/A | type: TrafficControlData  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| conditionData | It contains the condition data for a PCC rule.  allowedValues: N/A | type: ConditionData  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| tscaiInputUl | It contains transports TSCAI input parameters for TSC traffic at the ingress interface of the DS-TT/UE (uplink flow direction).  allowedValues: N/A | type: TscaiInputContainer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| tscaiInputDl | It contains transports TSCAI input parameters for TSC traffic at the ingress of the NW-TT (downlink flow direction).  allowedValues: N/A | type: TscaiInputContainer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| flowDescription | It defines a packet filter for an IP flow.  allowedValues: see TS 29.214 [62]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ethFlowDescription | It defines a packet filter for an Ethernet flow.  allowedValues: see TS 29.514 [62]. | type: EthFlowDescription  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| destMacAddr | It specifies the destination MAC address formatted in the hexadecimal notation according to clause 1.1 and clause 2.1 of IETF RFC 7042 [63].  Pattern: '^([0-9a-fA-F]{2})((-[0-9a-fA-F]{2}){5})$'.  allowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ethType | A two-octet string that represents the Ethertype, as described in IEEE 802.3 [64] and IETF RFC 7042 [63] in hexadecimal representation.  Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the ethType shall appear first in the string, and the character representing the 4 least significant bits of the ethType shall appear last in the string.  allowedValues: see IEEE 802.3 [64] and IETF RFC 7042 [63]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| fDesc | It contains the flow description for the Uplink or Downlink IP flow. It shall be present when the ethtype is IP.  allowedValues: see flowDescription in TS 29.214 [62]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| fDir | It indicates the packet filter direction.  allowedValues: "DOWNLINK", "UPLINK". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sourceMacAddr | It specifies the source MAC address formatted in the hexadecimal notation according to clause 1.1 and clause 2.1 of IETF RFC 7042 [63].  Pattern: '^([0-9a-fA-F]{2})((-[0-9a-fA-F]{2}){5})$'.  allowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| vlanTags | It specifies the Customer-VLAN and/or Service-VLAN tags containing the VID, PCP/DEI fields as defined in IEEE 802.1Q [65] and IETF RFC 7042 [63]. The first/lower instance in the array stands for the Customer-VLAN tag and the second/higher instance in the array stands for the Service-VLAN tag.  Each field is encoded as a two-octet string in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the PCP/DEI field shall appear first in the string, followed by character representing the 4 most significant bits of the VID field, and the character representing the 4 least significant bits of the VID field shall appear last in the string.  If only Service-VLAN tag is provided, empty string for Customer-VLAN tag shall be provided.  allowedValues: see IEEE 802.1Q [65] and IETF RFC 7042 [63]. | type: String  multiplicity: \*  isOrdered: True  isUnique: True  defaultValue: None  isNullable: False |
| srcMacAddrEnd | It specifies the source MAC address end. If this attribute is present, the sourceMacAddr attribute specifies the source MAC address start. E.g. srcMacAddrEnd with value 00-10-A4-23-3E-FE and sourceMacAddr with value 00-10-A4-23-3E-02 means all MAC addresses from 00-10-A4-23-3E-02 up to and including 00-10-A4-23-3E-FE.  allowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| destMacAddrEnd | It specifies the destination MAC address end. If this attribute is present, the destMacAddr attribute specifies the destination MAC address start.  allowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| packFiltId | It is the identifier of the packet filter.  allowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| packetFilterUsage | It indicates if the packet shall be sent to the UE.  The default value is "FALSE".  allowedValues: TRUE, FALSE | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| tosTrafficClass | It contains the Ipv4 Type-of-Service and mask field or the Ipv6 Traffic-Class field and mask field.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| spi | It is the security parameter index of the IPSec packet, see IETF RFC 4301 [66].  allowedValues: see IETF RFC 4301 [66]. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| flowLabel | It specifies the Ipv6 flow label header field.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| flowDirection | It indicates the direction/directions that a filter is applicable.  AllowedValues: “DOWNLINK”, “UPLINK”, “BIDIRECTIONAL”, “UNSPECIFIED”. | type: ENUM  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qosId | It identifies the QoS control policy data for a PCC rule.  AllowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| maxbrUl | It represents the maximum uplink bandwidth formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$', see TS 29.512 [60].  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps"  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| maxbrDl | It represents the maximum downlink bandwidth formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$', see TS 29.512 [60].  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps".  AllowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gbrUl | It represents the guaranteed uplink bandwidth formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$', see TS 29.512 [60].  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps".  AllowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gbrDl | It represents the guaranteed downlink bandwidth formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$', see TS 29.512 [60].  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps".  AllowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| extMaxDataBurstVol | It denotes the largest amount of data that is required to be transferred within a period of 5G-AN PDB, see TS 29.512 [60].  AllowedValues: 4096..2000000. | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| arp | It indicates the allocation and retention priority.  AllowedValues: N/A. | type: ARP  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ARP.priorityLevel | It defines the relative importance of a resource request.  AllowedValues: 1..15. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| preemptCap | It defines whether a service data flow may get resources that were already assigned to another service data flow with a lower priority level.  AllowedValues: "NOT\_PREEMPT", "MAY\_PREEMPT". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| preemptVuln | It defines whether a service data flow may lose the resources assigned to it in order to admit a service data flow with higher priority level.  AllowedValues: "NOT\_PREEMPTABLE", "PREEMPTABLE". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qosNotificationControl | It indicates whether notifications are requested from 3GPP NG-RAN when the GFBR can no longer (or again) be guaranteed for a QoS Flow during the lifetime of the QoS Flow. The default value is "FALSE".  AllowedValues: "TRUE", "FALSE". | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| reflectiveQos | Indicates whether the QoS information is reflective for the corresponding non-GBR service data flow. The default value is "FALSE".  AllowedValues: "TRUE", "FALSE". | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| sharingKeyDl | It indicates, by containing the same value, what PCC rules may share resource in downlink direction.  AllowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sharingKeyUl | It indicates, by containing the same value, what PCC rules may share resource in uplink direction.  AllowedValues: N/A. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| maxPacketLossRateDl | It indicates the downlink maximum rate for lost packets that can be tolerated for the service data flow.  AllowedValues: 0..1000. | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| maxPacketLossRateUl | It indicates the uplink maximum rate for lost packets that can be tolerated for the service data flow.  AllowedValues: 0..1000. | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| tcId | It univocally identifies the traffic control policy data within a PDU session.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| flowStatus | It represents whether the service data flow(s) are enabled or disabled. The default value is "ENABLED". See TS 29.514 [67].  AllowedValues: “ENABLED-UPLINK”, “ENABLED-DOWNLINK”, “ENABLED”, “DISABLED”, “REMOVED”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “ENABLED”  isNullable: False |
| redirectInfo | It indicates whether the detected application traffic should be redirected to another controlled address.  AllowedValues: N/A. | type: RedirectInformation  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “ENABLED”  isNullable: False |
| addRedirectInfo | It contains the additional redirect information indicating whether the detected application traffic should be redirected to another controlled address.  AllowedValues: N/A. | type: RedirectInformation  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: “ENABLED”  isNullable: False |
| redirectEnabled | It indicates whether the redirect instruction is enabled.  AllowedValues: "TRUE", "FALSE". | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| redirectAddressType | It indicates the type of redirect address, see TS 29.512 [60].  AllowedValues: " IPV4\_ADDR", "IPV6\_ADDR", “URL”, “SIP\_URI”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| redirectServerAddress | It indicates the address of the redirect server.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| muteNotif | It indicates whether applicat'on's start or stop notification is to be muted. The default value is "FALSE".  AllowedValues: "TRUE", "FALSE". | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| trafficSteeringPolIdDl | It references to a pre-configured traffic steering policy for downlink traffic at the SMF, see TS 29.512 [60].  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| trafficSteeringPolIdUl | It references to a pre-configured traffic steering policy for uplink traffic at the SMF, see TS 29.512 [60].  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| routeToLocs | It provides a list of location which the traffic shall be routed to for the AF request.  AllowedValues: N/A. | type: RouteToLocation  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| traffCorreInd | It indicates the traffic correlation.  AllowedValues: "TRUE", "FALSE". | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| dnai | It represents the DNAI (Data network access identifier), see 3GPP TS 23.501 [2].  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| routeInfo | It provides the traffic routing information.  AllowedValues: N/A. | type: RouteInformation  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ipv4Addr | It defines the Ipv4 address of the tunnel end point in the data network, formatted in the "dotted decimal" notation.  Pattern: '^(([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])$'.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ipv6Addr | It defines the Ipv6 address of the tunnel end point in the data network.  Pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))$'  and  Pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))$'.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ipv6AddrPrefix | String identifying an IPv6 address prefix formatted according to clause 4 of IETF RFC 5952 [82]. IPv6Prefix data type may contain an individual /128 IPv6 address.  Pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))(\/(([0-9])|([0-9]{2})|(1[0-1][0-9])|(12[0-8])))$'  and  Pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))(\/.+)$' | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| portNumber | It defines the UDP port number of the tunnel end point in the data network, see TS 29.571 [61].  AllowedValues: N/A. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| routeProfId | It identifies the routing profile.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| upPathChgEvent | It contains the information about the AF subscriptions of the UP path change.  AllowedValues: N/A. | type: UpPathChgEvent  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| notificationUri | It provides notification address (Uri) of AF receiving the event notification.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| notifCorreId | It is used to set the value of Notification Correlation ID in the notification sent by the SMF, see TS 29.512 [60].  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| dnaiChgType | It indicates the type of DNAI change, see TS 29.512 [60].  AllowedValues: “EARLY”, “EARLY\_LATE”, “LATE”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| afAckInd | It identifies whether the AF acknowledgement of UP path event notification is expected.The default value is "FALSE".  AllowedValues: “TRUE”, “FALSE”. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| steerFun | It indicates the applicable traffic steering functionality, see TS 29.512 [60].  AllowedValues: “MPTCP”, “ATSSS\_LL”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| steerModeDl | It provides the traffic distribution rule across 3GPP and Non-3GPP accesses to apply for downlink traffic.  AllowedValues: N/A. | type: SteeringMode  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| steerModeUl | It provides the traffic distribution rule across 3GPP and Non-3GPP accesses to apply for uplink traffic.  AllowedValues: N/A. | type: SteeringMode  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mulAccCtrl | It indicates whether the service data flow, corresponding to the service data flow template, is allowed or not allowed. The default value is "NOT\_ALLOWED".  AllowedValues: "ALLOWED", "NOT\_ALLOWED". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: "NOT\_ALLOWED"  isNullable: False |
| steerModeValue | It indicates the value of the steering mode, see TS 29.512 [60].  AllowedValues: “ACTIVE\_STANDBY”, “LOAD\_BALANCING”, “SMALLEST\_DELAY”, “PRIORITY\_BASED”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| active | It indicates the active access, see TS 29.571 [61].  AllowedValues: "3GPP\_ACCESS", "NON\_3GPP\_ACCESS". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| standby | It indicates the Standby access, see TS 29.571 [61].  AllowedValues: "3GPP\_ACCESS", "NON\_3GPP\_ACCESS". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| threeGLoad | It indicates the traffic load to steer to the 3GPP Access expressed in one percent.  AllowedValues: 0..100. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| prioAcc | It indicates the high priority access, see TS 29.571 [61].  AllowedValues: "3GPP\_ACCESS", "NON\_3GPP\_ACCESS". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| condId | It uniquely identifies the condition data.  AllowedValues: N/A. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| activationTime | It indicates the time (in date-time format) when the decision data shall be activated, see TS 29.512 [60] and TS 29.571 [61].  AllowedValues: N/A. | type: DateTime  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| deactivationTime | It indicates the time (in date-time format) when the decision data shall be deactivated, see TS 29.512 [60] and TS 29.571 [61].  AllowedValues: N/A. | type: DateTime  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| accessType | It provides the condition of access type of the UE when the session AMBR shall be enforced, see TS 29.512 [60].  AllowedValues: "3GPP\_ACCESS", "NON\_3GPP\_ACCESS". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ratType | It provides the condition of RAT type of the UE when the session AMBR shall be enforced, see TS 29.512 [60] and TS 29.571 [61].  AllowedValues: "NR", "EUTRA", “WLAN”, “VIRTUAL”, “NBIOT”, “WIRELINE”, “WIRELINE\_CABLE”, “WIRELINE\_BBF”, “LTE-M”, “NR\_U”, “EUTRA\_U”, “TRUSTED\_N3GA”, “TRUSTED\_WLAN”, “UTRA”, “GERA”. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| periodicity | It identifies the time period between the start of two bursts in reference to the TSN GM.  AllowedValues: see TS 29.571 [61]. | type: integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| burstArrivalTime | Indicates the arrival time (in date-time format) of the data burst in reference to the TSN GM.  AllowedValues: see TS 29.571 [61]. | type: DateTime  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nsacfInfoSnssaiList | It represents a list of NSACF information per S-NSSAI.  AllowedValues: N/A | type: NsacfInfoSnssai  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| snssaiInfo | It defines generic information for a S-NSSAI. The information includes global unique identifier of a Network Slice (see [2] for definition of Network Slice) and adminstrativeState of the Network Slice  AllowedValues: N/A. | type: SnssaiInfo  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| isSubjectToNsac | It defines if the Network Slice subjects to network slice admission control. The value is set to False if the maxNumberofUEs attribute in corresponding SliceProfile is absent.  AllowedValues: True, False | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| NsacfInfoSnssai.maxNumberofUEs | It defines the maximum number of UEs which are allowed to be served by the Network Slice that is subject to network slice admission control. This number could be derived from maxNumberofUEs defined in corresponding SliceProfile.  AllowedValues: 0 - 65535 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: 0  isNullable: False |
| eACMode | It represents if early admission control (EAC) mode is activated.  AllowedValues: Active, Inactive | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Inactive  isNullable: False |
| activeEacThreshold | It defines threshold in percentage value of the number of the UEs registered with the network slice to the maximum number of UEs allowed to register with the network slice. The eACMode is set to active when the number of the UEs registered with the network slice is above this threshold.  AllowedValues: 0 - 100 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: 0  isNullable: False |
| deactiveEacThreshold | It defines threshold in percentage value of the number of the UEs registered with the network slice to the maximum number of UEs allowed to register with the network slice. The eACMode is set to inactive when the number of the UEs registered with the network slice is below this threshold.  AllowedValues: 0 - 100  Note: If this attribute is absent, activeEacThreshhold is used to trigger deactivation of eACMode. | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: 100  isNullable: False |
| numberofUEs | It represents the number of the UEs registered with the network slice. This attribute is updated by NSACF.  AllowedValues: 0 - 65535 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| uEIdList | It represents the UEs registered with the network slice. This attribute is updated by NSACF.  AllowedValues: N/A | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| networkSliceInfoList | The attribute specifies a list of NetworkSliceInfo which is defined as a datatype (see clause 5.3.95). It can be used by the NWDAF to facilitate the data collection from OAM.  allowedValues: N/A | type: NetworkSliceInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| networkSliceRef | This holds a DN of the NetworkSlice managed object relating to the NetworkSlice instance differentiated by sNSSAI and optional cNSIId. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sNSSAI | It represents the S-NSSAI the NetworkSlice managed object is supporting. The S-NSSAI is defined in TS 23.003 [13].  allowedValues: See TS 23.003 [13] | type: S-NSSAI  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| cNSIId | It represents NSI ID which is an identifier for identifying the Core Network part of a Network Slice instance when multiple Network Slice instances of the same Network Slice are deployed, and there is a need to differentiate between them in the 5GC. See NSI ID definition in clause 3.1 of TS 23.501 [2] and subclause 6.1.6.2.7 of TS 29.531 [24]. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| eCSAddrConfigInfo | It represents one or more FQDN(s) and/or IP address(es) of Edge Configuration Server(s), and of an ECS Provider ID. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| aMFSet.aMFRegionRef | This is the DN of AMFRegion instance of the AMFSet. This holds a DN of AMFRegion instance for which the AMFSet instance belongs to.  allowedValues: N/A | type: DN  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| aMFSetRef | This is the DN of AMFSet.  allowedValues: N/A | type: DN  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| aMFRegion.aMFSetListRef | This holds a list of DN of AMFSet instances in the same AMFRegion instance.  allowedValues: N/A | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ServerAddr | This attribute indicates the DNS server address for the PDU Session (see clause 6.2.2.2 in TS 23.548 [78])  allowedValues: Not applicable. | Type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NsacfInfoSnssai.maxNumberofPDUSessions | It defines the maximum number of concurrent PDU sessions supported by the network slic. This number could be derived from maxNumberofPDUSessions defined in corresponding SliceProfile. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues:N/A  isNullable: False |
| eASServiceArea | This parameter defines the EAS service area (see clause 7.3.3.6 in TS 23.558 [81]).  allowedValues: N/A | type: ServingLocation  multiplicity: 1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| eESServiceArea | This parameter defines the EES service area (see clause 7.3.3.5 in TS 23.558 [81]).  allowedValues: N/A | type: ServingLocation  multiplicity: 1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| eDNServiceArea | This parameter defines the EDN service area (see clause 7.3.3.4 in TS 23.558 [81]).  allowedValues: N/A | type: ServingLocation  multiplicity: 1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| 5GCNfConnEcmInfoList | The attribute specifies a list of 5GCNfConnInfo which is defined as a datatype (see clause 5.3.120). It is used to provide 5GC NFs, such as PCF, NEF, SCEF, that are connected EDN NFs, such as EAS, EES, and ECS.  allowedValues: N/A | type: 5GCNfConnEcmInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| 5GCNFType | It indicates the type of a NF instance.  AllowedValues:"PCF", "NEF", "SCEF". | type: ENUM  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| 5GCNFIpAddress | This parameter defines address of a NF instance, It can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38])) or FQDN (See TS 23.003 [13]).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| 5GCNFRef | This attribute holds the DN of a NF instance.  allowedValues: N/A | type: DN  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ednIdentifier | The identifier of the edge data network (See TS 23.558 [81]).  allowedValues: N/A | type: string  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| eASIpAddress | This parameter defines address of an EAS instance. It can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38]).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| eESIpAddress | This parameter defines address of an EES instance. It can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38])).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| eCSIpAddress | This parameter defines address of an ECS instance. It can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38])).  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| uPFConnectionInfo | The attribute is defined as a datatype UPFConnInfo (see clause 5.3.121). It is used to provide the UPF IP address and UPF DN.  allowedValues: N/A | type: UPFConnInfo  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| uPFRef | This attribute holds the DN of an UPF instance.  allowedValues: N/A | type: DN  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| UpfIpAddress | This parameter defines address of an UPF instance, It can be IP address (either IPv4 address (See RFC 791 [37]) or IPv6 address (See RFC 2373 [38])) or FQDN (See TS 23.003 [13]).  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ecmConnectionType | It indicates the type of ECM connection (i.e., user plane connection via UPF, control plane connection via PCF or NEF.  AllowedValues: "USERPLANE", "CONTROLPLANE", "BOTH". | type: ENUM  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| nwdafEvents | This attribute represents the Analytic functionalities (identified by nwdafEvent defined in TS 29.520 [85]) of the NWDAF instance. MnS consumer can configure this attribute to specify which Analytic functionalities (identified by nwdafEvent) can be performed the NWDAF instance. If the value of this attribute is not present, the NWDAF instance can perform any NWDAFEvents  allowedValues: the detailed ENUM value for NwdafEvent see the Table 5.1.6.3.4-1 in TS 29.520[85]. | type: NwdafEvent  multiplicity: \*  isOrdered: True  isUnique: True  defaultValue: None  isNullable: False |
| administrativeState | This attribute determines whether the NWDAF is enabled or disabled. MnS consumer can configure this attribute to activate or de-activate the analytic functionalities (identified by nwdafEvent defined in TS 29.520 [85]) of the NWDAF instance.  allowedValues: LOCKED, UNLOCKED. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| PCFFunction.groupId | It indicates the identity of the PCF group that is served by the PCF instance.  If not provided, the PCF instance does not pertain to any PCF group.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| dnnList | It represents the DNNs supported by the PCF. The DNN, as defined in clause 9A of TS 23.003 [13], shall contain the Network Identifier and it may additionally contain an Operator Identifier, as specified in TS 23.003 [13] clause 9.1.1 and 9.1.2. If the Operator Identifier is not included, the DNN is supported for all the PLMNs in the plmnList of the NF Profile.  If not provided, the PCF can serve any DNN.  allowedValues: N/A | type: string  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| supiRanges | It represents list of ranges of SUPIs that can be served by the PCF instance.  allowedValues: N/A | type: SupiRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| PcfInfo.gpsiRanges | It represents list of ranges of GPSIs that can be served by the PCF instance.  allowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SupiRange.start | It indicates the first value identifying the start of a SUPI range, to be used when the range of SUPI's can be represented as a numeric range (e.g., IMSI ranges). This string shall consist only of digits.  Pattern: "^[0-9]+$"  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| SupiRange.end | It indicates the last value identifying the end of a SUPI range, to be used when the range of SUPI's can be represented as a numeric range (e.g. IMSI ranges). This string shall consist only of digits.  Pattern: "^[0-9]+$"  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| SupiRange.pattern | It indicates the pattern (regular expression according to the ECMA-262 dialect [75]) representing the set of SUPI's belonging to this range. A SUPI value is considered part of the range if and only if the SUPI string fully matches the regular expression.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| IdentityRange.start | It indicates the first value identifying the start of an identity range, to be used when the range of identities can be represented as a numeric range (e.g., MSISDN ranges). This string shall consist only of digits.  Pattern: "^[0-9]+$"  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| IdentityRange.end | It indicates the last value identifying the end of an identity range, to be used when the range of identities can be represented as a numeric range (e.g. MSISDN ranges). This string shall consist only of digits.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| IdentityRange.pattern | It indicates the pattern (regular expression according to the ECMA-262 dialect [75]) representing the set of identities belonging to this range. An identity value is considered part of the range if and only if the identity string fully matches the regular expression.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| rxDiamHost | It indicates the Diameter host of the Rx interface for the PCF. See TS 29.571 [61]. String contains a Diameter Identity (FQDN).  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| rxDiamRealm | It indicates the Diameter realm of the Rx interface for the PCF. See TS 29.571 [61]. String contains a Diameter Identity (FQDN).  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| v2xSupportInd | It indicates whether V2X Policy/Parameter provisioning is supported by the PCF.  TRUE: Supported  FALSE (default): Not Supported  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseSupportInd | It indicates whether ProSe capability is supported by the PCF.  TRUE: Supported FALSE (default): Not Supported  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseCapability | It indicates the supported ProSe Capability by the PCF. | type: ProSeCapability  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| v2xCapability | It indicates the supported V2X Capability by the PCF. | type: V2xCapability  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| proseDirectDiscovery | It indicates whether the PCF supports ProSe Direct Discovery:  - true: ProSe Direct Discovery is supported by the PCF  - false (default): ProSe Direct Discovery is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseDirectCommunication | It indicates whether the PCF supports ProSe Direct Communication:  - true: ProSe Direct Communication is supported by the PCF  - false (default): ProSe Direct Communication is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseL2UetoNetworkRelay | It indicates whether the PCF supports ProSe Layer-2 UE-to-Network Relay:  - true: ProSe Layer-2 UE-to-Network Relay is supported by the PCF  - false (default): ProSe Layer-2 UE-to-Network Relay is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseL3UetoNetworkRelay | It indicates whether the PCF supports ProSe Layer-3 UE-to-Network Relay:  - true: ProSe Layer-3 UE-to-Network Relay is supported by the PCF  - false (default): ProSe Layer-3 UE-to-Network Relay is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseL2RemoteUe | It indicates whether the PCF supports ProSe Layer-2 Remote UE:  - true: ProSe Layer-2 Remote UE is supported by the PCF  - false (default): ProSe Layer-2 Remote UE is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| proseL3RemoteUe | It indicates whether the PCF supports ProSe Layer-3 Remote UE:  - true: ProSe Layer-3 Remote UE is supported by the PCF  - false (default): ProSe Layer-3 Remote UE is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| v2xCapability.lteV2x | It indicates whether the PCF supports LTE V2X capability:  - TRUE: LTE V2X capability is supported by the PCF  - FALSE (default): LTE V2X capability is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| v2xCapability.nrV2x | It indicates whether the PCF supports NR V2X capability:  - TRUE: NR V2X capability is supported by the PCF  - FALSE (default): NR V2X capability is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| UDMFunction.groupId | It indicates the identity of the UDM group that is served by the UDM instance.  If not provided, the UDM instance does not pertain to any UDM group.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| supiRanges | It represents list of ranges of SUPIs whose profile data is available in the UDM instance.  AllowedValues: N/A | type: SupiRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UdmInfo.gpsiRanges | It represents list of ranges of GPSIs whose profile data is available in the UDM instance.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UdmInfo.externalGroupIdentifiersRanges | It represents list of ranges of external groups whose profile data is available in the UDM instance.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| routingIndicators | It represents list of Routing Indicator information that allows to route network signalling with SUCI (see TS 23.003 [12]) to the UDM instance.  If not provided, the UDM can serve any Routing Indicator.  Pattern: '^[0-9]{1,4}$'  AllowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UdmInfo.internalGroupIdentifiersRanges | It represents list of ranges of Internal Group Identifiers whose profile data is available in the UDM instance.  If not provided, it does not imply that the UDM supports all internal groups.  AllowedValues: N/A | type: InternalGroupIdRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| InternalGroupIdRange.start | It indicates first value identifying the start of an identity range, to be used when the range of identities can be represented as a consecutive numeric range.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| InternalGroupIdRange.end | It indicates last value identifying the end of an identity range, to be used when the range of identities can be represented as a consecutive numeric range.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| InternalGroupIdRange.pattern | It indicates pattern (regular expression according to the ECMA-262 dialect [75]) representing the set of identities belonging to this range. An identity value is considered part of the range if and only if the identity string fully matches the regular expression.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| suciInfos | It represents list of SuciInfo. A SUCI that matches this information can be served by the UDM .  A SUCI that matches all attributes of at least one entry in this array shall be considered as a match of this information.  AllowedValues: N/A | type: SuciInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| routingInds | It indicates served Routing Indicator (see TS 23.003 [13], clause 2.2B). If not provided, the AUSF/UDM can serve any Routing Indicator.  AllowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| hNwPubKeyIds | It indicating served Home Network Public Key (see TS 23.003 [13], clause 2.2B). If not provided, the AUSF/UDM can serve any public key.  AllowedValues: N/A | type: Integer  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UDRFunction.groupId | It indicates the identity of the UDR group that is served by the UDR instance.  If not provided, the UDR instance does not pertain to any UDR group.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| supiRanges | It represents list of ranges of SUPI's whose profile data is available in the UDR instance.  AllowedValues: N/A | type: SupiRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UdmInfo.gpsiRanges | It represents list of ranges of GPSIs whose profile data is available in the UDR instance.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| externalGroupIdentifiersRanges | It represents list of ranges of external groups whose profile data is available in the UDR instance.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| sharedDataIdRanges | It represents list of ranges of Shared Data IDs that identify shared data available in the UDR instance.  AllowedValues: N/A | type: SharedDataIdRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SharedDataIdRange.pattern | It indicates the pattern (regular expression according to the ECMA-262 dialect [75]) representing the set of SharedDataIds belonging to this range. A SharedDataId value is considered part of the range if and only if the SharedDataId string fully matches the regular expression.  EXAMPLE: sharedDataId range. "123456-sharedAmData{localID}" where "123456" is the HPLMN id (i.e. MCC followed by MNC) and "{localID}" can be any string.  JSON: { "pattern": "^123456-sharedAmData.+$" }  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| udsfInfo | This attribute represents information related to UDSF, as described in clause 6.1.6.2.63 of TS 29.510 [23].  AllowedValues: N/A | type: UdsFInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| UdsfInfo.grouId | This attribute represents the identity of the UDSF group that is served by the UDSF instance.  If not provided, the UDSF instance does not pertain to any UDSF group.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| UdsfInfo.supiRanges | This attribute represents a list of ranges of SUPIs whose profile data is available in the UDSF instance  If not provided, then the UDSF can serve any SUPI range.  AllowedValues: N/A | type: SupiRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UdsfInfo.storageIdRanges | It represents a map (list of key-value pairs) where realmId serves as key and each value in the map is an array of IdentityRanges. Each IdentityRange is a range of storageIds. A UDSF complying with this version of the specification shall include this IE.  Absence indicates that the UDSF's supported realms and storages are determined by the UDSF's consumer by other means such as local provisioning.  AllowedValues: N/A | type: IdentityRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| seppInfo | This attributes represents information of a SEPP Instance, as described in clause 6.1.6.2.72 of TS 29.510 [23].  AllowedValues: N/A | type: SeppInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| seppPrefix | This attributes represents optional deployment specific string used to construct the apiRoot of the next hop SEPP, as described in clause 6.10 of TS 29.500 [76].  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| seppPorts | This attributes represents SEPP port number(s) for HTTP and/or HTTPS.  This attribute shall be present if the SEPP uses non-default HTTP and/or HTTPS ports. When present, it shall contain the HTTP and/or HTTPS ports.  The key of the map shall be "http" or "https".  The value shall indicate the port number for HTTP or HTTPS respectively.  Minimum: 0 Maximum: 65535  AllowedValues: N/A | type: Integer  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| remotePlmnList | It represents a list of remote PLMNs reachable through the SEPP.  The absence of this attribute indicates that any PLMN is reachable through the SEPP.  AllowedValues: N/A | type: PlmnId  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| remoteSnpnList | This attributes represents list of remote SNPNs reachable through the SEPP.  The absence of this attribute indicates that no SNPN is reachable through the SEPP.  AllowedValues: N/A | type: PlmnIdNid  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| scpDomainInfoList | This attributes represents SCP domain specific information of the SCP that differs from the common information in NFProfile data type. The key of the map shall be the string identifying an SCP domain.  allowedValues: N/A | type: ScpDomainInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| scpPrefix | Optional deployment specific string used to construct the apiRoot of the next hop SCP, as described in clause 6.10 of TS 29.500 [76].  allowedValues: N/A | type: String  multiplicity: 0..1  Ordered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| scpPorts | This attributes represents SCP port number(s) for HTTP and/or HTTPS.  This attribute shall be present if the SCP uses non-default HTTP and/or HTTPS ports and if the SCP does not provision port information within ScpDomainInfo for each SCP domain it belongs to.  allowedValues: 0 - 65535 | type: Integer  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| addressDomains | Pattern (regular expression according to the ECMA-262 dialect [72]) representing the address domain names reachable through the SCP.  Absence of this IE indicates the SCP can reach any address domain names in the SCP domain(s) it belongs to.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| ScpInfo.ipv4Addresses | This attributes represents list of IPv4 addresses reachable through the SCP.  This IE may be present if IPv4 addresses are reachable via the SCP.  If IPv4 addresses are reachable via the SCP, absence of both this IE and ipv4AddrRanges IE indicates the SCP can reach any IPv4 addresses in the SCP domain(s) it belongs to. | type: Ipv4Addr  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ScpInfo.ipv6Prefixes | List of IPv6 prefixes reachable through the SCP.  This IE may be present if IPv6 addresses are reachable via the SCP.  If IPv6 addresses are reachable via the SCP, absence of both this IE and ipv6PrefixRanges IE indicates the SCP can reach any IPv6 prefixes in the SCP domain(s) it belongs to. | type: Ipv6Addr  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ScpInfo.ipv4AddrRanges | List of IPv4 addresses ranges reachable through the SCP.  This IE may be present if IPv4 addresses are reachable via the SCP.  If IPv4 addresses are reachable via the SCP, absence of both this IE and ipv4Addresses IE indicates the SCP can reach any IPv4 addresses in the SCP domain(s) it belongs to. | type: Ipv4AddressRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ScpInfo.ipv6PrefixRanges | List of IPv6 prefixes ranges reachable through the SCP.  This IE may be present if IPv6 addresses are reachable via the SCP.  If IPv6 addresses are reachable via the SCP, absence of both this IE and ipv6Prefixes IE indicates the SCP can reach any IPv6 prefixes in the SCP domain(s) it belongs to. | type: Ipv6PrefixRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servedNfSetIdList | List of NF set ID of NFs served by the SCP.  Absence of this IE indicates the SCP can reach any NF set in the SCP domain(s) it belongs to.  NF Set Identifier (see clause 28.12 of TS 23.003 [13]), formatted as the following string:  "set<Set ID>.<nftype>set.5gc.mnc<MNC>.mcc<MCC>", or "set<SetID>.<NFType>set.5gc.nid<NID>.mnc<MNC>.mcc<MCC>" with  <MCC> encoded as defined in clause 5.4.2 ("Mcc" data type definition)  <MNC> encoding the Mobile Network Code part of the PLMN, comprising 3 digits. If there are only 2 significant digits in the MNC, one "0" digit shall be inserted at the left side to fill the 3 digits coding of MNC. Pattern: '^[0-9]{3}$'  <NFType> encoded as a value defined in Table 6.1.6.3.3-1 of 3GPP TS 29.510 but with lower case characters <Set ID> encoded as a string of characters consisting of alphabetic characters (A-Z and a-z), digits (0-9) and/or the hyphen (-) and that shall end with either an alphabetic character or a digit.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| remotePlmnList | List of remote PLMNs reachable through the SCP.  Absence of this IE indicates that no remote PLMN is reachable through the SCP.  allowedValues: N/A | type: PlmnId  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| remoteSnpnList | This attribute represents the List of remote PLMNs reachable through the SCP.  Absence of this IE indicates that no remote PLMN is reachable through the SCP.  allowedValues: N/A | type: PlmnIdNid  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ipReachability | This attribute indicates the type(s) of IP addresses reachable via the SCP in the SCP domain(s) it belongs to.  Absence of this IE indicates that the SCP can be used to reach both IPv4 addresses and IPv6 addresses in the SCP domain(s) it belongs to.  AllowedValues:  "IPV4": Only IPv4 addresses are reachable.  "IPV6": Only IPv6 addresses are reachable.  "IPV4V6": Both IPv4 addresses and IPv6 addresses are reachable. | type: Enumeration  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| scpCapabilities | List of SCP capabilities supported by the SCP.  This IE shall be present if the SCP supports at least one SCP capability. It may be present otherwise, with an empty array, to indicate that the SCP does not support any capability of the ScpCapability data type. The absence of this attribute shall not be interpreted as an SCP that does not support any capability; this only means that the SCP (e.g. pre-Rel-17 SCP) did not register the capabilities it may support.  AllowedValues: "INDIRECT\_COM\_WITH\_DELEG\_DISC", which indicating Indirect communication with delegated discovery supported | type: Enumeration  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| PlmnIdNid.nid | This attribute represents network Identity; Shall be present if PlmnIdNid identifies an SNPN. (see clauses 5.30.2.3, 5.30.2.9, 6.3.4, and 6.3.8 in TS 23.501 [2]).  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| nwdafInfo | It represents specific data for the NWDAF.  allowedValues: N/A | type: NwdafInfo  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| eventIds | It represents the EventId(s) supported by the Nnwdaf\_AnalyticsInfo service, if none are provided the NWDAF can serve any eventId. (see clause TS 29.520)  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| nwdafCapability | This attribute indicates the capability of the NWDAF.  If not present, the NWDAF shall be regarded with no capability.  allowedValues: N/A | type: NwdafCapability  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| analyticsDelay | It represents the supported Analytics Delay related to the eventIds and nwdafEvents.  It is an unsigned integer identifying a period of time in units of seconds.(see clause 5.2.2 TS 29.571 [61]).  allowedValues: N/A | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| servingNfTypeList | It contains the list of NF type(s) from which the NWDAF NF can collect data. The absence of this attribute indicates that the NWDAF can collect data from any NF type.  allowedValues: N/A | type: NFType  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servingNfSetIdList | It contains the list of NF type(s) from which the NWDAF NF can collect data. The absence of this attribute indicates that the NWDAF can collect data from any NF type. (see clause 5.4.2 NfSetId in TS 29.571 [61])  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mlAnalyticsList | It represents ML Analytics Filter information supported by the Nnwdaf\_MLModelProvision service.  allowedValues: N/A | type: MlAnalyticsInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| analyticsAggregation | It indicates whether the NWDAF supports analytics aggregation:  - true: analytics aggregation capability is supported by the NWDAF  - false (default): analytics aggregation capability is not supported by the NWDAF. | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| analyticsMetadataProvisioning | It indicate whether the NWDAF supports analytics metadata provisioning:  - true: analytics metadata provisioning capability is supported by the NWDAF  - false (default): analytics metadata provisioning capability is not supported by the NWDAF. | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| mlAnalyticsIds | This attribute represents the Analytic functionalities (identified by nwdafEvent defined in TS 29.520 [85]) of the NWDAF instance. MnS consumer can configure this attribute to specify which Analytic functionalities (identified by nwdafEvent) can be performed the NWDAF instance. If the value of this attribute is not present, the NWDAF instance can perform any NWDAFEvents  Analytics Id(s) supported by the Nnwdaf\_MLModelProvision service, if none are provided the NWDAF can serve any mlAnalyticsId.  allowedValues: the detailed ENUM value for NwdafEvent see the Table 5.1.6.3.4-1 in TS 29.520 [85]. | type: NwdafEvent  multiplicity: \*  isOrdered: True  isUnique: True  defaultValue: None  isNullable: False |
| trackingAreaList | This attribute represents area of Interest of the ML model, if none are provided the ML model for the analytics can apply to any TAIs.  If present, it represents the list of TAIs, it may contain one or more non-3GPP access TAIs.  allowedValues: N/A | type: Tai  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| nsacfInfo | This attribute represents the information of an NSACF NF Instance. (see TS 29.510 [23]).  AllowedValues: N/A | type: NsacfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| nsacfCapability | It represents NSACF service capability.  AllowedValues: N/A | type: NsacfCapability  multiplicity: 0..1  isOrdered: N/A  isUnique: NA  defaultValue: None  isNullable: False |
| NSACFFunction.taiList | This attribute represents the list of TAIs the NSACF can serve. It may contain one or more non-3GPP access TAIs. The absence of this attribute and the taiRangeList attribute indicate that the NSACF can be selected for any TAI in the serving network.  AllowedValues: N/A | type: Tai  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| NSACFFunction.taiRangeList | This attribute represents the range of TAIs the NSACF can serve. It may contain non-3GPP access TAIs. The absence of this attribute and the taiList attribute indicate that the NSACF can be selected for any TAI in the serving network.  AllowedValues: N/A | type: TaiRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| supportUeSAC | This attribute indicates the service capability of the NSACF to monitor and control the number of registered UEs per network slice for the network slice that is subject to NSAC.  AllowedValues:  true: Supported false (default): Not Supported | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| supportPduSAC | This attribute indicates the service capability of the NSACF to monitor and control the number of established PDU sessions per network slice for the network slice that is subject to NSAC.  AllowedValues:  true: Supported false (default): Not Supported | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: “FALSE”  isNullable: False |
| nefId | It represents the NEF ID. (see clause 6.1.6.3.2 of TS 29.510 [23])  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| appIds | It represents list of internal application identifiers of the managed PFDs.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| afIds | It represents list of application function identifiers of the managed PFDs.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| pfdData | It represents PFD data, containing the list of internal application identifiers and/or the list of application function identifiers for which the PFDs can be provided.  Absence of this attribute indicates that the PFDs for any internal application identifier and for any application function identifier can be provided.  allowedValues: N/A | type: PfdData  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| AfEventExposureData.afEvents | It represents AF Event(s) exposed by the NEF after registration of the AF(s) at the NEF.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| afEeData | It represents the AF provided event exposure data. The NEF registers such information in the NRF on behalf of the AF.  allowedValues: N/A | type: AfEventExposureData  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servedFqdnList | It represents pattern (regular expression according to the ECMA-262 dialect [75]) representing the Domain names served by the NEF.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| dnaiList | It represents list of Data network access identifiers supported by the NEF. The absence of this attribute indicates that the NEF can be selected for any DNAI.  allowedValues: N/A | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| unTrustAfInfoList | It represents list of information corresponding to the AFs.  allowedValues: N/A | type: UnTrustAfInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UnTrustAfInfo.afId | It represents associated AF id.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| UnTrustAfInfo. sNssaiInfoList | It represents S-NSSAIs and DNNs supported by the untrust AF.  allowedValues: N/A | type: SnssaiInfoItem  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| UnTrustAfInfo. mappingInd | When present, this attribute indicates whether the AF supports mapping between UE IP address (IPv4 address or IPv6 prefix) and UE ID (i.e. GPSI).  allowedValues: True, False  True: the AF supports mapping between UE IP address and UE ID;  False (default): the AF does not support mapping between UE IP address and UE ID. | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| SnssaiInfoItem.sNssai | It represents supported S-NSSAI.  allowedValues: N/A | type: ExtSnssai  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SnssaiInfoItem.dnnInfoList | It represents list of parameters supported by the NF per DNN.  allowedValues: N/A | type: DnnInfoItem  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| snssaiExtension | It represents extensions to the Snssai.  allowedValues: N/A | type: SnssaiExtension  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SnssaiExtension.sdRanges | It shall contain the range(s) of Slice Differentiator values supported for the Slice/Service Type value indicated in the sst attribute of the Snssai data type (see clause 5.4.4.2 in TS 29.571[61). | type: SdRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SnssaiExtension.wildcardSd | It indicates that all SD values are supported for the Slice/Service Type value indicated in the sst attribute of the Snssai data type (see clause 5.4.4.2 in TS 29.571[61]).  allowedValues: True, False | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| SdRange.start | First value identifying the start of an SD range.  This string shall be formatted as specified for the sd attribute of the Snssai data type in clause 5.4.4.2 of TS 29.571 [61].  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SdRange.end | Last value identifying the end of an SD range.  This string shall be formatted as specified for the sd attribute of the Snssai data type in clause 5.4.4.2 in TS 29.571 [61].  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| DnnInfoItem.dnn | It represents supported DNN or Wildcard DNN if the NF supports all DNNs for the related S-NSSAI. The DNN shall contain the Network Identifier and it may additionally contain an Operator Identifier. If the Operator Identifier is not included, the DNN is supported for all the PLMNs in the plmnList of the NF Profile.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| uasNfFunctionalityInd | When present, this attribute shall indicate whether the NEF supports UAS NF functionality:  allowedValues: True, False  - True: UAS NF functionality is supported by the NEF.  - False (default): UAS NF functionality is not supported by the NEF. | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| ausfInfo | It represents the information of an AUSF NF Instance (see TS 29.510 [23]).  AllowedValues: N/A | type: AusfInfo  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| AUSFFunction.supiRanges | This attribute represents a list of ranges of SUPIs that can be served by the AUSF instance. (NOTE 1)  AllowedValues: N/A | type: SupiRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| AUSFFunction.routingIndicators | This attribute represents a list of Routing Indicator information that allows to route network signalling with SUCI (see TS 23.003 [13]) to the AUSF instance.  If not provided, the AUSF can serve any Routing Indicator.  Pattern: '^[0-9]{1,4}$'  AllowedValues: N/A | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| AUSFFunction.suciInfos | This attribute represents a list of SuciInfo. A SUCI that matches this information can be served by the AUSF. (NOTE 2, NOTE 3)  A SUCI that matches all attributes of at least one entry in this array shall be considered as a match of this information.  AllowedValues: N/A | type: SuciInfo  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| smsfInfo | This attribute represents specific data for a SMSF.  AllowedValues: N/A | type: SmsfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| roamingUeInd | This attribute indicates whether the SMSF can serve roaming UE:  - TRUE: the SMSF can support roaming UEs.  - FALSE: the SMSF can not support roaming UEs.  Absence of this IE indicates whether the SMSF can serve roaming UEs is not specified.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| remotePlmnRangeList | This attribute indicates the list of ranges of remote PLMNs served by the SMSF, i.e. the SMSF can serve the roaming UEs which belong to the indicated remote PLMNs.  If the roamingUeInd attribute is present with the value "true", absence of remotePlmnRangeList indicates that the SMSF can serve roaming UEs from any remote PLMN.  AllowedValues: N/A | type: PlmnRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| PlmnRange.start | This attribute indicates the first value identifying the start of a PLMN range.  The string shall be encoded as follows:  <MCC><MNC>  Pattern: '^[0-9]{3}[0-9]{2,3}$'  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| PlmnRange.end | This attribute indicates the last value identifying the end of a PLMN range.  The string shall be encoded as follows:  <MCC><MNC>  Pattern: '^[0-9]{3}[0-9]{2,3}$'  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| PlmnRange.pattern | This attribute indicates pattern (regular expression according to the ECMA-262 dialect [8]) representing the set of PLMNs belonging to this range. A PLMN value is considered part of the range if and only if the PLMN string (formatted as <MCC><MNC>) fully matches the regular expression.  To be noted, either the start and end attributes, or the pattern attribute, shall be present.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| udrInfo | This attribute represents the information of an UDR NF Instance (see TS 29.510 [23]).  AllowedValues: N/A | type: UdrInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| udmInfo | This attribute represents the information of an UDM NF Instance (see TS 29.510 [23]).  AllowedValues: N/A | type: UdmInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| lmfInfo | This attribute represents information of an LMF NF Instance  AllowedValues: N/A | type: LmfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| servingClientTypes | This attribute represents a list of external client type(s), e.g. emergency client. The NRF should only include this LMF instance to NF discovery with "client-type" query parameter indicating one of the external client types in the list.  Absence of this attribute means the LMF is not dedicated to serve specific client types.  AllowedValues: see clause 6.1.6.3.3 of TS 29.572 [86]  "EMERGENCY\_SERVICES": External client for emergency services  "VALUE\_ADDED\_SERVICES": External client for value added services  "PLMN\_OPERATOR\_SERVICES": External client for PLMN operator services  "LAWFUL\_INTERCEPT\_SERVICES": External client for Lawful Intercept services  "PLMN\_OPERATOR\_BROADCAST\_SERVICES": External client for PLMN Operator Broadcast services  "PLMN\_OPERATOR\_OM": External client for PLMN Operator O&M  "PLMN\_OPERATOR\_ANONYMOUS\_STATISTICS": External client for PLMN Operator anonymous statistics  "PLMN\_OPERATOR\_TARGET\_MS\_SERVICE\_SUPPORT": External client for PLMN Operator target MS service support | type: ENUM  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| lmfId | This attribute represents the LMF identification. See clause 6.1.6.3.6 TS 29.572 [8]  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| servingAccessTypes | This attribute contains the access type (3GPP\_ACCESS and/or NON\_3GPP\_ACCESS) supported by the SMF.  If not included, it shall be assumed the both access types are supported.  AllowedValues: "3GPP\_ACCESS", "NON\_3GPP\_ACCESS". | type: ENUM  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servingAnNodeTypes | This attribute contains the AN node type (i.e. gNB or NG-eNB) supported by the LMF.  If not included, it shall be assumed that all AN node types are supported.  AllowedValues: "GNB","NG\_ENB" | type: ENUM  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servingRatTypes | This attribute contains the RAT type (e.g. 5G NR, eLTE or any of the RAT Types specified for NR satellite access) supported by the LMF.  If not included, it shall be assumed that all RAT types are supported  AllowedValues: see clause 5.4.3.2 of TS 29.571 [61]. | type: String  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| LmfInfo.taiList | This attribute contains TAI list that the LMF can serve. It may contain one or more non-3GPP access TAIs.  The absence of both this attribute and the taiRangeList attribute indicates that the LMF can be selected for any TAI in the serving network.  AllowedValues: N/A | type: TAI  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| LmfInfo.taiRangeList | This attribute contains TAI range list that the LMF can serve. It may contain one or more non-3GPP access TAI ranges. The absence of both this attribute and the taiList attribute indicates that the LMF can be selected for any TAI in the serving network.  AllowedValues: N/A | type: TAIRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| supportedGADShapes | This attribute contains the GAD shapes supported by the LMF.  If not included, it doesn't indicate that the LMF doesn't support any GAD shapes.  The allowedValues are: see clause 6.1.6.3.4 of TS 29.572 [86]  "POINT" indicates Ellipsoid Point  "POINT\_UNCERTAINTY\_CIRCLE" indicates Ellipsoid point with uncertainty circle  "POINT\_UNCERTAINTY\_ELLIPSE" indicates Ellipsoid point with uncertainty ellipse  "POLYGON" indicates Polygon  "POINT\_ALTITUDE" indicates Ellipsoid point with altitude  "POINT\_ALTITUDE\_UNCERTAINTY" indicates Ellipsoid point with altitude and uncertainty ellipsoid  "ELLIPSOID\_ARC" indicates Ellipsoid Arc  "LOCAL\_2D\_POINT\_UNCERTAINTY\_ELLIPSE" indicates Local 2D point with uncertainty ellipse  "LOCAL\_3D\_POINT\_UNCERTAINTY\_ELLIPSOID" indicates Local 3D point with uncertainty ellipsoid | type: ENUM  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SnssaiInfoItem | This attribute represents a list of S-NSSAIs and DNNs supported by the trusted AF.  AllowedValues: N/A | type: SnssaiInfoItem  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TrustAfInfo.afEvents | This attribute represents list of AF Event(s) supported by the trusted AF.  AllowedValues: "SVC\_EXPERIENCE","UE\_MOBILITY", "UE\_COMM", "EXCEPTIONS", "USER\_DATA\_CONGESTION", "PERF\_DATA", "COLLECTIVE\_BEHAVIOUR", "DISPERSION", "MS\_QOE\_METRICS", "MS\_CONSUMPTION", "MS\_NET\_ASSIST\_INVOCATION", "MS\_DYN\_POLICY\_INVOCATION", "MS\_ACCESS\_ACTIVITY"  See clause 5.6.3.3 TS 29.517 [87]. | type: Enumeration  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TrustAfInfo.appIds | This attribute represents a list of Application ID(s) supported by the trusted AF. The absence of this attribute indicate that the AF can be selected for any Application.  AllowedValues: N/A | type: String  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| internalGroupId | This attribute represents a list of Internal Group Identifiers supported by the trusted AF.  If not provided, it does not imply that the AF supports all internal groups.  String pattern: '^[A-Fa-f0-9]{8}-[0-9]{3}-[0-9]{2,3}-([A-Fa-f0-9][A-Fa-f0-9]){1,10}$'.  AllowedValues: N/A | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mappingInd | This attribute indicates whether the trusted AF supports mapping between UE IP address (IPv4 address or IPv6 prefix) and UE ID (i.e. SUPI).  TRUE: the trusted AF supports mapping between UE IP address and UE ID;  FALSE (default): the trusted AF does not support mapping between UE IP address and UE ID.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| sNssaiEasdfInfoList | This attribute represents a list of parameters supported by the EASDF per S-NSSAI.  AllowedValues: N/A | type: SnssaiEasdfInfoItem  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| easdfN6IpAddressList | This attribute represents N6 IP addresses of the EASDF.  AllowedValues: N/A | type: IpAddr  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| upfN6IpAddressList | This attribute represents N6 IP addresses of PSA UPFs.  AllowedValues: N/A | type: IpAddr  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SnssaiEasdfInfoItem.sNssai | This attribute represents a S-NSSAI.  AllowedValues: N/A | type: SnssaiExtension  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SnssaiEasdfInfoItem.dnnEasdfInfoList | This attribute represents a list of parameters supported by the EASDF per DNN.  AllowedValues: N/A | type: DnnEasdfInfoItem  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnEasdfInfoItem.dnn | This attribute represents a supported DNN or Wildcard DNN if the EASDF supports all DNNs for the related S-NSSAI.  The DNN shall contain the Network Identifier and it may additionally contain an Operator Identifier. If the Operator Identifier is not included, the DNN is supported for all the PLMNs in the plmnList of the NF Profile.  AllowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NssafInfo.supiRanges | This attribute represents a List of ranges of SUPIs that can be served by the NSSAAF instance.  AllowedValues: N/A | type: SupiRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| NssafInfo.internalGroupIdentifiersRanges | This attribute represents a List of ranges of Internal Group Identifiers that can be served by the NSSAAF instance. If not provided, it does not imply that the NSSAAF supports all internal groups.  AllowedValues: N/A | type: InternalGroupIdRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUdrInfo | This attribute contains all the udrInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the udrInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUdmInfo | This attribute contains all the udmInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the udmInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedAusfInfo | This attribute contains all the ausfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the ausfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedNwdafInfo | This attribute contains all the nwdafInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the nwdafInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedLmfInfo | This attribute contains all the lmfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the lmfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUdsfInfo | This attribute contains all the udsfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedTrustAfInfo | This attribute contains the trustAfInfo attribute locally configured in the NRF or that the NRF received during AF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedNssaafInfo | This attribute contains all the nssaafInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the nssaafInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 1..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| chfInfo | It represents the information of an AUSF NF Instance (see TS 29.510 [23]).  AllowedValues: N/A | type: ChfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ChfInfo.supiRangeList | This attribute represents the list of ranges of SUPIs that can be served by the CHF instance.  allowedValues: N/A | type: SupiRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ChfInfo.gpsiRangeList | This attribute represents the list of ranges of GPSI that can be served by the CHF instance.  allowedValues: N/A | type: IdentityRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ChfInfo.plmnRangeList | This attribute represents the list of ranges of PLMNs (including the PLMN IDs of the CHF instance) that can be served by the CHF instance. If not provided, the CHF can serve any PLMN.  allowedValues: N/A | type: PlmnRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| ChfInfo.groupId | This attribute represents the identity of the CHF group that is served by the CHF instance.  If not provided, the CHF instance does not pertain to any CHF group.  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ChfInfo.primaryChfInstance | This attribute represents the NF Instance Id of the primary CHF instance.  This attribute shall be absent if the secondaryChfInstance is present.  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ChfInfo.secondaryChfInstance | This attribute represents the NF Instance Id of the secondary CHF instance.  This attribute shall be absent if the primaryChfInstance is present.  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mfafInfo | This attribute represents information of an MFAF NF Instance.  AllowedValues: N/A | type: MfafInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| MfafInfo.servingNfTypeList | This attribute represents a List of NF type(s) served by MFAF NF. The absence of this attribute indicates that the MFAF can be selected for any NF type  AllowedValues: N/A | type: NFType  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MfafInfo.servingNfSetIdList | This attribute represents a List of NF Set Id(s) served by MFAF NF. The absence of this attribute indicates that the MFAF can be selected for any NF Set Id.  AllowedValues: N/A | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MfafInfo.taiList | This attribute represents a List of TAIs the MFAF can serve. It may contain one or more non-3GPP access TAIs. The absence of both this attribute and the taiRangeList attribute indicates that the MFAF can be selected for any TAI in the serving network.  AllowedValues: N/A | type: Tai  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MfafInfo.taiRangeList | This attribute represents the range of TAIs the MFAF can serve. It may contain one or more non-3GPP access TAI ranges. The absence of both this attribute and the taiList attribute indicates that the MFAF can be selected for any TAI in the serving network.  AllowedValues: N/A | type: TaiRange  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| dccfInfo | This attribute represents information of an DCCF NF Instance  AllowedValues: N/A | type: DccfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| DccfInfo.servingNfTypeList | This attribute represents the list of NF type(s) from which the DCCF NF can collect data. The absence of this attribute indicates that the DCCF can collect data from any NF type.  allowedValues: N/A | type: NFType  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DccfInfo.servingNfSetIdList | This attribute represents the list of NF Set Id(s) from which the DCCF NF can collect data. The absence of this attribute indicates that the DCCF can collect data from any NF Set.  allowedValues: N/A | type: String  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DccfInfo.taiList | This attribute represents the list of TAIs the DCCF can serve. It may contain one or more non-3GPP access TAIs. The absence of both this attribute and the taiRangeList attribute indicates that the DCCF can be selected for any TAI in the serving network.  allowedValues: N/A | type: TAI  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DccfInfo.taiRangeList | This attribute represents the range of TAIs the DCCF can serve. It may contain one or more non-3GPP access TAI ranges. The absence of both this attribute and the taiList attribute indicates that the DCCF can be selected for any TAI in the serving network.  allowedValues: N/A | type: TAIRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| amfInfo | This attribute represents information of an AMF NF Instance.  AllowedValues: N/A | type: AmfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| smfInfo | This attribute represents information of an SMF NF Instance.  AllowedValues: N/A | type: SmfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| upfInfo | This attribute represents information of an UPF NF Instance.  AllowedValues: N/A | type: UpfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| pcfInfo | This attribute represents information of a PCF NF Instance.  AllowedValues: N/A | type: PcfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nefInfo | This attribute represents information of an NEF NF Instance.  AllowedValues: N/A | type: NefInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| servedUdrInfoList | This attribute contains list of UdrInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUdmInfoList | This attribute contains list of UdmInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedAusfInfoList | This attribute contains list of AusfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedAmfInfo | This attribute contains all the amfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the amfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedAmfInfoList | This attribute contains list of AmfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedSmfInfo | This attribute contains all the smfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the smfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedSmfInfoList | This attribute contains list of SmfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUpfInfo | This attribute contains all the upfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the upfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUpfInfoList | This attribute contains list of UpfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedPcfInfo | This attribute contains all the pcfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the pcfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedPcfInfoList | This attribute contains list of PcfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedBsfInfo | This attribute contains all the bsfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the bsfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedBsfInfoList | This attribute contains list of BsfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedChfInfo | This attribute contains all the chfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the chfInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedChfInfoList | This attribute contains list of ChfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedNefInfo | This attribute contains all the nefInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the nefInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedNwdafInfoList | This attribute contains all the nwdafInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedGmlcInfo | This attribute contains all the gmlcInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of which the nefInfo belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedUdsfInfoList | This attribute contains list of UdsfInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedScpInfoList | This attribute contains list of ScpInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedSeppInfoList | This attribute contains list of SeppInfo attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| AanfInfo.routingIndicators | This attribute represents the List of Routing Indicators supported by the AAnf instance. If not provided, the AAnf can serve any Routing Indicator.  Pattern: '^[0-9]{1,4}$'  allowedValues: N/A | type: String  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| aanfInfo | This attribute represents information of an AANF NF Instance  AllowedValues: N/A | type: AanfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| TsctsfInfo | This attribute represents information of an TSCTSF NF Instance  allowedValues: N/A | type: TsctsfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| TsctsfInfo.sNssaiInfoList | This attribute represents the S-NSSAIs and DNNs supported by the TSCTSF. The key of the map shall be a (unique) valid JSON string per clause 7 of IETF RFC 8259 [92], with a maximum of 32 characters.  allowedValues: N/A | type: SnssaiTsctsfInfoItem  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TsctsfInfo.externalGroupIdentifiersRanges | This attribute represents the ranges of External Group Identifiers that can be served by the TSCTSF.  The absence of this IE indicates that the TSCTSF can serve any external group managed by the PLMN (or SNPN) of the TSCTSF instance.  allowedValues: N/A | type: IdentityRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TsctsfInfo.supiRanges | This attribute represents the ranges of SUPIs that can be served by the TSCTSF instance.  allowedValues: N/A | type: SupiRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TsctsfInfo.gpsiRanges | This attribute represents the ranges of GPSIs that can be served by the TSCTSF instance.  allowedValues: N/A | type: IdentityRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TsctsfInfo.internalGroupIdentifiersRanges | This attribute represents the ranges of Internal Group Identifiers that can be served by the TSCTSF instance.  The absence of this IE indicates that the TSCTSF can serve any internal group managed by the PLMN (or SNPN) of the TSCTSF instance.  allowedValues: N/A | type: InternalGroupIdRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servingClientTypes | This attribute shall be present if the GMLC is dedicated to serve the listed external client type(s), e.g. emergency client.  Absence of this attribute means the GMLC is not dedicated to serve specific client types.  See clause 6.1.6.3.3 TS 29.572 [86].  allowedValues:  "EMERGENCY\_SERVICES": External client for emergency services  "VALUE\_ADDED\_SERVICES": External client for value added services  "PLMN\_OPERATOR\_SERVICES": External client for PLMN operator services  "LAWFUL\_INTERCEPT\_SERVICES": External client for Lawful Intercept services  "PLMN\_OPERATOR\_BROADCAST\_SERVICES": External client for PLMN Operator Broadcast services  "PLMN\_OPERATOR\_OM": External client for PLMN Operator O&M  "PLMN\_OPERATOR\_ANONYMOUS\_STATISTICS": External client for PLMN Operator anonymous statistics  "PLMN\_OPERATOR\_TARGET\_MS\_SERVICE\_SUPPORT": External client for PLMN Operator target MS service support | type: <<enumeration>>  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| gmlcNumbers | This attribute represents each item of the array shall carry an OctetString indicating the ISDN number of the GMLC in international number format as described in ITU-T Rec. E.164 [94] and shall be encoded as a TBCD-string.  Pattern for string: "^[0-9]{5,15}$"  allowedValues: N/A | type: String  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| gmlcInfo | This attribute represents information of an GMLC NF Instance.  AllowedValues: N/A | type: GmlcfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nTNPLMNInfoList | This attribute defines the location restrictions per PLMN that relates to non-terrestrial network access. | type: NTNPLMNRestrictionsInfo  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| blockedLocationInfoList | This defines the information related with the location for which the access restrictions are to be applied in case of NTN. | type: BlockedLocationInfo  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| blockedLocation | This provides the geographical location at which the PLMN are not allowed in case of NTN. | type: string  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| blockedDurWindow | This provides the time durations for which the PLMN are not allowed at a given location in case of NTN | type: TimeWindow  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| blockedDurStartTime | This provides the start time starting which the PLMN is not allowed at a given location in case of NTN | type: DateTimeultiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| blockedDurEndTime | This provides the end time after which the PLMN is not allowed at a given location in case of NTN | type: DateTime  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| blockedSlice | This provides the slice for which the access is not allowed at a given location in case of NTN. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nwdafLogicalFuncSupported | It represents the logical functions supported by the NWDAF.  If not present, the NWDAF shall be regarded with no logical decomposition, in that case the NWDAF only supports the analytics services.  allowedValues:  “NWDAF\_WITH\_ANLF” indicates the NWDAF containing Analytics logical function (AnLF),  “NWDAF\_WITH\_MTLF” indicates the NWDAF containing Model Training logical function (MTLF),  “NWDAF\_WITH\_ANLF\_MTLF” indicates the NWDAF containing both Analytics logical function (AnLF) and Model Training logical function (MTLF). | type: ENUM  multiplicity: 0..1  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| satelliteCoverageInfoList | This attribute defines the information related to NR Satellite RAT type and corresponding information of satellite coverage | type: SatelliteCoverageInfo  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nRSatelliteRATtype | This attribute defines the RAT Type for NR satellite access.  Allowed Values:  “NRLEO”  “NRMEO”  “NRGEO”  “NROTHERSAT” | type: ENUM  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| locationInfo | This attribute defines the information about location and corresponding time windows for which the satellite coverage will be available or unavailable. | type: NtnLocationInfo  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| location | This defines the Location (geographical area) under consideration to which the satellite coverage info belongs | type: GeoArea  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| availabilityWindows | This attribute defines the list of time windows at which the satellite coverage will be available for this location. Either availabilityWindows or nonAvailabilityWindows shall be present. | type: TimeWindow  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| nonAvailabilityWindows | This attribute defines the list of time windows at which the satellite coverage will not be available for this location. Either availabilityWindows or nonAvailabilityWindows shall be present. | type: TimeWindow  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| N2InterfaceAmfInfo.ipv4EndpointAddresses | This attribute represents available AMF endpoint IPv4 address(es) for N2.  AllowedValues: N/A | type: Ipv4Addr  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| N2InterfaceAmfInfo.ipv6EndpointAddresses | This attribute represents available AMF endpoint IPv6 address(es) for N2.  AllowedValues: N/A | type: Ipv6Addr  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| N2InterfaceAmfInfo.amfName | This attribute represents AMF Name FQDN as defined in clause 28.3.2.5 of TS 23.003 [13]  AllowedValues: N/A | type: Fqdn  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| amfOnboardingCapability | This attribute indicates the AMF supports SNPN Onboarding capability. This is used for the case of Onboarding of UEs for SNPNs (see TS 23.501 [2], clause 5.30.2.10).  - FALSE (default): AMF does not support SNPN Onboarding;  - TRUE: AMF supports SNPN Onboarding.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| highLatencyCom | This attribute indicates whether the AMF supports High Latency communication (e.g. for NR RedCap UE). This is used for CP NF to discover AMF supporting High Latency communication (see TS 23.501 [2], clause 6.3.5).  - FALSE: AMF does not support High Latency communication e.g. for NR RedCap UE;  - TRUE: AMF supports High Latency communication e.g. for NR RedCap UE;  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ismfSupportInd | This attribute may be used by an SMF to explicitly indicate the support of I-SMF capability and its preference to be selected as I-SMF.  When present, this attribute shall indicate whether the I-SMF capability are supported by the SMF:  - TRUE: I-SMF capability supported by the SMF  - FALSE: I-SMF capability not supported by the SMF.  Absence of this attribute indicates the I-SMF capability support of the SMF is not specified.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| smfOnboardingCapability | This attribute indicates the SMF supports SNPN Onboarding capability and User Plane Remote Provisioning. This is used for the case of Onboarding of UEs for SNPNs (see TS 23.501 [2], clauses 5.30.2.10 and 6.2.6.2).  - FALSE (default): SMF does not support SNPN Onboarding;  - TRUE: SMF supports SNPN Onboarding.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| smfUPRPCapability | This attribute IE indicates the SMF supports User Plane Remote Provisioning (UPRP) capability. This is used for the case of Onboarding of UEs for SNPNs (see TS 23.501 [2], clauses 5.30.2.10 and 6.2.6.2).  - FALSE (default): SMF does not support UPRP;  - TRUE: SMF supports UPRP.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| sNssaiUpfInfoList | This attribute represents a list of parameters supported by the UPF per S-NSSAI.  AllowedValues: N/A | type: SnssaiUpfInfoItem  multiplicity: 1..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| sxaInd | This attribute indicates whether the UPF is configured to support Sxa interface.  TRUE: Supported  FALSE: Not Supported  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| a2xSupportInd | This attribute indicates whether A2X Policy/Parameter provisioning is supported by the PCF.  TRUE: Supported FALSE (default): Not Supported  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| a2xCapability | This attribute shall be present if the PCF supports A2X Capability.  When present, this attribute shall indicate the supported A2X Capability by the PCF.  AllowedValues: N/A | type: A2xCapability  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| rangingSlPosSupportInd | Indicates whether ranging and sidelink positioning capability is supported by the PCF.  TRUE: Supported FALSE (default): Not Supported  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| A2xCapability.lteA2x | This attribute indicates whether the PCF supports LTE A2X capability:  - TRUE: LTE A2X capability is supported by the PCF  - FALSE (default): LTE A2X capability is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| A2xCapability.nrA2x | This attribute indicates whether the PCF supports NR A2X capability:  - TRUE: NR A2X capability is supported by the PCF  - FALSE (default): NR A2X capability is not supported by the PCF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| multiMemAfSessQosInd | This attribute indicates whether the NEF supports Multi-member AF session with required QoS functionality:  - TRUE: Multi-member AF session with required QoS functionality is supported by the NEF  - FALSE (default): Multi-member AF session with required QoS functionality is not supported by the NEF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| memberUESelAssistInd | This attribute indicates whether the NEF supports member UE selection assistance functionality:  - TRUE: member UE selection assistance functionality is supported by the NEF  - FALSE (default): member UE selection assistance functionality is not supported by the NEF.  AllowedValues: TRUE, FALSE | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| mbUpfInfo | This attribute represents information of an MB-UPF NF Instance.  AllowedValues: N/A | type: MbUpfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mbUpfInfo.sNssaiMbUpfInfoList | This attribute represents the list of parameters supported by the MB-UPF per S-NSSAI.  allowedValues: N/A | type: SnssaiUpfInfoItem  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbUpfInfo.mbSmfServingArea | This attribute represents the MB-SMF service area(s) the MB-UPF can serve.  If not provided, the MB-UPF can serve any MB-SMF service area.  allowedValues: N/A | type: String  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbUpfInfo.interfaceMbUpfInfoList | This attribute represents the list of User Plane interfaces configured on the MB-UPF. When this IE is provided in the NF Discovery response, the NF Service Consumer (e.g. MB-SMF) may use this information for MB-UPF selection.  allowedValues: N/A | type: InterfaceUpfInfoItem  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbUpfInfo.taiList | This attribute represents the list of TAIs the MB-UPF can serve.  The absence of this attribute and the taiRangeList attribute indicates that the MB-UPF can serve the whole MB-SMF service area defined by the MbSmfServingArea attribute.  allowedValues: N/A | type: Tai  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbUpfInfo.taiRangeList | This attribute represents the range of TAIs the MB-UPF can serve.  The absence of this attribute and the taiList attribute indicates that the MB-UPF can serve the whole MB-SMF service area defined by the MbSmfServingArea attribute.  allowedValues: N/A | type: Tairange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbUpfInfo.priority | This attribute represents priority (relative to other NFs of the same type) in the range of 0-65535, to be used for NF selection for a service request matching the attributes of the MbUpfInfo; lower values indicate a higher priority.  See the precedence rules in the description of the priority attribute in NFProfile, if Priority is also present in NFProfile.  The NRF may overwrite the received priority value when exposing an NFProfile with the Nnrf\_NFDiscovery service.  allowedValues: N/A | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SnssaiUpfInfoItem.sNssai | It represents supported S-NSSAI.  allowedValues: N/A | type: ExtSnssai  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SnssaiUpfInfoItem.dnnUpfInfoList | This attribute represents a list of parameters supported by the UPF per DNN.  allowedValues: N/A | type: DnnUpfInfoItem  multiplicity: 1..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SnssaiUpfInfoItem.redundantTransport | This attribute indicates whether the UPF supports redundant transport path on the transport layer in the corresponding network slice.  allowedValues:  TRUE: supported FALSE (default): not supported | type: Boolean  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: FALSE  isNullable: False |
| DnnUpfInfoItem.dnaiList | This attribute represents a list of Data network access identifiers supported by the UPF for this DNN. The absence of this attribute indicates that the UPF can be selected for this DNN for any DNAI.  Each item in the list is the DNAI (Data network access identifier), see TS 23.501 [2].  allowedValues: N/A | type: String  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.pduSessionTypes | This attribute represents a list of PDU session type(s) supported by the UPF for a specific DNN. The absence of this attribute indicates that the UPF can be selected for this DNN for any PDU session type supported by the UPF (see clause 6.1.6.2.13).  allowedValues:  “IPv4” “IPv6” “IPv4v6” as per clause 5.8.2.2.1 TS 23.501 [2] “UNSTRUCTURED” “ETHERNET” | type: <<enumeration>>  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.ipv4AddressRanges | This attribute represents a list of ranges of IPv4 addresses handled by UPF.  allowedValues: N/A | type: Ipv4AddressRange  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.ipv6PrefixRanges | This attribute represents a list of ranges of IPv6 prefixes handled by the UPF.  allowedValues: N/A | type: Ipv6PrefixRange  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.natedIpv4AddressRanges | This attribute represents a list of ranges of NATed IPv4 addresses.  allowedValues: N/A | type: Ipv4AddressRange  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.natedIpv6PrefixRanges | This attribute represents a list of ranges of NATed IPv6 prefixes.  allowedValues: N/A | type: Ipv6PrefixRange  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.ipv4IndexList | This attribute represents a list of Ipv4 Index supported by the UPF.  This <<choice>> represents the IP Index to be sent from UDM to the SMF. (See clause 6.1.6.2.77 TS 29.503 [97])  It is a list of non-exclusive alternatives (Integer or String).  allowedValues: N/A | type: <<choice>>  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.ipv6IndexList | This attribute represents a list of Ipv6 Index supported by the UPF.  This <<choice>> represents the IP Index to be sent from UDM to the SMF. (See clause 6.1.6.2.77 TS 29.503 [97])  It is a list of non-exclusive alternatives (Integer or String).  allowedValues: N/A | type: <<choice>>  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.networkInstance | This attribute represents the N6 Network Instance (See TS 29.244 [56]) associated with the S-NSSAI and DNN.  allowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| DnnUpfInfoItem.dnaiNwInstanceList | This attribute represents a map of a network instance per DNAI for the DNN, where the key of the map is the DNAI (Data network access identifier), see TS 23.501 [2].  When present, the value of each entry of the map shall contain a N6 network instance that is configured for the DNAI indicated by the key.  allowedValues: N/A | type: String  multiplicity: 0..N  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbSmfInfo | This attribute represents information of an MB-SMF NF Instance  AllowedValues: N/A | type: MbSmfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| MbSmfInfo.sNssaiInfoList | This attribute represents the list of S-NSSAIs and DNNs supported by the MB-SMF.  The key of the map shall be a (unique) valid JSON string per clause 7 of IETF RFC 8259 [92], with a maximum of 32 characters.  allowedValues: N/A | type: NFType  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MbSmfInfo.tmgiRangeList | This attribute represents the list of TMGI range(s) supported by the MB-SMF  The key of the map shall be a (unique) valid JSON string per clause 7 of IETF RFC 8259 [92], with a maximum of 32 characters.  allowedValues: N/A | type: TmgiRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MbSmfInfo.taiList | This attribute represents the list of TAIs the MB-SMF can serve.  The absence of this attribute and the taiRangeList attribute indicates that the MB-SMF can be selected for any TAI in the serving network.  allowedValues: N/A | type: TAI  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MbSmfInfo.taiRangeList | This attribute represents the range of TAIs the MB-SMF can serve.  The absence of this attribute and the taiList attribute indicates that the MB-SMF can be selected for any TAI in the serving network.  allowedValues: N/A | type: TAIRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MbSmfInfo.mbsSessionList | This attribute represents the list of MBS sessions currently served by the MB-SMF  The key of the map shall be a (unique) valid JSON string per clause 7 of IETF RFC 8259 [92], with a maximum of 32 characters.  allowedValues: N/A | type: MbsSession  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mbsServiceIdStart | This attribute represents the first MBS Service ID value identifying the start of a TMGI range.  The value shall be coded as defined for the mbsServiceId attribute of the Tmgi data type defined in 3GPP TS 29.571 [61].  Pattern: '^[A-Fa-f0-9]{6}$'s.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mbsServiceIdEnd | This attribute represents the last MBS Service ID value identifying the end of a TMGI range.  The value shall be coded as defined for the mbsServiceId attribute of the Tmgi data type defined in 3GPP TS 29.571 [61].  Pattern: '^[A-Fa-f0-9]{6}$  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mbsServiceId | This attribute represents MBS Service ID consisting of a 6-digit fixed-length hexadecimal number between 000000 and FFFFFF.  Each character in the string shall take a value of "0" to "9", "a" to "f" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the MBS Service ID shall appear first in the string, and the character representing the 4 least significant bit of the MBS Service ID shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{6}$'  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| Ssm.sourceIpAddr | This attribute represents IP unicast address used as source address in IP packets for identifying the source of the multicast service (e.g. AF/AS).  allowedValues: N/A | type: IpAddr  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| Ssm.destIpAddr | This attribute represents IP multicast address used as destination address in related IP packets for identifying the multicast service associated with the source.  allowedValues: N/A | type: IpAddr  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| MbsSession.mbsSessionId | This attribute represents the MBS Session Identifier.  allowedValues: N/A | type: MbsSessionId  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| MbsSession.mbsAreaSessions | This attribute represents map of Area Session Id and related MBS Service Area information used for MBS session with location dependent content. The Area Session ID together with the mbsSessionId (TMGI) uniquely identifies the MBS session in a specific MBS service area.  For an MBS session with location dependent content, one map entry shall be registered for each MBS Service Area served by the MBS session.  The key of the map shall be the areaSessionId. | type: MbsServiceAreaInfo  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MbsServiceAreaInfo.areaSessionId | This attribute represents Area Session Identifier used for MBS session with location dependent content.  allowedValues: 0..65535 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| MbsServiceAreaInfo.mbsServiceArea | This attribute represents MBS Service Area for MBS session with location dependent content.  allowedValues: N/A | type: MbsServiceArea  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| MbsServiceArea.ncgiList | This attribute represents a list of NR cell ids with their pertaining TAIs.  allowedValues: N/A | type: Ncgi  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| plmnId | This attribute represents a PLMN Identity.  allowedValues: N/A | Type: PLMNId  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nrCellId | This attribute represents NR Cell Identity.  It's a 36-bit string identifying an NR Cell Id as specified in clause 9.3.1.7 of TS 38.413 [5], in hexadecimal representation. Each character in the string shall take a value of "0" to "9", "a" to "f" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the Cell Id shall appear first in the string, and the character representing the 4 least significant bit of the Cell Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{9}$'  Example:  An NR Cell Id 0x225BD6007 shall be encoded as "225BD6007".  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| HssInfo.groupId | This attribute defines the identity of the HSS group that is served by the HSS instance.  If not provided, the HSS instance does not pertain to any HSS group.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| HssInfo.imsiRanges | This attribute defines the list of ranges of IMSIs whose profile data is available in the HSS instance.  AllowedValues: N/A | type: ImsiRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| HssInfo.imsPrivateIdentityRanges | This attribute defines the list of ranges of IMS Private Identities whose profile data is available in the HSS instance.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| HssInfo.imsPublicIdentityRanges | This attribute defines the list of ranges of IMS Public Identities whose profile data is available in the HSS instance (NOTE 1)  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| HssInfo.msisdnRanges | This attribute defines the list of ranges of MSISDNs whose profile data is available in the HSS instance.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| HssInfo.externalGroupIdentifiersRanges | This attribute defines the list of ranges of external group IDs that can be served by this HSS instance.  If not provided, the HSS instance does not serve any external groups.  AllowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| HssInfo.hssDiameterAddress | This attribute defines the Diameter Address of the HSS  AllowedValues: N/A | type: NetworkNodeDiameterAddress  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| HssInfo.additionalDiamAddresses | This attribute defines the Additional Diameter Addresses of the HSS;  may be present if hssDiameterAddress is present  AllowedValues: N/A | type: NetworkNodeDiameterAddress  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| NetworkNodeDiameterAddress.name | This attribute indicates the Diameter name of the network node diameter address. See TS 29.571 [61]. String contains a Diameter Identity (FQDN).  AllowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkNodeDiameterAddress.realm | This attribute indicates the Diameter realm of the network node diameter addres. See TS 29.571 [61]. String contains a Diameter Identity (FQDN).  AllowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ImsiRange.start | This attribute indicates the first value identifying the start of a IMSI range.  Pattern: "^[0-9]+$"  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ImsiRange.end | This attribute indicates the last value identifying the end of a IMSI range.  Pattern: "^[0-9]+$"  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ImsiRange.pattern | This attribute indicates pattern (regular expression according to the ECMA-262 dialect [75]) representing the set of IMSIs belonging to this range. An IMSI value is considered part of the range if and only if the IMSI string fully matches the regular expression.  Either the start and end attributes, or the pattern attribute, shall be present.  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mnpfInfo | This attribute represents information of an MNPF NF Instance  AllowedValues: N/A | type: MnpfInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| MnpfInfo.msisdnRanges | This attribute represents the list of ranges of MSISDNs whose portability status is available in the MNPF.  allowedValues: N/A | type: IdentityRange  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| activationStatus | It describes the activation status.  allowedValues: ACTIVATED, DEACTIVATED. | Type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mLModelRefList | This attribute holds a DN list of MLModel (See TS 28.105 [105]) . | type: DN  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| aIMLInferenceFunctionRefList | This attribute holds a DN list of AIMLInferenceFunction (See TS 28.105 [105]) . | type: DN  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TrustAfInfo.sNssaiInfoList | It represents S-NSSAIs and DNNs supported by the trust AF.  allowedValues: N/A | type: SnssaiInfoItem  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SnssaiTsctsfInfoItem.dnnInfoList | It represents list of parameters supported by the TSCTSF per DNN.  allowedValues: N/A | type: DnnTsctsfInfoItem  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnnTsctsfInfoItem.dnn | It represents supported DNN or Wildcard DNN if the TSCTSF supports all DNNs for the related S-NSSAI. The DNN shall contain the Network Identifier and it may additionally contain an Operator Identifier. If the Operator Identifier is not included, the DNN is supported for all the PLMNs in the plmnList of the NF Profile.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mlModelInterInfo | This attribute defines the list of NWDAF vendors that are allowed to retrieve ML models from the NWDAF containing MTLF. The absence of this attribute indicates that none of the NWDAF vendors can retrieve the ML models.  allowedValues: 6 decimal digits; if the SMI code has less than 6 digits, it shall be padded with leading digits "0" to complete a 6-digit string value. | type: string  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| flCapabilityType | This attribute defines the federated learning capability type supported by NWDAF containing MTLF.  allowedValues:  “FL\_SERVER” indicates NWDAF containing MTLF as Federated Learning Server,  “FL\_CLIENT” indicates NWDAF containing MTLF as Federated Learning Client,  “FL\_SERVER\_AND\_CLIENT” indicates NWDAF containing MTLF as Federated Learning Server and Client. | type: ENUM  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| flTimeInterval | This attribute defines the time window at which the indicated flCapabilityType supported by NWDAF MTLF is available. This attribute shall be present only if flCapabilityType attribute is present.  allowedValues: N/A | type: TimeWindow  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: True |
| qFMonitoredSatelliteBackhaulCategories | It specifies the satellite backhaul categories for which the QoS monitoring per QoS flow per UE is to be performed.  AllowedValues:  "DYNAMIC\_GEO"  "DYNAMIC\_MEO"  "DYNAMIC\_LEO"  "DYNAMIC\_OTHER\_SAT" | type: Enumeration  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| AMFFunction.sliceExpiryInfo | This provides information related to a network slice validity. | type: SliceExpiryInfo  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| expiryTime | This attribute provides information about the time at which the slice is scheduled to be expired as it is not required anymore.  This attribute will be set based on the sliceAvailability coming as part of ServiceProfile. | type: DateTime  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| servedPcscfInfoList | This attribute contains all the pcscfInfo attributes locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedNfInfo | This attribute contains information of other NFs without corresponding NF type specific Info extensions locally configured in the NRF or the NRF received during NF registration. The key of the map is the nfInstanceId of the NF.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| servedAanfInfoList | This attribute contains the aanfInfoList attribute locally configured in the NRF or that the NRF received during NF registration. The key of the map is the nfInstanceId to which the map entry belongs to.  AllowedValues: N/A | type: AttributeValuePair  multiplicity: 0..\*  isOredred: False  isUnique: True  defaultValue: None  isNullable: False |
| PcscfInfo.dnnList | This attribute represents DNNs supported by the P-CSCF. The DNN shall contain the Network Identifier and it may additionally contain an Operator Identifier. If the Operator Identifier is not included, the DNN is supported for all the PLMNs in the plmnList of the NF Profile.  If not provided, the P-CSCF can serve any DNN.  allowedValues: N/A | type: string  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| gmFqdn | This attribute represents FQDN of the P-CSCF for the Gm interface.  AllowedValues: N/A | type: string  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gmIpv4Addresses | This attribute represents list of IPv4 addresses of of the P-CSCF for the Gm interface.  AllowedValues: N/A | type: Ipv4Addr  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| gmIpv6Addresses | This attribute represents list of IPv6 addresses of of the P-CSCF for the Gm interface.  AllowedValues: N/A | type: Ipv6Addr  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mwFqdn | This attribute represents FQDN of the P-CSCF for the Mw interface.  AllowedValues: N/A | type: string  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mwIpv4Addresses | This attribute represents list of IPv4 addresses of of the P-CSCF for the Mw interface.  AllowedValues: N/A | type: Ipv4Addr  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| mwIpv6Addresses | This attribute represents list of IPv6 addresses of of the P-CSCF for the Mw interface.  AllowedValues: N/A | type: Ipv6Addr  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servedIpv4AddressRanges | This attribute represents list of ranges of UE IPv4 addresses used on the Gm interface, served by P-CSCF.  The absence of this attribute does not mean the P-CSCF can serve any IPv4 address.  AllowedValues: N/A | type: Ipv4AddressRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| servedIpv6PrefixRanges | This attribute represents list of ranges of UE IPv6 prefixes used on the Gm interface, served by P-CSCF.  The absence of this attribute does not mean the P-CSCF can serve any IPv6 prefix.  AllowedValues: N/A | type: Ipv6PrefixRange  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| AMFFunction.satelliteBackhaulInfoList | This attribute defines the list of satellite backhaul information, including satellite backhaul categoty and corresponding information of (R)AN.  AllowedValues: N/A | type: SatelliteBackhaulInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| SatelliteBackhaulInfo.nTNGlobalRanNodeID | It specifies the unique identifier of a (R)AN node for NTN scenario. It is used to identify which (R)AN node the satellite backhaul type is applicable to.  AllowedValues: N/A | type: NTNGlobalRanNodeID  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SatelliteBackhaulInfo.satelliteBackhaulCategory | Define the type of the satellite used in the backhaul. Only a single backhaul category can be indicated.  AllowedValues:  "GEO"  "MEO"  "LEO"  "OTHER\_SAT"  "DYNAMIC\_GEO"  "DYNAMIC\_MEO"  "DYNAMIC\_LEO"  "DYNAMIC\_OTHER\_SAT"  "NON\_SATELLITE" | type: Enumeration  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SatelliteBackhaulInfo.geoSatelliteId | Unique identifier of a GEO satellite. See e.g. clause 5.43 in 3GPP TS 23.501 [2]. It shall be formatted as a fixed 5-digit string, padding with leading digits “0” to complete a 5-digit length.  Pattern: '^[0-9]{5}$'  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.plmnId | This attribute represents a PLMN Identity.  allowedValues: N/A | type: PLMNId  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.n3IwfId | This represents the identifier of the N3IWF ID. (Ref. clause 9.3.1.57 of 3GPP TS 38.413 [11])  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.gNbId | This represents the identifier of the gNB. (Ref. clause 8.2 of 3GPP TS 38.300 [3])  AllowedValues: 0..4294967295 | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.ngeNbId | This represents the identifier of the ng-eNB ID. (Ref. clause 9.3.1.8 of 3GPP TS 38.413 [11])  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.wagfId | This represents the identifier of the W-AGF ID. (Ref. clause 9.3.1.162 of 3GPP TS 38.413 [11])  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.tngfId | This represents the identifier of the TNGF ID. (Ref. clause 9.3.1.161 of 3GPP TS 38.413 [11])  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NTNGlobalRanNodeID.twifId | This represents the TWIF identification. (Ref. clause 9.3.1.153 of 3GPP TS 38.413 [11])  AllowedValues: N/A | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| SMFFunction.dnaiSatelliteMappingList | It specifies the mapping relationship between satellite ID and at least one DNAI.  AllowedValues: N/A | type: DnaiSatelliteMapping  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnaiSatelliteMapping.dnaiList | List of Data network access identifiers supported for this DNN.  allowedValues:  DNAI (Data network access identifier), see clause 5.6.7 of 3GPP TS 23.501 [2].  AllowedValues: N/A | type: string  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| DnaiSatelliteMapping.geoSatelliteId | Unique identifier of a GEO satellite. See e.g. clause 5.43 in 3GPP TS 23.501 [2].  AllowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NOTE 1: If none of these parameters are provided, the AUSF can serve any SUPI managed by the PLMN of the AUSF instance. If "supiRanges" attribute is absent, and "groupId" is present, the SUPIs served by this AUSF instance is determined by the NRF (see TS 23.501 [2], clause 6.2.6.2).  NOTE 2: The combination of SUCI informations, e.g. Routing Indicator and Home Network Public Key Id, can be used as criteria for AUSF discovery. This may only be used by the HPLMN in roaming scenarios in this release of the specification, i.e. an AMF in a visited network does not use the Home Network Public Key ID for AUSF selection.  NOTE 3: If the suciInfos attribute is present and contains the routingInds sub-attribute, then the routingIndicators attribute shall also be present. | | |

|  |
| --- |
| **Next change** |

### 6.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| ServiceProfile.availability | This parameter specifies the communication service availability requirement, expressed as a percentage. This parameter is applicable for an end-to-end communication service provided by a network slice. The communication service availability is defined in clause 3.1 of TS 22.261 [28]. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| serviceProfileId | A unique identifier of property of network slice related requirement should be supported by the network slice. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sliceProfileId | A unique identifier of the property of network slice subnet related requirement should be supported by the network slice subnet. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| operationalState | It indicates the operational state of the network slice or the network slice subnet. It describes whether or not the resource is physically installed and working.  allowedValues: "ENABLED", "DISABLED".  The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| administrativeState | It indicates the administrative state of the network slice or the network slice subnet. It describes the permission to use or prohibition against using the managed object instance, imposed through the OAM services.  allowedValues: “LOCKED”, “UNLOCKED”, SHUTTINGDOWN”  The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: LOCKED  allowedValues: N/A  isNullable: False |
| nsInfo | This attribute contains the NsInfo of the NS instance corresponding to the network slice subnet instance. The NsInfo is described in clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: NsInfo  multiplicity: 0..1  isOrdered: N/A  isUnique: True  defaultValue: No default value  isNullable: False |
| nsInstanceId | This attribute specifies the identifier of NS instance corresponding to the network slice subnet instance.  See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: No default value  isNullable: False |
| nsName | This attribute specifies the name of NS instance corresponding to the network slice subnet instance.  See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: No default value  isNullable: False |
| description | This attribute specifies the description of NS instance corresponding to the network slice subnet instance.  See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: No default value  isNullable: False |
| category | This attribute specifies the category of a service requirement/attribute of GST (see GSMA NG.116 [50]).  allowedValues: CHARACTER, SCALABILITY | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| tagging | This attribute specifies the tagging of a service requirement/attribute of GST in character category (see GSMA NG.116 [50]).  allowedValues: PERFORMANCE, FUNCTION, OPERATION | type: ENUM  multiplicity: 1…3  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| exposure | This attribute specifies exposure mode of a service requirement/attribute of GST (see GSMA NG.116 [50]).  allowedValues: API, KPI | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| maxNumberofUEs | An attribute specifies the maximum number of UEs may simultaneously access the network slice or network slice subnet instance. | type: MaxNumberofUEs  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxNumberofUE.3GPPNoOfUEs | An attribute specifies the maximum number of UEs may simultaneously access the network slice or network slice subnet instance on 3GPP access. | Type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxNumberofUE.non3GPPNoOfUEs | An attribute specifies the maximum number of UEs may simultaneously access the network slice or network slice subnet instance on non-3GPP access. | Type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| coverageAreaTAList | An attribute specifies a list of Tracking Areas for the network slice. TAI uniquely identifies a Tracking Area. TAI is defined in clause 9.3.3.11 of TS 38.413 [5].  allowedValues: N/A | type: Tai  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| dLLatency | An attribute specifies the required DL packet transmission latency (millisecond) through the RAN, CN, and TN part of 5G network and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uLLatency | An attribute specifies the required UL packet transmission latency (millisecond) through the RAN, CN, and TN part of 5G network and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| topSliceSubnetProfile.dLLatency | An attribute specifies the required DL packet transmission latency (millisecond) through all domains of the network slice and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| topSliceSubnetProfile.uLLatency | An attribute specifies the required UL packet transmission latency (millisecond) through all domains of the network slice and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| CNSliceSubnetProfile.dLLatency | An attribute specifies the required DL packet transmission latency (millisecond) through CN domain of the network slice and is used to evaluate the delay in CN domain, e.g. time between received DL packet on N6 interface of UPF and successfully sent out the packet on N3 interface. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| CNSliceSubnetProfile.uLLatency | An attribute specifies the required UL packet transmission latency (millisecond) through CN domain of the network slice and is used to evaluate the delay in CN domain, e.g. time between received UL packet on N3 interface of UPF and successfully sent out the packet on N6 interface. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| RANSliceSubnetProfile.dLLatency | An attribute specifies the required DL packet transmission latency (millisecond) in RAN including the air interface of the network slice and is used to evaluate the delay between NR-RAN and UE, e.g. time between received DL packet from UPF and the packet successfully received by UE. See clause 5.1.1.1.6 in TS 28.552 [69]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| RANSliceSubnetProfile.uLLatency | An attribute specifies the required UL packet transmission latency (millisecond) in RAN including the air interface of the network slice and is used to evaluate the delay between UE and NG-RAN, e.g. time between the UL packet transmitted by UE and the packet transmitted by gNB to UPF. See clause 5.1.1.1.7 in TS 28.552 [69]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uEMobilityLevel | An attribute specifies the mobility level of UE accessing the network slice. See 6.2.1 of TS 22.261 [28].  allowedValues: STATIONARY, NOMADIC, RESTRICTED\_MOBILITY, FULL\_MOBILITY. | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| networkSliceSharingIndicator | The attribute specifies whether a service, defined by the ServiceProfile, can share a NetworkSlice instance with other services or not. If “non-shared” the service needs a dedicated NetworkSlice instance. If “shared” the service may share a NetworkSlice instance with other service(s).  allowedValues: SHARED, NON\_SHARED. | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| serviceProfile.pLMNInfoList | It defines which PLMN and S-NSSAI combinations that are assigned for the service to satisfy service requirements represented by the ServiceProfile in case of network slicing feature is supported.  allowedValues: Not applicable. | type: PLMNInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| sliceProfile.pLMNInfoList | It defines which PLMN and S-NSSAI combinations that are served by the SliceProfile in case of network slicing feature is supported.  allowedValues: Not applicable. | type: PLMNInfo  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| sliceProfile.resourceSharingLevel | An attribute specifies whether the resources to be allocated to the network slice subnet may be shared with another network slice subnet(s).  allowedValues: SHARED, NON\_SHARED. | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: Yes  isNullable: False |
| serviceProfileList | An attribute specifies a list of ServiceProfile (see clause 6.3.3) supported by the network slice | type: ServiceProfile  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| sliceProfileList | An attribute specifies a list of SliceProfile (see clause 6.3.4) supported by the network slice subnet.  All members of the list, instances of SliceProfile, shall contain the same datatype representing slice profile requirements: TopSliceSubnetProfile, RANSliceSubnetProfile or CNSliceSubnetProfile. E.g. the sliceProfileList may contain only instances of sliceProfile containing RANSliceSubnetProfile datatype; the sliceProfileList may not contain instances of sliceProfile containing RANSliceSubnetProfile and CNSliceSubnetProfile datatypes  Members of the list may contain TopSliceSubnetProfile datatype only when this attribute (sliceProfileList) belongs to a NetworkSliceSubnet that is directly referenced by a NetworkSlice | type: SliceProfile  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| sST | This attribute specifies the slice/service type in a ServiceProfile to be supported by a network slice.  See standardised SST values in clause 5.15.2 of TS 23.501 [2]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| delayTolerance | An attribute specifies the properties of service delivery flexibility, especially for the vertical services that are not chasing a high system performance. See clause 4.3 of TS 22.104 [51]. | type: DelayTolerance  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DelayTolerance.support | An attribute specifies whether or not the network slice supports service delivery flexibility, especially for the vertical services that are not chasing a high system performance.  allowedValues:  "NOT\_SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| dLDeterministicComm | An attribute specifies the properties of the deterministic communication in downlink for periodic user traffic, see clause 4.3 of TS 22.104 [51]. | type: DeterministicComm  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| uLDeterministicComm | An attribute specifies the properties of the deterministic communication in uplink for periodic user traffic, see clause 4.3 of TS 22.104 [51]. | type: DeterministicComm  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DeterministicComm.availability | An attribute specifies whether or not the network slice supports deterministic communication for period user traffic.  allowedValues:  "NOT\_SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DeterministicComm.periodicityList | An attribute specifies a list of periodicities supported by the network slice for deterministic communication. Each instance of periodicity is expressed in seconds, refer to NG.116 [50]. | type: Integer  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: False  isNullable: False |
| dLThptPerSlice | This attribute defines achievable data rate of the network slice in downlink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dLThptPerSliceSubnet | This attribute defines required data rate of the network slice subnet in downlink that should be available ubiquitously across the coverage area of the slice. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dLThptPerUE | This attribute defines data rate supported by the network slice per UE, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| guaThpt | This attribute describes the guaranteed data rate. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| maxThpt | This attribute describes the maximum data rate. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| uLThptPerSlice | This attribute defines achievable data rate of the network slice in uplink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uLThptPerUE | This attribute defines data rate supported by the network slice per UE, refer NG.116 [50]. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uLThptPerSliceSubnet | This attribute defines required data rate of the network slice subnet in uplink that should be available ubiquitously across the coverage area of the slice. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| dLMaxPktSize | This parameter specifies the maximum packet size supported by the network slice or the network slice subnet, in downlink refer NG.116 [50]. | type: MaxPktSize  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| uLMaxPktSize | This parameter specifies the maximum packet size supported by the network slice or the network slice subnet in uplink, refer NG.116 [50]. | type: MaxPktSize  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxPktSize.maxsize | This parameter specifies the maximum packet size supported by the network slice, refer NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| maxNumberofPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice on 3GPP access type, refer NG.116 [50]. | type: MaxNumberofPDUSessions  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxNumberofPDUSessions.3GPPNoOfPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice, refer NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| MaxNumberofPDUSessions.non3GPPNoOfPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice on non 3GPP access type, refer NG.116 [50]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| ServiceProfile.kPIMonitoring | An attribute specifies the name list of KQIs and KPIs, related to the network slice available for performance monitoring. | type: KPIMonitoring  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| KPIMonitoring.kPIList | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: False  isNullable: False |
| nBIoT | An attribute specifies whether NB-IoT is supported in the RAN in the network slice, see NG.116 [50]. | type: NBIoT  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| NBIoT.support | An attribute specifies whether NB-IoT is supported in the RAN in the network slice, see NG.116 [50].  allowedValues:  "NOT\_SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| synchronicity | An attribute specifies whether synchronicity of communication devices is supported, Two cases are most important in this context, see clause 3.4.29 of NG.116 [50]:  - Synchronicity between a base station and a mobile device and  - Synchronicity between mobile devices. | type: Synchronicity  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Synchronicity.availability | An attribute specifies whether synchronicity of communication devices is supported, see NG.116 [50].  allowedValues:  "NOT\_SUPPORTED", "BETWEEN\_BS\_AND\_UE", "BETWEEN\_BS\_AND\_UE\_AND\_UE\_AND\_UE". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| Synchronicity.accuracy | An attribute specifies the accuracy of the synchronicity, see NG.116 [50]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| RANSliceSubnetProfile.synchronicity | An attribute specifies whether synchronicity of communication devices is supported in the RAN domain, Two cases are most important in this context, see clause 3.4.29 of NG.116 [50]:  - Synchronicity between a base station and a mobile device and  - Synchronicity between mobile devices. | type: Synchronicity  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| userMgmtOpen | An attribute specifies whether or not the network slice supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements. | type: UserMgmtOpen  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| UserMgmtOpen.support | An attribute specifies whether or not the network slice supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements.  allowedValues:  "NOT\_SUPPORTED", "SUPPORTED". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| v2XCommModels | An attribute specifies whether or not the V2X communication mode is supported by the network slice. | type: V2XCommMode  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| V2XCommMode.v2XMode | An attribute specifies whether or not the V2X communication mode is supported by the network slice.  allowedValues:  "NOT\_SUPPORTED", "SUPPORTED\_BY\_NR". | type: <<enumeration>>  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| coverageArea | An attribute specifies the coverage area of the network slice, i.e. the geographic region where a 3GPP communication service is accessible, see Table 7.1-1 of TS 22.261 [28]) and NG.116 [50]. | type: GeoArea  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: False  isNullable: False |
| termDensity | An attribute specifies the overall user density over the coverage area of the network slice. See Table 7.1-1 of TS 22.261 [28]). | type: TermDensity  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| TermDensity.density | An attribute specifies the overall user density over the coverage area of the network slice. See Table 7.1-1 of TS 22.261 [28]). | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| positioning | An attribute specifies whether the network slice provides geo-localization methods or supporting methods, see clause 3.4.20 of NG.116 [50]. | type: Positioning  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| RANSliceSubnetProfile.positioning | An attribute specifies whether the RAN domain of the network slice provides geo-localization methods or supporting methods, see clause 3.4.20 of NG.116 [50]. | type: PositioningRANSubnet  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| PositioningRANSubnet.availability | An attribute specifies if this attribute is provided by the RAN domain of the network slice and contains a list of positioning methods provided by the RAN domain. If the list is empty this attribute is not available in the RAN domain and the other parameters might be ignored, see NG.116 [50]. Comma separated multiple values are allowed:  CIDE\_CID, OTDOA, RF\_FINGERPRINTING, AECID, HYBRID\_POSITIONING, NET\_RTK. | type: ENUM  multiplicity: 1..6  isOrdered: False  isUnique: True  defaultValue: False  isNullable: False |
| PositioningRANSubnet.predictionFrequency | An attribute specifies how often location information is provided. This parameter simply defines how often the customer is allowed to request location information. This is not related to the time it takes to determine the location, which is a characteristic of the positioning method, see NG.116 [50].  allowedValues:  "PERSEC", "PERMIN", "PERHOUR". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| PositioningRANSubnet.accuracy | An attribute specifies the accuracy of the location information. Accuracy depends on the respective positioning solution applied in the RAN domain of the network slice, measurement unit is meter, see NG.116 [50]. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| activityFactor | An attribute specifies the percentage value of the amount of simultaneous active UEs to the total number of UEs where active means the UEs are exchanging data with the network. See Table 7.1-1 of TS 22.261 [28]). | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| uESpeed | An attribute specifies the maximum speed (in km/hour) supported by the network slice or network slice subnet at which a defined QoS can be achieved. See Table 7.1-1 of TS 22.261 [28]). | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| ServiceProfile.dLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in DL packet spacing at the receiver compared to the sender for a pair of packets through the RAN, CN and TN part of an end-to-end network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| ServiceProfile.uLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in UL packet spacing at the receiver compared to the sender for a pair of packets through the RAN, CN and TN part of an end-to-end network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| TopSliceSubnetProfile.dLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in DL packet spacing at the receiver compared to the sender for a pair of packets through the RAN, CN and TN part of an end-to-end network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| TopSliceSubnetProfile.uLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in UL packet spacing at the receiver compared to the sender for a pair of packets through the RAN, CN and TN part of an end-to-end network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| CNSliceSubnetProfile.dLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in DL packet spacing at the receiver compared to the sender for a pair of packets through CN domain of the network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| CNSliceSubnetProfile. uLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in UL packet spacing at the receiver compared to the sender for a pair of packets through CN domain of the network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| RANSliceSubnetProfile.dLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in DL packet spacing at the receiver compared to the sender for a pair of packets through RAN domainof the network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| RANSliceSubnetProfile.uLPktDelayVariation | An attribute specifies the required deviation (millisecond) of the difference in UL packet spacing at the receiver compared to the sender for a pair of packets through RAN domainof the network slice.  How to measure inter-packet delay variation is documented by IETF in RFC 3393 [102] as measuring the IP packet delay variation and its applicability to use it as metric is documented in Section 4.1 of RFC 5481 [103]. The deviation is also defined in Annex C.4.4 of TS 22.104 [51] | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| survivalTime | An attribute specifies the time (millisecond) that an application consuming a communication service may continue without an anticipated message. See clause 5 of TS 22.104 [51]). | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| dLReliability | An attribute specifies in the context of network layer DL packet transmissions, percentage value of the amount of sent network layer packets successfully delivered to a given system entity within the time constraint required by the targeted service, divided by the total number of sent network layer packets, see TS 22.261. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| uLReliability | An attribute specifies in the context of network layer UL packet transmissions, percentage value of the amount of sent network layer packets successfully delivered to a given system entity within the time constraint required by the targeted service, divided by the total number of sent network layer packets, see TS 22.261. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| NetworkSlice.networkSliceSubnetRef | This holds a DN of NetworkSliceSubnet relating to the NetworkSlice instance. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceSubnet.networkSliceSubnetRef | This holds a list of DN of constituent NetworkSliceSubnet supporting NetworkSliceSubnet instance | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| managedFunctionRef | This holds a list of DN of ManagedFunction instances supporting the NetworkSliceSubnet instance. | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| ipAddress | This parameter specifies the IP address assigned to a logical transport interface/endpoint which is part of a RAN or CN SubNetwork.  It can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).  See note 1 | type: IpAddress  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| localLogicalInterfaceInfo | This parameter specifies the information of a local logical transport interface. | type: LogicalInterfaceInfo  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| logicalInterfaceType | This parameter specifies the type of a logical transport interface. It could be VLAN, MPLS or SEGMENT.  Allowed Value: VLAN,MPLS, SEGMENT | type:Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| logicalInterfaceId | This parameter specifies the identify of a logical transport interface which is part of a RAN or CN SubNetwork. It could be VLAN ID (See IEEE 802.1Q [39]), MPLS Tag or Segment ID.  In case logical transport interface is VLAN, it is VLAN Id (See IEEE 802.1Q [39]).  In case logical transport interface is MPLS, it is MPLS Tag.  In case logical transport interface is Segment, it is Segment ID. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| externalEndPointRefList | This parameter is used to identify a list of connection point info(s). | Type: ConnectionPointInfo  multiplicity: \*  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| connectionPointId | This parameter specifies the identifier of a TN object. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| connectionPointIdType | This parameter specifies the type of the connection point identifier.  Allowed values: VLAN, MPLS, SEGMENT, IPV4, IPV6, ATTACHMENT\_CIRCUIT | type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| LogicalInterfaceInfo.systemName | This parameter specifies the identifier for a system. | Type: String  Multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| LogicalInterfaceInfo.portName | This parameter specifies the identifier for a port. | Type: String  Multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| LogicalInterfaceInfo.routingProtocol | This parameter specifies the Routing protocol.  Allowed values: RIP, IGMP, OSPF, EGP, EIGRP, BGP, IS-IS, STATIC | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qosProfile | This parameter specifies the QoS Profile for a logical transport interface. A QoS profile includes a set of parameters which are locally provisioned on both sides of a logical transport interface.  An example of the parameter value could be “DSCP” (See RFC 8436 [74]). | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| maxDLDataVolume | An attribute specifies the maximum DL PDCP data volume supported by the network slice instance (performance measurement definition see in TS 28.552[69]). The unit is MByte/day. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| maxULDataVolume | An attribute specifies the maximum UL PDCP data volume supported by the network slice instance (performance measurement definition see in TS 28.552[69]). The unit is MByte/day. | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| radioSpectrum | This attribute represents the radio spectrum in which the network slice should be supported (see clause 3.4.21 of GSMA NG.116 [50]). | type: RadioSpectrum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nROperatingBands | This attribute represents which 5G NR frequency bands can be used to access the network slice. 5G NR operating bands are defined in 3GPP TS 38.101-1 [42]. | type: String  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| epApplicationRef | This parameter specifies a list of application level EPs (i.e. EP\_N3 or EP\_NgU or EP\_F1U) associated with the logical transport interface. | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| epTransportRef | This parameter specifies a list of transport level EPs associated with the application level EP (i.e. EP\_N3 or EP\_NgU or EP\_F1U) or network slice subnet. | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| sliceSimultaneousUse | This attribute describes whether a network slice can be simultaneously used by a device together with other network slices and if so, with which other classes of network slices.  allowedValues: “0”, “1”, “2”, “3”, “4”.  “0”: Can be used with any network slice  “1”: Can be used with network slices with same SST value  “2”: Can be used with any network slice with same SD value  “3”: Cannot be used with another network slice  “4”: Cannot be used by a UE in a specific location | type: integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| energyEfficiency | An attribute which describes the energy efficiency of a network slice, i.e. the ratio between the performance of a network slice and its energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: EnergyEfficiency  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| EnergyEfficiency.performance | Depending on the sST value, EnergyEfficiency.performance will be  - eMBBEEPerfReq  or  - uRLLCEEPerfReq  or  - mIoTEEPerfReq  allowedValues:  - eMBBEEPerfReq identifies the requirement in terms of energy efficiency, i.e. the performance per consumed Joule in type Real, where performance can take one of the following forms (type: ENUM):  - number of bits (Integer) (see TS 28.554 [27] clause 6.7.2.2).  - number of bits (Integer) for RAN-based network slice (see TS 28.554 [27] clause 6.7.2.2a).  - uRLLCEEPerfReq identifies the requirement in terms of energy efficiency, i.e. the performance per consumed Joule in type Real, where performance can take one of the following forms (type: ENUM):  - inverse of the latency in 0.1ms (Real) (see TS 28.554 [27] clause 6.7.2.3.2).  - number of bits multiplied by the inverse of the latency in 0.1ms (Real) (see TS 28.554 [27] clause 6.7.2.3.3).  - mIoTEEPerfReq identifies the requirement in terms of energy efficiency, i.e. the performance per consumed Joule in type Real, where performance can take one of the following forms (type: ENUM):  - maximum number of registered subscribers (Integer) (see TS 28.554 [27] clause 6.7.2.4.1),  - mean number of active UEs (Integer) (see TS 28.554 [27] clause 6.7.2.4.2).  See NOTE 3. | type: ENUM  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| topSliceSubnetProfile.energyEfficiency | An attribute which describes the energy efficiency through all domains of the network slice, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: EnergyEfficiency  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| CNSliceSubnetProfile.energyEfficiency | An attribute which describes the energy efficiency through CN domain of the network slice, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| RANSliceSubnetProfile.energyEfficiency | An attribute which describes the energy efficiency through RAN domain of the network slice, i.e. the ratio between the performance and the energy consumption (EC) when assessed during the same time frame, see clause 3.4.7 of NG.116 [50]. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nssaaSupport | An attribute specifies whether for the Network Slice, devices need to be also authenticated and authorized by a AAA server using additional credentials different than the ones used for  the primary authentication, see clause 3.4.37 of NG.116 [50].  allowedValues: N/A | type: NSSAASupport  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| nssaaSupport.support | An attribute specifies whether or not the Network Slice, devices need to be also authenticated and authorized by a AAA server using additional credentials different than the ones used for  the primary authentication.  allowedValues:  "NOT\_SUPPORTED", "SUPPORTED". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| ServiceProfile.n6Protection | An attribute which includes required security functions and corresponding rules of each function for network slice N6 interface protection.  allowedValues: N/A | type: N6Protection  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| CNSliceSubnetProfile.n6Protection | An attribute which includes required security functions and corresponding rules of each function for network slice N6 interface protection.  allowedValues: N/A | type: N6Protection  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| secFuncList | An attribute which holds the list of security control functions/features required by the Network Slice or Network Slice Subnet consumer.  allowedValues: N/A | type: SecFunc  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| secFunId | An attribute which identifies a security function.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| secFunType | An attribute which describes the type of the security function. E.g. Firewall, NAT, antimalware, parental control, DDoS protection function, etc.  allowedValues: N/A | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| secRules | An attribute which could be configured on each function. If it's absent, the default rules could be applied.  allowedValues: N/A | type: String  multiplicity: 0..\*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| networkSliceSubnetType | An attribute indicating type of network slice subnet, including:  - Top network slice subnet  - RAN network slice subnet  - CN network slice subnet  Allowed Value:  TOP\_SLICESUBNET,RAN\_SLICESUBNET,CN\_SLICESUBNET | type:Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| priorityLabel | An attribute specifies a label that consumer would assign a value on an instance of network slice subnet. The management system takes the value of this attribute into account. The effect of this attribute value to the subject managed entity is not standardized  allowedValues: N/A | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceSubnetProviderCapabilities.dLlatency | This attribute specifies the achievable packet transmission latency in downlink (millisecond) through the network slice subnet. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| NetworkSliceSubnetProviderCapabilities.uLlatency | This attribute specifies the achievable packet transmission latency in uplink (millisecond) through the network slice subnet. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| NetworkSliceSubnetProviderCapabilities.dLThptPerSliceSubnet | This attribute defines achievable data rate of the network slice subnet in downlink that is available ubiquitously across the coverage area of the slice. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| NetworkSliceSubnetProviderCapabilities.uLThptPerSliceSubnet | This attribute defines achievable data rate of the network slice subnet in uplink that is available ubiquitously across the coverage area of the slice. | type: XLThpt  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| NetworkSliceSubnetProviderCapabilities.coverageAreaTAList | An attribute specifies a list of Tracking Areas that a network slice subnet can serve. TAI uniquely identifies a Tracking Area. TAI is defined in clause 9.3.3.11 of TS 38.413 [5].  allowedValues: N/A | type: Tai  multiplicity: 1..\*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| processMonitor | An attribute describes the process monitoring information of the feasibility check and reservation job. See corresponding processMonitor definition in TS 28.622[30]. | type: ProcessMonitor  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| feasibilityResult | An attribute which specifies the feasibility check result for the feasibility check and reservation job. This attribute is configured by MnS producer and can be read by MnS consumer. The feasibilityResult is configured once the "status" is "FINISHED"  Allowed Value:  FEASIBLE: which means the specified network slicing related requirements (i.e. ServiceProfile, SliceProfile) can be satisfied by the MnS producer.  INFEASIBLE: which means the specified network slicing related requirements (i.e. ServiceProfile, SliceProfile) cannot be satisfied by the MnS producer. | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| inFeasibleReason | An attribute that specifies the additional reason information if the feasibility check result is infeasible. This attribute can be absent if the feasibility check result is feasibile.  Allowed Value: the detailed content (Enum Value) for the inFeasibleReason is not defined in the present document. | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| resourceReservation | An attribute represents MnS consumer's requirements for resource reservation.  Allowed Value:  TRUE: MnS producer need to reserve corresponding resources  FALSE (DeaultValue): no guarantee for the corresponding resources. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: ‘FALSE’  isNullable: False |
| recommendationRequest | An attribute represents MnS consumer's request for recommended network slice related requirements  Allowed Value:  TRUE: MnS producer need to derive and provide the recommended network slicing related requirements  FALSE (DeaultValue): no guarantee for derive and provide the recommended network slicing related requirements. | type: Boolean  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: ’FALSE’  isNullable: False |
| requestedReservationExpiration | An attribute which specifies MnS consumer's requirememts for the validity period of the resource reservation. The value of requestedReservationExpiration is specified by MnS consumer. | type: Timestamp  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| reservationExpiration | An attribute which specifies the actual validity period of the resource reservation. After the period expires, no guarantees are given for the resources associated to the corresponding network slicing related requirements (i.e. ServiceProfile, SliceProfile). which is specified by MnS producer based on requested reservation expiration from MnS consumer and its own reservation capabilities. In case MnS produer have the enpugh capability to satisfy MnS consumer's reservation requirememts, the value of reservationExpiration is same as requestedReservationExpiration. | type: Timestamp  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| resourceReservationStatus | An attribute which specifies the resource reservation result for the feasibility check and reservation job. This attribute is configured by MnS producer and can be read by MnS consumer.  Allowed Value:  RESERVED: which means the resources for the specified network slicing related requirements (i.e. ServiceProfile, SliceProfile) is reserved.  UNRESERVED: which means the resources for the specified network slicing related requirements (i.e. ServiceProfile, SliceProfile) is not reserved.  USED: which means the reserved resource for the specified network slicing related requirements is used. | type: Enum  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| recommendedRequirements | An attribute which specifies the recommended network slicing related requirements (i.e. ServiceProfile and SliceProfile information) which can be supported by the MnS producer. This information is provided when the feasibility check result is infeasible. This information can be used by MnS consumer to adjust the network slicing related requirements. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| reservationFailureReason | An attribute that specifies the additional reason information if the reservation is failed. This attribute can be absent if the reservation is successful.  Allowed Value: the detailed content (Enum Value) for the reservationFailureReason is not defined in the present document. | type: Enum  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| FeasibilityCheckAndReservationJob.serviceProfile | An attribute specifies the network slice related requirements for the feasibility check and resource reservation job | type: ServiceProfile  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: None  isNullable: False |
| FeasibilityCheckAndReservationJob.sliceProfile | An attribute specifies the network slice subnet related requirements for the feasibility check and resource reservation job | type: SliceProfile  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: None  isNullable: False |
| feasibilityTimeWindow | An attribute represents MnS consumer's request for checking whether the network slicing related requirements (i.e. ServiceProfile and SliceProfile information) can be satisfied at a specified time window.  If this attribute specified by MnS consumer, MnS producer determine whether the network slicing related requirements can be satisfied at the specified time window and reserve corresponding resources at the specified time window if resourceReservation is “TRUE”. | type: TimeWindow  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: None  isNullable: False |
| NetworkSlice.networkSliceControllerRef | This holds a list of DN of NetworkSliceController supported by the NetworkSlice MOI. | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| NetworkSliceSubnet.networkSliceSubnetControllerRef | This holds a list of DN of NetworkSliceSubnetController supported by the NetworkSliceSubnet MOI. | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| NetworkSliceController.inputServiceProfile | This attribute specifies the input network slice related requirements provided by the MnS consumer. | type: ServiceProfile  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: N/A  isNullable: False |
| NetworkSliceController.serviceProfileId | This attribute specifies the service profile identifier provided by the MnS producer for the network slice related requirements specified in inputServiceProfile attribute or as specified as part of AllocateNsi operation (defined in TS 28.531 [26]). | type: String  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceController.processMonitor | This attribute describes the process monitoring information of the fulfilment of the network slice life cycle management. | type: ProcessMonitor  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceController.networkSliceRef | This attribute specifies the DN of the NetworkSlice MOI, that the MnS producer has selected to fulfil the network slice related requirements specified in inputServiceProfile attribute or as specified as part of AllocateNsi operation (defined in TS 28.531 [26]). | type: DN  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: N/A  isNullable: False |
| NetworkSliceSubnetController. inputSliceProfile | This attribute specifies the network slice subnet related requirements. | type: SliceProfile  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: N/A  isNullable: False |
| NetworkSliceSubnetController.sliceProfileId | This attribute specifies the service profile identifier provided by the MnS producer for the network slice subnet related requirements specified in inputSliceProfile attribute or as specified as part of AllocateNssi operation (defined in TS 28.531 [26]). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceSubnetController.processMonitor | This attribute describes the process monitoring information of the fulfilment of the network slice subnet life cycle management. | type: ProcessMonitor  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceSubnetController.networkSliceSubnetRef | This attribute specifies the DN of the NetworkSliceSubnet MOI, that the MnS producer has selected to fulfil the network slice subnet related requirements specified in inputSliceProfile attribute or as specified as part of AllocateNssi operation (defined in TS 28.531 [26]). | type: DN  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: N/A  isNullable: False |
| availabilityStatus | It indicates the availability status of the fulfilment of network slice or the network slice subnet related requirements by the MnS producer.  allowedValues: "IN\_TEST", "FAILED", "POWER\_OFF", "OFF\_LINE ", "OFF\_DUTY", "DEPENDENCY", "DEGRADED", "NOT\_INSTALLED", "LOG\_FULL".  The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  allowedValues: N/A  isNullable: False |
| nonIPSupport | An attribute specifies the non-IP Session support (Ethernet session and forwarding support) of the slice or slice subnet. See Clause 3.4.27 of GSMA NG.116 [50]. | type: NonIPSupport  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| NonIPSupport.support | An attribute specifies the non-IP Session support (Ethernet session and forwarding support) of the slice or slice subnet. See Clause 3.4.27 of GSMA NG.116 [50].  allowedValues:  "NOT SUPPORTED", "SUPPORTED". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| NetworkSlice. isolationProfileRef | This holds the DN of IsolationProfile MOI representing the isolation requirements applied for the NetworkSlice MOI.  allowedValues: N/A | type: DN  multiplicity: 0..1  isOrdered: False  isUnique: N/A  defaultValue: None  isNullable: False |
| NetworkSliceSubnet. isolationProfileRef | This holds the DN of IsolationProfile MOI representing the isolation requirements applied for the NetworkSliceSubnet MOI.  allowedValues: N/A | type: DN  multiplicity: 0..1  isOrdered: False  isUnique: N/A  defaultValue: None  isNullable: False |
| IsolationProfileRef.networkSliceSubnetRefList | This holds a list of DN of NetworkSliceSubnet MOI to which the isolation is applicable.  allowedValues: N/A | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| IsolationProfileRef.networkSliceRefList | This holds a list of DN of NetworkSlice MOI to which the isolation is applicable.  allowedValues: N/A | type: DN  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| IsolationProfileRef.resourceIsolationRuleList | An attribute which describes a set of isolation rules for the managed resources. | type: ResourceIsolationRule  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| resourceType | An attribute which describes the managed resource type for isolation.  MANAGED\_FUNCTION: Indicates the managed function instances are selected using the the isolation rule which is specified by isolationRule attribute.  NETWORK\_SERVICE: Indicates the Network Service (NS) information are selected using the isolation rule which is specified by isolationRule attribute.  allowedValues: “MANAGED\_FUNCTION”, “NETWORK\_SERVICE” | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| isolationRule | An attribute which describes the isolation requirement.  DEDICATED: The network slices are provided with exclusive network resources, preventing any interference between other network slices.  SHARED: Allows the network slice resources to be shared with other network slices.  allowedValues: DEDICATED, SHARED | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| networkSlicingApplicability | An attribute which describes if the isolation requirements are associated with NetworkSlice(s) or NetworkSliceSubnet(s).  allowedValues: NETWORKSLICE, NETWORKSLICESUBNET | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| TopSliceSubnetProfile.availability | An attribute specifies the required communication service availability (percentage) through the RAN, CN, and TN part of an end-to-end network slice. See clause 3.1 of TS 22.261 [28]. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| CNSliceSubnetProfile.availability | An attribute specifies the required communication service availability (percentage) through the CN domain of a network slice, i.e., CN slice subnet. The percentage value of the amount of time the CN slice subnet is delivered according to all the slice subnet related requirements listing in the CNSliceSubnetProfile, divided by the amount of time the system is expected to deliver the CN slice subnet. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| RANSliceSubnetProfile.availability | An attribute specifies the required communication service availability (percentage) through the RAN domain of a network slice, i.e., RAN slice subnet. The percentage value of the amount of time the RAN slice subnet is delivered according to all the slice subnet related requirements listing in the RANSliceSubnetProfile, divided by the amount of time the system is expected to deliver the RAN slice subnet. | type: Real  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| TopSliceSubnetProfile.kPIMonitoring | An attribute specifies the name list of KPIs, related to all domains of the network slice, available for performance monitoring. | type: KPIMonitoring  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| RANSliceSubnetProfile.kPIMonitoring | An attribute specifies the name list of KPIs, related to the RAN domain network slice subnet, available for performance monitoring. | type: KPIMonitoring  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: True |
| supportedDataNetworks | An attribute specifies the supported data network of the slice or slice subnet. See Clause 3.4.39 of GSMA NG.116 [50]. | type: DataNetwork  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DataNetwork.dnnList | An attribute specifies the list of supported data network (DNN, see ) of the slice or slice subnet. See Clause 3.4.39 of GSMA NG.116 [50]. | type: String  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| dataNetworkAccess | An attribute specifies how the supported data networks handle the user data of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: DataNetworkAccess  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DataNetworkAccess.dataAccessList | An attribute specifies Data access per data network for the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: DataAccess  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DataNetworkAccess.tunnellingMechanismList | An attribute specifies Tunnelling mechanism per data network for the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: TunnellingMechanism  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DataNetworkAccess.localBreakoutAllowedList | An attribute specifies whether a data network is available in Local Breakout while roaming for the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: LboAllowed  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DataAccess.dataNetworkName | An attribute specifies data network name of the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| DataAccess.dataAccessUsed | An attribute specifies Data access per data network for the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50].  "DIRECT\_INTERNET\_ACCESS": Direct access to the Internet  "TERM\_PVT\_NETWORK": Termination in a private network (e.g., via tunnelling mechanism such as L2TP, VPN Virtual Private Network, tunnel, etc.)  "LOCAL\_TRAFFIC": All data traffic stays local to an operator network and the devices do not have access to the Internet or private network.  allowedValues:  "DIRECT\_INTERNET\_ACCESS", "TERM\_PVT\_NETWORK", "LOCAL\_TRAFFIC". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| TunnellingMechanism.dataNetworkName | An attribute specifies data network name of the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| TunnellingMechanism.tunellingMechanismUsed | An attribute specifies Tunnelling mechanism for the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50].  allowedValues:  "L2TP\_TUNNEL", "GRE\_TUNNEL", "VPN\_TUNNEL", "LABEL\_BASED\_ROUTING", “802.1Q\_VLAN”, “SRV6”, "OTHER". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| LboAllowed.dataNetworkName | An attribute specifies data network name of the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50]. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
| LboAllowed.localBreakoutAllowed | An attribute specifies whether a data network is available in Local Breakout while roaming for the supported data networks of the slice or slice subnet. See Clause 3.4.34 of GSMA NG.116 [50].  allowedValues:  "YES", "NO". | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: False  isNullable: False |
|  |  |  |
|  |  |  |
| ServiceProfile.sliceAvailability | This attribute provides information about the time at which the slice or slice subnet instance is scheduled to be available. | type: SchedulingTime  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| CNSliceSubnetProfile.sliceSubnetAvailability | This attribute provides information about the time at which the slice or slice subnet instance is scheduled to be available. | type: SchedulingTime  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| TopSliceSubnetProfile.sliceSubnetAvailability | This attribute provides information about the time at which the slice or slice subnet instance is scheduled to be available. | type: SchedulingTime  multiplicity: \*  isOrdered: False  isUnique: True  defaultValue: None  isNullable: False |
| NOTE 1: There is no direct relationship between localAddress/remoteAddress in EP\_RP and ipAddress in EP\_transport. While the localAddress/remoteAddress in EP\_RP could be exchanged as part of signalling between GTP-u tunnel end points, ipAddress in EP\_transport is used for transport routing.  NOTE 2: void  NOTE 3: energy efficiency requirement for V2X is not part of the current document. | | |

|  |
| --- |
| **Next change** |

Forge MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1153> at commit 4d5ff5bd5fcf783899c775cf14a283ea903da7f5

\*\*\* START OF CHANGE 1 \*\*\*

\*\*\* OpenAPI/TS28541\_NrNrm.yaml \*\*\*

<CODE BEGINS>

openapi: 3.0.1

info:

title: NR NRM

version: 18.7.0

description: >-

OAS 3.0.1 specification of the NR NRM

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.541; 5G NRM, NR NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

GnbId:

type: integer

minimum: 0

maximum: 4294967295

GnbIdLength:

type: integer

minimum: 22

maximum: 32

GnbName:

type: string

maxLength: 150

GnbDuId:

type: integer

minimum: 0

maximum: 68719476735

GnbCuUpId:

type: integer

minimum: 0

maximum: 68719476735

Sst:

type: integer

minimum: 0

maximum: 255

Snssai:

type: object

properties:

sst:

$ref: '#/components/schemas/Sst'

sd:

type: string

pattern: '^[A-Fa-f0-9]{6}$'

PlmnIdList:

type: array

items:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

PlmnInfo:

type: object

properties:

plmnId:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

snssai:

$ref: '#/components/schemas/Snssai'

sliceExpiryTime:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

PlmnInfoList:

type: array

items:

$ref: '#/components/schemas/PlmnInfo'

cagId:

type: string

nid:

type: string

NpnIdentity:

type: object

oneOf:

- required: [ plmnId, cagidList ]

- required: [ plmnId, nidList ]

properties:

plmnId:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

cagidList:

type: array

items:

$ref: '#/components/schemas/cagId'

minItems: 1

maxItems: 12

nidList:

type: array

items:

$ref: '#/components/schemas/nid'

minItems: 1

maxItems: 12

NpnIdentityList:

type: array

items:

$ref: '#/components/schemas/NpnIdentity'

GGnbId:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-(22|23|24|25|26|27|28|29|30|31|32)-[0-9]{1,10}'

GEnbId:

type: string

pattern: '^[0-9]{3}[0-9]{2,3}-(18|20|21|22)-[0-9]{1,7}'

GGnbIdList:

type: array

items:

$ref: '#/components/schemas/GGnbId'

GEnbIdList:

type: array

items:

$ref: '#/components/schemas/GEnbId'

NrPci:

type: integer

maximum: 503

NrTac:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Tac'

NrTacList:

type: array

items:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Tac'

TaiList:

type: array

items:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Tai'

BackhaulAddress:

type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

tai:

$ref: "TS28623\_GenericNrm.yaml#/components/schemas/Tai"

MappingSetIDBackhaulAddress:

type: object

properties:

setID:

type: integer

backhaulAddress:

$ref: '#/components/schemas/BackhaulAddress'

IntraRatEsActivationOriginalCellLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

IntraRatEsActivationCandidateCellsLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

IntraRatEsDeactivationCandidateCellsLoadParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

EsNotAllowedTimePeriod:

type: object

properties:

startTimeandendTime:

type: string

periodOfDay:

type: string

daysOfWeekList:

type: string

listoftimeperiods:

type: string

InterRatEsActivationOriginalCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

InterRatEsActivationCandidateCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

InterRatEsDeactivationCandidateCellParameters:

type: object

properties:

loadThreshold:

type: integer

timeDuration:

type: integer

UeAccProbabilityDist:

type: object

properties:

targetProbability:

type: integer

numberofpreamblessent:

type: integer

UeAccDelayProbabilityDist:

type: object

properties:

targetProbability:

type: integer

accessdelay:

type: integer

NRPciList:

type: array

items:

$ref: '#/components/schemas/NrPci'

minItems: 0

maxItems: 1007

CSonPciList:

type: array

items:

$ref: '#/components/schemas/NrPci'

minItems: 1

maxItems: 100

MaximumDeviationHoTrigger:

type: integer

minimum: -20

maximum: 20

MaximumDeviationHoTriggerLow:

type: integer

minimum: -20

maximum: 20

MaximumDeviationHoTriggerHigh:

type: integer

minimum: -20

maximum: 20

MinimumTimeBetweenHoTriggerChange:

type: integer

minimum: 0

maximum: 604800

TstoreUEcntxt:

type: integer

minimum: 0

maximum: 1023

CellState:

type: string

enum:

- IDLE

- INACTIVE

- ACTIVE

CyclicPrefix:

type: string

enum:

- '15'

- '30'

- '60'

- '120'

TxDirection:

type: string

enum:

- DL

- UL

- DL\_AND\_UL

BwpContext:

type: string

enum:

- DL

- UL

- SUL

IsInitialBwp:

type: string

enum:

- INITIAL

- OTHER

- SUL

IsESCoveredBy:

type: string

enum:

- NO

- PARTIAL

- FULL

RrmPolicyMember:

type: object

properties:

plmnId:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

snssai:

$ref: '#/components/schemas/Snssai'

RrmPolicyMemberList:

type: array

items:

$ref: '#/components/schemas/RrmPolicyMember'

AddressWithVlan:

type: object

properties:

ipv4Address:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv6Addr'

vlanId:

type: integer

minimum: 0

maximum: 4096

LocalAddress:

type: object

properties:

addressWithVlan:

$ref: '#/components/schemas/AddressWithVlan'

port:

type: integer

minimum: 0

maximum: 65535

RemoteAddress:

type: object

properties:

ipv4Address:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv4Addr'

ipv6Address:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv6Addr'

CellIndividualOffset:

type: object

properties:

rsrpOffsetSSB:

type: integer

rsrqOffsetSSB:

type: integer

sinrOffsetSSB:

type: integer

rsrpOffsetCSI-RS:

type: integer

rsrqOffsetCSI-RS:

type: integer

sinrOffsetCSI-RS:

type: integer

QOffsetRange:

type: integer

enum:

- -24

- -22

- -20

- -18

- -16

- -14

- -12

- -10

- -8

- -6

- -5

- -4

- -3

- -2

- -1

- 0

- 24

- 22

- 20

- 18

- 16

- 14

- 12

- 10

- 8

- 6

- 5

- 4

- 3

- 2

- 1

QOffsetRangeList:

type: object

properties:

rsrpOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

rsrqOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

sinrOffsetSSB:

$ref: '#/components/schemas/QOffsetRange'

rsrpOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

rsrqOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

sinrOffsetCSI-RS:

$ref: '#/components/schemas/QOffsetRange'

QOffsetFreq:

type: number

TReselectionNRSf:

type: integer

enum:

- 25

- 50

- 75

- 100

SsbPeriodicity:

type: integer

enum:

- 5

- 10

- 20

- 40

- 80

- 160

SsbDuration:

type: integer

enum:

- 1

- 2

- 3

- 4

- 5

SsbSubCarrierSpacing:

type: integer

enum:

- 15

- 30

- 120

- 240

CoverageShape:

type: integer

maximum: 65535

DigitalTilt:

type: integer

minimum: -900

maximum: 900

DigitalAzimuth:

type: integer

minimum: -1800

maximum: 1800

RSSetId:

type: integer

maximum: 4194303

RSSetType:

type: string

enum:

- RS1

- RS2

FrequencyDomainPara:

type: object

properties:

rimRSSubcarrierSpacing:

type: integer

rIMRSBandwidth:

type: integer

nrofGlobalRIMRSFrequencyCandidates:

type: integer

rimRSCommonCarrierReferencePoint:

type: integer

rimRSStartingFrequencyOffsetIdList:

type: array

items:

type: integer

SequenceDomainPara:

type: object

properties:

nrofRIMRSSequenceCandidatesofRS1:

type: integer

rimRSScrambleIdListofRS1:

type: array

items:

type: integer

nrofRIMRSSequenceCandidatesofRS2:

type: integer

rimRSScrambleIdListofRS2:

type: array

items:

type: integer

enableEnoughNotEnoughIndication:

type: string

enum:

- ENABLE

- DISABLE

RIMRSScrambleTimerMultiplier:

type: integer

RIMRSScrambleTimerOffset:

type: integer

TimeDomainPara:

type: object

properties:

dlULSwitchingPeriod1:

type: string

enum:

- MS0P5

- MS0P625

- MS1

- MS1P25

- MS2

- MS2P5

- MS3

- MS4

- MS5

- MS10

- MS20

symbolOffsetOfReferencePoint1:

type: integer

dlULSwitchingPeriod2:

type: string

enum:

- MS0P5

- MS0P625

- MS1

- MS1P25

- MS2

- MS2P5

- MS3

- MS4

- MS5

- MS10

- MS20

symbolOffsetOfReferencePoint2:

type: integer

totalnrofSetIdofRS1:

type: integer

totalnrofSetIdofRS2:

type: integer

nrofConsecutiveRIMRS1:

type: integer

nrofConsecutiveRIMRS2:

type: integer

consecutiveRIMRS1List:

type: array

items:

type: integer

consecutiveRIMRS2List:

type: array

items:

type: integer

enablenearfarIndicationRS1:

type: string

enum:

- ENABLE

- DISABLE

enablenearfarIndicationRS2:

type: string

enum:

- ENABLE

- DISABLE

RimRSReportInfo:

type: object

properties:

detectedSetID:

type: integer

propagationDelay:

type: integer

functionalityOfRIMRS:

type: string

enum:

- RS1

- RS2

- RS1\_FOR\_ENOUGH\_MITIGATION

- RS1\_FOR\_NOT\_ENOUGH\_MITIGATION

RimRSReportConf:

type: object

properties:

reportIndicator:

type: string

enum:

- ENABLE

- DISABLE

reportInterval:

type: integer

nrofRIMRSReportInfo:

type: integer

maxPropagationDelay:

type: integer

rimRSReportInfoList:

type: array

items:

$ref: '#/components/schemas/RimRSReportInfo'

TceMappingInfo:

type: object

properties:

TceIPAddress:

oneOf:

- $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv4Addr'

- $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv6Addr'

TceID:

type: integer

PlmnTarget:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

TceMappingInfoList:

type: array

items:

$ref: '#/components/schemas/TceMappingInfo'

ResourceType:

type: string

enum:

- PRB

- PRB\_UL

- PRB\_DL

- RRC\_CONNECTED\_USERS

- DRB

ParameterRange:

type: object

properties:

maxValue:

type: integer

minValue:

type: integer

NTNTAClist:

type: array

items:

$ref: '#/components/schemas/NrTac'

Ephemeris:

type: object

oneOf:

- required: [ positionVelocity ]

- required: [ orbital ]

required:

- satelliteId

- epochTime

properties:

satelliteId:

type: string

pattern: '^[0-9]{5}$'

epochTime:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

positionVelocity:

$ref: '#/components/schemas/PositionVelocity'

orbital:

$ref: '#/components/schemas/Orbital'

EphemerisInfos:

type: array

items:

$ref: '#/components/schemas/Ephemeris'

PositionVelocity:

type: object

properties:

positionX:

type: integer

minimum: 0

maximum: 604800

positionY:

type: integer

minimum: 0

maximum: 604800

positionZ:

type: integer

minimum: 0

maximum: 604800

velocityVX:

type: integer

minimum: -131072

maximum: 131071

velocityVY:

type: integer

minimum: -131072

maximum: 131071

velocityVZ:

type: integer

minimum: -131072

maximum: 131071

Orbital:

type: object

properties:

semiMajorAxis:

type: integer

minimum: 0

maximum: 8589934591

eccentricity:

type: integer

minimum: -524288

maximum: 524287

periapsis:

type: integer

minimum: 0

maximum: 16777215

longitude:

type: integer

minimum: 0

maximum: 2097151

inclination:

type: integer

minimum: -524288

maximum: 524287

meanAnomaly:

type: integer

minimum: 0

maximum: 16777215

MappedCellIdInfo:

type: object

properties:

ntnGeoArea:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/GeoArea'

mappedCellId:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Ncgi'

MappedCellIdInfoList:

type: array

items:

$ref: '#/components/schemas/MappedCellIdInfo'

#-------- Definition of types for name-containments ------

SubNetwork-ncO-NrNrm:

type: object

properties:

NRFrequency:

$ref: '#/components/schemas/NRFrequency-Multiple'

ExternalGnbCuCpFunction:

$ref: '#/components/schemas/ExternalGnbCuCpFunction-Multiple'

ExternalGnbCuUpFunction:

$ref: '#/components/schemas/ExternalGnbCuUpFunction-Multiple'

ExternalGnbDuFunction:

$ref: '#/components/schemas/ExternalGnbDuFunction-Multiple'

ExternalENBFunction:

$ref: '#/components/schemas/ExternalENBFunction-Multiple'

EUtranFrequency:

$ref: '#/components/schemas/EUtranFrequency-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

Configurable5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

RimRSGlobal:

$ref: '#/components/schemas/RimRSGlobal-Single'

Dynamic5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

CCOFunction:

$ref: '#/components/schemas/CCOFunction-Single'

ManagedElement-ncO-NrNrm:

type: object

properties:

GnbDuFunction:

$ref: '#/components/schemas/GnbDuFunction-Multiple'

GnbCuUpFunction:

$ref: '#/components/schemas/GnbCuUpFunction-Multiple'

GnbCuCpFunction:

$ref: '#/components/schemas/GnbCuCpFunction-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

Configurable5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

#-------- Definition of abstract IOCs --------------------------------------------

RrmPolicy\_-Attr:

type: object

properties:

resourceType:

$ref: '#/components/schemas/ResourceType'

rRMPolicyMemberList:

$ref: '#/components/schemas/RrmPolicyMemberList'

#-------- Definition of concrete IOCs --------------------------------------------

MnS:

oneOf:

- type: object

properties:

SubNetwork:

type: array

items:

$ref: '#/components/schemas/SubNetwork-ncO-NrNrm'

- type: object

properties:

ManagedElement:

type: array

items:

$ref: '#/components/schemas/ManagedElement-ncO-NrNrm'

GnbDuFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbDuId:

$ref: '#/components/schemas/GnbDuId'

gnbDuName:

$ref: '#/components/schemas/GnbName'

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

rimRSReportConf:

$ref: '#/components/schemas/RimRSReportConf'

configurable5QISetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NrCellDu:

$ref: '#/components/schemas/NrCellDu-Multiple'

Bwp-Multiple:

$ref: '#/components/schemas/Bwp-Multiple'

NrSectorCarrier-Multiple:

$ref: '#/components/schemas/NrSectorCarrier-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

OperatorDU:

$ref: '#/components/schemas/OperatorDu-Multiple'

BWPSet:

$ref: '#/components/schemas/BWPSet-Multiple'

Configurable5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

OperatorDu-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- type: object

properties:

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

configurable5QISetRef:

description: This attribute is condition optional. The condition is NG-RAN Multi-Operator Core Network (NG-RAN MOCN) network sharing with operator specific 5QI is supported.

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

dynamic5QISetRef:

description: This attribute is condition optional. The condition is NG-RAN Multi-Operator Core Network (NG-RAN MOCN) network sharing with operator specific 5QI is supported.

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

NrOperatorCellDu:

$ref: '#/components/schemas/NrOperatorCellDu-Multiple'

GnbCuUpFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

gnbCuUpId:

$ref: '#/components/schemas/GnbCuUpId'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

configurable5QISetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Single'

EP\_XnU:

$ref: '#/components/schemas/EP\_XnU-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

EP\_NgU:

$ref: '#/components/schemas/EP\_NgU-Multiple'

EP\_X2U:

$ref: '#/components/schemas/EP\_X2U-Multiple'

EP\_S1U:

$ref: '#/components/schemas/EP\_S1U-Multiple'

Configurable5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

GnbCuCpFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

gnbCuName:

$ref: '#/components/schemas/GnbName'

plmnId:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

x2BlockList:

$ref: '#/components/schemas/GGnbIdList'

xnBlockList:

$ref: '#/components/schemas/GGnbIdList'

x2AllowList:

$ref: '#/components/schemas/GGnbIdList'

xnAllowList:

$ref: '#/components/schemas/GGnbIdList'

x2HOBlockList:

$ref: '#/components/schemas/GEnbIdList'

xnHOBlackList:

$ref: '#/components/schemas/GGnbIdList'

mappingSetIDBackhaulAddress:

$ref: '#/components/schemas/MappingSetIDBackhaulAddress'

tceMappingInfoList:

$ref: '#/components/schemas/TceMappingInfoList'

configurable5QISetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

dynamic5QISetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

ephemerisInfoSetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

dCHOControl:

type: boolean

dDAPSHOControl:

type: boolean

mappedCellIdInfoList:

$ref: '#/components/schemas/MappedCellIdInfoList'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NrCellCu:

$ref: '#/components/schemas/NrCellCu-Multiple'

EP\_XnC:

$ref: '#/components/schemas/EP\_XnC-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

EP\_NgC:

$ref: '#/components/schemas/EP\_NgC-Multiple'

EP\_X2C:

$ref: '#/components/schemas/EP\_X2C-Multiple'

DANRManagementFunction:

$ref: '#/components/schemas/DANRManagementFunction-Single'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

Configurable5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Configurable5QISet-Multiple'

Dynamic5QISet:

$ref: 'TS28541\_5GcNrm.yaml#/components/schemas/Dynamic5QISet-Multiple'

NrCellCu-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

cellLocalId:

type: integer

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nRFrequencyRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

NRCellRelation:

$ref: '#/components/schemas/NRCellRelation-Multiple'

EUtranCellRelation:

$ref: '#/components/schemas/EUtranCellRelation-Multiple'

NRFreqRelation:

$ref: '#/components/schemas/NRFreqRelation-Multiple'

EUtranFreqRelation:

$ref: '#/components/schemas/EUtranFreqRelation-Multiple'

DESManagementFunction:

$ref: '#/components/schemas/DESManagementFunction-Single'

DMROFunction:

$ref: '#/components/schemas/DMROFunction-Single'

DLBOFunction:

$ref: '#/components/schemas/DLBOFunction-Single'

CESManagementFunction:

$ref: '#/components/schemas/CESManagementFunction-Single'

DPCIConfigurationFunction:

$ref: '#/components/schemas/DPCIConfigurationFunction-Single'

NrCellDu-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

administrativeState:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/OperationalState'

cellLocalId:

type: integer

cellState:

$ref: '#/components/schemas/CellState'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

npnIdentityList:

$ref: '#/components/schemas/NpnIdentityList'

nrPci:

$ref: '#/components/schemas/NrPci'

nrTac:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Tac'

arfcnDL:

type: integer

arfcnUL:

type: integer

arfcnSUL:

type: integer

bSChannelBwDL:

type: integer

bSChannelBwUL:

type: integer

bSChannelBwSUL:

type: integer

ssbFrequency:

type: integer

minimum: 0

maximum: 3279165

ssbPeriodicity:

$ref: '#/components/schemas/SsbPeriodicity'

ssbSubCarrierSpacing:

$ref: '#/components/schemas/SsbSubCarrierSpacing'

ssbOffset:

type: integer

minimum: 0

maximum: 159

ssbDuration:

$ref: '#/components/schemas/SsbDuration'

nrSectorCarrierRef:

type: array

items:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

bwpRef:

description: "Condition is BWP sets are not supported"

type: array

items:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

bwpSetRef:

description: "Condition is BWP sets are supported"

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

rimRSMonitoringStartTime:

type: string

rimRSMonitoringStopTime:

type: string

rimRSMonitoringWindowDuration:

type: integer

rimRSMonitoringWindowStartingOffset:

type: integer

rimRSMonitoringWindowPeriodicity:

type: integer

rimRSMonitoringOccasionInterval:

type: integer

rimRSMonitoringOccasionStartingOffset:

type: integer

nRFrequencyRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

victimSetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

aggressorSetRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

RRMPolicyRatio:

$ref: '#/components/schemas/RRMPolicyRatio-Multiple'

CPCIConfigurationFunction:

$ref: '#/components/schemas/CPCIConfigurationFunction-Single'

DRACHOptimizationFunction:

$ref: '#/components/schemas/DRACHOptimizationFunction-Single'

BWPSet-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

bWPlist:

type: array

items:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

maxItems: 12

NrOperatorCellDu-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

cellLocalId:

type: integer

administrativeState:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/AdministrativeState'

plmnInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nrTac:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Tac'

NRFrequency-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

absoluteFrequencySSB:

type: integer

minimum: 0

maximum: 3279165

ssbSubCarrierSpacing:

$ref: '#/components/schemas/SsbSubCarrierSpacing'

multiFrequencyBandListNR:

type: integer

minimum: 1

maximum: 256

EUtranFrequency-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

earfcnDL:

type: integer

minimum: 0

maximum: 262143

multiBandInfoListEutra:

type: integer

minimum: 1

maximum: 256

NrSectorCarrier-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

txDirection:

$ref: '#/components/schemas/TxDirection'

configuredMaxTxPower:

type: integer

arfcnDL:

type: integer

arfcnUL:

type: integer

bSChannelBwDL:

type: integer

bSChannelBwUL:

type: integer

sectorEquipmentFunctionRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

CommonBeamformingFunction:

$ref: '#/components/schemas/CommonBeamformingFunction-Single'

Bwp-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

bwpContext:

$ref: '#/components/schemas/BwpContext'

isInitialBwp:

$ref: '#/components/schemas/IsInitialBwp'

subCarrierSpacing:

type: integer

cyclicPrefix:

$ref: '#/components/schemas/CyclicPrefix'

startRB:

type: integer

numberOfRBs:

type: integer

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

CommonBeamformingFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

coverageShape:

$ref: '#/components/schemas/CoverageShape'

digitalAzimuth:

$ref: '#/components/schemas/DigitalAzimuth'

digitalTilt:

$ref: '#/components/schemas/DigitalTilt'

- type: object

properties:

Beam:

$ref: '#/components/schemas/Beam-Multiple'

Beam-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

beamIndex:

type: integer

beamType:

type: string

enum:

- SSB\_BEAM

beamAzimuth:

type: integer

minimum: -1800

maximum: 1800

beamTilt:

type: integer

minimum: -900

maximum: 900

beamHorizWidth:

type: integer

minimum: 0

maximum: 3599

beamVertWidth:

type: integer

minimum: 0

maximum: 1800

RRMPolicyRatio-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: '#/components/schemas/RrmPolicy\_-Attr'

- type: object

properties:

rRMPolicyMaxRatio:

type: integer

default: 100

minimum: 0

maximum: 100

rRMPolicyMinRatio:

type: integer

default: 0

minimum: 0

maximum: 100

rRMPolicyDedicatedRatio:

type: integer

default: 0

minimum: 0

maximum: 100

NRCellRelation-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

nRTCI:

type: integer

cellIndividualOffset:

$ref: '#/components/schemas/CellIndividualOffset'

adjacentNRCellRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

nRFreqRelationRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

isRemoveAllowed:

type: boolean

isHOAllowed:

type: boolean

isESCoveredBy:

$ref: '#/components/schemas/IsESCoveredBy'

isENDCAllowed:

type: boolean

isMLBAllowed:

type: boolean

EUtranCellRelation-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

adjacentEUtranCellRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

NRFreqRelation-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

offsetMO:

$ref: '#/components/schemas/QOffsetRangeList'

blockListEntry:

type: array

items:

type: integer

minimum: 0

maximum: 1007

blockListEntryIdleMode:

type: integer

cellReselectionPriority:

type: integer

cellReselectionSubPriority:

type: number

minimum: 0.2

maximum: 0.8

multipleOf: 0.2

pMax:

type: integer

minimum: -30

maximum: 33

qOffsetFreq:

$ref: '#/components/schemas/QOffsetFreq'

qQualMin:

type: number

qRxLevMin:

type: integer

minimum: -140

maximum: -44

threshXHighP:

type: integer

minimum: 0

maximum: 62

threshXHighQ:

type: integer

minimum: 0

maximum: 31

threshXLowP:

type: integer

minimum: 0

maximum: 62

threshXLowQ:

type: integer

minimum: 0

maximum: 31

tReselectionNr:

type: integer

minimum: 0

maximum: 7

tReselectionNRSfHigh:

$ref: '#/components/schemas/TReselectionNRSf'

tReselectionNRSfMedium:

$ref: '#/components/schemas/TReselectionNRSf'

nRFrequencyRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

EUtranFreqRelation-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cellIndividualOffset:

$ref: '#/components/schemas/CellIndividualOffset'

blackListEntry:

type: array

items:

type: integer

minimum: 0

maximum: 1007

blackListEntryIdleMode:

type: integer

cellReselectionPriority:

type: integer

cellReselectionSubPriority:

type: number

minimum: 0.2

maximum: 0.8

multipleOf: 0.2

pMax:

type: integer

minimum: -30

maximum: 33

qOffsetFreq:

$ref: '#/components/schemas/QOffsetFreq'

qQualMin:

type: number

qRxLevMin:

type: integer

minimum: -140

maximum: -44

threshXHighP:

type: integer

minimum: 0

maximum: 62

threshXHighQ:

type: integer

minimum: 0

maximum: 31

threshXLowP:

type: integer

minimum: 0

maximum: 62

threshXLowQ:

type: integer

minimum: 0

maximum: 31

tReselectionEutran:

type: integer

minimum: 0

maximum: 7

tReselectionNRSfHigh:

$ref: '#/components/schemas/TReselectionNRSf'

tReselectionNRSfMedium:

$ref: '#/components/schemas/TReselectionNRSf'

eUTranFrequencyRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

DANRManagementFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

intrasystemANRManagementSwitch:

type: boolean

intersystemANRManagementSwitch:

type: boolean

DESManagementFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

desSwitch:

type: boolean

intraRatEsActivationOriginalCellLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

intraRatEsActivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationCandidateCellsLoadParameters"

intraRatEsDeactivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsDeactivationCandidateCellsLoadParameters"

esNotAllowedTimePeriod:

$ref: "#/components/schemas/EsNotAllowedTimePeriod"

interRatEsActivationOriginalCellParameters:

$ref: "#/components/schemas/InterRatEsActivationOriginalCellParameters"

interRatEsActivationCandidateCellParameters:

$ref: "#/components/schemas/InterRatEsActivationCandidateCellParameters"

interRatEsDeactivationCandidateCellParameters:

$ref: "#/components/schemas/InterRatEsDeactivationCandidateCellParameters"

isProbingCapable:

type: string

enum:

- YES

- NO

energySavingState:

type: string

enum:

- IS\_NOT\_ENERGY\_SAVING

- IS\_ENERGY\_SAVING

mLModelRefList:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

aIMLInferenceFunctionRefList:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

DRACHOptimizationFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

drachOptimizationControl:

type: boolean

ueAccProbabilityDist:

$ref: "#/components/schemas/UeAccProbabilityDist"

ueAccDelayProbabilityDist:

$ref: "#/components/schemas/UeAccDelayProbabilityDist"

DMROFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dmroControl:

type: boolean

maximumDeviationHoTriggerLow:

$ref: '#/components/schemas/MaximumDeviationHoTriggerLow'

maximumDeviationHoTriggerHigh:

$ref: '#/components/schemas/MaximumDeviationHoTriggerHigh'

minimumTimeBetweenHoTriggerChange:

$ref: '#/components/schemas/MinimumTimeBetweenHoTriggerChange'

tstoreUEcntxt:

$ref: '#/components/schemas/TstoreUEcntxt'

mLModelRefList:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

aIMLInferenceFunctionRefList:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

DLBOFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dlboControl:

type: boolean

maximumDeviationHoTrigger:

$ref: '#/components/schemas/MaximumDeviationHoTrigger'

minimumTimeBetweenHoTriggerChange:

$ref: '#/components/schemas/MinimumTimeBetweenHoTriggerChange'

mLModelRefList:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

aIMLInferenceFunctionRefList:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

DPCIConfigurationFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dPciConfigurationControl:

type: boolean

nRPciList:

$ref: "#/components/schemas/NRPciList"

CPCIConfigurationFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cPciConfigurationControl:

type: boolean

cSonPciList:

$ref: "#/components/schemas/CSonPciList"

CESManagementFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cesSwitch:

type: boolean

intraRatEsActivationOriginalCellLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

intraRatEsActivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsActivationCandidateCellsLoadParameters"

intraRatEsDeactivationCandidateCellsLoadParameters:

$ref: "#/components/schemas/IntraRatEsDeactivationCandidateCellsLoadParameters"

esNotAllowedTimePeriod:

$ref: "#/components/schemas/EsNotAllowedTimePeriod"

interRatEsActivationOriginalCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsActivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

interRatEsDeactivationCandidateCellParameters:

$ref: "#/components/schemas/IntraRatEsActivationOriginalCellLoadParameters"

energySavingControl:

type: string

enum:

- TO\_BE\_ENERGY\_SAVING

- TO\_BE\_NOT\_ENERGY\_SAVING

energySavingState:

type: string

enum:

- IS\_NOT\_ENERGY\_SAVING

- IS\_ENERGY\_SAVING

RimRSGlobal-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

frequencyDomainPara:

$ref: '#/components/schemas/FrequencyDomainPara'

sequenceDomainPara:

$ref: '#/components/schemas/SequenceDomainPara'

timeDomainPara:

$ref: '#/components/schemas/TimeDomainPara'

RimRSSet:

$ref: '#/components/schemas/RimRSSet-Multiple'

RimRSSet-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

setId:

$ref: '#/components/schemas/RSSetId'

setType:

$ref: '#/components/schemas/RSSetType'

nRCellDURefs:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

ExternalGnbDuFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

ExternalGnbCuUpFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1U:

$ref: '#/components/schemas/EP\_F1U-Multiple'

EP\_XnU:

$ref: '#/components/schemas/EP\_XnU-Multiple'

ExternalGnbCuCpFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: >-

TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr

- type: object

properties:

gnbId:

$ref: '#/components/schemas/GnbId'

gnbIdLength:

$ref: '#/components/schemas/GnbIdLength'

plmnId:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

ExternalNrCellCu:

$ref: '#/components/schemas/ExternalNrCellCu-Multiple'

EP\_XnC:

$ref: '#/components/schemas/EP\_XnC-Multiple'

EP\_E1:

$ref: '#/components/schemas/EP\_E1-Multiple'

EP\_F1C:

$ref: '#/components/schemas/EP\_F1C-Multiple'

ExternalNrCellCu-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

cellLocalId:

type: integer

nrPci:

$ref: '#/components/schemas/NrPci'

plmnIdList:

$ref: '#/components/schemas/PlmnIdList'

nRFrequencyRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

ExternalENBFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

eNBId:

type: integer

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

- type: object

properties:

ExternalEUTranCell:

$ref: '#/components/schemas/ExternalEUTranCell-Multiple'

ExternalEUTranCell-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

- type: object

properties:

EUtranFrequencyRef:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

EP\_XnC-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_E1-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_F1C-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_NgC-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_X2C-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_XnU-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_F1U-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

epTransportRefs:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

EP\_NgU-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

epTransportRefs:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

EP\_X2U-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

EP\_S1U-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/EP\_RP-Attr'

- type: object

properties:

localAddress:

$ref: '#/components/schemas/LocalAddress'

remoteAddress:

$ref: '#/components/schemas/RemoteAddress'

CCOFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

cCOControl:

type: boolean

cCOWeakCoverageParameters:

$ref: '#/components/schemas/CCOWeakCoverageParameters-Single'

cCOPilotPollutionParameters:

$ref: '#/components/schemas/CCOPilotPollutionParameters-Single'

cCOOvershootCoverageParameters-Single:

$ref: '#/components/schemas/CCOOvershootCoverageParameters-Single'

CCOParameters-Attr:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

coverageShapeList:

type: integer

downlinkTransmitPowerRange:

$ref: '#/components/schemas/ParameterRange'

antennaTiltRange:

$ref: '#/components/schemas/ParameterRange'

antennaAzimuthRange:

$ref: '#/components/schemas/ParameterRange'

digitalTiltRange:

$ref: '#/components/schemas/ParameterRange'

digitalAzimuthRange:

$ref: '#/components/schemas/ParameterRange'

CCOWeakCoverageParameters-Single:

allOf:

- $ref: '#/components/schemas/CCOParameters-Attr'

- type: object

CCOPilotPollutionParameters-Single:

allOf:

- $ref: '#/components/schemas/CCOParameters-Attr'

- type: object

CCOOvershootCoverageParameters-Single:

allOf:

- $ref: '#/components/schemas/CCOParameters-Attr'

- type: object

NTNFunction-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

nTNpLMNInfoList:

$ref: '#/components/schemas/PlmnInfoList'

nTNTAClist:

$ref: '#/components/schemas/NrTacList'

ephemerisInfoSet:

$ref: '#/components/schemas/EphemerisInfoSet-Multiple'

EphemerisInfoSet-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

ephemerisInfos:

$ref: '#/components/schemas/EphemerisInfos'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

GnbDuFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbDuFunction-Single'

OperatorDu-Multiple:

type: array

items:

$ref: '#/components/schemas/OperatorDu-Single'

GnbCuUpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbCuUpFunction-Single'

GnbCuCpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/GnbCuCpFunction-Single'

BWPSet-Multiple:

type: array

items:

$ref: '#/components/schemas/BWPSet-Single'

NrCellDu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrCellDu-Single'

NrOperatorCellDu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrOperatorCellDu-Single'

NrCellCu-Multiple:

type: array

items:

$ref: '#/components/schemas/NrCellCu-Single'

NRFrequency-Multiple:

type: array

minItems: 1

items:

$ref: '#/components/schemas/NRFrequency-Single'

EUtranFrequency-Multiple:

type: array

minItems: 1

items:

$ref: '#/components/schemas/EUtranFrequency-Single'

NrSectorCarrier-Multiple:

type: array

items:

$ref: '#/components/schemas/NrSectorCarrier-Single'

Bwp-Multiple:

type: array

items:

$ref: '#/components/schemas/Bwp-Single'

Beam-Multiple:

type: array

items:

$ref: '#/components/schemas/Beam-Single'

RRMPolicyRatio-Multiple:

type: array

items:

$ref: '#/components/schemas/RRMPolicyRatio-Single'

NRCellRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/NRCellRelation-Single'

EUtranCellRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/EUtranCellRelation-Single'

NRFreqRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/NRFreqRelation-Single'

EUtranFreqRelation-Multiple:

type: array

items:

$ref: '#/components/schemas/EUtranFreqRelation-Single'

RimRSSet-Multiple:

type: array

items:

$ref: '#/components/schemas/RimRSSet-Single'

ExternalGnbDuFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbDuFunction-Single'

ExternalGnbCuUpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbCuUpFunction-Single'

ExternalGnbCuCpFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalGnbCuCpFunction-Single'

ExternalNrCellCu-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalNrCellCu-Single'

ExternalENBFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalENBFunction-Single'

ExternalEUTranCell-Multiple:

type: array

items:

$ref: '#/components/schemas/ExternalEUTranCell-Single'

EP\_E1-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_E1-Single'

EP\_XnC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_XnC-Single'

EP\_F1C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_F1C-Single'

EP\_NgC-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NgC-Single'

EP\_X2C-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_X2C-Single'

EP\_XnU-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_XnU-Single'

EP\_F1U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_F1U-Single'

EP\_NgU-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_NgU-Single'

EP\_X2U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_X2U-Single'

EP\_S1U-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_S1U-Single'

EphemerisInfoSet-Multiple:

type: array

items:

$ref: '#/components/schemas/EphemerisInfoSet-Single'

#-------- Definitions in TS 28.541 for TS 28.532 ---------------------------------

resources-nrNrm:

oneOf:

- $ref: '#/components/schemas/MnS'

- $ref: '#/components/schemas/GnbDuFunction-Single'

- $ref: '#/components/schemas/GnbCuUpFunction-Single'

- $ref: '#/components/schemas/GnbCuCpFunction-Single'

- $ref: '#/components/schemas/OperatorDu-Single'

- $ref: '#/components/schemas/NrCellCu-Single'

- $ref: '#/components/schemas/NrCellDu-Single'

- $ref: '#/components/schemas/NrOperatorCellDu-Single'

- $ref: '#/components/schemas/NRFrequency-Single'

- $ref: '#/components/schemas/EUtranFrequency-Single'

- $ref: '#/components/schemas/NrSectorCarrier-Single'

- $ref: '#/components/schemas/Bwp-Single'

- $ref: '#/components/schemas/BWPSet-Single'

- $ref: '#/components/schemas/CommonBeamformingFunction-Single'

- $ref: '#/components/schemas/Beam-Single'

- $ref: '#/components/schemas/RRMPolicyRatio-Single'

- $ref: '#/components/schemas/NRCellRelation-Single'

- $ref: '#/components/schemas/EUtranCellRelation-Single'

- $ref: '#/components/schemas/NRFreqRelation-Single'

- $ref: '#/components/schemas/EUtranFreqRelation-Single'

- $ref: '#/components/schemas/DANRManagementFunction-Single'

- $ref: '#/components/schemas/DESManagementFunction-Single'

- $ref: '#/components/schemas/DRACHOptimizationFunction-Single'

- $ref: '#/components/schemas/DMROFunction-Single'

- $ref: '#/components/schemas/DLBOFunction-Single'

- $ref: '#/components/schemas/DPCIConfigurationFunction-Single'

- $ref: '#/components/schemas/CPCIConfigurationFunction-Single'

- $ref: '#/components/schemas/CESManagementFunction-Single'

- $ref: '#/components/schemas/RimRSGlobal-Single'

- $ref: '#/components/schemas/RimRSSet-Single'

- $ref: '#/components/schemas/ExternalGnbDuFunction-Single'

- $ref: '#/components/schemas/ExternalGnbCuUpFunction-Single'

- $ref: '#/components/schemas/ExternalGnbCuCpFunction-Single'

- $ref: '#/components/schemas/ExternalNrCellCu-Single'

- $ref: '#/components/schemas/ExternalENBFunction-Single'

- $ref: '#/components/schemas/ExternalEUTranCell-Single'

- $ref: '#/components/schemas/EP\_XnC-Single'

- $ref: '#/components/schemas/EP\_E1-Single'

- $ref: '#/components/schemas/EP\_F1C-Single'

- $ref: '#/components/schemas/EP\_NgC-Single'

- $ref: '#/components/schemas/EP\_X2C-Single'

- $ref: '#/components/schemas/EP\_XnU-Single'

- $ref: '#/components/schemas/EP\_F1U-Single'

- $ref: '#/components/schemas/EP\_NgU-Single'

- $ref: '#/components/schemas/EP\_X2U-Single'

- $ref: '#/components/schemas/EP\_S1U-Single'

- $ref: '#/components/schemas/CCOFunction-Single'

- $ref: '#/components/schemas/CCOWeakCoverageParameters-Single'

- $ref: '#/components/schemas/CCOPilotPollutionParameters-Single'

- $ref: '#/components/schemas/CCOOvershootCoverageParameters-Single'

- $ref: '#/components/schemas/NTNFunction-Single'

- $ref: '#/components/schemas/EphemerisInfoSet-Single'

<CODE ENDS>

\*\*\* END OF CHANGE 1 \*\*\*

|  |
| --- |
| **End of change** |