**3GPP TSG-SA5 Meeting #155 *S5-243288***

Jeju, South Korea, 27 – 31 May 2024

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.622** | **CR** | **0395** | **rev** | **1** | **Current version:** | **18.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Rel-19 CR 28.622 areaScope clarifications  |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | **TraceQoE\_OAM** |  | ***Date:*** | 2024-05-15 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Area Scope defined in TS28.622 is used in TraceJob for Trace and MDT, it is also used in QMCJob for QoE. However, Area Scope definiation is not excetly same for Trace and QMC. The current areaScope datatype is only referring to areaScope for TraceJob. The reference to QMCJob is missing.  |
|  |  |
| ***Summary of change:*** | Adding clairfications on area scope definition |
|  |  |
| ***Consequences if not approved:*** | Unclear statement which may mislead on implementations  |
|  |  |
| ***Clauses affected:*** | 4.3.38.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of 242829 |

\*\*\* START OF NEXT CHANGE \*\*\*

#### 4.3.38.1 Definition

This <<dataType>> defines the area scope of MDT and QoE. The Area Scope for MDT is specified in clause 5.10.2 of TS 32.422 [30]. The Area Scope for QoE is specified in clause 5.4 of TS 28.405 [50].

\*\*\* END OF CHANGE \*\*\*