**3GPP TSG- Meeting #**

**Jeju, South Korea, 27 – 31 May 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | 8 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In SA5#154, a new attribute in QMC job has been agreed as part of S5-242029. This has not been added to the stage 3 YAML code. This CR propose to update the Stage 3 aligning with Stage 2 agreement. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The stage 3 for QMC job YAML is updated with the attribute mBSCommunicationServiceType | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplete stage 3 YAML code | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | FORGE | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1156> | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | S5-243370 is a revision of S5-242676 | | | | | | | | |

Forge MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1156> at commit 6d720f3703f73367784f9dc1256c4343a5d3a2a8

\*\*\* START OF CHANGE 1 \*\*\*

\*\*\* OpenAPI/TS28623\_QoEMeasurementCollectionNrm.yaml \*\*\*

<CODE BEGINS>

openapi: 3.0.1

info:

title: QoE Measurement Collection NRM

version: 18.6.0

description: >-

OAS 3.0.1 definition of the QoE Measurement Collection NRM

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.623; Generic NRM,QoE Measurement Collection NRM fragment

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.623/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

#-------- Definition of concrete IOCs --------------------------------------------

QMCJob-Single:

allOf:

- $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

serviceType:

type: string

enum:

- DASH

- MTSI

- VR

areaScope:

type: array

items:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/AreaScope'

qoECollectionEntityAddress:

$ref: 'TS28623\_GenericNrm.yaml#/components/schemas/IpAddr'

pLMNTarget:

$ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

qoETarget:

type: string

qoEReference:

type: string

jobId:

type: string

sliceScope:

type: array

items:

$ref: 'TS28541\_NrNrm.yaml#/components/schemas/Snssai'

qMCConfigFile:

type: string

mDTAlignmentInformation:

$ref: 'TS28623\_TraceControlNrm.yaml#/components/schemas/traceReference-Type'

availableRANqoEMetrics:

type: array

items:

type: string

enum:

- APPLAYERBUFFERLEVELLIST

- PLAYOUTDELAYFORMEDIA\_STARTUP

minItems: 0

maxItems: 2

mBSCommunicationServiceType:

type: string

enum:

- BROADCAST

- MULTICAST

#-------- Definition of YAML arrays for name-contained IOCs ----------------------

QMCJob-Multiple:

type: array

items:

$ref: '#/components/schemas/QMCJob-Single'

#-------- Definitions in TS 28.623 for TS 28.532 ---------------------------------

resources-qoEMeasuremetCollectionNrm:

oneOf:

- $ref: '#/components/schemas/QMCJob-Single'

<CODE ENDS>

\*\*\* END OF CHANGE 1 \*\*\*