**3GPP TSG- Meeting #**

**Jeju, South Korea, 27 – 31 May 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | 8 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In SA5#154, a new attribute in QMC job has been agreed as part of S5-242029. This has not been added to the stage 3 YAML code. This CR propose to update the Stage 3 aligning with Stage 2 agreement. |
|  |  |
| ***Summary of change:*** | The stage 3 for QMC job YAML is updated with the attribute mBSCommunicationServiceType |
|  |  |
| ***Consequences if not approved:*** | Incomplete stage 3 YAML code |
|  |  |
| ***Clauses affected:*** | FORGE |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** | MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1156> |
|  |  |
| ***This CR's revision history:*** | S5-243370 is a revision of S5-242676 |

Forge MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1156> at commit 6d720f3703f73367784f9dc1256c4343a5d3a2a8

\*\*\* START OF CHANGE 1 \*\*\*

\*\*\* OpenAPI/TS28623\_QoEMeasurementCollectionNrm.yaml \*\*\*

<CODE BEGINS>

openapi: 3.0.1

info:

 title: QoE Measurement Collection NRM

 version: 18.6.0

 description: >-

 OAS 3.0.1 definition of the QoE Measurement Collection NRM

 © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.623; Generic NRM,QoE Measurement Collection NRM fragment

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.623/

paths: {}

components:

 schemas:

#-------- Definition of types-----------------------------------------------------

#-------- Definition of concrete IOCs --------------------------------------------

 QMCJob-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 serviceType:

 type: string

 enum:

 - DASH

 - MTSI

 - VR

 areaScope:

 type: array

 items:

 $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/AreaScope'

 qoECollectionEntityAddress:

 $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/IpAddr'

 pLMNTarget:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/PlmnId'

 qoETarget:

 type: string

 qoEReference:

 type: string

 jobId:

 type: string

 sliceScope:

 type: array

 items:

 $ref: 'TS28541\_NrNrm.yaml#/components/schemas/Snssai'

 qMCConfigFile:

 type: string

 mDTAlignmentInformation:

 $ref: 'TS28623\_TraceControlNrm.yaml#/components/schemas/traceReference-Type'

 availableRANqoEMetrics:

 type: array

 items:

 type: string

 enum:

 - APPLAYERBUFFERLEVELLIST

 - PLAYOUTDELAYFORMEDIA\_STARTUP

 minItems: 0

 maxItems: 2

 mBSCommunicationServiceType:

 type: string

 enum:

 - BROADCAST

 - MULTICAST

#-------- Definition of YAML arrays for name-contained IOCs ----------------------

 QMCJob-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/QMCJob-Single'

#-------- Definitions in TS 28.623 for TS 28.532 ---------------------------------

 resources-qoEMeasuremetCollectionNrm:

 oneOf:

 - $ref: '#/components/schemas/QMCJob-Single'

<CODE ENDS>

\*\*\* END OF CHANGE 1 \*\*\*