**3GPP TSG RAN #106 RP-243265**

**Madrid, Spain, December 10th – 13th, 2024**

**Title: Moderator Summary for 3T3R SRS Antennas Switching in Rel-19**

**Source: RAN1 Chair (Samsung)**

# Introduction

Rel-19 MIMO work item objectives were updated in RAN#105. In particular the following update was made for 3T3R (RP-242394):

|  |
| --- |
| 1. Specify non-coherent UL codebook to facilitate 3-antenna-port codebook-based transmissions, enhancement(s) to enable 3T6R SRS antenna switching, as well as UE capability signaling for 3T3R antenna switching and 3-antenna-port non-codebook-based transmissions, without enhancement on UL full power transmission and without enhancement on SRS resource

Note: UL full power transmission mode 1 and 2 are not supported.Note: Other than UE capability signaling, no other enhancement is specified for 3T3R SRS antenna switching. |

In RAN1, there is debate whether or not the above WID objective precludes specification change on SRS configuration details and SRS resource/set definition for ‘3T3R’ antenna switching. In RAN#106, the following tdocs were submitted on this issue:

* RP-242488 On the Scope of Rel-19 NR MIMO Phase 5 InterDigital, Inc.
* RP-242618 Discussion on 3T3R SRS antenna switching capability in Rel-19 MIMO vivo
* RP-243173 on Rel-19 MIMO 3T3R Apple

# Discussions

Moderator proposes to select one of the following 3 alternatives in RAN#106.

* Alt 1: RAN clarifies that for ‘3T3R’ antenna switching, SRS configuration details including SRS resource/set definition for ‘3T3R’ antenna switching can be discussed and supported as part of Rel-19 MIMO in RAN1
	+ Update WID accordingly
* Alt 2: Other than UE capability signaling, no other enhancement is specified for 3T3R SRS antenna switching (i.e. SRS configuration details including SRS resource/set definition for ‘3T3R’ antenna switching is not supported) as part of Rel-19 MIMO in RAN1
* Alt 3: 3T3R SRS antenna switching is not supported as part of Rel-19 MIMO
	+ Update WID accordingly

Note that the RAN1 workload required for each of the three alternatives is marginal.

Companies are invited to provide their views using the table below.

|  |  |  |
| --- | --- | --- |
| **Company** |  | **Comments** |
| vivo | Alt1 or alt 3 | In our view alt2 is not reasonable. We should not intentionally introduce a broken feature in the spec. Either we introduce a complete UE feature or we remove the UE feature. |
| Apple | Alt 1 or Alt 3 | We are fine with either Alt 1 or Alt 3. Alt 2 should be avoided. Without specifying the 3T3R features in the specification, e.g., TS38.214, we fail to see the justification to specify the corresponding UE capability. |
| OPPO | Alt.1 | We support Alt.1 in principle. In our view, the WID can kept as it is (RAN clarification is sufficient for this case) or modify it to avoid the potential confusion as suggested by Alt.1. For all the antenna configuration xTxR (x=1,2,4,8), there are descriptions on the UE capability from the perspective of the SRS configuration. Thus, it is nature to have similar description for 3T3R. If without such kind of description, the spec is broken. Thus, Alt.1 is our preference.For Alt.2, the spec will be broken. Thus, we should avoid it. For Alt.3, it will revert RAN agreement. Thus, we should avoid it. The main concern from Huawei is on a UE with only 3 physical antennas (that is the intention of the proponents). Thus, not sure whether it can address Huawei’s concern if we can agree some conclusion like: A UE supporting 3T3R antenna switching should be equipped with 4 or more physical antennas.  |
| Nokia | Alt.1 or Alt.3 | We agree with vivo and Apple above that we should only add UE feature for something that has corresponding support in specifications.  |
| InterDigital | Alt 1 with a note | We are supportive Alt 1 but we may add a note to address Huawei’s concern on introducing new type of UEs (i.e., standalone capability of 3T3R) as following:* Alt 1: RAN clarifies that for ‘3T3R’ antenna switching, SRS configuration details including SRS resource/set definition for ‘3T3R’ antenna switching can be discussed and supported as part of Rel-19 MIMO in RAN1
	+ Update WID accordingly
	+ Note: ‘3T3R’ is a downgrade antenna switching configuration of ‘3T6R’ and it doesn’t imply that standalone ‘3T3R’ capability is introduced.
 |
| Ericsson | Alt.1 (no WID change) | In favour of Alt.1 as it implies that we complete the feature RAN agreed to have in September (whereas Alt.2 is leaving a broken feature and Alt.3 is reverting previous agreement).However, we don’t see a WID update is needed in Alt.1 since the WID mentions no further *enhancements*, we don’t want to set a precedence that completing a half-done feature is seen by 3GPP as an enhancement. 3GPP should specify complete and working features. We think RAN clarification is sufficient in the line of:**Conclusion:**As a RAN guidance on the 3T3R issue, necessary specification changes needed to enable the capability “3T3R SRS antenna switching” is expected by the WIDIn addition, OPPO’s suggestion to address Huawei’s concern by a short sentence in such conclusion can be helpful to close this issue.  |
| CMCC | Alt. 1 | In our understanding, Alt.1 is the intention to support 3T3R antenna switching when we discussed the scope expansion for Rel-19 MIMO WI. The confusion in RAN1 comes from the NOTE statement in the WID “Note: Other than UE capability signaling, no other enhancement is specified for 3T3R SRS antenna switching.”Hence, we support to directly clarify in the WID that SRS configuration including SRS resource/set definition for 3T3R antenna switching should be specified in Rel-19.And to avoid the potential risk to open the door for 3R UE (not sure any company propose this), the NOTE proposal from InterDigital can be considered. |

# Conclusions

TBD