**3GPP TSG RAN WG2#127 *R2-240xxxx***

**Maastricht, Netherlands, 19th - 23rd August 2024**

**Title:** LS on IUC Scheme-2 and Random Selection

**Response to:** -

**Release:** Rel-17

**Work Items:** NR\_SL\_enh-Core

**Source:** RAN WG2

**To:** RAN WG1

**CC:**

**Contact Person:**

#### Name: Qianxi Lu

E-mail Address: qianxi.lu@oppo.com

**Attachment:**

**1. Overall Description:**

In TS 38.321, it is specified that

5.22.1.2b Re-selection for using a received resource conflict indication

If the MAC entity has been configured with Sidelink resource allocation mode 2 to transmit using pool(s) of resources in a carrier as indicated in TS 38.331 [5] based on full sensing, or partial sensing or random selection or any combination(s), the MAC entity shall for each Sidelink process:

<Text Removed>

But it is not clear to RAN2 whether the configuration of both Inter-UE coordination scheme-2 and random-selection is supported or not.

**Q1**: Is configuration of both Inter-UE coordination scheme-2 and random-selection supported or not?

**2. Actions:**

**To RAN WG1**

**ACTION:** RAN2 respectfully asks RAN1 to provide answer to **Q1** above.

**3. Date of Next RAN WG2 Meetings:**

RAN2#127-bis 2024-10-14~2024-10-18 Hefei, CN

RAN2#128 2024-11-18~2024-11-22 Orlando, US