**3GPP TSG-RAN WG2 Meeting #127**  draft-**R2-2407612**

**Maastricht, Netherlands, 19th - 23rd August 2024**

**Agenda item: 7.7.2**

**Source: Qualcomm Incorporated**

**Title: Report of [AT127][301][R18 NR NTN] corrections for satellite switch with re-sync**

**Document for: Discussion and Decision**

# Introduction

In this document, the report of the following offline discussions is provided.

**[AT127][301][R18 NR NTN] corrections for satellite switch with re-sync (Qualcomm)**

Scope: Continue the discussion on p1 and p2 in [R2-2406641](file:///C:\Data\3GPP\Extracts\R2-2406641%20issue%20on%20PCI%20unchanged.docx)

Intended outcome: report of offline discussion

Deadline for companies' feedback: Thursday 2024-08-22 20:00

Deadline for rapporteur's summary (in R2-2407612): Friday 2024-08-23 08:00

# Discussion

Following was captured during the discussion.

[R2-2406641](file:///C:\Data\3GPP\Extracts\R2-2406641%20issue%20on%20PCI%20unchanged.docx) Discussion on soft satellite switch with re-sync Qualcomm Incorporated discussion Rel-18 NR\_NTN\_enh-Core

*Proposal 1 Based on LS response, keep the reference point of ssb-TimeOffset at ULSRP and clarify the field description of ssb-TimeOffset that the source satellite and target satellite may have its own different ULSRP as below:*

*Indicates the time offset between the SSB from source and target satellite at the uplink time synchronization reference point between a SSB burst of the target cell at its uplink time synchronization reference point and the SSB burst of the source cell at its uplink time synchronization reference point. It is given in number of subframes.*

1. **Continue in offline 301 to discuss a clarification for ssb-TimeOffset based on the text proposal in p1**

There was a question whether the SSB time offset can have negative value. However, as per current signaling, the value of SSB time offset is always positive.

SatSwitchWithReSync-r18 ::= SEQUENCE {

ntn-Config-r18 NTN-Config-r17,

t-ServiceStart-r18 INTEGER (0..549755813887) OPTIONAL, -- Need R

ssb-TimeOffset-r18 INTEGER (0..159) OPTIONAL -- Need R

}

In this case, we need to clarify whether the positive offset is applied with respect to source ULSRP or target ULSRP. We have options:

#1: Target SSB at ULSRP = Source SSB at ULSRP + ssb-TimeOffset

#2: Source SSB at ULSRP = Target SSB at ULSRP + ssb-TimeOffset

It was also discussed whether it is beneficial to have option of signaling negative value of ssb-TimeOffset.

Q1: Do you think negative value of SSB time offset is needed?

|  |  |  |
| --- | --- | --- |
| Company name | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

Q2: If we stick to current positive value of the ssb-TimeOffset, what is current understanding?

Option#1: Target SSB at ULSRP = Source SSB at ULSRP + ssb-TimeOffset

Option#2: Source SSB at ULSRP = Target SSB at ULSRP + ssb-TimeOffset

|  |  |  |
| --- | --- | --- |
| Company name | Option 1 or Option 2 | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

Q2: Based on above, how should we clarify the field description of *ssb-TimeOffset*?

Option#1: *Indicates the time offset between a SSB of the target cell at its uplink time synchronization reference point and the SSB burst of the source cell at its uplink time synchronization reference point. It is given in number of subframes.*

Option#2: *Indicates the time offset between a SSB of the source cell at its uplink time synchronization reference point and the SSB burst of the target cell at its uplink time synchronization reference point. It is given in number of subframes.*

Option#3: *Indicates the time offset of the SSB of the target cell at its uplink time synchronization reference point from the SSB burst of the source cell at its uplink time synchronization reference point. It is given in number of subframes.*

Option#4: others

|  |  |  |
| --- | --- | --- |
| Company name | Option 1 or Option 2 | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

Following was also discussed.

*Proposal 2 Confirm that there is no impact to running timers (e.g., HARQ RTT timer) due to cell timing change after soft satellite switch with resync. Consider updating NOTE 1 in section 3.1 by adding another example as “due to soft satellite switch with resynchronization” in addition to “due to BWP switching”.*

- Ericsson and Apple confirm the understanding but think we don’t need any further clarification

**Continue the discussion in offline 301**

Q2: Do you agree to confirm the following?

* *Confirm that there is no impact to running timers (e.g., HARQ RTT timer) due to cell timing change after soft satellite switch with resync. No further clarification is needed.*

|  |  |  |
| --- | --- | --- |
| Company name | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |

Following conclusion is made.

1. To be updated

# Conclusion

Following proposals are made.

Proposal 1 To be updated