**3GPP TSG-RAN WG2 Meeting #127 *R2-2407618***

**Maastricht, Netherlands, August 19th – 23rd, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **36.306** | **CR** | **draftCR** | **rev** | **-** | **Current version:** | **18.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of LTE TN to NR NTN Mobility UE Capability |
|  |  |
| ***Source to WG:*** | vivo |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | LTE\_TN\_NR\_NTN\_mob-Core |  | ***Date:*** | 2024-08-23 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Introduction of UE capability for inter-RAT cell measurement on NR NTN cell |
|  |  |
| ***Summary of change:*** | A new optional UE capability without siganlling is introduced to allow inter-RAT measurement for cell reselection from LTE TN cell to NR NTN cell. |
|  |  |
| ***Consequences if not approved:*** | Inter-RAT cell reselection from LTE TN to NR NTN is not supported. |
|  |  |
| ***Clauses affected:*** | 3.3, 6.8.x (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.331 CR |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

START OF CHANGE

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

1xRTT CDMA2000 1x Radio Transmission Technology

ACK Acknowledgement

ACDC Application specific Congestion control for Data Communication

ANDSF Access Network Discovery and Selection Function

ANR Automatic Neighbour Relation

BCCH Broadcast Control Channel

CAS Cell Acquisition Subframes

CFI Control Format Indicator

CG Cell Group

CRS Cell-specific Reference Signal

CSG Closed Subscriber Group

CSI Channel State Information

DC Dual Connectivity

DCI Downlink Control Information

DL-SCH Downlink Shared Channel

EHC Ethernet Header Compression

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRAN Evolved Universal Terrestrial Radio Access Network

FDD Frequency Division Duplex

GERAN GSM/EDGE Radio Access Network

HARQ Hybrid Automatic Repeat Request

HRPD High Rate Packet Data

HSDN High Speed Dedicated Network

IRC Interference Rejection Combining

MAC Medium Access Control

MMSE Minimum Mean Squared Error

MO-EDT Mobile Originated Early Data Transmission

MRO Mobility Robustness Optimisation

MT-EDT Mobile Terminated Early Data Transmission

MTSI Multimedia Telephony Service for IMS

MUST MultiUser Superposition Transmission

NAICS Network Assisted Interference Cancellation/Suppression

NB-IoT Narrow Band Internet of Things

NTN Non-Terrestrial Network

OS OFDM Symbol

PCell Primary Cell

PDCCH Physical Downlink Control Channel

PDCP Packet Data Convergence Protocol

PDSCH Physical Downlink Shared Channel

PHR Power Headroom Reporting

ProSe Proximity-based Services

PUCCH Physical Uplink Control Channel

PUR Preconfigured Uplink Resource

PUSCH Physical Uplink Shared Channel

QoE Quality of Experience

RACH Random Access CHannel

RAI Release Assistance Indication

RAT Radio Access Technology

RLC Radio Link Control

RLF Radio Link Failure

ROHC RObust Header Compression

RRC Radio Resource Control

SC-PTM Single Cell Point to Multipoint

SCC Secondary Component Carrier

SCell Secondary Cell

SI System Information

SL Sidelink

SL-DCH Sidelink Discovery CHannel

SL-SCH Sidelink Shared CHannel

SON Self Organizing Networks

SPT Short Processing Time

SR Scheduling Request

SSAC Service Specific Access Control

SSTD SFN and Subframe Timing Difference

STTI Short TTI

TDD Time Division Duplex

TTI Transmission Time Interval

UCI Uplink Control Information

UDC Uplink Data Compression

UE User Equipment

UL-SCH Uplink Shared Channel

UMTS Universal Mobile Telecommunications System

UTRA UMTS Terrestrial Radio Access

V2X Vehicle-to-Everything

WLAN Wireless Local Area Network

NEXT CHANGE

## 6.8 Other features

### 6.8.1 System Information Block Type 16

It is optional for UE, including UEs of any *ue- Category-NB*, to support the reception of *SystemInformationBlockType16* as specified in TS 36.331 [5].

### 6.8.2 QCI1 indication in Radio Link Failure Report

It is optional for the UE to include *drb-EstablishedWithQCI-1* in *RLF-Report* as specified in TS 36.331 [5].

### 6.8.3 Enhanced random access power control

It is optional for UE to support enhanced random access power control for FDD as specified in TS 36.321 [4] and TS 36.213 [22], clauses 16.2.1.1.1 and 16.3.1. This feature is only applicable if the UE supports any *ue-Category-NB*.

### 6.8.4 MO-EDT for Control Plane CIoT EPS Optimization

It is optional for UE to support MO-EDT for Control Plane CIoT EPS optimizations as specified in TS 24.301 [28]. This feature is only applicable if the UE supports *ce-ModeA-r13*, or for FDD if the UE supports any *ue-Category-NB*.

### 6.8.5 Void

### 6.8.6 Enhanced PHR

It is optional for UE to support enhanced PHR in MSG3 for FDD, as defined in TS 36.321 [4]. This feature is only applicable if the UE supports any *ue-Category-NB*.

### 6.8.7 void

### 6.8.8 Resynchronization Signals

It is optional for UE to support resynchronization signals, as defined in TS 36.211 [17]. This feature is only applicable if the UE supports *ce-ModeA-r13*.

### 6.8.9 Measurement gaps for higher UE velocity

It is optional for UE to support measurement gaps for higher UE velocity, as defined in TS 36.331 [5] and TS 36.133[16]. This feature is only applicable if the UE supports *ce-ModeA-r13*.

### 6.8.10 MT-EDT for Control Plane CIoT EPS Optimisation

It is optional for UE to support MT-EDT for Control Plane CIoT EPS Optimisation, as defined in TS 24.301 [28]. If the UE supports 'MT-EDT for Control Plane CIoT EPS Optimisation' it shall support 'MO-EDT for Control Plane CIoT EPS Optimisation' as described in clause 6.8.4. This feature is only applicable if the UE supports *ce-ModeA-r13,* or for FDD if the UE supports any *ue-Category-NB*.

### 6.8.11 MT-EDT for User Plane CIoT EPS Optimisation

It is optional for UE to support MT-EDT for User Plane CIoT EPS Optimisation, as defined in TS 24.301 [28]. If the UE supports 'MT-EDT for User Plane CIoT EPS Optimisation' it shall support *earlyData-UP-r15* as described in clause 4.3.8.7. This feature is only applicable if the UE supports *ce-ModeA-r13,* or for FDD if the UE supports any *ue-Category-NB*.

### 6.8.12 Void

### 6.8.13 Reduced MIB/SIB1-BR acquisition time

It is optional for UE to support reduced MIB/SIB1-BR acquisition time requirements as specified in TS 36.133 [16]. This feature is only applicable if the UE supports *ce-ModeB-r13.*

### 6.8.14 High speed dedicated network features

It is optional for UE to support HSDN cell reselection handling in RRC\_IDLE and RRC\_INACTIVE (if the UE supports *eutra-5GC-r15*) as specified in TS 36.304 [14] and TS 36.331 [5].

### 6.8.15 Carrier specific NRSRP thresholds for NPRACH resource selection

It is optional for UE to support carrier specific NRSRP thresholds for NPRACH resource selection as specified in TS 36.321 [4]. This feature is only applicable if the UE supports any *ue-Category-NB* and *multiCarrier-NPRACH-r14* or *multiCarrierPagingTDD-r15*.

### 6.8.16 Protection against improper reselection to GERAN/UTRAN

It is optional for UE to support protection against improper reselection to GERAN/UTRAN as specified in TS 36.304 [14].

### 6.8.17 Inter-RAT cell reselection of an NR mobile IAB cell

It is optional for UE to support inter-RAT cell reselection priority handling of an NR mobile IAB cell in RRC\_IDLE and RRC\_INACTIVE (if the UE supports *eutra-5GC-r15*) as specified in TS 36.304 [14] and TS 36.331 [5].

### 6.8.x Inter-RAT measurement on an NR NTN cell

It is optional for UE in RRC\_IDLE, or in RRC\_INACTIVE (if the UE supports *eutra-5GC-r15*) to support inter-RAT measurement for cell reselection from E-TURA terrestrial network cell to NR NTN cell as specified in TS 36.304 [14] and TS 36.331 [5].

END OF CHANGE