**3GPP TSG-RAN WG3 #125R3-244682**

**Maastricht, NL,** **19th – 23th Aug 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.423** | **CR** | **1325** | **rev** | **1** | **Current version:** | **15.19.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on asymmetric UL and DL for TDD Carrier |
|  |  |
| ***Source to WG:*** | China Telecom,ZTE, CATT,China Unicom, Ericsson, Nokia, Nokia Shanghai Bell, Huawei |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_newRAT\_Core |  | ***Date:*** | 2024-08-21 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Per TS38.104, TDD Band can be configured with asymmetric UL and DL,i.e, n50 for TDD (see Table 5.3.6-2 in TS38.101-1). However, the existing *Served Cell Information* *NR* IE the UL and DL bandwidth for TDD can only be set to symmetric. Therefore, it is needed to introduce a new UL and DL Transmission Bandwidth for asymmetric TDD Band. |
|  |  |
| ***Summary of change:*** | * To introduce a new UL and DL Transmission Bandwidth for asymmetric TDD Band in existing *Served Cell Information NR* IE.
* To add semantics description for the exisiting TDD Transmission Bandwidth IE

Impact Analysis:Impact assessment towards the previous version of the specification (same release):This CR has an isolated impact towards the previous version of the specification (same release). This CR only has an impact on the Served Cell Information by introducing the asymmetric TDD transmission bandwidth. |
|  |  |
| ***Consequences if not approved:*** | Asymmetric bandwidth configuration for TDD cell can not be exchanged between two nodes |
|  |  |
| ***Clauses affected:*** | 9.2.2.11,9.3.5,9.3.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.473 CR 1449  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev 1: Correct the IE tabular format issue, current version and add more co-source companies |

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

#### 9.2.2.11 Served Cell Information NR

This IE contains cell configuration information of an NR cell that a neighbouring NG-RAN node may need for the Xn AP interface.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| NR-PCI | M |  | INTEGER (0..1007, …) | NR Physical Cell ID | – |  |
| NR CGI | M |  | 9.2.2.7 |  | – |  |
| TAC | M |  | 9.2.2.5 | Tracking Area Code | – |  |
| RANAC | O |  | RAN Area Code9.2.2.6 |  | – |  |
| **Broadcast PLMNs** |  | *1..<maxnoofBPLMNs>* |  | Broadcast PLMNs in SIB1 associated to the NR Cell Identity in the *NR CGI* IE. | – |  |
| >PLMN Identity | M |  | 9.2.2.4 |  | – |  |
| CHOICE *NR-Mode-Info* | M |  |  |  | – |  |
| >*FDD* |  |  |  |  |  |  |
| >>**FDD Info** |  | *1* |  |  | – |  |
| >>>UL NR Frequency Info | M |  | NR Frequency Info9.2.2.19 |  | – |  |
| >>>DL NR Frequency Info | M |  | NR Frequency Info9.2.2.19 |  | – |  |
| >>>UL Transmission Bandwidth | M |  | NR Transmission Bandwidth9.2.2.20 |  | – |  |
| >>>DL Transmission Bandwidth | M |  | NR Transmission Bandwidth9.2.2.20 |  | – |  |
| >*TDD* |  |  |  |  |  |  |
| >>**TDD Info** |  | *1* |  |  | – |  |
| >>>Frequency Info | M |  | NR Frequency Info9.2.2.19 |  | – |  |
| >>>Transmission Bandwidth | M |  | NR Transmission Bandwidth9.2.2.20 | This IE is ignored if the *Transmission Bandwidth asymmetric* IE is present. | – |  |
| **>>>Transmission Bandwidth asymmetric** |  | *0..1* |  | Indicates the asymmetric UL and DL transmission bandwidth. | YES | ignore |
| >>>>UL Transmission Bandwidth | M |  | Transmission Bandwidth9.2.2.20 |  | – |  |
| >>>>DL Transmission Bandwidth | M |  | Transmission Bandwidth9.2.2.20 |  | – |  |
| Measurement Timing Configuration | M |  | OCTET STRING | Contains the *MeasurementTimingConfiguration* inter-node message for the served cell, as defined in TS 38.331 [10]. | – |  |
| Connectivity Support | M |  | 9.2.2.28 |  | – |  |
| **Broadcast PLMN Identity Info List NR** |  | *0..<maxnoofBPLMNs>* |  | This IE corresponds to the *PLMN-IdentityInfoList* IE in *SIB1* as specified in TS 38.331 [8]. All PLMN Identities and associated information contained in the *PLMN-IdentityInfoList* IE are included and provided in the same order as broadcast in SIB1. | YES | ignore |
| **>Broadcast PLMNs** |  | *1..<maxnoofBPLMNs>* |  | Broadcast PLMNs in SIB1 associated to the *NR Cell Identity* IE | – |  |
| >>PLMN Identity | M |  | 9.2.2.4 |  | – |  |
| >TAC | M |  | 9.2.2.5 |  | – |  |
| >NR Cell Identity | M |  | BIT STRING (SIZE(36)) |  | – |  |
| >RANAC | O |  | RAN Area Code9.2.2.6 |  | – |  |
| >Configured TAC Indication | O |  | 9.2.2.39a | NOTE: This IE is associated with the TAC in the *Broadcast PLMN Identity Info List NR* IE | YES | ignore |
| Configured TAC Indication | O |  | 9.2.2.39a | NOTE: This IE is associated with the TAC on top-level of the *Served Cell Information NR* IE | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBPLMNs | Maximum no. of broadcast PLMNs by a cell. Value is 12. |
|  |  |

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

### 9.3.5 Information Element definitions

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

 id-Secondary-MN-Xn-U-TNLInfoatM,

 id-ULForwardingProposal,

 id-DRB-IDs-takenintouse,

 id-SplitSessionIndicator,

 id-secondary-SN-UL-PDCP-UP-TNLInfo,

 id-pdcpDuplicationConfiguration,

 id-duplicationActivation,

 id-AdditionLocationInformation,

 id-SecurityIndication,

 id-QosFlowMappingIndication,

 id-NRTransmissonBandwidth-asymmetric,

 maxEARFCN,

 maxnoofAllowedAreas,

 maxnoofAMFRegions,

 maxnoofAoIs,

 maxnoofBPLMNs,

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

-- N

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

 nrFrequencyInfo NRFrequencyInfo,

 nrTransmissonBandwidth NRTransmissionBandwidth,

 iE-Extension ProtocolExtensionContainer { {NRModeInfoTDD-ExtIEs} } OPTIONAL,

 ...

}

NRModeInfoTDD-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

 {ID id-IntendedTDD-DL-ULConfiguration-NR CRITICALITY ignore EXTENSION IntendedTDD-DL-ULConfiguration-NR PRESENCE optional }|

 {ID id-TDDULDLConfigurationCommonNR CRITICALITY ignore EXTENSION TDDULDLConfigurationCommonNR PRESENCE optional }|

 { ID id-CarrierList CRITICALITY ignore EXTENSION NRCarrierList PRESENCE optional }|

 {ID id-tdd-GNB-DU-Cell-Resource-Configuration CRITICALITY ignore EXTENSION GNB-DU-Cell-Resource-Configuration PRESENCE optional }|

 { ID id-NRTransmissonBandwidth-asymmetric CRITICALITY ignore EXTENSION NRTransmissonBandwidth-asymmetric PRESENCE optional },

 ...

}

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

NRTransmissionBandwidth-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

 ...

}

NRTransmissonBandwidth-asymmetric ::= SEQUENCE {

 uL-NRTransmissonBandwidth NRTransmissionBandwidth,

 dL-NRTransmissonBandwidth NRTransmissionBandwidth,

 iE-Extensions ProtocolExtensionContainer { { NRTransmissonBandwidth-asymmetric-ExtIEs} } OPTIONAL,

 ...

}

NRTransmissonBandwidth-asymmetric-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

 ...

}

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

### 9.3.7 Constant definitions

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////

id-TAINSAGSupportList ProtocolIE-ID ::= 364

id-SCGreconfigNotification ProtocolIE-ID ::= 365

id-earlyMeasurement ProtocolIE-ID ::= 366

id-BeamMeasurementsReportConfiguration ProtocolIE-ID ::= 367

id-CoverageModificationCause ProtocolIE-ID ::= 368

id-AdditionalListofPDUSessionResourceChangeConfirmInfo-SNterminated ProtocolIE-ID ::= 369

id-UERLFReportContainerLTEExtension ProtocolIE-ID ::= 370

id-ExcessPacketDelayThresholdConfiguration ProtocolIE-ID ::= 371

id-HashedUEIdentityIndexValue ProtocolIE-ID ::= 372

id-QosFlowMappingIndication ProtocolIE-ID ::= 373

id-Full-and-Short-I-RNTI-Profile-List ProtocolIE-ID ::= 374

id-MBS-DataForwarding-Indicator ProtocolIE-ID ::= 375

id-IABAuthorizationStatus ProtocolIE-ID ::= 376

id-NRTransmissonBandwidth-asymmetric ProtocolIE-ID ::= xxx

//////////////////////////////////////////////////////////////irrelevant operations skipped/////////////////////////////////////////////////////////////////////