**3GPP TSG- Meeting #111**

**Fukuoka, Japan, 20th May – 24th May 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **2216** | **rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR Bug Fixes 38101-1-i50\_s0505A03-0505A03 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Apple | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_3BDL\_xBUL-Core, NR\_CADC\_R18\_yBDL\_xBUL-Core | | | | |  | ***Date:*** | | | 2024-05-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Band combinations bug fixing | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Correcting three notation bugs and adding four missing fallbacks including their ΔTIB,c.and ΔRIB,c values and MSD for one missing 3CA combination. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Bugs are still in the band combinations tables and combinations cannot be supported as they are not correctly specified | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.2, 5.5A.3.3, 6.2A.4.2.4, 6.2A.4.2.5, 7.3A.3.2.3, 7.3A.3.2.4, 7.3A.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

#### 5.5A.3.2 Configurations for inter-band CA (three bands)

Table 5.5A.3.2-1: Void

##### Table 5.5A.3.2-1a

Table 5.5A.3.2-1a: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n1A-n3A-n5A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n3A-n5A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3(2A)-n7A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3A-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3B-n7A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3B-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3(2A)-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3B-n7B | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n8A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n18A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n3A-n18A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n18 | 5, 10, 15 |  |
| CA\_n1A-n3A-n20A | CA\_n1A-n3A CA\_n1A-n20A CA\_n3A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n26A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n26(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n26A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n1A-n3B-n26(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n3A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 201, 301 |  |
| CA\_n1A-n3B-n28A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3B-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3A-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3B-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3(2A)-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3(2A)-n38A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n40A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n3A-n40A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n41A | n417  CA\_n1A-n3A  CA\_n1A-n41A7  CA\_n3A-n41A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n67A | CA\_n1A-n3A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n75A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77A | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n77(2A) | n777,9  CA\_n1A-n3A  CA\_n1A-n77A7  CA\_n3A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n77(3A) | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n1A-n3A-n78A | CA\_n1A-n3A  CA\_n1A-n78A7  CA\_n3A-n78A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n78C | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n3B-n78A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n78(2A) | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n79A | CA\_n1A-n3A  CA\_n1A-n79A  CA\_n3A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3B-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3B-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3B-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3B-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3(2A)-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3(2A)-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3(2A)-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3(2A)-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3A-n105A | CA\_n1A-n3A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n5A-n7A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n5A-n7B | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n5A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n5A-n28A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n40A | CA\_n1A-n5A  CA\_n1A-n40A  CA\_n5A-n40A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n78A | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
|  |  | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n78C | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n5A-n79A | CA\_n1A-n5A  CA\_n1A-n79A  CA\_n5A-n79A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n8A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n26A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n26(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n7B-n26A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n7B-n26(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n7A-n26A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n7A-n28A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7B-n28A | CA\_n1A-n28A  CA\_n1A-n7A  CA\_n7A-n28A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n38A10 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n7A-n38A10 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n7A-n40A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n7A-n67A | CA\_n1A-n7A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n75A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901,100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 901, 100 |  |
|  | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7B-n78A | CA\_n1A-n78A  CA\_n1A-n7A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n1A-n7B-n78(2A) | CA\_n1A-n78A  CA\_n1A-n7A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7A-n78C | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n7A-n105A | CA\_n1A-n7A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n7A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n8A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 10, 15, 20 |  |
| CA\_n1A-n8A-n40A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n8A-n78A | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | - | n1 | 5, 10, 15, 20 | 1 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n8A-n78C | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | See n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n1A-n8A-n78(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
| CA\_n1A-n8A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n18A-n28A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n18A-n41A | CA\_n1A-n18A  CA\_n1A-n41A  CA\_n18A-n41A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77A | n777  CA\_n1A-n18A  CA\_n1A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77(2A) | CA\_n1A-n18A  CA\_n1A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n20A-n67A | CA\_n1A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n20A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26A-n78A | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26(2A)-n78A | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n26A-n78(2A) | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n26(2A)-n78(2A) | CA\_n1A-n26A  CA\_n1A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n28A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n28A-n40A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n40B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
| CA\_n1A-n28A-n41A | n417  CA\_n1A-n28A  CA\_n1A-n41A7  CA\_n28A-n41A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n28A-n46A | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
| CA\_n1A-n28A-n46C | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46C\_BCS0 |  |
| CA\_n1A-n28A-n46D | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46D\_BCS0 |  |
| CA\_n1A-n28A-n46(2A) | CA\_n1A-n28A  CA\_n1A-n46A  CA\_n28A-n46A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
| CA\_n1A-n28A-n75A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n28A-n77A | n777,9  CA\_n1A-n28A  CA\_n1A-n77A7  CA\_n28A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n77(2A) | n777,9  CA\_n1A-n28A  CA\_n1A-n77A7  CA\_n28A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n28A-n77(3A) | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n1A-n28A-n78A | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n28A-n78C | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n1A-n28A-n79A | CA\_n1A-n28A  CA\_n1A-n79A  CA\_n28A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n28A-n102A | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n28A-n102B | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n1A-n102B  CA\_n28A-n102A  CA\_n28A-n102B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n28A-n102C | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n1A-n102C  CA\_n28A-n102A  CA\_n28A-n102C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n28A-n102D | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n28A-n102E | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n28A-n102(2A) | CA\_n1A-n28A  CA\_n1A-n102A  CA\_n28A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n77A | CA\_n1A-n40A  CA\_n1A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n77(2A) | CA\_n1A-n40A  CA\_n1A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n40A-n78A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n40B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n40A-n105A | CA\_n1A-n40A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n41A-n77A | n417  n777,9  CA\_n1A-n41A7  CA\_n1A-n77A7  CA\_n41A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n41A-n77(2A) | n417  n777,9  CA\_n1A-n41A7  CA\_n1A-n77A7  CA\_n41A-n77A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n41A-n77(3A) | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n1A-n41A-n79A | CA\_n1A-n41A  CA\_n1A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n46A-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 10, 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46C-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46D-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46(2A)-n78A | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n46A-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | 10, 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46C-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46D-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n46(2A)-n78(2A) | CA\_n1A-n46A  CA\_n1A-n78A  CA\_n46A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n67A-n78A | CA\_n1A-n78A | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n67A-n78(2A) | CA\_n1A-n78A CA\_n78(2A) | n1 | 5, 10, 15, 20, 30, 40, 45, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n75A-n78A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n77A-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n77(2A)-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n77(3A)-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78A-n79A5 | CA\_n1A-n78A  CA\_n1A-n79A  CA\_n78A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n78(2A)-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78A-n102A | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n78A-n102B | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102B  CA\_n78A-n102A  CA\_n78A-n102B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n78A-n102C | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102C  CA\_n78A-n102A  CA\_n78A-n102C | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n78A-n102D | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n78A-n102E | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n78A-n102(2A) | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n78(2A)-n102A | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n1A-n78(2A)-n102B | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102B  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n1A-n78(2A)-n102C | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n1A-n102C  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n1A-n78(2A)-n102D | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n1A-n78(2A)-n102E | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n1A-n78(2A)-n102(2A) | CA\_n1A-n78A  CA\_n1A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n1A-n78A-n105A | CA\_n1A-n78A  CA\_n1A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n2A-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n41A | CA\_n2A-n5A  CA\_n2A-n41A  CA\_n5A-n41A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
| CA\_n2A-n5A-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A  CA\_n48B | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n2A-n5A-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
| CA\_n2A-n5A-n48(A-B) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
| CA\_n2(2A)-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n5A-n66(3A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n5A-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n77C | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n5A-n77(2A) | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n5A-n77A | n777,9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n77(2A) | n777  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n7A-n12A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n12 | 5, 10, 15 |  |
| CA\_n2A-n7A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2A-n7A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n7A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n12A-n41A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n2A-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66(3A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n12A-n71A | CA\_n2A-n12A  CA\_n2A-n71A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n12A-n77A | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n77A | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n77(2A) | n777,9  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n77(2A) | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(3A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n14A-n77A | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n77(2A) | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n14A-n77A | n777,9  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n14A-n77(2A) | n777  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A | CA\_n2A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n29A-n30A | CA\_n2A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n29A-n66A | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n66A | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n66(2A) | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n66(2A) | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n77A | n777,9  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n77A | n777,9  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n77(2A) | 777,9  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n77(2A) | n777  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n30A-n66(3A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n30A-n77A | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n77(2A) | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n30A-n77A | n777,9  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n30A-n77(2A) | n777  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n41A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2A-n41A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n48A-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48(A-B)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48B-n66A | CA\_n48B  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48(2A)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48A-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48(2A)-n77C | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48B-n77C | n777,9  CA\_n48B  CA\_n2A-n48A  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48B-n77A | n777,9  CA\_n48B  CA\_n2A-n48A  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48(2A)-n77A | n777,9  CA\_n2A-n48A  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n66A-n77A | n777, 9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n66A-n77A | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66(2A)-n77A | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n77C | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n66A-n77(2A) | n777,9  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n66(2A)-n77A | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n66(2A)-n77(2A) | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n66A-n77(2A) | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66(2A)-n77(2A) | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66(3A)-n77A | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66(3A)-n77(2A) | n777  CA\_n2A-n66A  CA\_n2A-n77A7  CA\_n66A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n2A-n71A-n77A | CA\_n2A-n71A  CA\_n2A-n77A  CA\_n71A-n77A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n71A-n77(2A) | CA\_n2A-n71A  CA\_n2A-n77A  CA\_n71A-n77A | n2 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n71A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n71A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n7A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n3A-n5A-n7B | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n3A-n5A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n5A-n28A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n5A-n78A | CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n79A | CA\_n3A-n5A  CA\_n3A-n79A  CA\_n5A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | See n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n8A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
| CA\_n3A-n7A-n20A | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n7A-n20A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | See n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n26A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n26(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3A-n7B-n26A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n3A-n7B-n26(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n7A-n26A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3B-n7A-n26A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7A-n26(2A) | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3B-n7B-n26A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n3B-n7B-n26(2A) | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n3A-n7A-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3A-n7B-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3B-n7A-n28A | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3B-n7B-n28A | CA\_n7B  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n38A10 | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3B-n7A-n38A10 | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3(2A)-n7A-n38A10 | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3A-n7A-n40A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n7A-n40A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n3A-n7A-n67A | CA\_n3A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n75A | - | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78C | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n7B-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n3A-n7B-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7A-n78(2A) | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n7B-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7A-n79A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n79C | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3B-n7A-n79A | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3(2A)-n7A-n79A | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n79C | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3(2A)-n7A-n79C | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3A-n7A-n105A | CA\_n3A-n7A  CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n7A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n8A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n8A-n41A | CA\_n3A-n8A  CA\_n3A-n41A  CA\_n8A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77(2A) | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n8A-n78A | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n79A | CA\_n3A-n8A  CA\_n3A-n79A  CA\_n8A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n18A-n28A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n18A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n28 | 5, 10 |
| CA\_n3A-n18A-n41A | CA\_n3A-n41A  CA\_n3A-n18A  CA\_n18A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |
| CA\_n3A-n18A-n77A | n777  CA\_n3A-n18A  CA\_n3A-n77A7  CA\_n18A-n77A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |
| CA\_n3A-n18A-n77(2A) | n777  CA\_n3A-n18A  CA\_n3A-n77A7  CA\_n18A-n77A7 | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n20A-n67A | CA\_n3A-n20A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n28A | CA\_n3A-n20A  CA\_n3A-n28A  CA\_n20A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n20A-n78A | CA\_n3A-n20A CA\_n3A-n78A CA\_n20A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n78(2A) | CA\_n3A-n20A CA\_n3A-n78A CA\_n20A-n78A  CA\_n78(2A) | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n3A-n26A-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n26A-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n28A-n38A | - | n3 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n38 | 5, 10, 15, 20, 30, 40 |  |
| CA\_n3A-n28A-n40A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n28A-n40A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n40 | 20, 40 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A | n417,9  CA\_n3A-n28A  CA\_n3A-n41A7  CA\_n28A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n41B | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n3A-n28A-n77A | n777,9  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35,40 | 2 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n77(2A) | n777,9  CA\_n3A-n28A  CA\_n3A-n77A7  CA\_n28A-n77A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  | CA\_n77(2A)7 | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n28A-n77(3A) | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n3A-n28A-n78A | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n78C | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n3A-n28A-n78(2A) | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n78(2A)  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n28A-n78A | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n28A-n78(2A) | CA\_n78(2A)  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n28A-n79A | n797,9  CA\_n3A-n28A  CA\_n3A-n79A7  CA\_n28A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n38A-n40A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n38A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n78A | CA\_n3A-n40A  CA\_n3A-n78A  CA\_n40A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n105A | CA\_n3A-n40A  CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n77A-n79A4 | n777,9  n797,9  CA\_n3A-n77A7  CA\_n3A-n79A7  CA\_n77A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n77(2A)-n79A4 | n777,9  n797,9  CA\_n3A-n77A7  CA\_n3A-n79A7  CA\_n77A-n79A7 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n77(3A)-n79A4 | CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n40A-n41A | CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n40A-n41C | CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n3A-n40A-n77A | CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n40A-n77(2A) | CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 30, 35, 40, 45, 50 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n41A-n77A | n417  n777  CA\_n3A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A7 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41B-n77A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41A-n77(2A) | n417  n777  CA\_n3A-n41A7 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n41A-n77(3A) | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n3A-n41A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  | CA\_n3A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n78A | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n41A-n78(2A) | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n78A | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n41A-n79A | CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 2 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n41A-n79C | CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n3A-n41C-n79A | CA\_n41C  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n41C-n79C | CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n3 | See n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n3A-n67A-n78A | CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n67A-n78(2A) | CA\_n78(2A)  CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n75A-n78A | - | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n78A-n79A | n787,9 | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n78A-n79C | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3B-n78A-n79A | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3B-n78A-n79C | - | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3(2A)-n78A-n79A | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3(2A)-n78A-n79C | - | n3 | CA\_n3(2A)\_BCS1 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n3A-n78A-n105A | CA\_n3A-n78A  CA\_n3A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n7A-n25A | CA\_n5A-n7A  CA\_n5A-n25A  CA\_n7A-n25A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n5A-n7A-n25(2A) | CA\_n5A-n7A  CA\_n5A-n25A  CA\_n7A-n25A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n25 | CA\_n25(2A) |  |
| CA\_n5A-n7A-n28A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n5A-n7A-n66A | CA\_n5A-n7A  CA\_n5A-n66A  CA\_n7A-n66A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n5A-n7A-n77A | n777,9  CA\_n5A-n7A  CA\_n5A-n77A7  CA\_n7A-n77A7 | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n7A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n5A-n7A  CA\_n5A-n77A7  CA\_n7A-n77A7 | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n5A-n7A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n5A-n7A  CA\_n5A-n77A7  CA\_n7A-n77A7 | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n5A-n7A-n78A | CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n7B-n78A | CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n12A-n77A | n777  CA\_n5A-n12A  CA\_n5A-n77A7  CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n12A-n77(2A) | n777  CA\_n5A-n12A CA\_n5A-n77A7 CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n14A-n77A | n777  CA\_n5A-n14A  CA\_n5A-n77A7  CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n14A-n77(2A) | n777  CA\_n5A-n14A CA\_n5A-n77A7 CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n29A | CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n29 | 5, 10 |  |
| CA\_n5A-n25A-n41A | CA\_n5A-n25A  CA\_n5A-n41A  CA\_n25A-n41A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
| CA\_n5A-n25(2A)-n41A | CA\_n5A-n25A  CA\_n5A-n41A  CA\_n25A-n41A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n25 | CA\_n25(2A) |  |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
| CA\_n5A-n25A-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25(2A)-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25A-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77A | n777,9  CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  | CA\_n5A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n77A7 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n77A | n777,9  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n77(2A) | n777,9  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77(3A) | n777,9  CA\_n77(2A)  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n77(2A) | n777,9  CA\_n5A-n25A  CA\_n5A-n77A7  CA\_n25A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n78A | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n78A | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n78(2A) | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n78(2A) | n787,9  CA\_n5A-n25A  CA\_n5A-n78A7  CA\_n25A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n28A-n78A | CA\_n5A-n28A  CA\_n5A-n78A  CA\_n28A-n78A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n28A-n79A | CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n5A-n28A-n105A | CA\_n5A-n28A  CA\_n5A-n105A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n5A-n29A-n66A | CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n29A-n77A | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n29A-n77(2A) | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n30A-n66A | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n5A-n30A-n66(2A) | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n5A-n30A-n66(3A) | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n5A-n30A-n77A | n777,9  CA\_n5A-n30A  CA\_n5A-n77A7  CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n30A-n77(2A) | n777,9  CA\_n5A-n30A CA\_n5A-n77A7 CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n40A-n78A | CA\_n5A-n40A  CA\_n5A-n78A  CA\_n40A-n78A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n40 | 58, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
| CA\_n5A-n41A-n66A | CA\_n5A-n41A CA\_n5A-n66A CA\_n41A-n66A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n5A-n41A-n77A | CA\_n5A-n41A  CA\_n5A-n77A  CA\_n41A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n41A-n77(2A) | CA\_n5A-n41A  CA\_n5A-n77A  CA\_n41A-n77A | n5 | 5, 10, 15, 20, 25 | 0 |
|  |  | n41 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n77 | CA\_n77(2A) |  |
| CA\_n5A-n48A-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48(A-B)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48B-n66A | CA\_n48B  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48(2A)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48A-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48A-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n48B-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48B-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C BCS1 |  |
| CA\_n5A-n48(2A)-n77A | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48(2A)-n77C | n777,9  CA\_n5A-n48A  CA\_n5A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n66A-n77A | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n77A | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n77(2A) | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66(3A)-n77A | n777,9  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(3A)-n77(2A) | n777  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66A-n77C | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7  CA\_n77C | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n66A-n77(2A) | n777,9  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7  CA\_n77(2A)7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n5A-n66A-n77(3A) | CA\_n77(2A)  CA\_n5A-n66A  CA\_n5A-n77A7  CA\_n66A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n5A-n66A-n78A | CA\_n5A-n66A  CA\_n5A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n78A | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66A-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n66(2A)-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n78A-n79A | CA\_n5A-n78A  CA\_n5A-n79A  CA\_n78A-n79A | n5 | See n5 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n8A-n28A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n7A-n8A-n40A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n7A-n8A-n78A | CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n12A-n25A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n12A-n66A | - | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 35, 40, 45 |  |
| CA\_n7A-n12A-n71A | CA\_n7A-n12A  CA\_n7A-n71A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n7A-n12A-n77A | - | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n20A-n67A | CA\_n7A-n20A | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | See n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n78A | CA\_n7A-n20A CA\_n7A-n78A CA\_n20A-n78A | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n20A-n78(2A) | CA\_n7A-n20A CA\_n7A-n78A CA\_n20A-n78A  CA\_n78(2A) | n7 | See n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n7A-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n71A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n7A-n25A-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n77(2A) | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25(2A)-n77A | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n77(2A) | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n77(2A) | n777,9  CA\_n7A-n25A  CA\_n7A-n77A7  CA\_n25A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n78A | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25A-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25(2A)-n78A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25(2A)-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25A-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n25(2A)-n78(2A) | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7(2A)-n25(2A)-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n26A-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n26A-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n26(2A)-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n26(2A)-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7B-n26A-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7B-n26A-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n7B  CA\_n26A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7B-n26(2A)-n78A | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7B-n26(2A)-n78(2A) | CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n28A-n38A11 | - | n7 | 5, 10, 15, 20, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n38 | 5, 10, 15, 20, 30, 40 |  |
| CA\_n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n28A-n78A | CA\_n7A-n78A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n28A-n78A7 | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7A-n28A-n78C | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n7B-n28A-n78A | CA\_n7A-n78A7  CA\_n28A-n78A7 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A  CA\_n7B | n7 | CA\_n7B\_BCS0 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n38A-n78A10 | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n40A-n78A | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n40A-n105A | CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5,10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n7A-n46A-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46C-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46D-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46(2A)-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46(2A)-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46A-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46C-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n46D-n78(2A) | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n66A-n71A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n7A-n66A-n77A | n777,9  CA\_n7A-n66A  CA\_n7A-n77A7  CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n77A | n777,9  CA\_n7A-n66A  CA\_n7A-n77A7  CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n77(2A) 7  CA\_n7A-n66A  CA\_n7A-n77A7  CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n7A-n66(2A)-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66A-n77A | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n77A | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66A-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66(2A)-n77(2A) | n777,9  CA\_n7A-n66A CA\_n7A-n77A7 CA\_n66A-n77A7 | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66A-n78A | n787,9  CA\_n7A-n66A  CA\_n7A-n78A7  CA\_n66A-n78A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78(2A) | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66(2A)-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n67A-n78A | CA\_n7A-n78A | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n67A-n78(2A) | CA\_n7A-n78A CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n71A-n77A | n777,9  CA\_n7A-n71A  CA\_n7A-n77A7  CA\_n71A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n71A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n7A-n71A  CA\_n7A-n77A7  CA\_n71A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n7A-n71A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n7A-n71A  CA\_n7A-n77A7  CA\_n71A-n77A7 | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n71 | 5, 10, 15, 20, 25, 30, 35 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n7A-n75A-n78A | - | n7 | n7 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n7A-n78A-n102A | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n7A-n78A-n102B | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102B  CA\_n78A-n102A  CA\_n78A-n102B | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n7A-n78A-n102C | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102C  CA\_n78A-n102A  CA\_n78A-n102C | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n7A-n78A-n102D | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n7A-n78A-n102E | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n7A-n78A-n102(2A) | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n7A-n78(2A)-n102A | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n7A-n78(2A)-n102B | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102B  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n7A-n78(2A)-n102C | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n7A-n102C  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n7A-n78(2A)-n102D | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n7A-n78(2A)-n102E | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n7A-n78(2A)-n102(2A) | CA\_n7A-n78A  CA\_n7A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n7A-n78A-n105A | CA\_n7A-n78A  CA\_n7A-n105A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

##### Table 5.5A.3.2-1b

Table 5.5A.3.2-1b: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n8A-n20A-n28A | CA\_n8A-n20A | n8 | 5, 10, 15, 20 | 0 |
|  | CA\_n8A-n28A | n20 | 5, 10, 15, 20 |  |
|  | CA\_n20A-n28A | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n8A-n20A-n75A | - | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n75A | - | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n78A | - | n8 | 5, 10, 15, 20 | 0 |
|  | n28 | 5, 10, 15, 20 |
|  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
| CA\_n8A-n38A-n40A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n39A-n41A | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  | - | n8 | 5, 10, 15, 20 | 1 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n39A-n41C | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n8A-n39A-n79A | CA\_n8A-n39A  CA\_n8A-n79A  CA\_n39A-n79A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n40A-n41A | CA\_n8A-n40A  CA\_n8A-n41A  CA\_n40A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n40A-n41C | CA\_n41C  CA\_n8A-n40A  CA\_n8A-n41A  CA\_n40A-n41A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n8A-n40A-n78A | CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n41A-n79A | CA\_n8A-n41A  CA\_n8A-n79A  CA\_n41A-n79A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n8 | 5, 10, 15, 20 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n41C-n79A | CA\_n41C  CA\_n8A-n41A  CA\_n8A-n79A  CA\_n41A-n79A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n78A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n78(2A)-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n12A-n25A-n41A | - | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n12A-n25A-n66A | - | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n12A-n30A-n66A | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n12A-n30A-n66(2A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n12A-n30A-n66(3A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n12A-n30A-n77A | n777,9  CA\_n12A-n30A,  CA\_n12A-n77A7  CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n77(2A) | n777,9  CA\_n12A-n30A  CA\_n12A-n77A7  CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n41A-n66A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n12A-n41A-n77A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77A | n777,9  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(2A)-n77A | n777,9  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77(2A) | n777,9  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66(2A)-n77(2A) | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66(3A)-n77A | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(3A)-n77(2A) | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n71A-n77A | CA\_n12A-n77A  CA\_n71A-n77A | n12 | 5, 10, 15 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n25A-n66A | CA\_n13A-n25A  CA\_n13A-n66A  CA\_n25A-n66A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n25A-n77A | n777,9  CA\_n13A-n25A  CA\_n13A-n77A7  CA\_n25A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n25A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n13A-n25A  CA\_n13A-n77A7  CA\_n25A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n66A-n77A | n777, 9  CA\_n13A-n66A  CA\_n13A-n77A7  CA\_n66A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n66A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n13A-n66A  CA\_n13A-n77A7  CA\_n66A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66A | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n14A-n30A-n66(2A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66(3A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n14A-n30A-n77A | n777,9  CA\_n14A-n30A  CA\_n14A-n77A7  CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n77(2A) | n777,9  CA\_n14A-n30A  CA\_n14A-n77A7  CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66A-n77A | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(2A)-n77A | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66A-n77(2A) | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66(2A)-n77(2A) | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66(3A)-n77A | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(3A)-n77(2A) | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A-n41A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77A | n777  CA\_n18A-n28A  CA\_n18A-n77A7  CA\_n28A-n77A7 | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77(2A) | n777  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n41A-n77A | n417  n777  CA\_n18A-n41A7  CA\_n18A-n77A7  CA\_n41A-n77A7 | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n41A-n77(2A) | n777  CA\_n18A-n41A7  CA\_n18A-n77A7  CA\_n41A-n77A7 | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n20A-n28A-n75A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20 |  |
| CA\_n20A-n28A-n78A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n20A-n28A-n78C | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n20A-n67A-n78A | CA\_n20A-n78A | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | See n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n20A-n67A-n78(2A) | CA\_n20A-n78A  CA\_n78(2A) | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | See n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n24A-n41A-n48A | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
| CA\_n24A-n41(2A)-n48A | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
| CA\_n24A-n41A-n48(2A) | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n48(2A) | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41A-n77A | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41(2A)-n77A | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41A-n77(2A) | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n77(2A) | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48A-n77A | - | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48(2A)-n77A | - | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48A-n77(2A) | - | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48(2A)-n77(2A) | - | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n25A-n29A-n66A | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41C-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7  CA\_n25A-n41C  CA\_n41C-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(3A)-n66A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(A-C)-n66A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41A-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(3A)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41C-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7  CA\_n25A-n41C  CA\_n41C-n71A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41C-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(3A)-n71A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(A-C)-n71A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(3A)-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77(2A) | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n77(2A) | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n77(2A) | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77(2A) | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(3A)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(A-C)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n78A | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n78(2A) | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n48A-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48(2A)-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48C-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n66A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25A-n66(2A)-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66(2A)-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n78A | n787,9  CA\_n25A-n66A  CA\_n25A-n78A7  CA\_n66A-n78A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78A | n787,9  CA\_n25A-n66A CA\_n25A-n78A7 CA\_n66A-n78A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n78(2A) | n787  CA\_n78(2A)7  CA\_n25A-n66A CA\_n25A-n78A7 CA\_n66A-n78A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66A-n85A | CA\_n25A-n66A  CA\_n25A-n85A  CA\_n66A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A) BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A) BCS1 |  |
| CA\_n25A-n71B-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B-n77(2A) | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71(2A)-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71(2A)-n77(2A) | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71A-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71A-n77(2A) | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71B-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71B-n77(2A) | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71(2A)-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71(2A)-n77(2A) | n77  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71A-n78A | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n71A-n78(2A) | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n71A-n85A | CA\_n25A-n71A  CA\_n25A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n77A-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n77(2A)-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n77A-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n26A-n29A-n66A | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n29A-n66(2A) | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n26A-n29A-n66(3A) | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n26A-n29A-n70A | CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
| CA\_n26A-n48A-n66A | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n48(2A)-n66A | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n48A-n66(2A) | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n48(2A)-n66(2A) | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n48A-n70A | CA\_n26A-n48A  CA\_n26A-n70A  CA\_n48A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
| CA\_n26A-n66A-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66(2A)-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66(3A)-n70A | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66A-n71A | CA\_n26A-n66A  CA\_n66A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n66(2A)-n71A | CA\_n26A-n66A  CA\_n66A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n66(3A)-n71A | CA\_n66A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n66A-n77A | CA\_n26A-n66A  CA\_n26A-n77A  CA\_n66A-n77A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n70A-n71A | CA\_n26A-n70A  CA\_n70A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n70A-n77A | CA\_n26A-n70A  CA\_n26A-n77A  CA\_n70A-n77A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n28A-n38A-n78A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n39A-n40A | CA\_n28A-n39A  CA\_n28A-n40A  CA\_n39A-n40A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
| CA\_n28A-n39A-n41A | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n39A-n41C | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n28A-n39A-n79A | CA\_n28A-n39A  CA\_n28A-n79A  CA\_n39A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n40A-n41A | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n41C | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C\_BCS0 |  |
| CA\_n28A-n40A-n78A | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40A-n77A | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n77(2A) | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n28A-n40B-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n40A-n79A | CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41A-n77A | n417,9  n777,9  CA\_n28A-n41A7 | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41B-n77A | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41A-n77(2A) | n417,9  n777,9  CA\_n28A-n41A7 | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n28A-n41A-n77(3A) | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n28A-n41A-n78A | CA\_n28A-n41A  CA\_n41A-n78A  CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n41A-n78(2A) | CA\_n78(2A) | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n41A-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41A-n79C | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n28A-n41C-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41C-n79C | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n28A-n46A-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46C-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46D-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46(2A)-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46(2A)-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46A-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46C-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46D-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n75A-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n77A-n79A4 | n777,9  n797,9  CA\_n28A-n77A7  CA\_n28A-n79A7  CA\_n77A-n79A7 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(2A)-n79A4 | n777,9  n797,9  CA\_n28A-n77A7  CA\_n28A-n79A7  CA\_n77A-n79A7 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(3A)-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n79A | n787,9  n797,9  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n102A | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n78A-n102B | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102B  CA\_n78A-n102A  CA\_n78A-n102B | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n78A-n102C | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102C  CA\_n78A-n102A  CA\_n78A-n102C | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n78A-n102D | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n78A-n102E | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n78A-n102(2A) | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n28A-n78(2A)-n102A | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n78(2A)-n102B | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102B  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n78(2A)-n102C | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102C  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n78(2A)-n102D | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n78(2A)-n102E | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n78(2A)-n102(2A) | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n29A-n30A-n66A | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n29A-n30A-n66(2A) | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n29A-n30A-n77A | n777,9  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n30A-n77(2A) | n777,9  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66B-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66(2A)-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66(3A)-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66A-n71A | CA\_n66A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n66(2A)-n71A | CA\_n66A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n66(3A)-n71A | CA\_n66A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n66A-n77A | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77A | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66A-n77(2A) | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66(3A)-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77(2A) | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66(3A)-n77(2A) | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n70A-n71A | CA\_n70A-n71A | n29 | 5, 10 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n30A-n66A-n77A | n777,9  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(2A)-n77A | n777,9  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66A-n77(2A) | n777,9  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66(2A)-n77(2A) | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66(3A)-n77A | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(3A)-n77(2A) | n777  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n34A-n39A-n40A | CA\_n34A-n39A  CA\_n34A-n40A  CA\_n39A-n40A | n34 | 5, 10, 15 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n39A-n41A | CA\_n34A-n39A  CA\_n34A-n41A  CA\_n39A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n39A-n41C | CA\_n34A-n39A  CA\_n34A-n41A  CA\_n39A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n34A-n40A-n41A | CA\_n34A-n40A  CA\_n34A-n41A  CA\_n40A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n40A-n41C | CA\_n34A-n40A  CA\_n34A-n41A  CA\_n40A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n34A-n41A-n79A | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41A-n79C | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n34A-n41C-n79A | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41C-n79C | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n38A-n66A-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n38A-n66(2A)-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66(2A)-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n39A-n40A-n41A | CA\_n39A-n40A  CA\_n39A-n41A  CA\_n40A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n40A-n41C | CA\_n39A-n40A  CA\_n39A-n41A  CA\_n40A-n41A | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n39A-n40A-n79A | CA\_n39A-n40A  CA\_n40A-n79A  CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41A-n79C | CA\_n39A-n41A  CA\_n39A-n79A  CA\_n41A-n79A | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n39A-n41A-n79A | CA\_n39A-n41A  CA\_n39A-n79A  CA\_n41A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n40A-n41A-n79A | CA\_n40A-n41A  CA\_n40A-n79A  CA\_n41A-n79A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n41C-n79A | CA\_n41C  CA\_n41A-n79A  CA\_n40A-n41A  CA\_n40A-n79A | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n78A-n105A | CA\_n40A-n78A  CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n41A-n66A-n70A | CA\_n41A-n66A  CA\_n41A-n70A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n41A-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41A-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71A | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71B | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n66A-n71A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66(2A)-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n71B | CA\_n41A-n71A  CA\_n41A-n66A CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66(2A)-n71A | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66A-n71B | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41C-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A)-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n41C  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n71B | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n41C  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n71A | n417,9  CA\_n41C7  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n66A-n71B | CA\_n41A-n66A CA\_n41A-n71A CA\_n41C CA\_n66A-n71A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41C | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n66(2A)-n71A | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41C | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n77A7  CA\_n41A-n66A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66(2A)-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66(2A)-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A)-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n41C  CA\_n66A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n66(2A)-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n41C  CA\_n66A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66(2A)-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66(2A)-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66A-n85A | CA\_n41A-n66A  CA\_n41A-n85A  CA\_n66A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n85A | CA\_n41A-n66A  CA\_n41A-n85A  CA\_n66A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n85A | CA\_n41A-n66A CA\_n41A-n85A CA\_n66A-n85A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n85A | CA\_n41A-n66A CA\_n41A-n85A CA\_n41C CA\_n66A-n85A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n70A-n78A | CA\_n41A-n70A  CA\_n41A-n78A  CA\_n70A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71(2A)-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n71B-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n71(2A)-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n71B-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n71(2A)-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n71B-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n71(2A)-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n71B-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n71(2A)-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n78A | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n78(2A) | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n71A-n85A | CA\_n41A-n71A  CA\_n41A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n85A | CA\_n41A-n71A  CA\_n41A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71(2A)-n85A | CA\_n41A-n71A  CA\_n41A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n77A-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77(2A)-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77(3A)-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77A-n85A | CA\_n41A-n77A  CA\_n41A-n85A  CA\_n77A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n77A-n85A | CA\_n41A-n77A CA\_n41A-n85A CA\_n77A-n85A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n77(2A)-n85A | CA\_n41A-n77A CA\_n41A-n85A CA\_n77A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n77A-n85A | CA\_n41A-n77A CA\_n41A-n85A CA\_n41C CA\_n77A-n85A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |

##### Table 5.5A.3.2-1c

Table 5.5A.3.2-1c: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n46A-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48A-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48C-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 1001 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48A-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48A-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48A-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48A-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48A-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48A-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48A-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48B-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48C-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48C-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48C-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48C-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48C-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48C-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48A-n96D | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48A-n96D | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48A-n96D | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48A-n96D | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48A-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48A-n96D | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48C-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48A-n96E | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48A-n96E | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48A-n96E | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48A-n96E | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48A-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48A-n96E | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48C-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(2A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(2A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(2A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(2A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(2A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(3A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(3A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(3A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(3A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(3A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(4A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(4A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(4A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(4A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46A-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46A-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46A-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46A-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46A-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46(2A)-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46(2A)-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46(2A)-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46(2A)-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46(2A)-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46(2A)-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46C-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46C-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46C-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46C-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46C-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46C-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46D-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46D-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46D-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46D-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46D-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46D-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46A-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46A-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46A-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46A-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46A-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46A-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46(2A)-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  | CA\_n78(2A) | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46C-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46C-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46C-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46C-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46C-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46C-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46D-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46D-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46D-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46D-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46D-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46D-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n48A-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66(2A)-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48(2A)-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48B-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66(2A)-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66A-n71(2A) | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(2A)-n77A | CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66A-n77C | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7  CA\_n77C | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77C | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7  CA\_n77C | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77C | n777,9  CA\_n77C  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 3 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48A-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n70A-n71(2A) | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n70A-n77A | CA\_n48A-n70A  CA\_n70A-n77A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n70A-n77A | CA\_n48A-n70A  CA\_n70A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n71A-n77A | CA\_n48A-n71A  CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n71A-n77A | CA\_n48A-n71A  CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n78A | CA\_n66A-n78A CA\_n70A-n78A | n66 | 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71(2A) | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66B-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201,251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(2A)-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(3A)-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n77A | CA\_n66A-n77A  CA\_n70A-n77A | n66 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n70A-n77A | CA\_n66A-n77A  CA\_n70A-n77A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71(2A)-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71(2A)-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71A-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n66(2A)-n71B-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71B-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71(2A)-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71A-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  | n71 | 5, 10, 15, 20 |  |
|  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71(2A)-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n78A | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n78(2A) | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66(2A)-n71A-n78A | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n71A-n78(2A) | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66A-n71A-n85A | CA\_n66A-n71A  CA\_n66A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n77A-n85A | CA\_n66A-n77A  CA\_n66A-n85A  CA\_n77A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n77(2A)-n85A | CA\_n66A-n77A CA\_n66A-n85A CA\_n77A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n77A-n85A | CA\_n66A-n77A  CA\_n66A-n85A  CA\_n77A-n85A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n70A-n71A-n77A | CA\_n70A-n71A  CA\_n70A-n77A  CA\_n71A-n77A | n70 | 5, 10, 15, 20, 25 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |

The following notes are applied to the above tables.

NOTE 1: This UE channel bandwidth is applicable only to downlink

NOTE 2: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz.

NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.

NOTE 4: The minimum requirements only apply for non-simultaneous Tx/Rx between all carriers for TDD combinations.

NOTE 5: Simultaneous Rx/Tx capability for TDD combinations does not apply for UEs supporting band n78 with an n77 implementation.

NOTE 6: Only single uplink carriers with power class other than PC3 are listed.

NOTE 7: Minimum requirements for Power Class 2 are applicable for this uplink combination or single uplink carrier in this downlink/uplink combination

NOTE 8: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.

NOTE 9: Minimum requirements for Power Class 1.5 are applicable for single uplink carrier in this downlink/uplink combination

NOTE 10: For a band combination which include band n7 and n38 simultaneously, carriers in band n7 and n38 can only be configured as downlink carriers. Power imbalance between downlink carriers on Band n7 and Band n38 is assumed to be within 6dB.

NOTE 11: UL carrier shall be supported in Band n28 only. Power imbalance between downlink carriers on Band 7 and Band 38 is assumed to be within 6dB.

NOTE 12: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as a downlink SCell part of CA configuration

#### 5.5A.3.3 Configurations for inter-band CA (four bands)

Table 5.5A.3.3-1: Void

##### Table 5.5A.3.3-1a

Table 5.5A.3.3-1a: NR CA configurations and bandwidth combinations sets defined for inter-band CA (four bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier 4 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n1A-n3A-n5A-n7A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3A-n5A-n7B | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n5A-n28A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n28A  CA\_n3A-n5A  CA\_n3A-n28A  CA\_n5A-n28A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n5A-n78A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n78A  CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n8A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n26A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7A-n26A | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7B-n26A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7B-n26A | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n26(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7A-n26(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7B-n26(2A) | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7B-n26(2A) | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7A-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
| CA\_n1A-n3A-n7B-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  | CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7A-n28A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3B-n7B-n28A | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3A-n7A-n38A7 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3B-n7A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3B-n7A-n38A7 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3(2A)-n7A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3(2A)-n7A-n38A7 | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n7A-n40A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n40A  CA\_n3A-n7A  CA\_n3A-n40A  CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n67A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n75A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3B-n7A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7B-n78A | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n7B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n7B-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3B-n7B-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3A-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3A-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3B-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3B-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3B-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3B-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3(2A)-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3(2A)-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n3(2A)-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n3(2A)-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n3A-n7A-n105A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n105A  CA\_n3A-n7A  CA\_n3A-n105A  CA\_n7A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n105 | 5, 10,15, 20, 25, 30, 35 |  |
| CA\_n1A-n3A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n8A-n78A | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901, 100 |  |
| CA\_n1A-n3A-n18A-n28A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n28A  CA\_n3A-n18A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n3A-n18A-n41A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n41A  CA\_n3A-n18A  CA\_n3A-n41A  CA\_n18A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n18A-n77A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n77A  CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n20A-n67A | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n3A-n20A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A) BCS0 |  |
| CA\_n1A-n3A-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3B-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3B-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n28A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n28A-n41A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n77A | n775,6  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | n775  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n77(2A) | n775  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n3A-n28A-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202,302 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202, 302 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3B-n28A-n78A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n28A-n79A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n40A-n77A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n40A-n78A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n40A-n105A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n105A  CA\_n3A-n40A  CA\_n3A-n105A  CA\_n40A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n3A-n41A-n77A | n415  n775  CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n41A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n3A-n41A-n79A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n67A-n78A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n67A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n75A-n78A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n77A-n79A | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n77(2A)-n79A | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n78A-n105A | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25,30, 35 |  |
| CA\_n1A-n5A-n7A-n78A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n7B-n78A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n28A-n78A | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n5A-n28A  CA\_n5A-n78A  CA\_n28A-n78A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n28A-n79A | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n5A-n40A-n78A | CA\_n1A-n5A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n5A-n40A  CA\_n5A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n78A-n79A | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n5A-n78A  CA\_n5A-n79A  CA\_n78A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n8A-n40A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n40A  CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n7A-n8A-n78A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n26A-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n26A-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n26(2A)-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n26A-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A) BCS0 |  |
| CA\_n1A-n7A-n26(2A)-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7B-n26(2A)-n78A | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n26A-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7B-n26(2A)-n78(2A) | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n7A-n28A-n38A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n7A-n28A-n78A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n28A-n78A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7A-n38A-n78A7 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n40A-n78A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n40A-n105A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n105A  CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n7A-n67A-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n67A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7A-n75A-n78A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n78A-n105A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n8A-n40A-n78A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n8A-n78A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n8A-n78(2A)-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A-n41A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n28A-n77A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n18A-n41A-n77A | CA\_n1A-n18A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40A-n77A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40A-n78A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40B-n78A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n41A-n77A | n41**5**  n775,6  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n41A-n77(2A) | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n1A-n28A-n41A-n79A | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n28A-n75A-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n77A-n79A | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n28A-n78A-n79A | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n28A-n77(2A)-n79A | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n40A-n78A-n105A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n41A-n77A-n79A | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n41A-n77(2A)-n79A | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A-n30A-n66A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n30A-n66A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  | n5 | 5, 10, 15, 20 |
|  | n30 | 5, 10 |
|  | n66 | 10, 15, 20, 25, 30, 40 |
| CA\_n2A-n5A-n30A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  | n5 | 5, 10, 15, 20 |
|  | n30 | 5, 10 |
|  | n66 | CA\_n66(2A)\_BCS1 |
| CA\_n2A-n5A-n30A-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n30A-n77A | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n30A-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n30A-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n48A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48B-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48(2A)-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48(A-B)-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A-n77C | n775,6  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  | n775,6 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n5A-n48B-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48(2A)-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A5  CA\_n5A-n48A  CA\_n5A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n66A-n77A | n775,6  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n66A-n77A | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30,40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n66(2A)-n77A | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n66A-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66(2A)-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n5A-n66A-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66A-n77C | n775,6  CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n77A5  CA\_n5A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n12A-n30A-n66A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n30A-n66A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n30A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n30A-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n30A-n77A | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A-n77(2A) | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n30A-n77(2A) | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66A-n77A | n775,6  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n66A-n77A | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n66(2A)-n77A | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n66A-n77(2A) | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66(2A)-n77(2A) | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n66A-n77(2A) | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A-n66A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n30A-n66A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  | n14 | 5, 10 |
|  | n30 | 5, 10 |
|  | n66 | 5, 10, 15, 20, 25, 30, 40 |
| CA\_n2A-n14A-n30A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  | n14 | 5, 10 |
|  | n30 | 5, 10 |
|  | n66 | CA\_n66(2A)\_BCS1 |
| CA\_n2A-n14A-n30A-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n14A-n30A-n77A | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n30A-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n14A-n30A-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66A-n77A | n775,6  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n14A-n66A-n77A | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n66(2A)-n77A | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n66A-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(2A)-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n14A-n66A-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n30A-n77A | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n30A-n77(2A) | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n30A-n77(2A) | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n66A-n77A | n775,6  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n66A-n77A | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n66(2A)-n77A | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n66A-n77(2A) | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n66A-n77(2A) | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n66(2A)-n77(2A) | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66A-n77A | n775,6  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n30A-n66A-n77A | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n66(2A)-n77A | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n66A-n77(2A) | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66(2A)-n77(2A) | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n30A-n66A-n77(2A) | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n41A-n66A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n48A-n66A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48B-n66A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48(2A)-n66A-n77A | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n775,6  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n66A-n77C | n775,6 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  | n775,6  CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n48A-n66A  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 508, 608, 708, 808, 908, 1008 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n66A-n71A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A-n77(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A) BCS1 |  |
| CA\_n2A-n66A-n71A-n78A | - | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A-n78(2A) | - | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n7A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n7B-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n28A-n78A | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n5A-n28A-n79A | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n8A-n78A | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n7A-n20A-n67A | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n7A-n20A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n20A-n78A | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n20A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n7A-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7B-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A) BCS0 |  |
| CA\_n3A-n7A-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7B-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7B-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7B-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | CA\_n7B BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n7A-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n7A-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n7B-n26A-n78A | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n26(2A)-n78A | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n26A-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3B-n7B-n26(2A)-n78(2A) | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n3A-n7A-n28A-n38A7 | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n3A-n7A-n28A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n7A CA\_n3A-n28A  CA\_n3A-n78A CA\_n7A-n28A  CA\_n7A-n78A CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n7B-n28A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7A-n28A-n78A | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3B-n7B-n28A-n78A | CA\_n7B  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3B-n7B-n28A-n78(2A) | CA\_n7B  CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | CA\_n3B\_BCS0 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n7A-n38A-n78A7 | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n40A-n78A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n40A-n105A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n3A-n105A  CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n7A-n67A-n78A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n67A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n78(2A) | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n7A-n75A-n78A | - | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n78A-n105A | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n18A-n28A-n41A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n18A-n28A-n77A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n18A-n41A-n77A | CA\_n3A-n18A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n20A-n67A-n78A | CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n20A-n67A-n78(2A) | CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n28A-n38A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n40A-n77A | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n40 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n77A | CA\_n3A-n28A  CA\_n3A-n41A5  CA\_n3A-n77A5  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A5 | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n77(2A) | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n28A-n41A-n78A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n78(2A) | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n28A-n41A-n79A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n28A-n77A-n79A | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n28A-n77(2A)-n79A | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n40A-n78A-n105A | CA\_n3A-n40A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25,30, 35 |  |
| CA\_n3A-n41A-n77A-n79A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n41A-n77(2A)-n79A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |

**< Unchanged sections omitted>**

##### 6.2A.4.2.4 ΔTIB,c for Inter-band CA (three bands)

Table 6.2A.4.2.4-1: ΔTIB,c due to NR CA (three bands)

|  |  |  |  |
| --- | --- | --- | --- |
| Inter-band CA combination | ΔTIB,c for NR bands (dB)8 | | |
| Component band in order of bands in configuration9 | | |
| CA\_n1-n3-n5 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n7 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n8 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n18 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n20 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n26 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n28 | 0.3 | 0.3 | 0.6 |
| CA\_n1-n3-n38 | 0.5 | 0.5 | 0.3 |
| CA\_n1-n3-n40 | 0.5 | 0.5 | 0.5 |
| CA\_n1-n3-n41 | 0.5 | 0.5 | 0.35 / 0.86 |
| CA\_n1-n3-n75 | 0.3 | 0.3 | N/A |
| CA\_n1-n3-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n79 | 0.3 | 0.3 | 0.8 |
| CA\_n1-n3-n105 | 0.3 | 0.3 | 0.6 |
| CA\_n1-n5-n7 | 0.5 | 0.3 | 0.6 |
| CA\_n1-n5-n28 | 0.3 | 0.6 | 0.6 |
| CA\_n1-n5-n40 | 0.6 | 0.3 | 0.5 |
| CA\_n1-n5-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n5-n79 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n8 | 0.5 | 0.6 | 0.6 |
| CA\_n1-n7-n26 | 0.5 | 0.6 | 0.3 |
| CA\_n1-n7-n28 | 0.5 | 0.6 | 0.6 |
| CA\_n1-n7-n38 | 0.5 | N/A | N/A |
| CA\_n1-n7-n40 | 0.6 | 0.8 | 0.9 |
| CA\_n1-n7-n67 | 0.5 | 0.5 | N/A |
| CA\_n1-n7-n75 | 0.5 | 0.6 | N/A |
| CA\_n1-n7-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n79 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n105 | 0.5 | 0.6 | 0.6 |
| CA\_n1-n8-n28 | 0.3 | 0.6 | 0.6 |
| CA\_n1-n8-n40 | 0.3 | 0.3 | 0.5 |
| CA\_n1-n8-n77 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n8-n78 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n8-n79 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n18-n28 | 0.3 | 0.5 | 0.5 |
| CA\_n1-n18-n41 | 0.5 | 0.3 | 0.5 |
| CA\_n1-n18-n77 | 0.3 | 0.3 | 0.8 |
| CA\_n1-n20-n67 | 0.5 | 0.6 | N/A |
| CA\_n1-n20-n78 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n26-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n38 | 0.5 | 0.6 | 0.5 |
| CA\_n1-n28-n40 | 0.6 | 0.3 | 0.5 |
| CA\_n1-n28-n41 | 0.5 | 0.6 | 0.6 |
| CA\_n1-n28-n46 | 0.3 | 0.6 | - |
| CA\_n1-n28-n75 | 0.3 | 0.6 | N/A |
| CA\_n1-n28-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n78 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n28-n79 | - | 0.2 | 0.5 |
| CA\_n1-n28-n102 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n38-n78 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n40-n77 | 0.3 | 0.5 | 0.8 |
| CA\_n1-n40-n78 | 0.3 | 0.5 | 0.8 |
| CA\_n1-n40-n105 | 0.5 | 0.5 | 0.6 |
| CA\_n1-n41-n77 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n41-n79 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n46-n78 | 0.3 | - | 0.8 |
| CA\_n1-n67-n78 | 0.3 | N/A | 0.8 |
| CA\_n1-n75-n78 | 0.3 | N/A | 0.8 |
| CA\_n1-n77-n79 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n78-n79 | 0.3 | 0.8 / 1.57 | 0.5 / 1.57 |
| CA\_n1-n78-n102 | 0.6 | 1.5 | 1.5 |
| CA\_n1-n78-n105 | 0.3 | 0.8 | 0.6 |
| CA\_n2-n5-n30 | 0.5 | 0.3 | 0.3 |
| CA\_n2-n5-n41 | 0.5 | 0.6 | 0.45 / 0.96 |
| CA\_n2-n5-n48 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n5-n66 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n5-n77 | 0.6 | 0.8 | 0.8 |
| CA\_n2-n7-n12 | 0.5 | 0.5 | 0.3 |
| CA\_n2-n7-n71 | 0.5 | 0.5 | 0.6 |
| CA\_n2-n7-n66 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n7-n77 | 0.6 | 0.5 | 0.8 |
| CA\_n2-n12-n30 | 0.5 | 0.3 | 0.3 |
| CA\_n2-n12-n41 | 0.5 | 0.3 | 0.45 / 0.96 |
| CA\_n2-n12-n66 | 0.5 | 0.8 | 0.5 |
| CA\_n2-n12-n71 | 0.3 | 1 | 1 |
| CA\_n2-n12-n77 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n14-n30 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n14-n66 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n14-n77 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n29-n30 | 0.5 | N/A | 0.3 |
| CA\_n2-n29-n66 | 0.5 | N/A | 0.5 |
| CA\_n2-n29-n77 | 0.6 | N/A | 0.8 |
| CA\_n2-n30-n66 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n30-n77 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n41-n66 | 0.5 | 0.86 / 1.37 | 0.5 |
| CA\_n2-n41-n71 | 0.5 | 0.45/0.96 | 0.6 |
| CA\_n2-n48-n66 | 0.6 | 0.8 | 0.6 |
| CA\_n2-n48-n77 | 0.6 | 0.8 | 0.8 |
| CA\_n2-n66-n71 | 0.5 | 0.5 | 0.3 |
| CA\_n2-n66-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n2-n66-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n2-n71-n77 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n71-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n5-n7 | 0.5 | 0.3 | 0.5 |
| CA\_n3-n5-n28 | 0.3 | 0.6 | 0.5 |
| CA\_n3-n5-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n5-n79 | 0.3 | 0.5 | 0.8 |
| CA\_n3-n7-n8 | 0.5 | 0.5 | 0.6 |
| CA\_n3-n7-n20 | 0.5 | 0.5 | 0.3 |
| CA\_n3-n7-n26 | 0.5 | 0.5 | 0.3 |
| CA\_n3-n7-n28 | 0.5 | 0.5 | 0.3 |
| CA\_n3-n7-n38 | 0.5 | N/A | N/A |
| CA\_n3-n7-n67 | 0.5 | 0.5 | N/A |
| CA\_n3-n7-n40 | 0.6 | 0.6 | 0.6 |
| CA\_n3-n7-n75 | 0.7 | 0.7 | N/A |
| CA\_n3-n7-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n79 | 0.5 | 0.5 | 0.8 |
| CA\_n3-n7-n105 | 0.5 | 0.5 | 0.6 |
| CA\_n3-n8-n28 | 0.3 | 0.6 | 0.5 |
| CA\_n3-n8-n41 | 0.5 | 0.3 | 0.31 / 0.82 |
| CA\_n3-n8-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n8-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n8-n79 | 0.3 | 0.3 | 0.5 |
| CA\_n3-n18-n28 | 0.3 | 0.5 | 0.3 |
| CA\_n3-n18-n41 | 0.5 | 0.3 | 0.31 / 0.82 |
| CA\_n3-n18-n77 | 0.6 | 0.3 | 0.8 |
| CA\_n3-n20-n28 | 0.3 | 0.5 | 0.5 |
| CA\_n3-n20-n67 | 0.3 | 0.5 | N/A |
| CA\_n3-n20-n78 | 0.5 | 0.3 | 0.8 |
| CA\_n3-n26-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n28-n38 | 0.5 | 0.5 | 0.3 |
| CA\_n3-n28-n40 | 0.5 | 0.3 | 0.5 |
| CA\_n3-n28-n41 | 0.5 | 0.3 | 0.31 / 0.82 |
| CA\_n3-n28-n77 | 0.6 | 0.5 | 0.8 |
| CA\_n3-n28-n78 | 0.5 | 0.3 | 0.8 |
| CA\_n3-n28-n79 | 0.3 | 0.5 | 0.8 |
| CA\_n3-n38-n40 | 0.5 | 0.51,3 | 0.5 |
| CA\_n3-n40-n78 | 0.6 | 0.5 | 0.8 |
| CA\_n3-n40-n105 | 0.5 | 0.5 | 0.6 |
| CA\_n3-n67-n78 | 0.5 | N/A | 0.8 |
| CA\_n3-n75-n78 | 0.6 | N/A | 0.8 |
| CA\_n3-n77-n79 | 0.6 | 0.8 | - |
| CA\_n3-n78-n79 | 0.6 | 0.8 | 0.8 |
| CA\_n3-n78-n105 | 0.6 | 0.8 | 0.6 |
| CA\_n3-n40-n41 | 0.5 | 0.5 | 0.51 / 0.823 |
| CA\_n3-n40-n77 | 0.6 | 0.5 | 0.8 |
| CA\_n3-n41-n77 | 0.6 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n41-n78 | 0.6 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n41-n79 | 0.3 | 0.31 / 0.82 | 0.8 |
| CA\_n5-n7-n25 | 0.3 | 0.5 | 0.5 |
| CA\_n5-n7-n28 | 0.5 | 0.3 | 0.6 |
| CA\_n5-n7-n66 | 0.3 | 0.5 | 0.5 |
| CA\_n5-n7-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n7-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n12-n77 | 0.8 | 0.4 | 0.5 |
| CA\_n5-n14-n77 | 0.5 | 0.3 | 0.8 |
| CA\_n5-n25-n29 | 0.5 | 0.3 | N/A |
| CA\_n5-n25-n41 | 0.6 | 0.5 | 0.45 / 0.96 |
| CA\_n5-n25-n66 | 0.3 | 0.5 | 0.5 |
| CA\_n5-n25-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n25-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n28-n105 | 0.7 | 1.0 | 1.0 |
| CA\_n5-n28-n78 | 0.7 | 0.7 | 0.8 |
| CA\_n5-n28-n79 | 0.7 | 0.7 | 0.8 |
| CA\_n5-n29-n66 | 0.5 | N/A | 0.3 |
| CA\_n5-n29-n77 | 0.8 | N/A | 0.5 |
| CA\_n5-n30-n66 | 0.3 | 0.3 | 0.5 |
| CA\_n5-n30-n77 | 0.6 | 0.3 | 0.8 |
| CA\_n5-n40-n78 | 0.6 | 0.5 | 0.8 |
| CA\_n5-n41-n66 | 0.6 | 0.85 / 1.36 | 0.5 |
| CA\_n5-n41-n77 | 0.6 | 0.3 | 0.8 |
| CA\_n5-n48-n66 | 0.3 | 0.8 | 0.6 |
| CA\_n5-n48-n77 | 0.6 | 0.8 | 0.8 |
| CA\_n5-n66-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n5\_n66-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n5\_n78-n79 | 0.5 | 0.8 / 1.57 | 0.5 / 1.57 |
| CA\_n7-n8-n28 | 0.3 | 0.6 | 0.5 |
| CA\_n7-n8-n40 | 0.5 | 0.6 | 0.6 |
| CA\_n7-n8-n78 | 0.5 | 0.6 | 0.8 |
| CA\_n7-n12-n25 | 0.5 | 0.3 | 0.5 |
| CA\_n7-n12-n66 | 0.5 | 0.3 | 0.5 |
| CA\_n7-n12-n71 | 0.3 | 1 | 1 |
| CA\_n7-n12-n77 | 0.5 | 0.5 | 0.8 |
| CA\_n7-n20-n67 | 0.3 | 0.3 | N/A |
| CA\_n7-n20-n78 | 0.3 | 0.3 | 0.8 |
| CA\_n7\_n25-n66 | 0.5 | 0.5 | 0.5 |
| CA\_n7-n25-n71 | 0.5 | 0.5 | 0.3 |
| CA\_n7-n25-n77 | 0.5 | 0.6 | 0.8 |
| CA\_n7-n25-n78 | 0.5 | 0.6 | 0.8 |
| CA\_n7-n26-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n28-n38 | N/A | 0.3 | N/A |
| CA\_n7\_n28-n78 | 0.3 | 0.3 | 0.8 |
| CA\_n7-n40-n105 | 0.5 | 0.6 | 0.6 |
| CA\_n7-n46-n78 | 0.5 | - | 0.8 |
| CA\_n7-n66-n71 | 0.5 | 0.5 | 0.5 |
| CA\_n7-n66-n77 | 0.5 | 0.6 | 0.8 |
| CA\_n7\_n66-n78 | 0.5 | 0.6 | 0.8 |
| CA\_n7-n67-n78 | 0.5 | - | 0.8 |
| CA\_n7-n71-n77 | 0.3 | 0.5 | 0.8 |
| CA\_n7-n75-n78 | 0.7 | N/A | 0.8 |
| CA\_n7-n78-n102 | 0.5 | 1.5 | 1.5 |
| CA\_n7-n78-n105 | 0.3 | 0.8 | 0.5 |
| CA\_n8-n20-n28 | 0.8 | 0.7 | 0.7 |
| CA\_n8-n20-n75 | 0.4 | 0.4 | N/A |
| CA\_n8-n28-n75 | 0.6 | 0.5 | N/A |
| CA\_n8-n28-n78 | 0.6 | 0.5 | 0.8 |
| CA\_n8-n38-n40 | 0.3 | 0.3 | 0.3 |
| CA\_n8-n39-n41 | 0.6 | 0.5 | 0.5 |
| CA\_n8-n39-n79 | 0.3 | 0.3 | - |
| CA\_n8-n40-n41 | 0.3 | 0.3 | 0.3 |
| CA\_n8-n40-n78 | 0.6 | 0.3 | 0.8 |
| CA\_n8-n41-n79 | 0.6 | 0.3 | 0.8 |
| CA\_n8-n78-n79 | 0.6 | 0.8 | 0.8 |
| CA\_n12-n25-n41 | 0.3 | 0.5 | 0.45 / 0.96 |
| CA\_n12-n25-n66 | 0.8 | 0.5 | 0.5 |
| CA\_n12-n30-n66 | 0.8 | 0.3 | 0.5 |
| CA\_n12-n30-n77 | 0.5 | 0.3 | 0.5 |
| CA\_n12-n41-n66 | 0.5 | 0.5 | 0.5 |
| CA\_n12-n41-n77 | 0.5 | 0.5 | 0.8 |
| CA\_n12-n66-n77 | 0.8 | 0.6 | 0.8 |
| CA\_n12-n71-n77 | 1 | 1 | 0.8 |
| CA\_n13-n25-n66 | 0.3 | 0.5 | 0.5 |
| CA\_n13-n25-n77 | 0.3 | 0.6 | 0.8 |
| CA\_n13-n66-n77 | 0.5 | 0.6 | 0.8 |
| CA\_n14-n30-n66 | 0.3 | 0.3 | 0.5 |
| CA\_n14-n30-n77 | 0.5 | 0.3 | 0.8 |
| CA\_n14-n66-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n18-n28-n41 | 0.4 | 0.4 | 0.3 |
| CA\_n18-n28-n77 | 0.5 | 0.5 | 0.8 |
| CA\_n18-n41-n77 | 0.3 | 0.3 | 0.8 |
| CA\_n20-n28-n75 | 0.5 | 0.5 | N/A |
| CA\_n20-n28-n78 | 0.6 | 0.5 | 0.8 |
| CA\_n20-n67-n78 | 0.6 | N/A | 0.8 |
| CA\_n24-n41-n48 | 0.6 | 0.41 / 0.92 | 0.8 |
| CA\_n24-n41-n77 | 0.6 | 0.45 / 0.96 | 0.8 |
| CA\_n24-n48-n77 | 0.6 | 0.8 | 0.8 |
| CA\_n25-n29-n66 | 0.5 | N/A | 0.5 |
| CA\_n25-n38-n78 | 0.5 | 0.4 | 0.8 |
| CA\_n25-n41-n66 | 0.5 | 0.85 / 1.36 | 0.5 |
| CA\_n25-n41-n71 | 0.5 | 0.5 | 0.6 |
| CA\_n25-n41-n77 | 0.5 | 0.5 | 0.6 |
| CA\_n25-n41-n78 | 0.6 | 0.5 | 0.8 |
| CA\_n25-n41-n85 | 0.5 | 0.5 | 0.3 |
| CA\_n25-n48-n66 | 0.6 | 0.8 | 0.6 |
| CA\_n25-n66-n71 | 0.5 | 0.5 | 0.6 |
| CA\_n25-n66-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n66-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n66-n85 | 0.5 | 0.5 | 0.8 |
| CA\_n25-n71-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n71-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n71-n85 | 0.3 | 1 | 1 |
| CA\_n25-n77-n85 | 0.6 | 0.8 | 0.3 |
| CA\_n26-n29-n66 | 0.5 | N/A | 0.3 |
| CA\_n26-n29-n70 | 0.5 | N/A | 0.3 |
| CA\_n26-n48-n66 | 0.3 | 0.8 | 0.6 |
| CA\_n26-n48-n70 | 0.3 | 0.8 | 0.6 |
| CA\_n26-n66-n70 | 0.3 | 0.5 | 0.5 |
| CA\_n26-n66-n71 | 0.5 | 0.3 | 0.5 |
| CA\_n26-n66-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n26-n70-n71 | 0.5 | 0.3 | 0.6 |
| CA\_n26-n70-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n28-n38-n78 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n39-n40 | 0.3 | 0.3 | 0.3 |
| CA\_n28-n39-n41 | 0.3 | 0.5 | 0.5 |
| CA\_n28-n39-n79 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n40-n41 | 0.3 | 0.5 | 0.5 |
| CA\_n28-n40-n77 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n40-n78 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n40-n79 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n41-n79 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n41-n77 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n41-n78 | 0.5 | 0.3 | 0.8 |
| CA\_n28-n46-n78 | 0.5 | - | 0.8 |
| CA\_n28-n75-n78 | 0.3 | N/A | 0.8 |
| CA\_n28-n77-n79 | 0.5 | 0.8 | 0.5 |
| CA\_n28-n78-n79 | 0.5 | 0.8 / 1.57 | 0.5 / 1.57 |
| CA\_n28-n78-n102 | 0.5 | 1.5 | 1.5 |
| CA\_n29-n30-n66 | N/A | 0.3 | 0.5 |
| CA\_n29-n30-n77 | N/A | 0.3 | 0.5 |
| CA\_n29-n66-n70 | N/A | 0.5 | 0.5 |
| CA\_n29-n66-n71 | N/A | 0.3 | 0.5 |
| CA\_n29-n66-n77 | N/A | 0.6 | 0.8 |
| CA\_n29-n70-n71 | N/A | 0.3 | 0.6 |
| CA\_n30-n66-n77 | 0.3 | 0.6 | 0.8 |
| CA\_n34-n39-n41 | 0.3 | 0.5 | 0.5 |
| CA\_n34-n40-n41 | 0.3 | 0.5 | 0.5 |
| CA\_n34-n41-n79 | 0.3 | 0.5 | 0.8 |
| CA\_n38-n66-n78 | 0.5 | 0.5 | 0.8 |
| CA\_n39-n40-n41 | 0.3 | 0.3 | 0.3 |
| CA\_n39-n40-n79 | 0.3 | - | 0.8 |
| CA\_n39-n41-n79 | 0.3 | 0.3 | 0.8 |
| CA\_n40-n41-n79 | 0.5 | 0.5 | 0.8 |
| CA\_n40-n78-n105 | 0.3 | 0.8 | 0.5 |
| CA\_n41-n66-n71 | 0.8 / 1.36 | 0.5 | 0.3 |
| CA\_n41-n66-n77 | 0.5 | 0.6 | 0.8 |
| CA\_n41-n66-n78 | 0.5 | 0.6 | 0.8 |
| CA\_n41-n66-n85 | 0.81 / 1.32 | 0.5 | 0.6 |
| CA\_n41-n70-n78 | 0.6 | 0.6 | 0.8 |
| CA\_n41-n71-n77 | 0.3 | 0.5 | 0.8 |
| CA\_n41-n71-n78 | 0.3 | 0.5 | 0.8 |
| CA\_n41-n71-n85 | 0.3 | 1 | 1 |
| CA\_n41-n77-n79 | 0.3 | 0.8 | 0.8 |
| CA\_n41-n77-n85 | 0.6 | 0.8 | 0.8 |
| CA\_n46-n48-n96 | 0.5 | 0.8 | 0.6 |
| CA\_n46-n78-n102 | - | 1.5 | 1.5 |
| CA\_n48-n66-n70 | 0.8 | 0.6 | 0.6 |
| CA\_n48-n66-n71 | 0.5 | 0.5 | 0.3 |
| CA\_n48-n66-n77 | 0.8 | 0.6 | 0.8 |
| CA\_n48-n70-n71 | 0.5 | 0.5 | 0.3 |
| CA\_n48-n70-n77 | 0.8 | 0.6 | 0.8 |
| CA\_n48-n71-n77 | 0.8 | 0.6 | 0.8 |
| CA\_n66-n70-n71 | 0.5 | 0.5 | 0.6 |
| CA\_n66-n70-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n66-n71-n77 | 0.6 | 0.6 | 0.8 |
| CA\_n66-n71-n78 | 0.6 | 0.5 | 0.8 |
| CA\_n66-n71-n85 | 0.8 | 1 | 1 |
| CA\_n66-n77-n85 | 0.6 | 0.8 | 0.8 |
| CA\_n70-n71-n77 | 0.6 | 0.3 | 0.8 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2515-2690 MHz.  NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496-2515 MHz.  NOTE 3: Void.NOTE 4: Void.  NOTE 5: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 6: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz.  NOTE 7: The requirements only apply for UE supporting inter-band carrier aggregation with simultaneous Rx/Tx capability, and NR UL carrier frequencies are confined to 3700 MHz-3800MHz for n78 and 4400 MHz-4500MHz for n79. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation.  NOTE 8: “-” denotes ΔTIB,c = 0.  NOTE 9: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5 the band order from left to right is n1, n3 and n5. | | | |

##### 6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands)

Table 6.2A.4.2.5-1: ΔTIB,c due to NR CA (four bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔTIB,c for NR bands (dB)5 | | | |
| Component band in order of bands in configuration6 | | | |
| CA\_n1-n3-n5-n7 | 0.6 | 0.6 | 0.3 | - |
| CA\_n1-n3-n5-n28 | 0.3 | 0.3 | 0.7 | 0.7 |
| CA\_n1-n3-n5-n78 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n1-n3-n7-n8 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n26 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n28 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n38 | 0.6 | 0.6 | N/A | N/A |
| CA\_n1-n3-n7-n67 | 0.6 | 0.6 | 0.6 | N/A |
| CA\_n1-n3-n7-n40 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n75 | 0.6 | 0.6 | 0.6 | N/A |
| CA\_n1-n3-n7-n78 | 0.7 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n3-n7-n79 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n7-n105 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n8-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n18-n28 | 0.3 | 0.3 | 0.5 | 0.5 |
| CA\_n1-n3-n18-n41 | 0.5 | 0.5 | 0.3 | 0.33 / 0.84 |
| CA\_n1-n3-n18-n77 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n1-n3-n20-n67 | 0.3 | 0.3 | 0.3 | - |
| CA\_n1-n3-n26-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n38 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n28-n41 | 0.5 | 0.5 | 0.5 | 0.33 / 0.84 |
| CA\_n1-n3-n28-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n79 | 0.3 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n3-n40-n77 | 0.7 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n3-n40-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n40-n105 | 0.7 | 0.7 | 0.7 | 0.5 |
| CA\_n1-n3-n41-n77 | 0.6 | 0.6 | 0.33 / 0.84 | 0.8 |
| CA\_n1-n3-n41-n79 | 0.5 | 0.5 | 0.53 / 0.84 | 0.8 |
| CA\_n1-n3-n67-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n3-n75-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n3-n77-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n5-n28-n78 | 0.3 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n5-n28-n79 | 0.3 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n5-n40-n78 | 0.6 | 0.6 | 0.5 | 0.8 |
| CA\_n1-n5-n78-n79 | 0.6 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n7-n8-n40 | 0.6 | 0.8 | 0.6 | 0.9 |
| CA\_n1-n7-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n26-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n28-n38 | 0.5 | N/A | 0.6 | N/A |
| CA\_n1-n7-n28-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n40-n78 | 0.6 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n7-n40-n105 | 0.6 | 0.5 | 0.5 | 0.5 |
| CA\_n1-n7-n67-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n7-n75-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n7-n78-n105 | 0.6 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n8-n40-n78 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n1-n8-n78-n79 | 0.3 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n18-n28-n41 | 0.6 | 0.5 | 0.6 | 0.5 |
| CA\_n1-n18-n28-n77 | 0.6 | 0.5 | 0.6 | 0.8 |
| CA\_n1-n18-n41-n77 | 0.5 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n28-n38-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n40-n77 | 0.3 | 0.6 | 0.5 | 0.8 |
| CA\_n1-n28-n40-n78 | 0.3 | 0.6 | 0.5 | 0.8 |
| CA\_n1-n28-n41-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n41-n79 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n75-n78 | 0.5 | 0.6 | - | 0.8 |
| CA\_n1-n28-n77-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n28-n78-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n41-n77-n79 | 0.6 | 0.5 | 0.8 | 0.8 |
| CA\_n2-n5-n30-n66 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n5-n30-n77 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n5-n48-n66 | 0.6 | 0.3 | 0.8 | 0.6 |
| CA\_n2-n5-n48-n77 | 0.6 | 0.3 | 0.8 | 0.8 |
| CA\_n2-n5-n66-n77 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n2-n12-n30-n66 | 0.5 | 0.8 | 0.3 | 0.5 |
| CA\_n2-n12-n30-n77 | 0.6 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n12-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n14-n30-n66 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n14-n30-n77 | 0.6 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n14-n66-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n2-n29-n30-n66 | 0.5 | N/A | 0.3 | 0.5 |
| CA\_n2-n29-n30-n77 | 0.6 | N/A | 0.3 | 0.8 |
| CA\_n2-n29-n66-n77 | 0.6 | N/A | 0.6 | 0.8 |
| CA\_n2-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n2-n41-n66-n71 | 0.5 | 0.83 / 1.34 | 0.5 | 0.6 |
| CA\_n2-n48-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n66-n71-n77 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n66-n71-n78 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n3-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n5-n28-n78 | 0.6 | 0.7 | 0.7 | 0.8 |
| CA\_n3-n5-n28-n79 | 0.6 | 0.7 | 0.7 | 0.8 |
| CA\_n3-n7-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n20-n67 | 0.5 | 0.5 | 0.3 | - |
| CA\_n3-n7-n20-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n26-n78 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n3-n7-n28-n38 | 0.5 | N/A | 0.3 | N/A |
| CA\_n3-n7-n28-n78 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n3-n7-n40-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n40-n105 | 0.6 | 0.6 | 0.6 | 0.5 |
| CA\_n3-n7-n67-n78 | 0.6 | 0.6 | N/A | 0.6 |
| CA\_n3-n7-n75-n78 | 0.6 | 0.6 | N/A | 0.6 |
| CA\_n3-n7-n78-n105 | 0.6 | 0.6 | 0.8 | 0.5 |
| CA\_n3-n18-n28-n41 | 0.5 | 0.4 | 0.4 | 0.33 / 0.84 |
| CA\_n3-n18-n28-n77 | 0.6 | 0.5 | 0.5 | 0.8 |
| CA\_n3-n18-n41-n77 | 0.6 | 0.4 | 0.33 / 0.84 | 0.8 |
| CA\_n3-n20-n67-n78 | 0.5 | 0.5 | - | 0.8 |
| CA\_n3-n28-n40-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n28-n41-n77 | 1 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n41-n78 | 1 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n41-n79 | 0.5 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n77-n79 | 0.6 | 0.5 | 0.8 | 0.8 |
| CA\_n3-n41-n77-n79 | 0.6 | 0.31 / 0.82 | 0.8 | 0.8 |
| CA\_n5-n25-n29-n66 | 0.5 | 0.5 | N/A | 0.5 |
| CA\_n5-n25-n66-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n25-n66-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n28-n78-n79 | 0.7 | 0.7 | 0.8 | 0.8 |
| CA\_n5-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n5-n48-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n7-n8-n40-n78 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n7-n12-n25-n66 | 0.5 | 0.3 | 0.5 | 0.5 |
| CA\_n7-n20-n67-n78 | 0.6 | 0.6 | - | 0.8 |
| CA\_n7-n25-n66-n71 | 0.5 | 0.5 | 0.5 | 0.6 |
| CA\_n7-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n25-n66-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n40-n78-n105 | 0.5 | 0.6 | 0.8 | 0.5 |
| CA\_n8-n20-n28-n75 | 0.8 | 0.7 | 0.7 | - |
| CA\_n12-n30-n66-n77 | 0.8 | 0.3 | 0.6 | 0.8 |
| CA\_n13-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n14-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n18-n28-n41-n77 | 0.5 | 0.5 | 0.33 / 0.84 | 0.8 |
| CA\_n25-n38-n66-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n41-n66-n71 | 0.5 | 0.5 | 0.5 | 0.3 |
| CA\_n25-n41-n66-n77 | 0.5 | 0.83 / 1.34 | 0.5 | 0.8 |
| CA\_n25-n41-n66-n78 | 0.5 | 0.83 / 1.34 | 0.5 | 0.8 |
| CA\_n25-n41-n66-n85 | 0.5 | 0.5 | 0.5 | 0.3 |
| CA\_n25-n41-n71-n77 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n41-n71-n78 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n41-n71-n85 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n25-n41-n77-n85 | 0.5 | 0.5 | 0.8 | 0.6 |
| CA\_n25-n66-n71-n77 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n66-n71-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n66-n77-n85 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n28-n41-n77-n79 | 0.5 | 0.3 | 0.8 | 0.8 |
| CA\_n29-n30-n66-n77 | N/A | 0.3 | 0.6 | 0.8 |
| CA\_n29-n66-n70-n71 | N/A | 0.5 | 0.5 | 0.6 |
| CA\_n41-n66-n70-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n41-n66-n71-n77 | 0.33 / 0.84 | 1 | 0.5 | 0.8 |
| CA\_n41-n66-n71-n78 | 0.33 / 0.84 | 1 | 0.5 | 0.8 |
| CA\_n41-n66-n71-n85 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n41-n66-n77-n85 | 0.33 / 0.84 | 1 | 0.8 | 0.5 |
| CA\_n48-n66-n70-n77 | 0.8 | 0.6 | 0.6 | 0.8 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz.  NOTE 3: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 4: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz.  NOTE 5: “-” denotes ΔTIB,c = 0.  NOTE 6: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n78 the band order from left to right is n1, n3, n5 and n78. | | | | |

**< Unchanged sections omitted>**

##### 7.3A.3.2.3 ΔRIB,c for three bands

Table 7.3A.3.2.3-1: ΔRIB,c due to CA (three bands)

|  |  |  |  |
| --- | --- | --- | --- |
| Inter-band CA combination | ΔRIB,c for NR bands (dB)9 | | |
| Component band in order of bands in configuration10 | | |
| CA\_n1-n3-n8 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28 | - | - | 0.2 |
| CA\_n1-n3-n38 | 0.2 | 0.2 | - |
| CA\_n1-n3-n41 | - | - | 05 / 0.56 |
| CA\_n1-n3-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n79 | - | - | 0.5 |
| CA\_n1-n3-n105 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n5-n28 | - | 0.2 | 0.2 |
| CA\_n1-n5-n40 | - | 0.2 | - |
| CA\_n1-n5-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n79 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n7-n8 | - | - | 0.2 |
| CA\_n1-n7-n28 | - | - | 0.2 |
| CA\_n1-n7-n40 | - | 0.3 | 0.8 |
| CA\_n1-n7-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n7-n79 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n7-n105 | - | - | 0.3 |
| CA\_n1-n8-n28 | - | 0.2 | 0.2 |
| CA\_n1-n8-n40 | - | 0.2 | 0.5 |
| CA\_n1-n8-n77 | - | 0.2 | 0.5 |
| CA\_n1-n8-n78 | - | 0.2 | 0.5 |
| CA\_n1-n8-n79 | - | 0.2 | 0.5 |
| CA\_n1-n18-n77 | - | - | 0.5 |
| CA\_n1-n20-n67 | - | 0.2 | 0.2 |
| CA\_n1-n20-n78 | - | - | 0.5 |
| CA\_n1-n26-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n28-n38 | - | 0.2 | - |
| CA\_n1-n28-n40 | - | 0.2 | - |
| CA\_n1-n28-n41 | - | 0.2 | - |
| CA\_n1-n28-n46 | - | - | 0.5 |
| CA\_n1-n28-n75 | - | 0.2 | - |
| CA\_n1-n28-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n28-n78 | - | 0.2 | 0.5 |
| CA\_n1-n28-n102 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n38-n78 | - | - | 0.5 |
| CA\_n1-n40-n77 | - | - | 0.5 |
| CA\_n1-n40-n78 | - | - | 0.5 |
| CA\_n1-n40-n105 | - | - | 0.3 |
| CA\_n1-n41-n77 | 0.2 | - | 0.5 |
| CA\_n1-n41-n79 | - | 0.5 | 0.5 |
| CA\_n1-n46-n78 | - | - | 0.5 |
| CA\_n1-n67-n78 | - | - | 0.5 |
| CA\_n1-n75-n78 | - | - | 0.5 |
| CA\_n1-n77-n79 | 0.2 | 0.5 | - |
| CA\_n1-n78-n79 | - | 0.5 | - |
| CA\_n1-n78-n102 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n78-n105 | - | 0.5 | 0.2 |
| CA\_n2-n5-n30 | 0.4 | - | 0.5 |
| CA\_n2-n5-n41 | - | 0.2 | - |
| CA\_n2-n5-n48 | 0.2 | - | 0.5 |
| CA\_n2-n5-n66 | 0.3 | - | 0.3 |
| CA\_n2-n5-n77 | 0.2 | 0.5 | 0.5 |
| CA\_n2-n7-n71 | - | - | 0.2 |
| CA\_n2-n7-n66 | 0.3 | 0.5 | 0.5 |
| CA\_n2-n7-n77 | 0.2 | - | 0.5 |
| CA\_n2-n12-n30 | 0.4 | - | 0.5 |
| CA\_n2-n12-n41 | 0.5 | 0.3 | 0.45 / 0.96 |
| CA\_n2-n12-n66 | 0.3 | 0.5 | 0.3 |
| CA\_n2-n12-n71 | - | 0.8 | 0.8 |
| CA\_n2-n12-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n2-n14-n30 | 0.3 | - | 0.3 |
| CA\_n2-n14-n66 | 0.3 | - | 0.3 |
| CA\_n2-n14-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n2-n29-n30 | 0.3 | - | 0.3 |
| CA\_n2-n29-n66 | 0.3 | - | 0.3 |
| CA\_n2-n29-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n2-n30-n66 | 0.4 | 0.5 | 0.4 |
| CA\_n2-n30-n77 | 0.2 | - | 0.5 |
| CA\_n2-n41-n66 | 0.3 | 0.56 / 17 | 0.5 |
| CA\_n2-n41-n71 | - | - | 0.3 |
| CA\_n2-n48-n66 | 0.3 | 0.5 | 0.3 |
| CA\_n2-n48-n77 | 0.2 | 0.5 | 0.5 |
| CA\_n2-n66-n71 | 0.3 | 0.3 | - |
| CA\_n2-n66-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n2-n66-n78 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n71-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n5-n28 | - | 0.2 | 0.1 |
| CA\_n3-n5-n79 | - | 0.2 | 0.5 |
| CA\_n3-n7-n8 | - | - | 0.2 |
| CA\_n3-n7-n38 | - | 0.5 | 0.5 |
| CA\_n3-n7-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n79 | - | - | 0.5 |
| CA\_n3-n7-n105 | - | - | 0.3 |
| CA\_n3-n8-n28 | - | 0.2 | 0.1 |
| CA\_n3-n8-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n8-n41 | - | - | 01 / 0.52 |
| CA\_n3-n5-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n40 | 0.2 | 0.2 | 0.3 |
| CA\_n3-n8-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n18-n41 | - | - | 01 / 0.52 |
| CA\_n3-n18-n77 | 0.2 | - | 0.5 |
| CA\_n3-n20-n28 | - | 0.1 | 0.1 |
| CA\_n3-n20-n67 | - | 0.1 | 0.1 |
| CA\_n3-n20-n78 | 0.2 | - | 0.5 |
| CA\_n3-n26-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n28-n41 | - | - | 01 / 0.52 |
| CA\_n3-n28-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n28-n78 | - | 0.2 | 0.5 |
| CA\_n3-n28-n79 | - | 0.2 | 0.5 |
| CA\_n3-n40-n78 | 0.2 | - | 0.5 |
| CA\_n3-n40-n105 | - | - | 0.3 |
| CA\_n3-n67-n78 | - | 0.2 | 0.5 |
| CA\_n3-n77-n79 | 0.2 | 0.5 | - |
| CA\_n3-n78-n79 | 0.2 | 0.5 | 0.5 |
| CA\_n3-n40-n41 | - | - | 01 / 0.52 |
| CA\_n3-n41-n77 | 0.2 | 01 / 0.52 | 0.5 |
| CA\_n3-n41-n78 | 0.2 | 01 / 0.52 | 0.5 |
| CA\_n3-n41-n79 | - | 0.5 | 0.5 |
| CA\_n3-n75-n78 | 0.2 | - | 0.5 |
| CA\_n3-n78-n105 | 0.2 | 0.5 | 0.3 |
| CA\_n5-n7-n28 | - | - | 0.2 |
| CA\_n5-n7-n66 | - | 0.5 | 0.5 |
| CA\_n5-n7-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n7-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n12-n77 | 0.5 | 0.3 | 0.5 |
| CA\_n5-n14-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n25-n29 | 0.5 | - | 0.3 |
| CA\_n5-n25-n41 | 0.2 | - | - |
| CA\_n5-n25-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n25-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n28-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n28-n79 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n28-n105 | 0.2 | 0.7 | 0.7 |
| CA\_n5-n29-n66 | 0.5 | 0.3 | - |
| CA\_n5-n29-n77 | 0.5 | 0.3 | 0.5 |
| CA\_n5-n30-n66 | - | 0.5 | 0.4 |
| CA\_n5-n30-n77 | 0.2 | - | 0.5 |
| CA\_n5-n40-n78 | 0.2 | 0.4 | 0.5 |
| CA\_n5-n41-n66 | 0.2 | 0.55 / 16 | 0.5 |
| CA\_n5-n41-n77 | 0.2 | - | 0.5 |
| CA\_n5-n48-n66 | - | 0.5 | 0.2 |
| CA\_n5-n48-n77 | 0.2 | 0.5 | 0.5 |
| CA\_n5-n66-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n5-n66-n78 | 0.5 | 0.2 | 0.5 |
| CA\_n5-n78-n79 | 0.2 | 0.5 | - |
| CA\_n7-n8-n28 | - | 0.2 | 0.1 |
| CA\_n7-n8-n40 | - | 0.2 | 0.5 |
| CA\_n7-n8-n78 | - | 0.2 | 0.5 |
| CA\_n7-n12-n71 | 0.2 | 0.8 | 0.8 |
| CA\_n7-n12-n77 | 0.2 | 0.5 | 0.5 |
| CA\_n7-n20-n67 | - | 0.2 | 0.2 |
| CA\_n7-n20-n78 | - | - | 0.5 |
| CA\_n7-n25-n66 | 0.5 | 0.3 | 0.5 |
| CA\_n7-n25-n71 | 0.3 | 0.3 | - |
| CA\_n7-n25-n77 | 0.5 | 0.2 | 0.5 |
| CA\_n7-n25-n78 | 0.5 | 0.2 | 0.5 |
| CA\_n7-n26-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n7-n28-n78 | - | - | 0.5 |
| CA\_n7-n40-n105 | - | 0.5 | 0.2 |
| CA\_n7-n46-n78 | 0.5 | - | 0.5 |
| CA\_n7-n66-n71 | 0.5 | 0.5 | 0.1 |
| CA\_n7-n66-n77 | 0.5 | 0.5 | 0.5 |
| CA\_n7-n66-n78 | 0.5 | 0.5 | 0.5 |
| CA\_n7-n67-n78 | - | - | 0.5 |
| CA\_n7-n71-n77 | - | 0.2 | 0.5 |
| CA\_n7-n75-n78 | - | - | 0.5 |
| CA\_n7-n78-n102 | - | 0.5 | 0.5 |
| CA\_n7-n78-n105 | - | 0.5 | 0.2 |
| CA\_n8-n20-n28 | 0.3 | 0.2 | 0.2 |
| CA\_n8-n28-n75 | 0.2 | 0.2 | - |
| CA\_n8-n28-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n8-n39-n41 | - | 0.24 | 0.2 |
| CA\_n8-n40-n78 | 0.2 | 0.4 | 0.5 |
| CA\_n8-n41-n79 | - | 0.5 | 0.5 |
| CA\_n8-n78-n79 | 0.2 | 0.5 | 0.5 |
| CA\_n12-n25-n66 | 0.5 | 0.3 | 0.3 |
| CA\_n12-n30-n66 | 0.5 | 0.5 | 0.4 |
| CA\_n12-n30-n77 | 0.2 | - | 0.5 |
| CA\_n12-n41-n66 | 0.1 | 0.5 | 0.5 |
| CA\_n12-n41-n77 | 0.5 | 0.2 | 0.5 |
| CA\_n12-n66-n77 | 0.5 | 0.5 | 0.5 |
| CA\_n12-n71-n77 | 0.8 | 0.8 | 0.5 |
| CA\_n13-n25-n66 | - | 0.3 | 0.3 |
| CA\_n13-n25-n77 | - | 0.2 | 0.5 |
| CA\_n13-n66-n77 | 0.3 | 0.3 | 0.5 |
| CA\_n14-n30-n66 | - | 0.5 | 0.4 |
| CA\_n14-n30-n77 | 0.2 | - | 0.5 |
| CA\_n14-n66-n77 | 0.2 | 0.5 | 0.5 |
| CA\_n18-n28-n77 | - | - | 0.5 |
| CA\_n18-n41-n77 | - | - | 0.5 |
| CA\_n20-n28-n75 | - | 0.2 | - |
| CA\_n20-n28-n78 | - | 0.2 | 0.5 |
| CA\_n20-n67-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n24-n41-n48 | - | - | 0.5 |
| CA\_n24-n41-n77 | 0.2 | - | 0.5 |
| CA\_n24-n48-n77 | 0.2 | 0.5 | 0.5 |
| CA\_n25-n29-n66 | 0.3 | - | 0.3 |
| CA\_n25-n38-n78 | 0.2 | 0.4 | 0.5 |
| CA\_n25-n41-n66 | 0.3 | 0.55 / 16 | 0.3 |
| CA\_n25-n41-n71 | - | - | 0.2 |
| CA\_n25-n41-n78 | 0.2 | 0.5 | 0.5 |
| CA\_n25-n48-n66 | 0.3 | 0.5 | 0.3 |
| CA\_n25-n66-n71 | 0.3 | 0.3 | 0.3 |
| CA\_n25-n66-n78 | 0.3 | 0.3 | 0.5 |
| CA\_n25-n66-n77 | 0.3 | 0.3 | 0.5 |
| CA\_n25-n66-n85 | 0.3 | 0.3 | 0.5 |
| CA\_n25-n71-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n25-n71-n78 | 0.2 | 0.3 | 0.5 |
| CA\_n25-n71-n85 | - | 0.8 | 0.8 |
| CA\_n25-n77-n85 | 0.2 | 0.5 | 0.2 |
| CA\_n26-n29-n66 | 0.5 | 0.3 | - |
| CA\_n26-n29-n70 | 0.5 | 0.3 | - |
| CA\_n26-n48-n66 | - | 0.5 | 0.2 |
| CA\_n26-n48-n70 | - | 0.5 | 0.2 |
| CA\_n26-n66-n71 | 0.5 | - | 0.3 |
| CA\_n26-n66-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n26-n70-n71 | 0.5 | - | 0.3 |
| CA\_n26-n70-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n28-n38-n78 | 0.2 | - | 0.5 |
| CA\_n28-n39-n40 | - | 0.3 | 0.3 |
| CA\_n28-n39-n41 | - | 0.2 | 0.2 |
| CA\_n28-n39-n79 | 0.2 | - | 0.5 |
| CA\_n28-n40-n77 | - | - | 0.5 |
| CA\_n28-n40-n78 | - | - | 0.5 |
| CA\_n28-n40-n79 | 0.2 | - | 0.5 |
| CA\_n28-n41-n77 | 0.2 | - | 0.5 |
| CA\_n28-n41-n78 | 0.2 | - | 0.5 |
| CA\_n28-n41-n79 | 0.2 | 0.5 | 0.5 |
| CA\_n28-n46-n78 | 0.2 | - | 0.5 |
| CA\_n28-n75-n78 | 0.2 | - | 0.5 |
| CA\_n28-n77-n79 | 0.2 | 0.5 | - |
| CA\_n28-n78-n79 | 0.2 | 0.5 | - |
| CA\_n28-n78-n102 | 0.2 | 0.5 | 0.5 |
| CA\_n29-n30-n66 | - | 0.5 | 0.4 |
| CA\_n29-n30-n77 | 0.2 | - | 0.5 |
| CA\_n29-n66-n71 | 0.5 | 0.3 | 0.7 |
| CA\_n29-n66-n77 | 0.5 | 0.5 | 0.5 |
| CA\_n29-n70-n71 | 0.2 | 0.2 | 0.2 |
| CA\_n30-n66-n77 | 0.5 | 0.4 | 0.5 |
| CA\_n34-n39-n40 | 0.3 | 0.3 | 0.3 |
| CA\_n34-n39-n41 | 0.3 | 0.3 | 0.2 |
| CA\_n34-n40-n41 | 0.3 | 0.3 | - |
| CA\_n34-n41-n78 | - | 0.5 | 0.5 |
| CA\_n39-n40-n79 | 0.3 | 0.3 | 0.5 |
| CA\_n39-n41-n79 | 0 | 0.5 | 0.8 |
| CA\_n40-n41-n79 | 08 | 0.58 | 0.5 |
| CA\_n40-n78-n105 | 0.4 | 0.5 | 0.2 |
| CA\_n41-n66-n71 | 0.51 / 12 | 0.5 | - |
| CA\_n41-n66-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n41-n66-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n41-n66-n85 | 0.51 / 12 | 0.5 | 0.5 |
| CA\_n41-n70-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n41-n71-n77 | - | 0.2 | 0.5 |
| CA\_n41-n71-n78 | - | 0.2 | 0.5 |
| CA\_n41-n71-n85 | - | 0.8 | 0.8 |
| CA\_n41-n77-n79 | 0.5 | 0.5 | 0.5 |
| CA\_n41-n77-n85 | 0.5 | 0.5 | 0.5 |
| CA\_n46-n48-n96 | 0.5 | 0.5 | 0.6 |
| CA\_n48-n66-n70 | 0.5 | 0.2 | 0.2 |
| CA\_n46-n78-n102 | - | 0.5 | - |
| CA\_n48-n66-n71 | 0.2 | 0.2 | 0.2 |
| CA\_n48-n66-n77 | 0.5 | 0.2 | 0.5 |
| CA\_n48-n70-n71 | 0.2 | 0.2 | 0.2 |
| CA\_n48-n70-n77 | 0.5 | 0.2 | 0.5 |
| CA\_n48-n71-n77 | 0.5 | 0.2 | 0.5 |
| CA\_n66-n70-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n66-n71-n77 | 0.2 | 0.2 | 0.5 |
| CA\_n66-n71-n78 | 0.2 | 0.2 | 0.5 |
| CA\_n66-n71-n85 | - | 0.8 | 0.8 |
| CA\_n66-n77-n85 | 0.5 | 0.5 | 0.5 |
| CA\_n70-n71-n77 | 0.2 | 0.2 | 0.5 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz.  NOTE 3: Void.  NOTE 4: Void.  NOTE 5: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 6: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz.  NOTE 7: Void.  NOTE 8: Void.  NOTE 9: “-” denotes ΔRIB,c = 0.  NOTE 10: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n8 the band order from left to right is n1, n3 and n8. | | | |

##### 7.3A.3.2.4 ΔRIB,c for four bands

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔRIB,c for NR bands (dB)7 | | | |
| Component band in order of bands in configuration8 | | | |
| CA\_n1-n3-n5-n28 | 0.2 | 0.2 | 0.2 | 0.2 |
| CA\_n1-n3-n5-n78 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n3-n7-n8 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n26 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n28 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n40 | 0.2 | 0.2 | 0.2 | 0.3 |
| CA\_n1-n3-n7-n67 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n78 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n1-n3-n7-n79 | 0.2 | - | 0.2 | 0.5 |
| CA\_n1-n3-n7-n105 | 0.2 | - | 0.2 | 0.3 |
| CA\_n1-n3-n8-n77 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n8-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n18-n28 | - | - | - | 0.2 |
| CA\_n1-n3-n18-n41 | - | - | - | 05 / 0.56 |
| CA\_n1-n3-n18-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n3-n20-n67 | - | - | - | 0.2 |
| CA\_n1-n3-n26-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28-n38 | - | - | 0.2 | - |
| CA\_n1-n3-n28-n41 | - | - | 0.2 | 05 / 0.56 |
| CA\_n1-n3-n28-n77 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28-n79 | - | - | 0.2 | 0.5 |
| CA\_n1-n3-n40-n77 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n1-n3-n40-n78 | 0.2 | 0.2 | 0.3 | 0.5 |
| CA\_n1-n3-n40-n105 | 0.3 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n41-n77 | 0.2 | 0.2 | 05 / 0.56 | 0.5 |
| CA\_n1-n3-n41-n79 | - | - | 05 / 0.56 | 0.5 |
| CA\_n1-n3-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n75-n78 | - | - | - | 0.5 |
| CA\_n1-n3-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n5-n7-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n28-n79 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n40-n78 | 0.2 | 0.2 | 0.4 | 0.5 |
| CA\_n1-n5-n78-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n7-n8-n40 | - | - | 0.3 | 0.8 |
| CA\_n1-n7-n8-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n7-n26-n78 | 0.2 | 0.2 | - | - |
| CA\_n1-n7-n28-n38 | - | - | 0.2 | - |
| CA\_n1-n7-n28-n78 | 0.2 | 0.2 | - | - |
| CA\_n1-n7-n40-n78 | 0.2 | - | 0.4 | 0.5 |
| CA\_n1-n7-n40-n105 | 0.2 | - | 0.4 | 0.3 |
| CA\_n1-n7-n67-n78 | 0.2 | 0.2 | - | - |
| CA\_n1-n7-n75-n78 | - | - | - | 0.5 |
| CA\_n1-n7-n78-n105 | 0.2 | 0.2 | 0.5 | 0.3 |
| CA\_n1-n8-n40-n78 | 0.2 | - | 0.4 | 0.5 |
| CA\_n1-n8-n78-n79 | 0.3 | 0.3 | 0.5 | - |
| CA\_n1-n18-n28-n41 | 0.2 | - | 0.2 | - |
| CA\_n1-n18-n28-n77 | 0.2 | - | 0.2 | 0.5 |
| CA\_n1-n18-n41-n77 | 0.2 | - | - | 0.5 |
| CA\_n1-n28-n38-n78 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n28-n40-n77 | - | 0.2 | - | 0.5 |
| CA\_n1-n28-n40-n78 | - | 0.2 | - | 0.5 |
| CA\_n1-n28-n41-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n28-n41-n79 | - | 0.2 | 0.5 | 0.5 |
| CA\_n1-n28-n75-n78 | - | 0.2 | - | 0.5 |
| CA\_n1-n28-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n28-n78-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n41-n77-n79 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n5-n30-n66 | 0.4 | - | 0.5 | 0.4 |
| CA\_n2-n5-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n5-n48-n66 | 0.2 | - | 0.5 | 0.2 |
| CA\_n2-n5-n48-n77 | 0.2 | - | 0.5 | 0.5 |
| CA\_n2-n5-n66-n77 | 0.3 | - | 0.3 | 0.5 |
| CA\_n2-n12-n30-n66 | 0.4 | 0.5 | 0.5 | 0.4 |
| CA\_n2-n12-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n12-n66-n77 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n14-n30-n66 | 0.4 | - | 0.5 | 0.4 |
| CA\_n2-n14-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n14-n66-n77 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n2-n29-n30-n66 | 0.4 | - | 0.5 | 0.4 |
| CA\_n2-n29-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n30-n66-n77 | 0.2 | 0.5 | 0.4 | 0.5 |
| CA\_n2-n41-n66-n71 | 0.3 | 0.51 / 12 | 0.5 | 0.3 |
| CA\_n2-n48-n66-n77 | 0.3 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n66-n71-n77 | 0.3 | 0.5 | - | 0.5 |
| CA\_n2-n66-n71-n78 | 0.3 | 0.5 | - | 0.5 |
| CA\_n3-n5-n7-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n5-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n5-n28-n79 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n8-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n20-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n26-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n40-n78 | 0.2 | 0.2 | 0.3 | 0.5 |
| CA\_n3-n7-n40-n105 | 0.2 | 0.2 | 0.2 | 0.3 |
| CA\_n3-n7-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n75-n78 | - | - | - | 0.5 |
| CA\_n3-n7-n78-n105 | 0.2 | 0.2 | 0.5 | 0.3 |
| CA\_n3-n18-n28-n41 | - | - | - | 05 / 0.56 |
| CA\_n3-n18-n28-n77 | 0.2 | - | 0.2 | 0.5 |
| CA\_n3-n18-n41-n77 | 0.2 | - | 05 / 0.56 | 0.5 |
| CA\_n3-n20-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n28-n40-n77 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n28-n41-n77 | 0.5 | 0.2 | 01 / 0.52 | 0.5 |
| CA\_n3-n28-n41-n78 | 0.5 | 0.2 | 01 / 0.52 | 0.5 |
| CA\_n3-n28-n41-n79 | - | 0.2 | 0.5 | 0.5 |
| CA\_n3-n28-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n3-n41-n77-n79 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n5-n25-n29-n66 | 0.5 | - | 0.3 | - |
| CA\_n5-n25-n66-n77 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n5-n25-n66-n78 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n5-n28-n78-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n5-n30-n66-n77 | 0.2 | 0.4 | 0.4 | 0.5 |
| CA\_n5-n48-n66-n77 | 0.2 | 0.5 | 0.2 | 0.5 |
| CA\_n7-n8-n40-n78 | - | 0.2 | 0.4 | 0.5 |
| CA\_n7-n12-n25-n66 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n7-n20-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n7-n25-n66-n71 | 0.5 | 0.3 | 0.5 | 0.3 |
| CA\_n7-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n25-n66-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n40-n78-n105 | 0.5 | 0.5 | 0.8 | 0.3 |
| CA\_n8-n20-n28-n75 | 0.3 | 0.2 | 0.2 | - |
| CA\_n12-n30-n66-n77 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n13-n25-n66-n77 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n14-n30-n66-n77 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n18-n28-n41-n77 | - | 0.2 | 05 / 0.56 | 0.5 |
| CA\_n25-n38-n66-n78 | 0.3 | 0.4 | 0.3 | 0.5 |
| CA\_n25-n41-n66-n71 | 0.3 | 0.5 | 0.5 | - |
| CA\_n25-n41-n66-n77 | 0.3 | 0.53 / 1.04 | 0.3 | 0.5 |
| CA\_n25-n41-n66-n78 | 0.3 | 0.53 / 1.04 | 0.3 | 0.5 |
| CA\_n25-n41-n66-n85 | 0.3 | 0.5 | 0.5 | - |
| CA\_n25-n41-n71-n77 | - | - | 0.2 | 0.5 |
| CA\_n25-n41-n77-n85 | - | - | 0.5 | 0.2 |
| CA\_n25-n41-n71-n78 | - | - | 0.2 | 0.5 |
| CA\_n25-n41-n71-n85 | 0.3 | 0.5 | - | 0.2 |
| CA\_n25-n66-n71-n77 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n25-n66-n71-n78 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n25-n66-n77-n85 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n28-n41-n77-n79 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n29-n30-n66-n77 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n29-n66-n70-n71 | 0.5 | 0.3 | 0.2 | 0.7 |
| CA\_n41-n66-n70-n78 | - | 0.2 | 0.2 | 0.5 |
| CA\_n41-n66-n71-n77 | 03 / 0.54 | 0.5 | 0.2 | 0.5 |
| CA\_n41-n66-n71-n78 | 03 / 0.54 | 0.5 | 0.2 | 0.5 |
| CA\_n41-n66-n71-n85 | 0.5 | 0.3 | - | 0.2 |
| CA\_n41-n66-n77-n85 | 03 / 0.54 | 0.5 | 0.5 | 0.2 |
| CA\_n48-n66-n70-n77 | 0.5 | 0.2 | 0.2 | 0.5 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz  NOTE 5: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 6: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz  NOTE 7: “-” denotes ΔRIB,c = 0.  NOTE 8: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n7-n78 the band order from left to right is n1 n3, n7 and n78. | | | | |

**< Unchanged sections omitted>**

Table 7.3A.5-2: 3DL/2UL interband Reference sensitivity QPSK PREFSENS and uplink/downlink configurations

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Band / Channel bandwidth / NRB / Duplex mode | | | | | | | | Source of IMD |
| NR CA band combination | NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | Duplex mode |  |
| CA\_n1-n3-n28 | n1 | 1975 | 5 | 25 | 2165 | N/A | FDD | N/A |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1818.5 | 4.0 | FDD | IMD5 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
|  | n1 | N/A | 5 | N/A | 2139 | 11.0 | FDD | IMD4 |
| CA\_n1-n3-n40 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | 1735 | 5 | 25 | 1830 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2380 | 8.0 | TDD | IMD5 |
| CA\_n1-n3-n41 | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | FDD | N/A |
|  | n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2507.5 | 5.0 | TDD | IMD5 |
| CA\_n1-n3-n77 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | 1750 | 5 | 25 | 1845 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3700 | 28.4 | TDD | IMD22 |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1807.5 | 31.5 | FDD | IMD21,2 |
|  | n77 | 3757.5 | 10 | 50 | 3757.5 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 31.0 | FDD | IMD21 |
|  | n3 | 1775 | 5 | 25 | 1870 | N/A | FDD | N/A |
|  | n77 | 3915 | 10 | 50 | 3915 | N/A | TDD | N/A |
| CA\_n1-n3-n78 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | 1750 | 5 | 25 | 1845 | N/A |  | N/A |
|  | n78 | N/A | 10 | N/A | 3700 | 28.4 | TDD | IMD2 |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A |  | N/A |
|  | n78 | N/A | 10 | N/A | 3360 | 11.2 | TDD | IMD4 |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1830 | 27.9 |  | IMD2 |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
| CA\_n1-n3-n79 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4950 | 4.7 | TDD | IMD5 |
|  | n3 | 1750 | 5 | 25 | 1845 | N/A | FDD | N/A |
|  | n79 | 4860 | 40 | 216 | 4860 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 3.6 | FDD | IMD5 |
| CA\_n1-n3-n105 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1855 | 4 | FDD | IMD5 |
|  | n105 | 695 | 5 | 25 | 644 | N/A | FDD | N/A |
|  | n1 | N/A | 5 | N/A | 2160 | 5 | FDD | IMD4 |
|  | n3 | 1775 | 5 | 25 | 1870 | N/A | FDD | N/A |
|  | n105 | 695 | 5 | 25 | 644 | N/A | FDD | N/A |
| CA\_n1-n5-n7 | n1 | 1968 | 5 | 25 | 2158 | N/A | FDD | N/A |
|  | n7 | 2512 | 10 | 50 | 2632 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 880 | 1.0 | FDD | IMD5 |
| CA\_n1-n5-n28 | n1 | N/A | 5 | N/A | 2123 | 4 | FDD | IMD5 |
|  | n5 | 829 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n28 | 738 | 5 | 25 | 793 | N/A | FDD | N/A |
|  | n1 | 1965 | 5 | 25 | 2155 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 875 | 4.6 | FDD | IMD5 |
|  | n28 | 710 | 5 | 25 | 765 | N/A | FDD | N/A |
| CA\_n1-n5-n40 | n1 | N/A | 5 | N/A | 2144 | 4.0 | FDD | IMD5 |
|  | n5 | 832 | 5 | 25 | 877 | N/A | FDD | N/A |
|  | n40 | 2320 | 5 | 25 | 2320 | N/A | TDD | N/A |
|  | n1 | 1945 | 5 | 25 | 2135 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 880 | 8.0 | FDD | IMD4 |
|  | n40 | 2385 | 5 | 25 | 2385 | N/A | TDD | N/A |
|  | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | FDD | N/A |
|  | n5 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2305 | 9.0 | TDD | IMD4 |
| CA\_n1-n5-n78 | n1 | N/A | 5 | N/A | 2122 | 18.1 | FDD | IMD3 |
|  | n5 | 829 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
|  | n1 | 1975 | 5 | 25 | 2165 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 885 | 3.1 | FDD | IMD5 |
|  | n78 | 3405 | 10 | 50 | 3405 | N/A | TDD | N/A |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3610 | 15.7 | TDD | IMD3 |
| CA\_n1-n5-n79 | n1 | N/A | 5 | N/A | 2160 | 1.2 | FDD | IMD4 |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n79 | 4650 | 40 | 100 | 4650 | N/A | TDD | N/A |
|  | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 890 | 15.2 | FDD | IMD3 |
|  | n79 | 4750 | 40 | 100 | 4750 | N/A | TDD | N/A |
|  | n1 | 1923 | 5 | 25 | 2113 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 879 | 10.3 | FDD | IMD4 |
|  | n79 | 4890 | 40 | 100 | 4890 | N/A | TDD | N/A |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n5 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4785 | 14.9 | TDD | IMD3 |
|  | n1 | 1940 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n5 | 830 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4430 | 9.4 | TDD | IMD4 |
| CA\_n1-n7-n8 | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | FDD | N/A |
|  | n7 | 2502.5 | 5 | 25 | 2622.5 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 927.5 | 1.0 | FDD | IMD5 |
| CA\_n1-n7-n26 | n1 | 1965 | 5 | 25 | 2155 | N/A | FDD | N/A |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 875 | 3.5 | FDD | IMD5 |
| CA\_n1-n7-n28 | n1 | 1935 | 5 | 25 | 2125 | N/A | FDD | N/A |
|  | n7 | N/A | 10 | N/A | 2653 | 30.0 | FDD | IMD2 |
|  | n28 | 718 | 5 | 25 | 773 | N/A | FDD | N/A |
|  | n1 | 1935 | 5 | 25 | 2125 | N/A | FDD | N/A |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | N/A |
|  | n28 | N/A | 10 | N/A | 785 | 4.5 | FDD | IMD5 |
| CA\_n1-n7-n40 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2630 | 23 | FDD | IMD3 |
|  | n40 | 2390 | 5 | 25 | 2390 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2120 | 16.4 | FDD | IMD3 |
|  | n7 | 2530 | 5 | 25 | 2650 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
| CA\_n1-n7-n67 | n1 | 1948 | 5 | 25 | 2138 | N/A | FDD | N/A |
|  | n7 | 2548 | 5 | 25 | 2668 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 748 | 3.3 | SDL | IMD5 |
| CA\_n1-n7-n78 | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2627.5 | 9.1 | FDD | IMD4 |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 8.7 | FDD | IMD4 |
|  | n7 | 2510 | 10 | 50 | 2630 | N/A | FDD | N/A |
|  | n78 | 3580 | 10 | 50 | 3580 | N/A | TDD | N/A |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n7 | 2520 | 5 | 25 | 2640 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3390 | 10.1 | TDD | IMD4 |
| CA\_n1-n7-n105 | n1 | 1935 | 5 | 25 | 2125 | N/A | FDD | N/A |
|  | n7 | 2565 | 10 | 50 | 2685 | N/A | FDD | N/A |
|  | n105 | N/A | 5 | N/A | 630 | 28.7 | FDD | IMD2 |
|  | n1 | 1925 | 5 | 25 | 2115 | N/A | FDD | N/A |
|  | n7 | 2565 | 10 | 50 | 2565 | N/A | FDD | N/A |
|  | n105 | N/A | 5 | N/A | 645 | 1 | FDD | IMD5 |
|  | n1 | 1968.5 | 5 | 25 | 2158.5 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2634.5 | 30 | FDD | IMD22 |
|  | n105 | 666 | 5 | 25 | 615 | N/A | FDD | N/A |
| CA\_n1-n8-n40 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 930 | 8.0 | FDD | IMD4 |
|  | n40 | 2395 | 5 | 25 | 2395 | N/A | TDD | N/A |
| CA\_n1-n8-n78 | n1 | 1945 | 5 | 25 | 2135 | N/A | FDD | N/A |
|  | n8 | 900 | 5 | 25 | 945 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3745 | 14.9 | TDD | IMD3 |
|  | n1 | 1940 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 940 | 3.3 | FDD | IMD5 |
|  | n78 | 3380 | 10 | 50 | 3380 | N/A | TDD | N/A |
| CA\_n1-n18-n28 | n1 | 1965 | 5 | 25 | 2155 | N/A | FDD | N/A |
|  | n28 | 708 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n18 | N/A | 5 | N/A | 867 | 4.6 | FDD | IMD5 |
|  | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n28 | 738 | 5 | 25 | 793 | N/A | FDD | N/A |
|  | n1 | N/A | 5 | N/A | 2127 | 4 | FDD | IMD5 |
| CA\_n1-n18-n41 | n1 | 1960 | 5 | 25 | 2150 | N/A | FDD | N/A |
|  | n41 | 2505 | 10 | 50 | 2505 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 870 | 3.3 | FDD | IMD5 |
| CA\_n1-n18-n77 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3600 | 15.7 | TDD | IMD31 |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3390 | 10 | 50 | 3390 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 870 | 3.5 | FDD | IMD5 |
|  | n1 | N/A | 5 | N/A | 2120 | 16.4 | FDD | IMD3 |
|  | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n77 | 3770 | 10 | 50 | 3770 | N/A | TDD | N/A |
| CA\_n1-n26-n78 | n1 | N/A | 5 | N/A | 2122 | 18.1 | FDD | IMD3 |
|  | n26 | 829 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
|  | n1 | 1975 | 5 | 25 | 2165 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 885 | 3.1 | FDD | IMD5 |
|  | n78 | 3405 | 10 | 50 | 3405 | N/A | TDD | N/A |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n26 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3610 | 15.7 | TDD | IMD3 |
| CA\_n1-n28-n41 | n1 | 1935 | 5 | 25 | 2125 | N/A | FDD | N/A |
|  | n28 | 718 | 5 | 25 | 773 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2653 | 30.1 | TDD | IMD22 |
|  | n1 | 1923 | 5 | 25 | 2113 | N/A | FDD | N/A |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 762 | 29.3 | FDD | IMD21 |
| CA\_n1-n28-n46 | n1 | 1975 | 5 | 25 | 2165 | N/A | FDD | N/A |
|  | n28 | 710 | 5 | 25 | 765 | N/A | FDD | N/A |
|  | n46 | N/A | 20 | N/A | 5215 | N/A | TDD | IMD4 |
|  | n1 | 1975 | 5 | 25 | 2165 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 765 | 10.5 | FDD | IMD4 |
|  | n46 | 5160 | 20 | 100 | 5160 | N/A | TDD | N/A |
| CA\_n1-n28-n77 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n28 | 733 | 5 | 25 | 788 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3416 | 15.7 | TDD | IMD32 |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 790 | 4.2 | FDD | IMD5 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n77 | 3630 | 10 | 50 | 3630 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2150 | 15.7 | FDD | IMD3 |
| CA\_n1-n28-n78 | n1 | N/A | 5 | N/A | 2150 | 15.7 | FDD | IMD3 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3630 | 10 | 50 | 3630 | N/A | TDD | N/A |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 794 | 4.2 | FDD | IMD5 |
|  | n78 | 3352 | 10 | 50 | 3352 | N/A | TDD | N/A |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n28 | 733 | 5 | 25 | 788 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3416 | 15.7 | TDD | IMD3 |
| CA\_n1-n28-n79 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n28 | 730 | 5 | 25 | 785 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4630 | 14.9 | TDD | IMD31 |
|  | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n79 | 4648 | 40 | 216 | 4648 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 788 | 15.2 | FDD | IMD32 |
|  | n28 | 745.5 | 5 | 25 | 800.5 | N/A | FDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2167.5 | 1.2 | FDD | IMD41 |
| CA\_n1-n28-n102 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n28 | 706 | 5 | 25 | 761 | N/A | FDD | N/A |
|  | n102 | N/A | 40 | N/A | 5978 | N/A12 | TDD | IMD5 |
| CA\_n1-n40-n77 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3480 | 9.8 | TDD | IMD41 |
|  | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2340 | 10.6 | TDD | IMD41 |
|  | n77 | 3450 | 10 | 50 | 3450 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 9.1 | FDD | IMD4 |
|  | n40 | 2380 | 5 | 25 | 2380 | N/A | TDD | N/A |
|  | n77 | 3450 | 10 | 50 | 3450 | N/A | TDD | N/A |
| CA\_n1-n40-n78 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3480 | 9.8 | TDD | IMD41 |
|  | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2340 | 10.6 | TDD | IMD4 |
|  | n78 | 3450 | 10 | 50 | 3450 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 9.1 | FDD | IMD4 |
|  | n40 | 2380 | 5 | 25 | 2380 | N/A | TDD | N/A |
|  | n78 | 3450 | 10 | 50 | 3450 | N/A | TDD | N/A |
| CA\_n1-n40-n105 | n1 | 1977 | 5 | 25 | 2167 | N/A | FDD | N/A |
|  | n40 | 2305 | 10 | 50 | 2305 | N/A | TDD | N/A |
|  | n105 | N/A | 5 | N/A | 649 | 1dB | FDD | IMD4 |
| CA\_n1-n41-n77 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n41 | 2650 | 10 | 50 | 2650 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3330 | 19.6 | TDD | IMD31,2 |
|  | n1 | 1975 | 5 | 10 | 2165 | N/A | FDD | N/A |
|  | n77 | 3410 | 10 | 50 | 3410 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2515 | 11.5 | TDD | IMD41 |
|  | n41 | 2640 | 10 | 50 | 2640 | N/A | TDD | N/A |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 9.3 | FDD | IMD4 |
| CA\_n1-n41-n79 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n41 | 2530 | 10 | 50 | 2530 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4500 | 19.0 | TDD | IMD21 |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n79 | 4500 | 40 | 216 | 4500 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2530 | 29.4 | TDD | IMD21 |
|  | n41 | 2530 | 10 | 50 | 2530 | N/A | TDD | N/A |
|  | n79 | 4690 | 40 | 216 | 4690 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2160 | 29.9 | FDD | IMD21 |
| CA\_n1-n46-n78 | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n46 | 5430 | 20 | 100 | 5430 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3500 | 29 | TDD | IMD2 |
|  | n1 | N/A | 5 | N/A | 2130 | 30 | FDD | IMD2 |
|  | n46 | 5630 | 20 | 100 | 5630 | N/A | TDD | N/A |
|  | n78 | 3500 | 10 | 50 | 3500 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2120 | 15 | FDD | IMD3 |
|  | n46 | 5160 | 20 | 100 | 5160 | N/A | TDD | N/A |
|  | n78 | 3640 | 10 | 50 | 3640 | N/A | TDD | N/A |
|  | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n46 | N/A | 20 | N/A | 5430 | N/A | TDD | IMD2 |
|  | n78 | 3500 | 10 | 50 | 3500 | N/A | TDD | N/A |
|  | n1 | 1930 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n46 | N/A | 20 | N/A | 5250 | N/A | TDD | IMD3 |
|  | n78 | 3590 | 10 | 50 | 3590 | N/A | TDD | N/A |
| CA\_n1-n67-n78 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 748 | 3.5 | SDL | IMD5 |
|  | n78 | 3329 | 10 | 50 | 3329 | N/A | TDD | N/A |
| CA\_n1-n77-n79 | n1 | N/A | 5 | N/A | 2140 | 15.6 | FDD | IMD31,2 |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n79 | 4660 | 40 | 216 | 4660 | N/A | TDD | N/A |
| CA\_n1-n78-n79 | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n78 | 3410 | 10 | 50 | 3410 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4870 | 15.9 | TDD | IMD31,3 |
|  | n1 | 1950 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3490 | 4.6 | TDD | IMD53 |
|  | n79 | 4670 | 40 | 216 | 4670 | N/A | TDD | N/A |
|  | n1 | N/A | 5 | N/A | 2140 | 15.6 | FDD | IMD31,2 |
|  | n78 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n79 | 4660 | 40 | 216 | 4660 | N/A | TDD | N/A |
| CA\_n1-n78-n102 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n78 | 3320 | 5 | 25 | 3320 | N/A | TDD | N/A |
|  | n102 | N/A | 40 | N/A | 6020 | N/A12 | TDD | IMD5 |
|  | n1 | N/A | 5 | N/A | 2155 | 29.9 | FDD | IMD21 |
|  | n78 | 3790 | 5 | 25 | 3790 | N/A | TDD | N/A |
|  | n102 | 5945 | 40 | 216 | 5945 | N/A | TDD | N/A |
| CA\_n1-n78-n105 | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n105 | N/A | 5 | N/A | 635 | 15.2 | FDD | IMD3 |
|  | n1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3342 | 15.7 | TDD | IMD3 |
|  | n105 | 686 | 5 | 25 | 635 | N/A | FDD | N/A |
|  | n1 | N/A | 5 | N/A | 2160 | 15.7 | FDD | IMD3 |
|  | n78 | 3532 | 10 | 50 | 3532 | N/A | TDD | N/A |
|  | n105 | 686 | 5 | 25 | 635 | N/A | FDD | N/A |
| CA\_n2-n5-n30 | n2 | 1870 | 5 | 25 | 1959 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 880 | 9.7 | FDD | IMD4 |
|  | n30 | 2310 | 10 | 50 | 2355 | N/A | FDD | N/A |
| CA\_n2-n5-n41 | n2 | 1855 | 10 | 50 | 1935 | N/A | FDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2685 | 30.0 | TDD | IMD2 |
| CA\_n2-n5-n48 | n2 | N/A | 5 | N/A | 1962 | 15.6 | FDD | IMD3 |
|  | n5 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n48 | 3640 | 10 | 50 | 3640 | N/A | TDD | N/A |
|  | n2 | 1905 | 5 | 25 | 1985 | N/A | FDD | N/A |
|  | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n48 | N/A | 10 | 50 | 3593 | 16.6 | TDD | IMD3 |
| CA\_n2-n5-n66 | n2 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2140 | 7.2 | FDD | IMD4 |
| CA\_n2-n5-n77 | n2 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 887.5 | 3.8 | FDD | IMD55 |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1987 | 16.5 | FDD | IMD35 |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n77 | 3680 | 10 | 50 | 3680 | N/A | TDD | N/A |
|  | n2 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3540 | 16.0 | TDD | IMD31 |
| CA\_n2-n12-n30 | n2 | 1885 | 5 | 25 | 1965 | N/A | FDD | N/A |
|  | n12 | 708.5 | 5 | 25 | 738.5 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2353 | 12.0 | FDD | IMD4 |
| CA\_n2-n12-n71 | n2 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n12 | N/A | 5 | N/A | 743.5 | 4.2 | FDD | IMD5 |
|  | n71 | 665.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
| CA\_n2-n12-n77 | n2 | N/A | 5 | N/A | 1960 | 16.5 | FDD | IMD32,5 |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n77 | 3375 | 10 | 50 | 3375 | N/A | TDD | N/A |
|  | n2 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3315 | 16.0 | TDD | IMD31,2,5 |
| CA\_n2-n14-n66 | n2 | 1874 | 5 | 25 | 1954 | N/A | FDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2162 | 7.6 | FDD | IMD4 |
|  | n2 | N/A | 5 | N/A | 1954 | 7.2 | FDD | IMD4 |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
| CA\_n2-n14-n77 | n2 | N/A | 5 | N/A | 1954 | 16.5 | FDD | IMD3 |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
|  | n2 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3466 | 16.0 | TDD | IMD31 |
| CA\_n2-n30-n77 | n2 | N/A | 5 | N/A | 1986 | 8.6 | FDD | IMD45 |
|  | n30 | 2312 | 5 | 25 | 2357 | N/A | FDD | N/A |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n2 | 1905 | 5 | 25 | 1985 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2354 | 10.6 | FDD | IMD45 |
|  | n77 | 3361 | 10 | 50 | 3361 | N/A | TDD | N/A |
|  | n2 | 1860 | 5 | 25 | 1940 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2354 | 3.4 | FDD | IMD5 |
|  | n77 | 3967 | 10 | 50 | 3967 | N/A | TDD | N/A |
|  | n2 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4180 | 29.4 | TDD | IMD22,5 |
| CA\_n2-n48-n66 | n2 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
|  | n48 | N/A | 10 | 50 | 3625 | 32.0 | TDD | IMD2 |
|  | n66 | 1770 | 5 | 25 | 2190 | N/A | FDD | N/A |
|  | n2 | 1905 | 5 | 25 | 1985 | N/A | FDD | N/A |
|  | n48 | 3560 | 10 | 50 | 3560 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2155 | 12.1 | FDD | IMD4 |
|  | n2 | N/A | 5 | N/A | 1960 | 28.3 | FDD | IMD21 |
|  | n48 | 3695 | 10 | 50 | 3695 | N/A | TDD | N/A |
|  | n66 | 1735 | 5 | 25 | 2135 | N/A | FDD | N/A |
| CA\_n2-n66-n77 | n2 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3620 | 29.4 | TDD | IMD25 |
|  | n2 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3900 | 8.9 | TDD | IMD4 |
|  | n2 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2115 | 29.2 | FDD | IMD2 |
|  | n77 | 3970 | 10 | 50 | 3970 | N/A | TDD | N/A |
|  | n2 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2140 | 10.4 | FDD | IMD4 |
|  | n77 | 3500 | 10 | 50 | 3500 | N/A | TDD | N/A |
|  | n2 | 1885 | 5 | 25 | 1965 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2175 | 4.0 | FDD | IMD5 |
|  | n77 | 3915 | 10 | 50 | 3915 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1960 | 32.1 | FDD | IMD2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1960 | 9.1 | FDD | IMD45 |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
|  | n77 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1960 | 2.1 | FDD | IMD55 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
| CA\_n3-n5-n7 | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n5 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n7 | N/A | 10 | N/A | 2625 | 30.0 | FDD | IMD24 |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 880 | 19.0 | FDD | IMD3 |
|  | n7 | 2560 | 10 | 50 | 2680 | N/A | FDD | N/A |
| CA\_n3-n5-n28 | n3 | N/A | 5 | N/A | 1829.5 | 8.7 | FDD | IMD4 |
|  | n5 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n28 | 705.5 | 5 | 25 | 760.5 | N/A | FDD | N/A |
|  | n3 | 1713 | 5 | 25 | 1808 | N/A | FDD | N/A |
|  | n5 | 827 | 5 | 25 | 872 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 768 | 9.4 | FDD | IMD4 |
| CA\_n3-n5-n78 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n5 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3408 | 16.1 | TDD | IMD3 |
|  | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n5 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3512 | 4.5 | TDD | IMD5 |
|  | n3 | N/A | 5 | N/A | 1862 | 15.7 | FDD | IMD3 |
|  | n5 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n3-n5-n79 | n3 | N/A | 5 | N/A | 1877.5 | 8.8 | FDD | IMD4 |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 860 | 15.3 | FDD | IMD3 |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 890 | 10.3 | FDD | IMD4 |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n3 | 1782.5 | 5 | 25 | 1875.5 | N/A | FDD | N/A |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4420 | 15.7 | TDD | IMD3 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n5 | 846 | 5 | 25 | 891 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4494 | 9.4 | TDD | IMD4 |
| CA\_n3-n7-n8 | n3 | 1735 | 5 | 25 | 1830 | N/A | FDD | N/A |
|  | n7 | 2530 | 10 | 50 | 2650 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 940 | 18.0 | FDD | IMD3 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n7 | N/A | 10 | N/A | 2670 | 29.0 | FDD | IMD24 |
|  | n8 | 890 | 5 | 25 | 935 | N/A | FDD | N/A |
| CA\_n3-n7-n20 | n3 | 1747 | 5 | 25 | 1842 | N/A | FDD | N/A |
|  | n7 | 2543 | 10 | 50 | 2663 | N/A | FDD | N/A |
|  | n20 | N/A | 5 | N/A | 796 | 20.0 | FDD | IMD2 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n7 | N/A | 10 | N/A | 2625 | 29.0 | FDD | IMD2 |
|  | n20 | 845 | 5 | 25 | 804 | N/A | FDD | N/A |
|  | n3 | 1750 | 5 | 25 | 1845 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | 25 | N/A | 17.0 | FDD | IMD3 |
|  | n20 | 835 | 5 | 25 | 794 | N/A | FDD | N/A |
| CA\_n3-n7-n26 | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n7 | 2560 | 10 | 50 | 2680 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 880 | 17.5 | FDD | IMD3 |
|  | n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
|  | n7 | N/A | 10 | N/A | 2625 | 29.0 | FDD | IMD24 |
|  | n26 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
| CA\_n3-n7-n28 | n3 | 1747 | 5 | 25 | 1842 | N/A | FDD | N/A |
|  | n7 | 2543 | 5 | 25 | 2663 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 796 | 20.0 | FDD | IMD2 |
|  | n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2682 | 17.0 | FDD | IMD3 |
|  | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1832.5 | 26 | FDD | IMD2 |
|  | n7 | 2543 | 5 | 25 | 2663 | N/A | FDD | N/A |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
| CA\_n3-n7-n40 | n3 | 1770 | 10 | 50 | 1865 | 4.5 | FDD | IMD5 |
|  | n7 | 2525 | 10 | 50 | 2645 | N/A | FDD | N/A |
|  | n40 | 2305 | 10 | 50 | 2305 | N/A | TDD | N/A |
| CA\_n3-n7-n67 | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n7 | 2520 | 5 | 25 | 2640 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 750 | 20 | SDL | IMD2 |
| CA\_n3-n7-n78 | n3 | N/A | 5 | N/A | 1820 | 17.6 | FDD | IMD3 |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | N/A |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1820 | 8.6 | FDD | IMD4 |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | N/A |
|  | n78 | 3475 | 10 | 50 | 3475 | N/A | TDD | N/A |
|  | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3390 | 16.1 | TDD | IMD3 |
| CA\_n3-n7-n105 | n3 | N/A | 5 | N/A | 1875 | 16.5 | FDD | IMD2 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n105 | 675 | 5 | 25 | 624 | N/A | FDD | N/A |
| CA\_n3-n8-n41 | n3 | 1722.5 | 5 | 25 | 1817.5 | N/A | FDD | N/A |
|  | n8 | 887.5 | 5 | 25 | 932.5 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2610 | 28.0 | FDD | IMD24 |
|  | n3 | 1725 | 5 | 25 | 1820 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 945 | 26.0 | FDD | IMD24 |
|  | n41 | 2516 | 10 | 50 | 2516 | N/A | FDD | N/A |
| CA\_n3-n8-n78 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3550 | 16.1 | TDD | IMD3 |
|  | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3370 | 4.5 | TDD | IMD5 |
|  | n3 | N/A | 5 | N/A | 1820 | 15.7 | FDD | IMD3 |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n78 | 3640 | 10 | 50 | 3640 | N/A | TDD | N/A |
| CA\_n3-n8-n79 | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n8 | 885 | 5 | 25 | 930 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4425 | 15.7 | TDD | IMD32 |
|  | n3 | 1755 | 5 | 25 | 1850 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 955 | 15.3 | FDD | IMD3 |
|  | n79 | 4465 | 40 | 216 | 4465 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1850 | 8.8 | FDD | IMD4 |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n79 | 4580 | 40 | 216 | 4580 | N/A | FDD | N/A |
| CA\_n3-n18-n28 | n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 770 | 9.4 | FDD | IMD4 |
|  | n18 | 827.5 | 5 | 25 | 872.5 | N/A | FDD | N/A |
| CA\_n3-n18-n41 | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2540 | [N/A]1 | TDD | IMD2 |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n3 | 1725 | 5 | 25 | 1820 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2630 | 16.0 | TDD | IMD3 |
|  | n18 | N/A | 5 | N/A | 865 | 28.9 | FDD | IMD2 |
|  | n3 | 1765 | 5 | 25 | 1860 | N/A | FDD | N/A |
|  | n41 | 2630 | 10 | 50 | 2630 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 875 | [19.0] | FDD | IMD3 |
|  | n3 | 1725 | 5 | 25 | 1820 | N/A | FDD | N/A |
|  | n41 | 2670 | 5 | 25 | 2670 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1850 | 28.8 | FDD | IMD2 |
|  | n41 | 2670 | 10 | 50 | 2670 | N/A | TDD | N/A |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
| CA\_n3-n18-n77 | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3410 | 16.3 | TDD | IMD31,2 |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n3 | N/A | 5 | N/A | 1865 | 15.7 | FDD | IMD3 |
|  | n77 | 3505 | 10 | 50 | 3505 | N/A | TDD | N/A |
| CA\_n3-n20-n28 | n3 | N/A | 5 | N/A | 1828 | 9.4 | FDD | IMD4 |
|  | n20 | 852 | 5 | 25 | 811 | N/A | FDD | N/A |
|  | n28 | 728 | 5 | 25 | 783 | N/A | FDD | N/A |
|  | n3 | 1748 | 5 | 25 | 1843 | N/A | FDD | N/A |
|  | n20 | 847 | 5 | 25 | 806 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 793 | 9.4 | FDD | IMD4 |
| CA\_n3-n20-n67 | n3 | 1775 | 5 | 25 | 1870 | N/A | FDD | N/A |
|  | n20 | 840 | 5 | 25 | 799 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 745 | 9.4 | FDD | IMD4 |
| CA\_n3-n20-n78 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n20 | 845 | 5 | 25 | 804 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3420 | 16.1 | TDD | IMD31 |
|  | n3 | N/A | 5 | N/A | 1820 | 17.3 | FDD | IMD3 |
|  | n20 | 845 | 5 | 25 | 804 | N/A | FDD | N/A |
|  | n78 | 3510 | 10 | 50 | 3510 | N/A | TDD | N/A |
| CA\_n3-n26-n78 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n26 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3408 | 16.1 | TDD | IMD3 |
|  | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n26 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3512 | 4.5 | TDD | IMD5 |
|  | n3 | N/A | 5 | N/A | 1862 | 15.7 | FDD | IMD3 |
|  | n26 | 839 | 5 | 25 | 884 | N/A | FDD | N/A |
|  | n78 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n3-n28-n41 | n3 | 1715 | 5 | 25 | 1810 | N/A | FDD | N/A |
|  | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2518 | 27.4 | TDD | IMD2 |
|  | n3 | 1715 | 5 | 25 | 1810 | N/A | FDD | N/A |
|  | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2687 | 15.9 | TDD | IMD3 |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n41 | 2510 | 5 | 25 | 2510 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 790 | 26.0 | FDD | IMD24 |
|  | n28 | 710.5 | 5 | 25 | 765.5 | N/A | FDD | N/A |
|  | n41 | 2543 | 10 | 50 | 2543 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1832.5 | 26.0 | FDD | IMD2 |
| CA\_n3-n28-n77 | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n28 | 733 | 5 | 25 | 788 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4173 | 15.9 | TDD | IMD3 |
|  | n28 | 735 | 5 | 25 | 790 | N/A | FDD | N/A |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1850 | 17.0 | FDD | IMD3 |
|  | n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | FDD | N/A |
|  | n77 | 4195 | 10 | 50 | 4195 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 770 | 15.3 | FDD | IMD3 |
| CA\_n3-n28-n78 | n28 | 735 | 5 | 25 | 790 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3320 | N/A | TDD | IMD3 |
|  | n3 | 1755 | 5 | 25 | 1850 | 17.3 | FDD | N/A |
|  | n3 | 1750 | 5 | 25 | 1845 | N/A | FDD | N/A |
|  | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3764 | 4.5 | TDD | IMD5 |
| CA\_n3-n28-n79 | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n28 | 725 | 5 | 25 | 780 | N/A | FDD | N/A |
|  | n79 | N/A | 40 | N/A | 4585 | 9.4 | TDD | IMD41 |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n79 | 4530 | 40 | 216 | 4530 | N/A | TDD | N/A |
|  | n28 | 725 | 5 | 25 | 780 | 10.3 | FDD | IMD4  |3\*fBn3-fBn79| |
|  | n28 | 725 | 5 | 25 | 780 | N/A | FDD | N/A |
|  | n79 | 4770 | 40 | 216 | 4770 | N/A | TDD | N/A |
|  | n3 | 1775 | 5 | 25 | 1870 | 5.7 | FDD | IMD5  |4\*fBn28-fBn79| |
| CA\_n3-40-n41 | n3 | N/A | 5 | N/A | 1842.5 | 1.0 | FDD | IMD5 |
|  | n40 | 2347.5 | 5 | 25 | 2347.5 | N/A | TDD | N/A |
|  | n41 | 2600 | 10 | 50 | 2600 | N/A | TDD | N/A |
| CA\_n3-n40-n77 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n40 | 2320 | 5 | 25 | 2320 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 4050 | 19.0 | TDD | IMD21 |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2310 | 29.4 | TDD | IMD21 |
|  | n77 | 4030 | 10 | 50 | 4030 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1820 | 29.9 | FDD | IMD22 |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n77 | 4130 | 10 | 50 | 4130 | N/A | TDD | N/A |
| CA\_n3-n40-n105 | n3 | 1745 | 5 | 25 | 1840 | N/A | FDD | N/A |
|  | n40 | 2380 | 10 | 50 | 2380 | N/A | TDD | N/A |
|  | n105 | N/A | 5 | N/A | 635 | 26.0 | FDD | IMD24 |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n40 | N/A | 10 | N/A | 2388 | 26.0 | TDD | IMD2 |
|  | n105 | 668 | 5 | 25 | 617 | N/A | FDD | N/A |
| CA\_n3-n41-n77 | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n77 | 3900 | 10 | 50 | 3900 | N/A | TDD | N/A |
|  | n41 | N/A | 5 | N/A | 2640 | 5.3 | TDD | IMD5 |
|  | n41 | 2620 | 5 | 25 | 2620 | N/A | TDD | N/A |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1840 | 16.4 | FDD | IMD3 |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3440 | 16.8 | TDD | IMD31 |
| CA\_n3-n41-n78 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n41 | 2560 | 10 | 50 | 2560 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3390 | 16.4 | TDD | IMD3 |
|  | n3 | N/A | 5 | N/A | 1840 | 16.4 | TDD | IMD3 |
|  | n41 | 2620 | 5 | 25 | 2620 | N/A | FDD | N/A |
|  | n78 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
| CA\_n3-n41-n79 | n3 | N/A | 5 | N/A | 1850 | 29.4 | FDD | IMD21 |
|  | n41 | 2570 | 10 | 50 | 2570 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2670 | 30.2 | TDD | IMD21 |
|  | n79 | 4440 | 40 | 216 | 4440 | N/A | TDD | N/A |
|  | n3 | 1770 | 5 | 25 | 1865 | N/A | FDD | N/A |
|  | n41 | 2670 | 10 | 50 | 2670 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4440 | 30.8 | TDD | IMD21 |
| CA\_n3-n67-n78 | n3 | N/A | 5 | N/A | 1877.5 | 2.2 | FDD | IMD7 |
|  | n67 | N/A | 5 | N/A | N/A | N/A | SDL | N/A |
|  | n7810 | 3305 | 10 | 1 (RBSTART=25) | 3305 | N/A | TDD | N/A |
|  |  | 3780 | 10 | 1 (RBSTART=25) | 3780 |  |  |  |
| CA\_n3-n77-n79 | n77 | 3350 | 10 | 50 | 3350 | N/A | FDD | N/A |
|  | n79 | 4840 | 40 | 216 | 4840 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 15.7 | TDD | IMD31, 2  |2\*fBn77-fBn79| |
| CA\_n3-n78-n105 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3740 | 17.3 | TDD | IMD44 |
|  | n105 | 670 | 5 | 25 | 619 | N/A | FDD | N/A |
| CA\_n5-n7-n25 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2685 | 30.0 | FDD | IMD2 |
|  | n25 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
| CA\_n5-n7-n66 | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2624 | 29.0 | FDD | IMD2 |
|  | n66 | 1777.5 | 5 | 25 | 2177.5 | N/A | FDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2670 | 13 | FDD | IMD3 |
|  | n66 | 1750 | 5 | 25 | 2150 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 880 | 13 | FDD | IMD3 |
|  | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
| CA\_n5-n7-n77 | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 30.1 | FDD | IMD2 |
|  | n77 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 879 | 30.2 | FDD | IMD21, 4 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n77 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n5 | 827 | 5 | 25 | 852 | N/A | FDD | N/A |
|  | n7 | 2503 | 5 | 25 | 2623 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3330 | 30.2 | TDD | IMD22, 4 |
| CA\_n5-n7-n78 | n5 | N/A | 5 | N/A | 879 | 30.2 | FDD | IMD2 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n78 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 875 | 3.3 | FDD | IMD5 |
|  | n7 | 2525 | 5 | 25 | 2645 | N/A | FDD | N/A |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 30.1 | FDD | IMD2 |
|  | n78 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n7 | 2540 | 5 | 25 | 2660 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3375 | 29.7 | TDD | IMD2 |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3430 | 9.7 | TDD | IMD4 |
| CA\_n5-n12-n77 | n5 | N/A | 5 | N/A | 880 | 3.9 | FDD | IMD5 |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n12 | N/A | 5 | N/A | 740 | 4.4 | FDD | IMD55 |
|  | n77 | 4080 | 10 | 50 | 4080 | N/A | TDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3905 | 4.4 | TDD | IMD5 |
| CA\_n5-n14-n77 | n5 | N/A | 5 | N/A | 880 | 3.9 | FDD | IMD55 |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n77 | 4052 | 10 | 50 | 4052 | N/A | TDD | N/A |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n14 | N/A | 5 | N/A | 765.5 | 11.6 | FDD | IMD41,5 |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n5 | 840 | 5 | 25 | 885 | N/A | FDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3313 | 10.3 | TDD | IMD41,5 |
| CA\_n5-n25-n41 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n25 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2685 | 30.0 | TDD | IMD2 |
| CA\_n5-n25-n66 | n5 | 834 | 5 | 25 | 879 | N/A | FDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2132 | 7.2 | FDD | IMD4 |
| CA\_n5-n25-n77 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3540 | 16.0 | TDD | IMD3 |
|  | n5 | N/A | 5 | N/A | 889 | 3.8 | FDD | IMD55 |
|  | n25 | 1907 | 5 | 25 | 1987 | N/A | FDD | N/A |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1987 | 16.5 | FDD | IMD3 |
|  | n77 | 3680 | 10 | 25 | 3680 | N/A | TDD | N/A |
| CA\_n5-n25-n78 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3560 | 16.1 | TDD | IMD3 |
|  | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1987 | 16.5 | FDD | IMD3 |
|  | n78 | 3680 | 10 | 50 | 3680 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 887.5 | 3.8 | FDD | IMD5 |
|  | n25 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
| CA\_n5-n28-n78 | n5 | N/A | 5 | N/A | 874 | 3.8 | FDD | IMD5 |
|  | n28 | 723 | 5 | 25 | 778 | N/A | FDD | N/A |
|  | n78 | 3766 | 10 | 50 | 3756 | N/A | TDD | N/A |
|  | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 778 | 11.6 | FDD | IMD4 |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n28 | 707 | 5 | 25 | 762 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3781 | 4.0 | TDD | IMD5 |
| CA\_n5-n28-n105 | n5 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n105 | 686 | 5 | 25 | 635 | 25.0 | FDD | IMD3 |
| CA\_n5-n29-n66 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n29 | N/A | 5 | N/A | 720 | 9.4 | SDL | IMD4 |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
| CA\_n5-n29-n77 | n5 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n29 | N/A | 5 | N/A | 720 | 4.4 | SDL | IMD55 |
|  | n77 | 4100 | 10 | 50 | 4100 | N/A | TDD | N/A |
| CA\_n5-n30-n66 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n30 | 2307.5 | 5 | 25 | 2352.5 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2125 | 4 | FDD | IMD5 |
| CA\_n5-n30-n77 | n5 | N/A | 5 | N/A | 880 | 15.2 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3740 | 10 | 50 | 3740 | N/A | TDD | N/A |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 13.2 | FDD | IMD35 |
|  | n77 | 4025 | 10 | 50 | 4025 | N/A | TDD | N/A |
|  | n5 | 840 | 5 | 25 | 885 | N/A | FDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3780 | 16.1 | TDD | IMD3 |
| CA\_n5-n40-n78 | n5 | N/A | 5 | N/A | 880 | 15.2 | FDD | IMD3 |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | 3740 | 10 | 50 | 3740 | N/A | TDD | N/A |
|  | n5 | 840 | 5 | 25 | 885 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3780 | 16.1 | TDD | IMD3 |
| CA\_n5-n41-n66 | n5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2624 | 29.0 | TDD | IMD24 |
|  | n66 | 1777.5 | 5 | 25 | 2177.5 | N/A | FDD | N/A |
|  | n5 | N/A | 5 | N/A | 875 | 28.9 | FDD | IMD24 |
|  | n41 | 2640 | 10 | 50 | 2640 | N/A | TDD | N/A |
|  | n66 | 1765 | 5 | 25 | 2165 | N/A | FDD | N/A |
| CA\_n5-n41-n77 | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n41 | 2540 | 5 | 25 | 2540 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3375 | 29.7 | TDD | IMD22 |
|  | n5 | 840 | 5 | 25 | 885 | N/A | FDD | N/A |
|  | n41 | 2500 | 5 | 25 | 2500 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 4160 | 16.1 | TDD | IMD3 |
|  | n5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2645 | 30.1 | TDD | IMD2 |
|  | n77 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2510 | 13.2 | FDD | IMD3 |
|  | n77 | 4180 | 10 | 50 | 4180 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 879 | 30.2 | FDD | IMD2 |
|  | n41 | 2550 | 5 | 25 | 2550 | N/A | TDD | N/A |
|  | n77 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 900 | 15.2 | FDD | IMD31 |
|  | n41 | 2500 | 5 | 25 | 2500 | N/A | TDD | N/A |
|  | n77 | 4100 | 10 | 50 | 4100 | N/A | TDD | N/A |
| CA\_n5-n48-n66 | n5 | 829 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n48 | N/A | 10 | N/A | 3622 | 3.6 | TDD | IMD5 |
|  | n66 | 1760 | 5 | 216 | 2160 | N/A | FDD | N/A |
| CA\_n5-n66-n77 | n5 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n66 | 1775 | 5 | 25 | 2175 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3465 | 16.1 | TDD | IMD3 |
|  | n5 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4192 | 8.2 | TDD | IMD45 |
|  | n5 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n66 | 1735 | 5 | 25 | 2135 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3535 | 3.3 | TDD | IMD5 |
|  | n5 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2142 | 13.2 | FDD | IMD3 |
|  | n77 | 3795 | 10 | 50 | 3795 | N/A | TDD | N/A |
| CA\_n5-n66-n78 | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3380 | 16.1 | TDD | IMD3 |
|  | n5 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2120 | 13.2 | FDD | IMD3 |
|  | n78 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
| CA\_n5-n78-n79 | n5 | 846 | 5 | 25 | 891 | N/A | FDD | N/A |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4636 | 26.2 | TDD | IMD2 |
|  | n5 | 827 | 5 | 25 | 872 | N/A | FDD | N/A |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4959 | 22 | TDD | IMD3 |
|  | n5 | 827 | 5 | 25 | 872 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3593 | 26.9 | TDD | IMD2 |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n5 | 827 | 5 | 25 | 872 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3326 | 17 | TDD | IMD3 |
|  | n79 | 4980 | 40 | 216 | 4980 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 880 | 16.2 | FDD | IMD2 |
|  | n78 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
|  | n79 | 4430 | 40 | 216 | 4430 | N/A | TDD | N/A |
|  | n5 | N/A | 5 | N/A | 875 | 3 | FDD | IMD5 |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n79 | 4520 | 40 | 216 | 4520 | N/A | TDD | N/A |
| CA\_n7-n8-n40 | n7 | 2530 | 5 | 25 | 2650 | N/A | FDD | N/A |
|  | n8 | 905 | 5 | 25 | 950 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2345 | 3.0 | TDD | IMD5 |
| CA\_n7-n8-n78 | n7 | 2555 | 5 | 25 | 2675 | N/A | FDD | N/A |
|  | n8 | 900 | 5 | 25 | 945 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3455 | 28.5 | TDD | IMD2 |
|  | n7 | 2555 | 5 | 25 | 2675 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 945 | 29.7 | FDD | IMD2 |
|  | n78 | 3500 | 10 | 50 | 3500 | N/A | TDD | N/A |
|  | n7 | 2520 | 5 | 25 | 2640 | N/A | FDD | N/A |
|  | n8 | N/A | 5 | N/A | 940 | 3.1 | FDD | IMD5 |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2650 | 28 | FDD | IMD2 |
|  | n8 | 895 | 5 | 25 | 940 | N/A | FDD | N/A |
|  | n78 | 3545 | 10 | 50 | 3545 | N/A | TDD | N/A |
| CA\_n7-n20-n67 | n7 | 2565 | 10 | 50 | 2685 | N/A | TDD | N/A |
|  | n20 | 834.5 | 5 | 25 | 793.5 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 773 | 3.9 | FDD | IMD5 |
| CA\_n7-n20-n78 | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n20 | N/A | 5 | N/A | 810 | 30.5 | FDD | IMD21 |
|  | n78 | 3370 | 10 | 50 | 3370 | N/A | TDD | N/A |
|  | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n20 | N/A | 5 | N/A | 810 | 3.0 | FDD | IMD5 |
|  | n78 | 3435 | 10 | 50 | 3435 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2675 | 30.8 | FDD | IMD2 |
|  | n20 | 845 | 5 | 25 | 804 | N/A | FDD | N/A |
|  | n78 | 3520 | 10 | 50 | 3520 | N/A | TDD | N/A |
|  | n7 | 2540 | 5 | 25 | 2660 | N/A | FDD | N/A |
|  | n20 | 835 | 5 | 25 | 794 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3375 | 29.7 | TDD | IMD22 |
| CA\_n7-n25-n77 | n7 | N/A | 5 | N/A | 2640 | 5.3 | FDD | IMD5 |
|  | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n77 | 4125 | 10 | 50 | 4125 | N/A | TDD | N/A |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 8.6 | FDD | IMD4 |
|  | n77 | 3525 | 10 | 50 | 3525 | N/A | TDD | N/A |
|  | n7 | 2520 | 5 | 25 | 2640 | N/A | FDD | N/A |
|  | n25 | 1905 | 5 | 25 | 1985 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3750 | 4.5 | TDD | IMD5 |
| CA\_n7-n25-n78 | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 8.6 | FDD | IMD4 |
|  | n78 | 3525 | 10 | 50 | 3525 | N/A | TDD | N/A |
|  | n7 | 2520 | 5 | 25 | 2640 | N/A | FDD | N/A |
|  | n25 | 1905 | 5 | 25 | 1985 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3750 | 4.5 | TDD | IMD5 |
| CA\_n7-n26-n78 | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 879 | 30.2 | FDD | IMD2 |
|  | n78 | 3429 | 10 | 50 | 3429 | N/A | TDD | N/A |
|  | n7 | 2525 | 5 | 25 | 2645 | N/A | FDD | N/A |
|  | n26 | N/A | 5 | N/A | 875 | 3.3 | FDD | IMD5 |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2645 | 30.1 | FDD | IMD2 |
|  | n26 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
|  | n78 | 3489 | 10 | 50 | 3489 | N/A | TDD | N/A |
|  | n7 | 2540 | 5 | 25 | 2660 | N/A | FDD | N/A |
|  | n26 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3375 | 29.7 | TDD | IMD2 |
| CA\_n7-n28-n78 | n7 | 2567.5 | 5 | 25 | 2687.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 782.5 | 28.8 | FDD | IMD2 |
|  | n78 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n7 | 2567.5 | 5 | 25 | 2687.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 782.5 | 3.0 | FDD | IMD5 |
|  | n78 | 3460 | 10 | 50 | 3460 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2650 | 30.5 | FDD | IMD2 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3390 | 10 | 50 | 3390 | N/A | TDD | N/A |
|  | n7 | 2565 | 5 | 25 | 2685 | N/A | FDD | N/A |
|  | n28 | 745 | 5 | 25 | 800 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3310 | 29.7 | TDD | IMD2 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n28 | 720 | 5 | 25 | 775 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3714 | 9.7 | TDD | IMD4 |
| CA\_n7-n40-n78 | n7 | N/A | 5 | N/A | 2630 | 10.1 | FDD | IMD4 |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | 3625 | 10 | 50 | 3625 | N/A | TDD | N/A |
|  | n7 | 2510 | 5 | 25 | 2630 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2310 | 8.7 | TDD | IMD4 |
|  | n78 | 3785 | 10 | 50 | 3785 | N/A | TDD | N/A |
| CA\_n7-n40-n105 | n7 | N/A | 5 | N/A | 2655 | 5.9 | FDD | IMD5 |
|  | n40 | 2352 | 5 | 25 | 2352 | N/A | TDD | N/A |
|  | n105 | 683 | 5 | 25 | 632 | N/A | FDD | N/A |
| CA\_n7-n46-n78 | n7 | 2530 | 5 | 25 | 2650 | N/A | FDD | N/A |
|  | n46 | 5840 | 20 | 100 | 5840 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3310 | 29,7 | TDD | IMD21 |
|  | n7 | 2530 | 5 | 25 | 2650 | N/A | FDD | N/A |
|  | n46 | N/A | 20 | N/A | 5840 | 25.2 | TDD | IMD21 |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
| CA\_n7-n66-n77 | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3390 | 16.1 | TDD | IMD3 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2150 | 8.7 | FDD | IMD4 |
|  | n77 | 3625 | 10 | 50 | 3625 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2640 | 3.4 | FDD | IMD5 |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n77 | 3900 | 10 | 50 | 3900 | N/A | TDD | N/A |
|  | n7 | 2520 | 5 | 25 | 2640 | N/A | FDD | N/A |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4040 | 4.2 | TDD | IMD5 |
| CA\_n7-n66-n78 | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3390 | 16.1 | TDD | IMD3 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2150 | 8.7 | FDD | IMD4 |
|  | n78 | 3625 | 10 | 50 | 3625 | N/A | TDD | N/A |
| CA\_n7-n67-n78 | n7 | 2562 | 5 | 25 | 2682 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 748 | 28.8 | SDL | IMD21 |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
| CA\_n7-n71-n77 | n7 | 2505 | 5 | 25 | 2625 | N/A | FDD | N/A |
|  | n71 | 666 | 5 | 25 | 620 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3837 | 16.0 | TDD | IMD3 |
|  | n7 | N/A | 5 | N/A | 2670 | 29.6 | FDD | IMD2 |
|  | n71 | 680 | 5 | 25 | 634 | N/A | FDD | N/A |
|  | n77 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
| CA\_n7-n78-n102 | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n78 | 3420 | 5 | 25 | 3420 | N/A | TDD | N/A |
|  | n102 | N/A | 40 | N/A | 5980 | N/A12 | TDD | IMD21 |
|  | n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
|  | n78 | N/A | 5 | N/A | 3420 | 29.6 | TDD | IMD21 |
|  | n102 | 5980 | 40 | 216 | 5980 | N/A | TDD | N/A |
|  | n7 | N/A | 5 | N/A | 2680 | 29.6 | FDD | IMD21 |
|  | n78 | 3320 | 5 | 25 | 3320 | N/A | TDD | N/A |
|  | n102 | 6000 | 40 | 216 | 6000 | N/A | TDD | N/A |
| CA\_n7-n78-n105 | n7 | 2555 | 5 | 25 | 2675 | N/A | FDD | N/A |
|  | n78 | 3520 | 10 | 50 | 3520 | N/A | TDD | N/A |
|  | n105 | N/A | 5 | N/A | 625 | 3.9 | FDD | IMD5 |
|  | n7 | 2550 | 5 | 25 | 2670 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3714 | 9.7 | TDD | IMD4 |
|  | n105 | 693 | 5 | 25 | 642 | N/A | FDD | N/A |
|  | n7 | N/A | 5 | N/A | 2625 | 28.7 | FDD | IMD2 |
|  | n78 | 3308 | 10 | 50 | 3308 | N/A | TDD | N/A |
|  | n105 | 683 | 5 | 25 | 632 | N/A | FDD | N/A |
| CA\_n8-n20-n28 | n8 | N/A | 5 | 25 | 951.5 | 24.3 | FDD | IMD3 |
|  | n20 | 834.5 | 5 | 25 | 793.5 | N/A | FDD | N/A |
|  | n28 | 717.5 | 5 | 25 | 772.5 | N/A | FDD | N/A |
|  | n8 | 887.5 | 5 | 25 | 932.5 | N/A | FDD | N/A |
|  | n20 | 834.5 | 5 | 25 | 793.5 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | 25 | 781.5 | 24 | FDD | IMD3 |
| CA\_n8-n39-n79 | n8 | 900 | 5 | 25 | 945 | N/A | FDD | N/A |
|  | n39 | 1890 | 10 | 50 | 1890 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4680 | 15.9 | TDD | IMD3 |
|  | n8 | 890 | 5 | 25 | 935 | N/A | FDD | N/A |
|  | n39 | 1890 | 10 | 50 | 1890 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4560 | 12.1 | TDD | IMD4 |
|  | n8 | 897.5 | 5 | 25 | 942.5 | N/A | FDD | N/A |
|  | n39 | N/A | 10 | N/A | 1907.5 | 13.8 | TDD | IMD4 |
|  | n79 | 4600 | 40 | 216 | 4600 | N/A | TDD | N/A |
|  | n8 | N/A | 5 | N/A | 940 | 15.1 | FDD | IMD3 |
|  | n39 | 1900 | 10 | 50 | 1900 | N/A | TDD | N/A |
|  | n79 | 4740 | 40 | 216 | 4740 | N/A | TDD | N/A |
|  | n8 | N/A | 5 | N/A | 940 | 7.1 | FDD | IMD4 |
|  | n39 | 1900 | 10 | 50 | 1900 | N/A | TDD | N/A |
|  | n79 | 4750 | 40 | 216 | 4750 | N/A | TDD | N/A |
| CA\_n8-n40-n78 | n8 | N/A | 5 | N/A | 950 | 30.5 | FDD | IMD2 |
|  | n40 | 2380 | 5 | 25 | 2380 | N/A | TDD | N/A |
|  | n78 | 3330 | 10 | 50 | 3330 | N/A | TDD | N/A |
|  | n8 | N/A | 5 | N/A | 935 | 19.8 | FDD | IMD3 |
|  | n40 | 2320 | 5 | 25 | 2320 | N/A | TDD | N/A |
|  | n78 | 3705 | 10 | 50 | 3705 | N/A | TDD | N/A |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2395 | 28 | TDD | IMD2 |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n40 | 2395 | 10 | 50 | 2395 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3305 | 28.8 | TDD | IMD24 |
| CA\_n8-n41-n79 | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n41 | 2650 | 10 | 50 | 2650 | N/A | TDD | N/A |
|  | n79 | 4470 | 10 | 50 | 4470 | 16.3 | TDD | IMD3 |
|  | n8 | 910 | 5 | 25 | 955 | N/A | FDD | N/A |
|  | n41 | 2650 | 10 | 50 | 2650 | 15.5 | TDD | IMD3 |
|  | n79 | 4470 | 10 | 50 | 4470 | N/A | TDD | N/A |
|  | n8 | 895 | 5 | 25 | 940 | 11.8 | FDD | IMD31 |
|  | n41 | 2680 | 10 | 50 | 2680 | N/A | TDD | N/A |
|  | n79 | 4420 | 10 | 50 | 4420 | N/A | TDD | N/A |
| CA\_n12-n30-n77 | n12 | N/A | 5 | N/A | 740 | 15.2 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3880 | 10 | 50 | 3880 | N/A | TDD | N/A |
|  | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 13.2 | FDD | IMD3 |
|  | n77 | 3770 | 10 | 50 | 3770 | N/A | TDD | N/A |
|  | n12 | 707 | 5 | 25 | 737 | N/A | FDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3913 | 16.0 | TDD | IMD3 |
| CA\_n12-n66-n77 | n12 | N/A | 5 | N/A | 740 | 15.2 | FDD | IMD35 |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n77 | 4180 | 10 | 50 | 4180 | N/A | TDD | N/A |
|  | n12 | 707 | 5 | 25 | 737 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2126 | 13.2 | FDD | IMD3 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
|  | n12 | 704 | 5 | 25 | 734 | N/A | FDD | N/A |
|  | n66 | 1723 | 5 | 25 | 2123 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4150 | 16.0 | TDD | IMD31,2,5 |
| CA\_n12-n71-n77 | n12 | N/A | 5 | N/A | 732 | 4.4 | FDD | IMD5 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3504 | 10 | 50 | 3504 | N/A | TDD | N/A |
|  | n12 | 711 | 5 | 25 | 741 | N/A | FDD | N/A |
|  | n71 | N/A | 5 | N/A | 646 | 3.9 | FDD | IMD5 |
|  | n77 | 3490 | 10 | 50 | 3490 | N/A | TDD | N/A |
| CA\_n13-n25-n66 | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2156 | 7..2 | FDD | IMD4 |
|  | n25 | 1860 | 5 | 25 | 1940 | N/A | FDD | N/A |
|  | n13 | 780 | 10 | 50 | 749 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1940 | 6.2 | FDD | IMD4 |
|  | n66 | 1750 | 5 | 25 | 2150 | N/A | FDD | N/A |
| CA\_n13-n25-n77 | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n25 | 1896 | 5 | 25 | 1976 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3460 | 17.3 | TDD | IMD31,2 |
|  | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 16.0 | FDD | IMD3 |
|  | n77 | 3524 | 10 | 50 | 3524 | N/A | TDD | N/A |
| CA\_n13-n66-n77 | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2146 | 17.1 | FDD | IMD3 |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n13 | N/A | 5 | N/A | 750 | 15.2 | FDD | IMD35 |
|  | n66 | 1710 | 5 | 25 | 2110 | N/A | FDD | N/A |
|  | n77 | 4170 | 10 | 50 | 4170 | N/A | TDD | N/A |
|  | n13 | 782 | 5 | 25 | 751 | N/A | FDD | N/A |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3334 | 16.3 | TDD | IMD31,2,5 |
| CA\_n14-n30-n77 | n14 | N/A | 5 | N/A | 763 | 15.2 | FDD | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3857 | 10 | 50 | 3857 | N/A | TDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 13.2 | FDD | IMD3 |
|  | n77 | 3941 | 10 | 50 | 3941 | N/A | TDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3896 | 16.0 | TDD | IMD3 |
| CA\_n14-n66-n77 | n14 | N/A | 5 | N/A | 763 | 15.2 | FDD | IMD35 |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
|  | n77 | 4188 | 10 | 50 | 4188 | N/A | TDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2155 | 13.2 | FDD | IMD3 |
|  | n77 | 3741 | 10 | 50 | 3741 | N/A | TDD | N/A |
|  | n14 | 793 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n66 | 1755 | 5 | 25 | 2155 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3341 | 16.0 | TDD | IMD31,2,5 |
| CA\_n18-n28-n41 | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n28 | 738 | 5 | 25 | 793 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2562 | 4.4 | TDD | IMD5 |
|  | n18 | 825 | 5 | 25 | 870 | N/A | FDD | N/A |
|  | n41 | 2505 | 10 | 50 | 2505 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 795 | 3.9 | FDD | IMD5 |
| CA\_n18-n28-n77 | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n28 | 710 | 5 | 25 | 765 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3770 | 4.0 | TDD | IMD5 |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n28 | N/A | 5 | N/A | 778 | 4.4 | FDD | IMD5 |
|  | n77 | 4058 | 10 | 50 | 4058 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 865 | 3.9 | FDD | IMD5 |
|  | n28 | 723 | 5 | 25 | 778 | N/A | FDD | N/A |
|  | n77 | 3757 | 10 | 50 | 3757 | N/A | TDD | N/A |
| CA\_n18-n41-n77 | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n41 | 2570 | 5 | 25 | 2570 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3390 | 30.1 | TDD | IMD22,4 |
|  | n18 | 820 | 5 | 25 | 865 | N/A | FDD | N/A |
|  | n77 | 3450 | 10 | 50 | 3450 | N/A | TDD | N/A |
|  | n41 | N/A | 5 | N/A | 2630 | 28.5 | TDD | IMD24 |
|  | n41 | 2590 | 10 | 50 | 2590 | N/A | TDD | N/A |
|  | n77 | 3460 | 10 | 50 | 3460 | N/A | TDD | N/A |
|  | n18 | N/A | 5 | N/A | 870 | 29.3 | FDD | IMD21,4 |
| CA\_n20-n67-n78 | n20 | 855 | 5 | 25 | 814 | N/A | FDD | N/A |
|  | n67 | N/A | 5 | N/A | 755 | 11.6 | FDD | IMD4 |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
| CA\_n24-n41-n48 | n24 | 1649 | 5 | 25 | 1528.5 | N/A | FDD | N/A |
|  | n41 | 2610 | 5 | 25 | 2610 | N/A | TDD | N/A |
|  | n48 | N/A | 10 | N/A | 3571 | 16.8 | TDD | IMD3 |
|  | n24 | 1630 | 5 | 25 | 1528.5 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2500 | 5.3 | TDD | IMD5 |
|  | n48 | 3695 | 10 | 50 | 3695 | N/A | TDD | N/A |
|  | n24 | N/A | 5 | N/A | 1530 | 16.4 | FDD | IMD3 |
|  | n41 | 2592.5 | 5 | 25 | 2592.5 | N/A | TDD | N/A |
|  | n48 | 3655 | 10 | 50 | 3655 | N/A | TDD | N/A |
| CA\_n24-n41-n77 | n24 | 1630 | 5 | 25 | 1528.5 | N/A | FDD | N/A |
|  | n41 | 2685 | 5 | 25 | 2685 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3735 | 16.8 | TDD | IMD31,5 |
|  | n24 | 1630 | 5 | 25 | 1528.5 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2610 | 5.3 | TDD | IMD55 |
|  | n77 | 3755 | 10 | 50 | 3755 | N/A | TDD | N/A |
|  | n24 | N/A | 5 | N/A | 1528.5 | 16.4 | FDD | IMD32,5 |
|  | n41 | 2500 | 5 | 25 | 2500 | N/A | TDD | N/A |
|  | n77 | 3465 | 10 | 50 | 3465 | N/A | TDD | N/A |
| CA\_n25-n38-n78 | n25 | N/A | 5 | N/A | 1932.5 | 16.4 | FDD | IMD3 |
|  | n38 | 2617.5 | 5 | 25 | 2617.5 | N/A | TDD | N/A |
|  | n78 | 3305 | 10 | 50 | 3305 | N/A | TDD | N/A |
|  | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n38 | 2610 | 5 | 25 | 2610 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3350 | 14.8 | TDD | IMD3 |
|  | n25 | N/A | 5 | N/A | 1960 | 8.6 | TDD | IMD4 |
|  | n38 | 2570 | 5 | 25 | 2570 | N/A | FDD | N/A |
|  | n78 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
| CA\_n25-n41-n66 | n25 | N/A | 5 | N/A | 1940 | 11.0 | FDD | IMD4 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | FDD | N/A |
| CA\_n25-n41-n66 | n25 | N/A | 5 | 25 | 1950 | 15.3 | FDD | IMD3 |
|  | n41 | 2546 | 100 | 1 (RBstart=24) | 2546 | N/A | TDD | N/A |
|  |  | 2641 | 90 | 1 (RBstart=232) | 2641 |  |  |  |
|  | n66 | 1775 | 5 | 25 | 2195 | N/A | FDD | N/A |
|  | n25 | 1912.5 | 5 | 25 | 1992.5 | N/A | FDD | N/A |
|  | n41 | 2546 | 100 | 1 (RBstart=260) | 2546 | N/A | TDD | N/A |
|  |  | 2641 | 90 | 1 (RBstart=121) | 2641 |  |  |  |
|  | n66 | N/A | 5 | 25 | 1962.5 | 15.3 | FDD | IMD3 |
| CA\_n25-n41-n77 | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n41 | 2670 | 5 | 25 | 2670 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3470 | 14.8 | TDD | IMD3 |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n41 | 2525 | 5 | 25 | 2645 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3775 | 4.2 | TDD | IMD5 |
|  | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2640 | 5.3 | TDD | IMD55 |
|  | n77 | 4125 | 10 | 50 | 4125 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 17.6 | FDD | IMD35 |
|  | n41 | 2675 | 5 | 25 | 2675 | N/A | TDD | N/A |
|  | n77 | 3400 | 10 | 50 | 3400 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 8.6 | FDD | IMD4 |
|  | n41 | 2550 | 5 | 25 | 2685 | N/A | TDD | N/A |
|  | n77 | 3525 | 10 | 50 | 3525 | N/A | TDD | N/A |
| CA\_n25-n41-n78 | n25 | 1870 | 5 | 25 | 1950 | N/A | FDD | N/A |
|  | n41 | 2610 | 5 | 25 | 2610 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3350 | 14.8 | TDD | IMD3 |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n41 | 2525 | 5 | 25 | 2645 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3775 | 4.2 | TDD | IMD5 |
|  | n25 | N/A | 5 | N/A | 1950 | 17.6 | FDD | IMD3 |
|  | n41 | 2565 | 5 | 25 | 2565 | N/A | TDD | N/A |
|  | n78 | 3180 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1950 | 8.6 | FDD | IMD4 |
|  | n41 | 2550 | 5 | 25 | 2685 | N/A | TDD | N/A |
|  | n78 | 3525 | 10 | 50 | 3475 | N/A | TDD | N/A |
| CA\_n25-n41-n85 | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n41 | 2638 | 10 | 50 | 2638 | N/A | TDD | N/A |
|  | n85 | N/A | 5 | N/A | 738 | 28.7 | FDD | IMD24 |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n41 | N/A | 5 | N/A | 2608 | 28.7 | TDD | IMD2 |
|  | n85 | 708 | 5 | 25 | 738 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1952 | 26 | FDD | IMD2 |
|  | n41 | 2660 | 10 | 50 | 2660 | N/A | TDD | N/A |
|  | n85 | 708 | 5 | 50 | 738 | N/A | FDD | N/A |
| CA\_n25-n48-n66 | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n48 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 10.4 | FDD | IMD4 |
|  | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n48 | N/A | 10 | N/A | 3620 | 29.4 | TDD | IMD2 |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 32.1 | FDD | IMD21 |
|  | n48 | 3700 | 10 | 50 | 3700 | N/A | TDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
| CA\_n25-n66-n77 | n25 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2115 | 29.2 | FDD | IMD2 |
|  | n77 | 3970 | 10 | 50 | 3970 | N/A | TDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 10.4 | FDD | IMD4 |
|  | n77 | 3540 | 10 | 50 | 3540 | 10 | TDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 4.0 | FDD | IMD5 |
|  | n77 | 3930 | 10 | 50 | 3930 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 32.1 | FDD | IMD2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 9.1 | FDD | IMD45 |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
|  | n77 | 3350 | 10 | 50 | 3350 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 2.1 | FDD | IMD55 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n77 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
|  | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3620 | 29.4 | TDD | IMD25 |
|  | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3900 | 8.9 | TDD | IMD4 |
| CA\_n25-n66-n78 | n25 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
|  | n66 | 1740 | 5 | 25 | 2140 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3620 | 29.4 | TDD | IMD2 |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2150 | 10.4 | FDD | IMD4 |
|  | n78 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
|  | n25 | N/A | 5 | N/A | 1960 | 32.1 | FDD | IMD21,2 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n78 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n25-n66-n85 | n25 | N/A | 5 | N/A | 1992.5 | 11.0 | FDD | IMD4 |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
|  | n85 | 713.5 | 5 | 25 | 743.5 | N/A | FDD | N/A |
| CA\_n25-n71-n77 | n25 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n71 | 695.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3305 | 8.0 | TDD | IMD31,2,5 |
|  | n25 | N/A | 5 | N/A | 1954 | 16.5 | FDD | IMD32,5 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3340 | 10 | 50 | 3340 | N/A | TDD | N/A |
| CA\_n25-n71-n78 | n25 | 1907.5 | 5 | 25 | 1987.5 | N/A | FDD | N/A |
|  | n71 | 695.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3305 | 8.0 | TDD | IMD3 |
|  | n25 | N/A | 5 | N/A | 1954 | 16.5 | FDD | IMD3 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n78 | 3340 | 10 | 50 | 3340 | N/A | TDD | N/A |
| CA\_n25-n71-n85 | n25 | 1912.5 | 5 | 25 | 1992,5 | N/A | FDD | N/A |
|  | n71 | 665.5 | 5 | 25 | 619.5 | N/A | FDD | N/A |
|  | n85 | N/A | 5 | 25 | 743.5 | 4.2 | FDD | IMD5 |
| CA\_n25-n77-n85 | n25 | N/A | 5 | N/A | 1960 | 16.5 | FDD | IMD32 |
|  | n77 | 3375 | 10 | 50 | 3375 | N/A | TDD | N/A |
|  | n85 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3315 | 16.0 | TDD | IMD31,2 |
|  | n85 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
| CA\_n26-n29-n66 | n26 | 830 | 5 | 25 | 875 | N/A | FDD | N/A |
|  | n29 | N/A | 5 | N/A | 720 | 9.4 | SDL | IMD4 |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
| CA\_n26-n48-n66 | n26 | 829 | 5 | 25 | 874 | N/A | FDD | N/A |
|  | n48 | N/A | 10 | N/A | 3622 | 3.6 | TDD | IMD5 |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
| CA\_n26-n48-n70 | n26 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n48 | 3653 | 10 | 50 | 3653 | N/A | TDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 13.2 | FDD | IMD3 |
| CA\_n26-n66-n71 | n26 | N/A | 5 | N/A | 892 | 4.2 | FDD | IMD5 |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
|  | n71 | 665.5 | 5 | 25 | 619.5 | N/A | FDD | N/A |
| CA\_n26-n66-n77 | n26 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n66 | 1775 | 5 | 25 | 2175 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3465 | 16.1 | TDD | IMD3 |
|  | n26 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4192 | 8.2 | TDD | IMD4 |
|  | n26 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n66 | 1735 | 5 | 25 | 2135 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3535 | 3.3 | TDD | IMD5 |
|  | n26 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2142 | 13.2 | FDD | IMD3 |
|  | n77 | 3795 | 10 | 50 | 3795 | N/A | TDD | N/A |
| CA\_n26-n70-n77 | n26 | 845 | 5 | 25 | 890 | N/A | FDD | N/A |
|  | n70 | 1700 | 5 | 25 | 2000 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3390 | 16.1 | TDD | IMD35 |
|  | n26 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n70 | 1700 | 5 | 25 | 2000 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4179.5 | 8.2 | TDD | IMD45 |
|  | n26 | 835 | 5 | 25 | 880 | N/A | FDD | N/A |
|  | n70 | 1700 | 5 | 25 | 2000 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3430 | 3.3 | TDD | IMD55 |
|  | n26 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 13.2 | FDD | IMD35 |
|  | n77 | 3653 | 10 | 50 | 3653 | N/A | TDD | N/A |
| CA\_n28-n39-n40 | n28 | N/A | 5 | N/A | 790 | 8.6 | FDD | IMD4 |
|  | n39 | 1915 | 5 | 25 | 1915 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | FDD | N/A |
| CA\_n28-n39-n41 | n28 | N/A | 5 | N/A | 762 | 29.3 | FDD | IMD2 |
|  | n39 | 1923 | 5 | 25 | 1923 | N/A | TDD | N/A |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
| CA\_n28-n39-n79 | n28 | 715 | 5 | 25 | 770 | N/A | FDD | N/A |
|  | n39 | 1902.5 | 5 | 25 | 1902.5 | N/A | TDD | N/A |
|  | n79 | 4520 | 40 | 216 | 4520 | 6.7 | TDD | IMD3 |
|  | n28 | 727.5 | 5 | 25 | 782.5 | N/A | FDD | N/A |
|  | n39 | 1902.5 | 5 | 25 | 1902.5 | N/A | TDD | N/A |
|  | n79 | 4980 | 40 | 216 | 4980 | 4.0 | TDD | IMD41 |
|  | n28 | 715.5 | 5 | 25 | 770.5 | N/A | FDD | N/A |
|  | n39 | 1898 | 5 | 25 | 1898 | 5.7 | TDD | IMD5 |
|  | n79 | 4760 | 40 | 216 | 4760 | N/A | TDD | N/A |
|  | n28 | 730 | 5 | 25 | 785 | 15.6 | FDD | IMD3 |
|  | n39 | 1887.5 | 5 | 25 | 1887.5 | N/A | TDD | N/A |
|  | n79 | 4560 | 40 | 216 | 4560 | N/A | TDD | N/A |
|  | n28 | 725 | 5 | 25 | 780 | 8.5 | FDD | IMD4 |
|  | n39 | 1900 | 5 | 25 | 1900 | N/A | TDD | N/A |
|  | n79 | 4920 | 40 | 216 | 4920 | N/A | TDD | N/A |
| CA\_n28-n40-n41 | n28 | N/A | 5 | N/A | 765 | 7.6 | FDD | IMD4 |
|  | n40 | 2302.5 | 5 | 25 | 2302.5 | N/A | TDD | N/A |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
| CA\_n28-n40-n77 | n28 | N/A | 5 | N/A | 800.5 | 11 | FDD | IMD31 |
|  | n40 | 2302.5 | 5 | 25 | 2302.5 | N/A | TDD | N/A |
|  | n77 | 3795 | 10 | 50 | 3795 | N/A | TDD | N/A |
|  | n28 | 708 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n77 | N/A | 10 | N/A | 3736 | 16.0 | TDD | IMD32 |
|  | n28 | 708 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2134 | 15.7 | TDD | IMD3 |
|  | n77 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
| CA\_n28-n40-n78 | n28 | N/A | 5 | N/A | 800.5 | 11 | FDD | IMD3 |
|  | n40 | 2302.5 | 5 | 25 | 2302.5 | N/A | TDD | N/A |
|  | n78 | 3795 | 10 | 50 | 3795 | N/A | TDD | N/A |
|  | n28 | 708 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3736 | 16.0 | TDD | IMD32 |
|  | n28 | 708 | 5 | 25 | 763 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2134 | 15.7 | TDD | IMD3 |
|  | n78 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
| CA\_n28-n40-n79 | n28 | 730 | 5 | 25 | 785 | N/A | FDD | N/A |
|  | n40 | 2350 | 5 | 50 | 2350 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4540 | 10.7 | TDD | IMD4 |
|  | n28 | 720 | 5 | 25 | 775 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2340 | 9.2 | TDD | IMD4 |
|  | n79 | 4500 | 40 | 216 | 4500 | N/A | TDD | N/A |
| CA\_n28-n41-n77 | n41 | 2642 | 5 | 25 | 2642 | N/A | TDD | N/A |
|  | n77 | 3440 | 10 | 50 | 3440 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 798 | 30.8 | FDD | IMD24 |
|  | n41 | 2567.5 | 10 | 50 | 2567.5 | N/A | TDD | N/A |
|  | n77 | 3460 | 10 | 50 | 3460 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 782.5 | 3.0 | FDD | IMD5 |
|  | n28 | 738 | 5 | 25 | 793 | N/A | FDD | N/A |
|  | n77 | 3380 | 10 | 50 | 3380 | N/A | TDD | N/A |
|  | n41 | N/A | 5 | N/A | 2642 | 29.5 | TDD | IMD2 |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n28 | 743 | 5 | 25 | 798 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3323 | 28.2 | TDD | IMD24 |
| CA\_n28-n41-n78 | n28 | 738 | 5 | 25 | 793 | N/A | FDD | N/A |
|  | n78 | 3380 | 10 | 50 | 3380 | N/A | TDD | N/A |
|  | n41 | N/A | 5 | N/A | 2642 | 29.5 | TDD | IMD2 |
|  | n41 | 2642 | 5 | 25 | 2642 | N/A | TDD | N/A |
|  | n78 | 3440 | 10 | 50 | 3440 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 798 | 30.8 | FDD | IMD21 |
|  | n41 | 2565 | 5 | 25 | 2565 | N/A | TDD | N/A |
|  | n28 | 745 | 5 | 25 | 800 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3310 | 29.7 | TDD | IMD22 |
| CA\_n28-n41-n79 | n28 | N/A | 5 | N/A | 780 | 13.0 | FDD | IMD31 |
|  | n41 | 2600 | 10 | 50 | 2600 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n28 | 720 | 5 | 25 | 775 | N/A | FDD | N/A |
|  | n41 | 2600 | 10 | 50 | 2600 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4480 | 10.1 | TDD | IMD32 |
|  | n28 | 735 | 5 | 25 | 790 | N/A | FDD | N/A |
|  | n41 | N/A | 10 | N/A | 2645 | 10.4 | TDD | IMD4 |
|  | n79 | 4850 | 40 | 216 | 4850 | N/A | TDD | N/A |
| CA\_n28-n46-n78 | n28 | 710 | 5 | 25 | 765 | N/A | FDD | N/A |
|  | n46 | 5170 | 20 | 100 | 5170 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3750 | 17 | TDD | IMD31 |
|  | n28 | N/A | 5 | N/A | 780 | 16 | FDD | IMD3 |
|  | n46 | 5900 | 20 | 100 | 5900 | N/A | FDD | N/A |
|  | n78 | 3340 | 10 | 50 | 3340 | N/A | TDD | N/A |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n46 | N/A | 20 | N/A | 5900 | 22 | TDD | IMD31,2 |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
| CA\_n28-n77-n79 | n77 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
|  | n28 | 745 | 5 | 25 | 800 | 16.2 | FDD | IMD21,2 |
| CA\_n28-n78-n79 | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | 3700 | 10 | 50 | 3700 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4440 | 26.2 | TDD | IMD21,3,4 |
|  | n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3700 | 26.9 | TDD | IMD23,4 |
|  | n79 | 4440 | 40 | 216 | 4440 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 800 | 16.2 | FDD | IMD21 |
|  | n78 | 3620 | 10 | 50 | 3620 | N/A | TDD | N/A |
|  | n79 | 4420 | 40 | 216 | 4420 | N/A | TDD | N/A |
| CA\_n28-n78-n102 | n28 | 710 | 5 | 25 | 765 | N/A | FDD | N/A |
|  | n78 | 3380 | 5 | 25 | 3380 | N/A | TDD | N/A |
|  | n102 | N/A | 40 | N/A | 6050 | 22 | TDD | IMD31,2 |
|  | n28 | 730 | 5 | 25 | 785 | N/A | FDD | N/A |
|  | n78 | N/A | 5 | N/A | 3755 | 10.3 | TDD | IMD41 |
|  | n102 | 5945 | 40 | 216 | 5945 | N/A | TDD | N/A |
|  | n28 | N/A | 5 | N/A | 775 | 16 | FDD | IMD31,2 |
|  | n78 | 3395 | 5 | 25 | 3395 | N/A | TDD | N/A |
|  | n102 | 6015 | 40 | 216 | 6015 | N/A | TDD | N/A |
| CA\_n29-n30-n66 | n29 | N/A | 5 | N/A | 719.5 | 4.5 | SDL | IMD5 |
|  | n30 | 2307.5 | 5 | 25 | 2352.5 | N/A | FDD | N/A |
|  | n66 | 1777.5 | 5 | 25 | 2177.5 | N/A | FDD | N/A |
| CA\_n29-n30-n77 | n29 | N/A | 5 | N/A | 722 | 15.2 | SDL | IMD31 |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n77 | 3898 | 10 | 50 | 3898 | N/A | TDD | N/A |
| CA\_n29-n66-n77 | n29 | N/A | 5 | N/A | 722 | 15.2 | SDL | IMD35 |
|  | n66 | 1734 | 5 | 25 | 2134 | N/A | FDD | N/A |
|  | n77 | 4190 | 10 | 50 | 4190 | N/A | TDD | N/A |
| CA\_n30-n66-n77 | n30 | N/A | 5 | N/A | 2355 | 29.2 | FDD | IMD25 |
|  | n66 | 1745 | 5 | 25 | 2145 | N/A | FDD | N/A |
|  | n77 | 4100 | 10 | 50 | 4100 | N/A | TDD | N/A |
|  | n30 | N/A | 5 | N/A | 2355 | 3.4 | FDD | IMD5 |
|  | n66 | 1735 | 5 | 25 | 2135 | N/A | FDD | N/A |
|  | n77 | 3780 | 10 | 50 | 3780 | N/A | TDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 8.7 | FDD | IMD45 |
|  | n77 | 3390 | 10 | 50 | 3390 | N/A | TDD | N/A |
|  | n30 | 2310 | 5 | 25 | 2355 | N/A | FDD | N/A |
|  | n66 | 1745 | 5 | 25 | 2145 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4055 | 28.4 | TDD | IMD21,5 |
| CA\_n34-n39-n40 | n34 | 2022.5 | 5 | 25 | 2022.5 | N/A | TDD | N/A |
|  | n39 | 1882.5 | 5 | 25 | 1882.5 | N/A | TDD | N/A |
|  | n40 | N/A | 5 | N/A | 2302.5 | 2.4 | TDD | IMD5 |
| CA\_n34-n40-n41 | n34 | N/A | 5 | N/A | 2015 | 18.3 | TDD | IMD31 |
|  | n40 | 2302.5 | 5 | 25 | 2302.5 | N/A | TDD | N/A |
|  | n41 | 2590 | 10 | 50 | 2590 | N/A | TDD | N/A |
|  | n34 | 2020 | 5 | 25 | 2020 | N/A | TDD | N/A |
|  | n40 | 2320 | 5 | 25 | 2320 | N/A | TDD | N/A |
|  | n41 | 2620 | 10 | 50 | 2620 | 16.5 | TDD | IMD3 |
| CA\_n34-n41-n79 | n34 | 2020 | 5 | 25 | 2020 | N/A | TDD | N/A |
|  | n41 | 2660 | 5 | 25 | 2660 | N/A | TDD | N/A |
|  | n79 | 4680 | 40 | 216 | 4680 | 19.3 | TDD | IMD2 |
|  | n34 | 2020 | 5 | 25 | 2020 | N/A | TDD | N/A |
|  | n41 | 2550 | 5 | 25 | 2550 | 27.2 | TDD | IMD2 |
|  | n79 | 4570 | 40 | 216 | 4570 | N/A | TDD | N/A |
|  | n34 | 2015 | 5 | 25 | 2015 | 28.6 | TDD | IMD2 |
|  | n41 | 2585 | 5 | 25 | 2585 | N/A | TDD | N/A |
|  | n79 | 4600 | 40 | 216 | 4600 | N/A | TDD | N/A |
|  | n34 | 2015 | 5 | 25 | 2015 | 7.5 | TDD | IMD5 |
|  | n41 | 2515 | 5 | 25 | 2515 | N/A | TDD | N/A |
|  | n79 | 4780 | 40 | 216 | 4780 | N/A | TDD | N/A |
| CA\_n38-n66-n78 | n38 | 2550 | 5 | 25 | 2550 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2150 | 8.7 | FDD | IMD4 |
|  | n78 | 3625 | 10 | 50 | 3625 | N/A | TDD | N/A |
|  | n38 | 2610 | 5 | 25 | 2610 | N/A | TDD | N/A |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3460 | 15.0 | TDD | IMD3 |
| CA\_n39-n40-n79 | n39 | 1917.5 | 5 | 25 | 1917.5 | N/A | TDD | N/A |
|  | n40 | 2302.5 | 5 | 25 | 2302.5 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4980 | 5.8 | TDD | IMD4 |
| CA\_n39-n41-n79 | n39 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
|  | n41 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
|  | n79 | N/A | N/A | N/A | N/A | N/A | TDD | IMD29 |
| CA\_n40-n41-n79 | n40 | 2340 | 5 | 25 | 2340 | N/A | TDD | N/A |
|  | n41 | 2600 | 10 | 50 | 2600 | N/A | TDD | N/A |
|  | n79 | N/A | 40 | N/A | 4940 | 30.5 | TDD | IMD2 |
| CA\_n40-n78-n105 | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | 3789 | 10 | 50 | 3789 | N/A | TDD | N/A |
|  | n105 | N/A | 5 | N/A | 648 | 3.3 | FDD | IMD5 |
|  | n40 | 2310 | 5 | 25 | 2310 | N/A | TDD | N/A |
|  | n78 | N/A | 10 | N/A | 3708 | 16 | TDD | IMD3 |
|  | n105 | 699 | 5 | 25 | 648 | N/A | FDD | N/A |
|  | n40 | N/A | 5 | N/A | 2310 | 15.7 | TDD | IMD3 |
|  | n78 | 3708 | 10 | 50 | 3708 | N/A | TDD | N/A |
|  | n105 | 699 | 5 | 25 | 648 | N/A | FDD | N/A |
| CA\_n41-n66-n77 | n41 | 2600 | 5 | 25 | 2600 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3470 | 16.1 | TDD | IMD31,2 |
|  | n41 | N/A | 5 | N/A | 2670 | 5.2 | TDD | IMD55 |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | FDD | N/A |
|  | n77 | 4190 | 10 | 50 | 4190 | N/A | TDD | N/A |
|  | n41 | 2640 | 5 | 25 | 2640 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 9.0 | FDD | IMD4 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n41-n66-n78 | n41 | 2560 | 5 | 25 | 2560 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3390 | 16.1 | TDD | IMD31 |
|  | n41 | 2530 | 5 | 25 | 2530 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 9.0 | FDD | IMD4 |
|  | n78 | 3610 | 10 | 50 | 3610 | N/A | TDD | N/A |
| CA\_n41-n66-n85 | n41 | N/A | 5 | N/A | 2498.5 | 27.6 | TDD | IMD2 |
|  | n66 | 1777.5 | 5 | 25 | 2197.5 | N/A | FDD | N/A |
|  | n85 | 713.5 | 5 | 25 | 743.5 | N/A | FDD | N/A |
|  | n41 | 2501 | 5 | 25 | 2501 | N/A | TDD | N/A |
|  | n66 | 1770 | 5 | 25 | 2190 | N/A | FDD | N/A |
|  | n85 | N/A | 5 | N/A | 731 | 31 | FDD | IMD21 |
| CA\_n41-n70-n78 | n41 | 2655 | 10 | 50 | 2655 | N/A | TDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 17.6 | FDD | IMD3 |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n41 | 2565 | 10 | 50 | 2565 | N/A | TDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 8.6 | FDD | IMD4 |
|  | n78 | 3565 | 10 | 50 | 3565 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2480 | 5.3 | TDD | IMD5 |
|  | n70 | 1700 | 5 | 25 | 2000 | N/A | FDD | N/A |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n41 | 2545 | 10 | 50 | 2545 | N/A | FDD | N/A |
|  | n70 | 1700 | 5 | 25 | 2000 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3390 | 16.1 | TDD | IMD3 |
| CA\_n41-n71-n77 | n41 | 2615 | 5 | 25 | 2615 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3308 | 29.1 | TDD | IMD21,5 |
|  | n41 | 2564 | 5 | 25 | 2564 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3950 | 16.3 | TDD | IMD31 |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3774 | 10.3 | TDD | IMD41 |
|  | n41 | N/A | 5 | N/A | 2615 | 28.7 | TDD | IMD25 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3308 | 10 | 50 | 3308 | N/A | TDD | N/A |
|  | n41 | N/A | 5 | N/A | 2564 | 15.5 | TDD | IMD3 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n77 | 3950 | 10 | 50 | 3950 | N/A | TDD | N/A |
|  | 41 | 2680 | 5 | 25 | 2680 | N/A | TDD | N/A |
|  | n71 | N/A | 5 | N/A | 640 | 30.8 | FDD | IMD25 |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
| CA\_n41-n71-n78 | n41 | 2615 | 5 | 25 | 2615 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3308 | 29.1 | TDD | IMD21 |
|  | n41 | 2580 | 5 | 25 | 2580 | N/A | TDD | N/A |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3774 | 10.3 | TDD | IMD41 |
|  | n41 | N/A | 5 | N/A | 2615 | 28.7 | TDD | IMD2 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n78 | 3308 | 10 | 50 | 3308 | N/A | TDD | N/A |
|  | 41 | 2642 | 5 | 25 | 2642 | N/A | TDD | N/A |
|  | n71 | N/A | 5 | N/A | 798 | 30.8 | FDD | IMD2 |
|  | n78 | 3440 | 10 | 50 | 3440 | N/A | TDD | N/A |
| CA\_n41-n77-n79 | n77 | 3600 | 10 | 50 | 3600 | N/A | TDD | N/A |
|  | n79 | 4600 | 40 | 216 | 4600 | N/A | TDD | N/A |
|  | n41 | N/A | 10 | N/A | 2600 | 10.7 | TDD | IMD31,2 |
| CA\_n41-n77-n85 | n41 | 2687 | 5 | 25 | 2687 | N/A | TDD | N/A |
|  | n77 | 3420 | 10 | 50 | 3420 | N/A | TDD | N/A |
|  | n85 | N/A | 5 | N/A | 733 | 30.8 | FDD | IMD25 |
|  | n41 | N/A | 5 | N/A | 2 619 | 29.5 | TDD | IMD24.5 |
|  | n77 | 3320 | 10 | 50 | 3320 | N/A | TDD | N/A |
|  | n85 | 701 | 5 | 25 | 731 | N/A | FDD | N/A |
|  | n41 | 2680 | 5 | 25 | 2680 | N/A | TDD | N/A |
|  | n77 | 3393 | 10 | N/A | 3393 | 28.2 | TDD | IMD24,5 |
|  | n85 | 713 | 5 | 25 | 743 | N/A | FDD | N/A |
| CA\_n46-n78-n102 | n46 | 5315 | 20 | 100 | 5315 | N/A | TDD | N/A |
|  | n78 | 3770 | 10 | 50 | 3770 | N/A | TDD | N/A |
|  | n102 | N/A | 40 | N/A | 5995 | N/A12 | TDD | IMD4 |
|  | n46 | N/A | 10 | N/A | 5530 | N/A12 | TDD | IMD4 |
|  | n78 | 3550 | 10 | 50 | 3550 | N/A | TDD | N/A |
|  | n102 | 6315 | 40 | 216 | 6315 | N/A | TDD | N/A |
| CA\_n48-n66-n70 | n48 | 3625 | 10 | 50 | 3625 | N/À | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2142.5 | 2.8 | FDD | IMD5 |
|  | n70 | 1702.5 | 5 | 25 | 2002.5 | N/A | FDD | N/A |
|  | n48 | 3645 | 10 | 50 | 3645 | N/À | TDD | N/A |
|  | n66 | 1762.5 | 5 | 25 | 2162.5 | N/A | FDD | N/A |
|  | n70 | N/A | 5 | N/A | 2002.5 | 3.1 | FDD | IMD5 |
| CA\_n48-n66-n71 | n48 | 3552.5 | 10 | 50 | 3552.5 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2161.5 | 14.4 | FDD | IMD3 |
|  | n71 | 695.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
|  | n48 | N/A | 10 | N/A | 3695 | 5.2 | TDD | IMD4 |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
|  | n71 | 665.5 | 5 | 25 | 619.5 | N/A | FDD | N/A |
| CA\_n48-n70-n71 | n48 | N/A | 10 | N/A | 3694 | 9 | TDD | IMD41 |
|  | n70 | 1697.5 | 5 | 25 | 1997.5 | N/A | FDD | N/A |
|  | n71 | 665.5 | 5 | 25 | 619.5 | N/A | FDD | N/A |
| CA\_n48-n71-n77 | n48 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n71 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n77 | N/A | N/A | N/A | N/A | N/A | FDD | IMD25 |
|  | n48 | N/A | N/A | N/A | N/A | N/A | FDD | IMD25 |
|  | n71 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n77 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
| CA\_n66-n70-n77 | n66 | 1757.5 | 5 | 25 | 2157.5 | N/A | FDD | N/A |
|  | n70 | N/A | 5 | N/A | 2007.5 | 32.1 | FDD | IMD22,1 |
|  | n77 | 3765 | 10 | 50 | 3765 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2162.5 | 29.2 | FDD | IMD21 |
|  | n70 | 1702.5 | 5 | 25 | 2002.5 | N/A | FDD | N/A |
|  | n77 | 3865 | 10 | 50 | 3865 | N/A | TDD | N/A |
| CA\_n66-n70-n78 | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 32.1 | FDD | IMD2 |
|  | n78 | 3760 | 10 | 50 | 3760 | N/A | TDD | N/A |
|  | n66 | 1770 | 5 | 25 | 2170 | N/A | FDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 9.1 | FDD | IMD4 |
|  | n78 | 3310 | 10 | 50 | 3310 | N/A | TDD | N/A |
|  | n66 | 1760 | 5 | 25 | 2160 | N/A | FDD | N/A |
|  | n70 | N/A | 5 | N/A | 2000 | 2.1 | FDD | IMD5 |
|  | n78 | 3640 | 10 | 50 | 3640 | N/A | TDD | N/A |
|  | n66 | N/A | 5 | N/A | 2160 | 5.0 | FDD | IMD5 |
|  | n70 | 1700 | 5 | 25 | 2000 | N/A | FDD | N/A |
|  | n78 | 3630 | 10 | 50 | 3630 | N/A | TDD | N/A |
| CA\_n66-n71-n77 | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n71 | 668 | 5 | 25 | 622 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 4108 | 15.9 | TDD | IMD31,2,5 |
|  | n66 | N/A | 5 | N/A | 2150 | 15.5 | FDD | IMD32 |
|  | n71 | 690 | 5 | 25 | 644 | N/A | FDD | N/A |
|  | n77 | 3530 | 10 | 50 | 3530 | N/A | TDD | N/A |
|  | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n71 | N/A | 5 | N/A | 640 | 15.3 | FDD | IMD35 |
|  | n77 | 4080 | 10 | 50 | 4080 | N/A | TDD | N/A |
| CA\_n66-n71-n78 | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n71 | 668 | 5 | 25 | 622 | N/A | FDD | N/A |
|  | n78 | N/A | 10 | N/A | 3724 | 9 | TDD | IMD41 |
|  | n66 | N/A | 5 | N/A | 2160 | 15.5 | FDD | IMD3 |
|  | n71 | 693 | 5 | 25 | 647 | N/A | FDD | N/A |
|  | n78 | 3546 | 10 | 50 | 3546 | N/A | TDD | N/A |
| CA\_n66-n77-n85 | n66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
|  | n77 | 4180 | 10 | 50 | 4180 | N/A | TDD | N/A |
|  | n85 | N/A | 5 | N/A | 740 | 23.5 | FDD | IMD35 |
|  | n66 | N/A | 5 | N/A | 2124 | 21.4 | FDD | IMD3 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
|  | n85 | 708 | 5 | 25 | 738 | N/A | FDD | N/A |
| CA\_n70-n71-n77 | n70 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n71 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | IMD35 |
|  | n70 | 1702.5 | 5 | 25 | 2002.5 | N/A | FDD | N/A |
|  | n71 | 680.5 | 5 | 25 | 834.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3745 | 8.2 | TDD | IMD4 |
|  | n70 | 1702.5 | 5 | 25 | 2002.5 | N/A | FDD | N/A |
|  | n71 | 680.5 | 5 | 25 | 834.5 | N/A | FDD | N/A |
|  | n77 | N/A | 10 | N/A | 3745 | 3.3 | TDD | IMD5 |
|  | n70 | N/A | N/A | N/A | N/A | N/A | FDD | IMD35 |
|  | n71 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
|  | n70 | N/A | N/A | N/A | N/A | N/A | FDD | IMD45 |
|  | n71 | N/A | N/A | N/A | N/A | N/A | FDD | N/A |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| NOTE 1: This band is subject to IMD5 also which MSD is not specified.  NOTE 2: This band is subject to IMD4 also which MSD is not specified.  NOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation.  NOTE 4: This band is subject to IMD3 also which MSD is not specified.  NOTE 5: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped.  NOTE 6: Void.  NOTE 7: Void.  NOTE 8: Both of the transmitters shall be set min(+20 dBm, PCMAX\_L,f,c) as defined in clause 6.2A.4  NOTE 9: There is no IMD2 product in band n79 downlink for n79 operating in 4800 – 5000 MHz frequency range.  NOTE 10: This band supports intra-band non-contiguous uplink configuration.  NOTE 11: Void.  NOTE 12: This is a share spectrum access band, hence no MSD is defined.  NOTE 13: This band is also subject to a near missed IMD2 that is not specified and is not applicable for band n77 spectrum ranges of 3450-3550MHz and 3700-3980MHz. | | | | | | | | |