**3GPP TSG-RAN WG4 Meeting # 111R4-2407853**

**Fukuoka, Japan, May 20 – May 24, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** |  | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | DraftCR on TC for MAC CE based TCI state activation in sDCI in Multi-RX |
|  |  |
| ***Source to WG:*** | Xiaomi |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_MIMO\_evo\_DL\_UL-Core |  | ***Date:*** | 2024-5-10 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* *Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In RAN4#110bis, it’s agreed to define TC for dual TCI state switch for s-DCI for PDCCH repetition* TC2: MAC-CE based dual TCI state switch for s-DCI for PDCCH repetition
	+ [RS1] to [RS2, RS3]
 |
|  |  |
| ***Summary of change:*** | Add TC for dual TCI state switch for s-DCI for PDCCH repetition. |
|  |  |
| ***Consequences if not approved:*** | The related testcase will be missing. |
|  |  |
| ***Clauses affected:*** | New A.7.5.8.x |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.533  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

# <Start of Change #1>

### A.7.5.8 Active TCI state switch delay

Unrelated part is omitted.

#### A.7.5.8.x MAC-CE based dual TCI state switch for sDCI

A.7.5.8.x.1 NR PCell FR2 active TCI state switch for a known TCI state

A.7.5.8.x.1.1 Test Purpose and Environment

The purpose of this test is to verify the active TCI state switch delay requirement defined in clause 8.10E.3. Supported test configuration is shown in Table A.7.5.8.x.1.1-1.

The test scenario comprises of one NR PCell (Cell 1) as given in Table A.7.5.8.x.1.1-2, which is configured with two TRPs(TRP0 and TRP1). Cell-specific parameters of NR PCell are specified in Table A.7.5.8.x.1.1-3 below. The OTA related test parameters for FR2 are shown in Table A.7.5.8.x.1.1-4.

PDCCHs indicating new transmissions shall be sent continuously on TRP0 to ensure that the UE would have ACK/NACK sending.

Before the test starts,

- UE is connected to Cell 1 (PCell) on radio channel 1 (PCC).

- UE is configured with 2 different TCI states for TRP0, PDCCH TCI state 0 (QCL’d to SSB0) and TCIstate 1 (QCL’d to SSB1).

- UE is indicated in TCI state 0 as the active PDCCH TCI state

- Target TCI state is not in the active TCI state list.

The test consists of two time periods, T1 and T2. Figure A.7.5.8.x.1.1-1 and Figure A.7.5.8.x.1.1-2 show the Time multiplexed (allocation in Frequency is symbolic) downlink transmissions from each Angle of Arrival. During T1 only SSB to which PDCCH-TCI-state0 is QCL’d is transmitted. At the beginning of T2, the SSB corresponding to TCI state 1 starts transmitting. The UE is configured to provide periodic L1-RSRP reports. In slot n which is within 1280ms of UE providing L1-RSRP report with results for both SSB0 and SSB1, UE receives a MAC-CE command indicating a switch to TCI state 1. *tci-PresentInDCI* is not configured in the PDSCH configuration, i.e. TCI state for the PDSCH is identical to the PDCCH TCI state.

The test equipment verifies that UE can be scheduled on TRP0 on TCI state 0 till n+ THARQ +3 ms. The test equipment also verifies the TCI state switch time in TRP0 by scheduling the UE on TCI state 1 after n+ THARQ +3 ms + (Tfirst-SSB + TSSB-proc).

Table A.7.5.8.x.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| Config | Description |
| 1 | NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |

Table A.7.5.8.x.1.1-2: General test parameters for TCI state switch

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Value | Comment |
| NR RF Channel Number |  | 1 | One NR radio channel is used for this test |
| Active PCell |  | Cell 1 | PCell on RF channel number 1. |
| CP length |  | Normal |  |
| DRX |  | OFF |  |
| T1 | s | 0.2 |  |
| T2 | s | 0.2 |  |

Table A.7.5.8.x.1.1-3: NR Cell specific test parameters for TCI state switch

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Cell 1 |
| Frequency Range |  | FR2 |
| Duplex mode |  | TDD |
| TDD configuration |  | TDDConf.3.1 |
| BWchannel |  | 100 MHz: NRB,c = 66 |
| Data RBs allocated |  | 24 |
| Initial DL BWP Configuration |  | DLBWP.0.2 |
| Dedicated DL BWP Configuration |  | DLBWP.1.1 |
| Initial UL BWP Configuration |  | ULBWP.0.2 |
| Dedicated UL BWP Configuration |  | ULBWP.1.1 |
| PDSCH Reference measurement channel |  | SR.3. 2 TDD  |
| RMSI CORESET parameters |  | CR.3.1 TDD  |
| Dedicated CORESET parameters |  | CCR.3.1 TDD  |
| OCNG Patterns |  | OP. 5 |
| SSB Configuration |  | SSB.1 FR2 |
| SMTC Configuration |  | SMTC.1  |
| TCI State 0 |  | TCI. State.2 |
| TCI State 1 |  | TCI.State.3 |
| TRS Configuration |  | TRS.2.1 TDD TRS.2.2 TDD  |
| Correlation Matrix and Antenna Configuration |  | 1x2 Low |
| EPRE ratio of PSS to SSS | dB | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |  |
| EPRE ratio of PBCH to PBCH DMRS |  |  |
| EPRE ratio of PDCCH DMRS to SSS |  |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |  |
| EPRE ratio of PDSCH to PDSCH  |  |  |
| EPRE ratio of OCNG DMRS to SSS(Note 1) |  |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |  |
| Propagation Condition |  | AWGN |
| Note 1: OCNG shall be used such that a constant total transmitted power spectral density is achieved for all OFDM symbols. |

Table A.7.5.8.x.1.1-4: OTA related test parameters for TCI state switch

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | TRP0 of Cell 1 |
|  |  | SSB0 | SSB1 |
|  |  | T1 | T2 | T1 | T2 |
| Angle of arrival configuration |  | Setup 3 according to clause A.3.15.3 |
|  |  | AoA1 | AoA2 |
| Assumption for UE beams Note 6 |  | Rough |
| Ês | dBm/SCS | -80.6 | -80.6 | -Infinity | -80.6 |
| SS B\_RP Note 2 | dBm/ SCS | -80.6 | -80.6 | -Infinity | -80.6 |
| BB Note 7 | dB | 8.3 | 8.3 | -Infinity | 8.3 |
| IoNote2 | dBm/95.04 MHz Note4 | -55.41 | -55.41 | - Infinity  | -55.41 |
| Note 1: VoidNote 2: SS B\_RP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 3: VoidNote 4: Equivalent power received by an antenna with 0 dBi gain at the centre of the quiet zoneNote 5: As observed with 0dBi gain antenna at the center of the quiet zone.Note 6: Information about types of UE beam is given in B.2.1.3 and does not limit UE implementation or test system implementation.Note 7: Calculation of Es/IotBB includes the effect of UE internal noise up to the value assumed for the associated Refsens requirement in clause 7.3.2 of TS 38.101-2 [19], and an allowance of 1dB for UE multi-band relaxation factor ΔMBP from TS 38.101-2 [19] Table 6.2.1.3-4. |



Figure A.7.5.8.x.1.1-1: Time multiplexed downlink transmissions during T1



Figure A.7.5.8.x.1.1-2: Time multiplexed downlink transmissions during T2

A.7.5.8.x.1.2 Test Requirements

During T2, UE shall send L1-RSRP report with results for both SSB0 and SSB1.

After receiving MAC-CE command in slot n, UE shall:

- be able to continue to receive on TCI state 0 till n+ THARQ +3 ms

- be able to start receiving on TCI state 1 after n+ THARQ +5 ms + Tfirst-SSB

The rate of correct events observed during repeated tests shall be at least 90%.

# <End of Change #1>