**3GPP TSG-RAN WG4 Meeting #111 R4-2410365**

**Fukuoka City, Fukuoka, Japan, 20th – 24th May, 2024**

**Title:** WF on core maintenance and performance part for BWP without restriction

**Agenda Item:** 7.6.3

**Source:** vivo, Vodafone

**Document for:** Approval

# Agreements for core part maintenance

**Issue 1-5: Configuration of SSB resources within CSI-ResourceConfig settings for option B-1-1**

* It is RAN4 common understanding that SSB outside a BWP can be configured within *CSI-ResourceConfig* for the BWP if UE supports option B-1-1.
* Remove the bracket in L1-RSRP/L1-SINR requirements for UE supporting option B-1-1.

# Agreements for performance part

* Add a note to clarify that the RedCap [SMTC] configuration can be applied to non-RedCap UE.

----EoD---