**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | To introduce measurement delay test case for RSCPD measurement reported together with RSTD measurement for positioning measurements in RRC\_CONNECTED state in FR1. |
|  |  |
| ***Summary of change:*** | New section is introduced for meaurement delay TC for RSCPD measurement reported together with RSTD in RRC\_CONNECTED in FR1. |
|  |  |
| ***Consequences if not approved:*** | UE capability to meet measurement reporting delay requirement for RSCPD reported together with RSTD measurement cannot be varified. |
|  |  |
| ***Clauses affected:*** | New clauses A.6.6.12.X is added. |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This DraftCR covers set 7-1 agreed in the work split document R4-2406382 in RAN4#110bis. |
|  |  |
| ***This CR's revision history:*** |  |

**START OF CHANGE 1**

##### A.6.6.12.X NR RSCPD with RSTD measurement reporting delay test case for single positioning frequency layer in FR1 SA in RRC\_CONNECTED state

###### A.6.6.12.X.1 Test Purpose and Environment

The purpose of the test is to verify that the DL RSCPD measurement reported together with the RSTD measurement meets the requirements specified in Clause 9.9.7 in an environment with AWGN propagation conditions in FR1 in standalone scenario when single positioning frequency layer is configured to the UE.

The supported test configurations are specified in Table A.6.6.12.X.1-1.

Table A.6.6.12.X.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 20 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 20 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 50 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. |

In the test there are three synchronous cells: Cell 1, Cell 2 and Cell 3. Cell 1 is the reference as well as the PCell. Cell 2 and Cell 3 are the neighbour cells. All 3 cells are on the same RF channel in FR1.

The test consists of two consecutive time intervals, with duration of T1 and T2. During time duration T1, the UE shall not have any timing information of Cell 2 and Cell 3. All three cells transmit PRS during T2.

***Note****: The information on when PRS is muted is conveyed to the UE using PRS muting information.*

The *NR-DL-TDOA-ProvideAssistanceData* and *nr-DL-TDOA-RequestLocationInformation* as defined in TS 37.355 [34, clause 6.5.10], shall be provided to the UE during T1. In *nr-DL-TDOA-RequestLocationInformation,* the UE is configured to perform DL RSCPD measurement via *nr-DL-PRS-RSCPD-Request*. The UE is configured to perform both RSCPD and RSTD measurements within the time window indicated to UE via *nr-DL-PRS-MeasurementTimeWindowsConfig*. The last TTI containing the two messages shall be provided to the UE ΔT ms before the start of T2, where ΔT = 50 ms is the maximum processing time of the DL-TDOA assistance data and location information request.

The beginning of the time interval T2 shall be aligned with the beginning of the first MG instance containing the PRS resources to be measured within the configured time window.

The UE is configured with measurement gap pattern ID # 24 or # 0 before T2.

The general test parameters are listed in Table A.6.6.12.X.1-2, and cell specific test parameters are listed in Table A.6.6.12.X.1-3.

Table A.6.6.12.X.1-2: General test parameters for RSTD measurement reporting delay.

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Value | Comment |
| Reference cell |  | Cell 1 | Reference cell is the cell in the DL-TDOA assistance data with respect to which the RSCPD and RSTD measurement is defined, as specified in TS 38.215 [4] and TS 37.355 [34]. The reference cell is the PCell in this test case. |
| Neighbor cells |  | Cell 2 and Cell 3 | Cell 2 and Cell 3 appear at the first and second places in the neighbour cell list in the DL-TDOA assistance data. |
| SSB configuration | Config 1 |  | SSB.1 FR1 |  |
| Config 2 |  | SSB.1 FR1 |
| Config 3 |  | SSB.2 FR1 |
| SMTC configuration | Config 1 |  | SMTC.2 |  |
| Config 2 |  | SMTC.1 |
| Config 3 |  | SMTC.1 |
| PDSCH RMC configuration | Config 1 |  | SR.1.1 FDD |  |
| Config 2 |  | SR.1.1 TDD |  |
| Config 3 |  | SR.2.1 TDD |  |
| RMSI CORESET RMC configuration | Config 1 |  | CR.1.1 FDD | As specified in clause A.3.1.2.1 |
| Config 2 |  | CR.1.1 TDD |  |
| Config 3 |  | CR.2.1 TDD |  |
| Dedicated CORESET RMC configuration | Config 1 |  | CCR.1.1 FDD |  |
| Config 2 |  | CCR.1.1 TDD |  |
| Config 3 |  | CCR.2.1 TDD |  |
| Initial BWP configuration | Config 1,2,3 |  | DLBWP.0.1 ULBWP.0.1 |  |
| Active DL BWP configuration | Config 1,2,3 |  | DLBWP.1.1 |  |
| Active UL BWP configuration | Config 1,2,3 |  | ULBWP.1.1 |  |
| PRS Configuration | Config 1 |  | PRS.1.1 FR1 | As specified in clause A.3.31 |
| Config 2 |  | PRS.1.1 FR1 |
| Config 3 |  | PRS.2.1 FR1 |
| Physical cell ID PCI |  | (PCI of Cell 1 – PCI of Cell 2) mod 6=0and(PCI of Cell 1 – PCI of Cell 3) mod 6=0  | The cell PCIs are selected such that the relative shifts of PRS patterns among cells are as given by the test parameters |
| CP length |  | Normal |  |
| DRX |  | OFF |  |
| Measurement gap |  | GP#24 or GP#0  | GP#24 is configured if UE supports MG#24, otherwise GP#0 is configured |
| Time window configuration |  | MTW.1 | As specified in clause A.3.Y |
| Radio frame receive time offset between the cells at the UE antenna connector | μs | Cell 2 to Cell 1: 0Cell 3 to Cell 1: 3 | PRS are transmitted from synchronous cells |
| Expected RSTD | μs | Cell 2: 3 Cell 3: 3Other neighbour cells: randomly between -3 and 3 | The expected RSTD is what is expected at the receiver. The corresponding parameter in the DL-TDOA assistance data specified in TS 37.355 [34] is the expectedRSTD indicator |
| Expected RSTD uncertainty for all neighbour cells | μs | 5 | The corresponding parameter in the DL-TDOA assistance ta specified in TS 37.355 [34] is the expectedRSTD-Uncertainty index |
| Number of cells provided in DL-TDOA assistance data |  | 4 | Including the reference cell |
| PRS muting info |  | Cell 1: ‘10’Cell 2: ‘01’Cell 3: ‘10’ | Correponds to *NR-MutingPattern* defined in TS 37.355 [34] |
| PRS resource RE offset |  | Cell 1: 0Cell 2: 0Cell 3: 1 | Cell 1 and Cell 3 are configured with different resource offsets |
| T1 | s | 3 | The length of the time interval from the beginning of each test |
| T2 | s | 1.28 | The length of the time interval that follows immediately after time interval T1 |

Table A.6.6.12.X.1-3: Cell-specific test parameters for RSCPD with RSTD measurement reporting delay during T1.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Cell 1 | Cell 2 | Cell 3 |
| NR RF Channel Number |  | 1 | 1 | 1 |
| Positiong frequency layer  |  | 1 | 1 | 1 |
| Correlation Matrix and Antenna Configuration |  | 12 Low | 12 Low | 12 Low |
| OCNG patterns defined in A.3.2.1 |  | OP.1 | N/A | N/A |
| EPRE ratio of PSS to SSS | dB | 0 | N/A | N/A |
| EPRE ratio of PBCH DMRS to SSS |
| EPRE ratio of PBCH to PBCH DMRS |
| EPRE ratio of PDCCH DMRS to SSS |
| EPRE ratio of PDCCH to PDCCH DMRS |
| EPRE ratio of PDSCH DMRS to SSS |
| EPRE ratio of PDSCH to PDSCH DMRS |
| EPRE ratio of OCNG DMRS to SSSNote 1 |
| EPRE ratio of OCNG to OCNG DMRS Note 1 |
| Note 3 | Config 1 | dBm/SCS | -98 |
| Config 2 | dBm/SCS | -98 |
| Config 3 | dBm/SCS | -95 |
| PRS  | dB | -Infinity | -Infinity | -Infinity |
| SSB  | dB | 10 | -Infinity | -Infinity |
| Io Note 4 | Config 1 | dBm/19.08MHz | -56.54 | -56.54 | -56.54 |
| Config 2 | dBm/19.08MHz | -56.54 | -56.54 | -56.54 |
| Config 3 | dBm/47.88MHz | -52.56 | -52.56 | -52.56 |
| SSB RP Note4 | Config 1 | dBm/SCS | -88 | -Infinity | -Infinity |
| Config 2 | dBm/SCS | -88 | -Infinity | -Infinity |
| Config 3 | dBm/SCS | -85 | -Infinity | -Infinity |
| Propagation Condition  |  | AWGN |
| Note 1: OCNG shall be used such that active cell (Cell 1) is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols other than those in the slots with transmitted PRS. Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for to be fulfilled.Note 4: SSB RP and Io levels have been derived from other parameters and are given for information purpose. These are not settable test parameters. |

Table A.6.6.12.X.1-4: Cell-specific test parameters for RSCPD with RSTD measurement reporting delay during T2.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Cell 1 | Cell 2 | Cell 3 |
| T2 | T2 | T2 |
| NR RF Channel Number |  | 1 | 1 | 1 |
| Correlation Matrix and Antenna Configuration |  | 12 Low | 12 Low | 12 Low |
| OCNG patterns defined in A.3.2.1 |  | OP.1 | OP.1 | OP.1 |
| PRACH configuration |  | FR1 PRACH configuration 1 | FR1 PRACH configuration 1 | FR1 PRACH configuration 1 |
| EPRE ratio of PSS to SSS | dB | 0 | 0 | 0 |
| EPRE ratio of PBCH DMRS to SSS |
| EPRE ratio of PBCH to PBCH DMRS |
| EPRE ratio of PDCCH DMRS to SSS |
| EPRE ratio of PDCCH to PDCCH DMRS |
| EPRE ratio of PDSCH DMRS to SSS |
| EPRE ratio of PDSCH to PDSCH DMRS |
| EPRE ratio of OCNG DMRS to SSSNote 1 |
| EPRE ratio of OCNG to OCNG DMRS Note 1 |
|  Note 3 | Config 1 | dBm/SCS | -98 | -98 | -98 |
| Config 2 | dBm/SCS | -98 | -98 | -98 |
| Config 3 | dBm/SCS | -95 | -95 | -95 |
| PRS  | Config 1 | dB | -5.45 | -11.67 | -11.67 |
| Config 2 | dB | -5.45 | -11.67 | -11.67 |
| Config 3 | dB | -5.45 | -11.67 | -11.67 |
| SSB  | Config 1~3 | dB | 10 | 3 | 3 |
| Io Note 4 | Config 1 | dBm/19.08MHz | -65.43 | -65.43 | -65.43 |
| Config 2 | dBm/19.08MHz | -65.43 | -65.43 | -65.43 |
| Config 3 | dBm/47.88MHz | -61.44 | -61.44 | -61.44 |
| SSB RP Note4 | Config 1 | dBm/SCS | -88 | -95 | -95 |
| Config 2 | dBm/SCS | -88 | -95 | -95 |
| Config 3 | dBm/SCS | -85 | -92 | -92 |
| PRS  | dB | -6.00 | -12.98 | -12.98 |
| Propagation Condition  |  | AWGN |
| Note 1: OCNG shall be used such that active cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols other than those in the slots with transmitted PRS.Note 2: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.Note 3: Interference from other cells and noise sources not specified in the test are assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for to be fulfilled.Note 4: SSB RP and Io levels have been derived from other parameters and are given for information purpose. These are not settable test parameters. The Io is calculated based only on the symbols in which PRS is transmitted. |

###### A.6.6.12.X.2 Test Requirements

The RSCPD reported together with RSTD measurement time fulfils the requirements specified in the clause 9.9.7.

The UE shall perform and report the RSCPD and RSTD measurements for Cell 2 and Cell 3 with respect to the reference cell in the DL-TDOA assistance data, Cell 1, within the time duration specified in section 9.9.7 starting from the beginning of time interval T2.

***NOTE****: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the time duration above because of TTI insertion uncertainty of the measurement report in DCCH.*

The rate of the correct events for DL RSCPD measurement for each neighbour cell observed during the repeated tests shall be at least 90%. The reported DL RSCPD measurement shall be within the DL RSCPD reporting range specified in the Clause 10.1.Y1 and the reported RSTD measurement shall be within the RSTD reporting range specified in the Clause 10.1.23.

**END OF CHANGE 1**