**3GPP TSG-RAN4 Meeting #111 *R4-2409264***

**Fukuoka, Japan, 20 – 24 May, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draftCR on RRM requirements for CPP | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_pos\_enh2-Core | | | | |  | ***Date:*** | | | 2024-04-23 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 1. For CPP measurement, it is unclear which requirements apply when the time window is not configured by LMF, for multiple PFL case. 2. Based on RAN1#115 agreement, legacy measurement (RSTD and Rx-Tx) can be performed within the time window only, or both within and outside the time window. The requirements for the latter are unclear. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | For RSCPD measurement with RSTD in RRC\_IDLE,   1. Clarify that when time window is not configured, legacy requirements for RSTD apply, for multiple PFL case. 2. Clarify that RSTD measurement is not performed within the time window only, legacy requirements for RSTD apply but UE is not required to report RSCPD. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Core equirements for RSCPD measurement with RSTD in RRC\_IDLE are incomplete. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.5.5.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | The draftCR is based on Big draftCR R4-2405983 | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<Start of Change 1>

4.5.5.5 Measurements Period Requirements

After receiving both *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message from the LMF via LPP [34] with *nr-DL-PRS-RSCPD-Request* and configuring a measurement time window via *nr-DL-PRS-MeasurementTimeWindowsConfig,* subject to UE capabilities *supportOfRSCPD-MeasurementInTimeWindow* and *supportOfLegacyMeasurementInTimeWindow*, the UE shall be able to measure multiple (up to the UE capability specified in Clause 4.5.5.3) DL RSTD and DL RSCPD measurements, defined in TS 38.215 [4], during the time window only.

If the UE is not configured with a measurement time window via *nr-DL-PRS-MeasurementTimeWindowsConfig*, the requirements in clause 4.5.2.5 apply. If multiple PFLs are configured in the assistance data, the UE is only required to measure DL RSCPD on one of the PFLs.

If the UE is configured with a measurement time window via *nr-DL-PRS-MeasurementTimeWindowsConfig*, but the UE does not support *supportOfRSCPD-MeasurementInTimeWindow*, the requirements in clause 4.5.2.5 apply. If multiple PFLs are configured in the assistance data, UE is only required to measure DL RSCPD on the PFL associated with the configured measurement time window.

If the UE is configured with a measurement time window via *nr-DL-PRS-MeasurementTimeWindowsConfig*, and UE supports *supportOfRSCPD-MeasurementInTimeWindow* but not *supportOfLegacyMeasurementInTimeWindow*, the requirements in clause 4.5.2.5 apply for DL RSTD measurement. For DL RSCPD measurement, requirements in clause 4.5.2.5 apply prvodied that the resources associated to the measurement time window have occasions only within the measurement time window.

If a periodic time window is configured, the UE shall be able to measure multiple (up to the UE capability specified in Clause 4.5.5.3) DL RSTD and DL RSCPD measurements, defined in TS 38.215 [4], based on the indicated PRS resource sets occurring inside the time window during the measurement period defined as:

Where:

- is the index of positioning frequency layer,

- is total number of positioning frequency layers, and

- is the periodicity of the PRS RSTD measurement in positioning frequency layer i

is the measurement period for PRS RSTD measurement in positioning frequency layer *i* as specified below:

,

Where:

- is the UE Rx beam sweeping factor:

- = 1 if positioning frequency layer *i* is in FR1, and if positioning frequency layer *i* is in FR2

- equals to the value as UE reported in *supportedLowerRxBeamSweepingFactor-FR2* if the capability is reported by the UE for the band containing positioning frequency layer i, and LMF indicates *lowerRxBeamSweepingFactor-FR2* in *NR-DL-TDOA-RequestLocationInformation*.

- equals to 8, otherwise.

- is a scaling factor for PRS-based NR positioning measurements in RRC\_INACTIVE. If the UE supports *parallelPRS-MeasRRC-Inactive-r17*, Kcarrier\_PRS = 1; otherwise,

- If Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ, , where is defined in clause 4.2.2.4

- If Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ, , where is defined in clause 4.2.2.7.

- is the Rx TEG specific scaling factor:

- =1 if the UE is not configured by the LMF to measure a PRS resource with multiple Rx TEGs via *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* [34].

- is defined as follows if the UE is configured by the LMF with *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* [34] to perform measurement on same DL PRS resource of a TRP using different Rx TEGs in *NR-DL-TDOA-RequestLocationInformation* [34]:

- , if the UE is not capable of receiving same DL PRS resource simultaneously from multiple Rx TEGs, where P is the number of UE Rx TEGs that the UE is requested by LMF to measure the same DL-PRS Resource of a TRP indicated by *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* in [34], and in case ‘n0’ is indicated, P is the maximum number of Rx TEGs with which UE can support to measure the same PRS resource as reported in *NR-UE-TEG-Capability*.

- , if the UE is capable of receiving the same DL PRS resource simultaneously from multiple Rx TEGs, where is the number of UE Rx TEGs for measuring the same DL-PRS Resource simultaneously indicated by *measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul-r17* in [34].

- is the maximum number of DL PRS resources in positioning frequency layer *i* configured in a slot.

- is the time duration of available PRS in positioning frequency layer *i* to be measured , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only the unmuted PRS resources in the indicated resources sets that are not fully overlapped with other higher-priority DL signals/channels are considered.

- is the number of PRS RSTD samples, where

- = 1 if the UE supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive* [34], and the LMF requests the UE to perform positioning measurements with reduced number of samples, and meets the following conditions:

- PRS bandwidth is within the initial BWP and

- Magnitude of difference between the serving cell’s SS-RSRP and the neighbor cell’s PRS-RSRP is within 6 dB.

- = 2 if the UE supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive* [34], and the LMF requests the UE to perform positioning measurements with reduced number of samples, and does not meet the following conditions:

- PRS bandwidth is within the initial BWP and

- Magnitude of difference between the serving cell’s SS-RSRP and the neighbor cell’s PRS-RSRP is within 6 dB.

- = 4 otherwise.

- is the measurement duration for the last PRS RSTD sample in positioning frequency layer *i*, including the sampling time and processing time, = + ,

- is the periodicity of the PRS RSTD measurement in positioning frequency layer i defined as:

=

Where:

- corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms-r17* in TS 37.355 [34],

- , the least common multiple between , the DRX cycle length and the time window periodicity ,

- is the periodicity of DL PRS resource with muting on positioning frequency layer *i,* and when calculating , only the PRS resources in the indicated resources sets and overlapped with both the MG and the indicated time window(s) are considered

- is the maximum periodicity of the indicated time window(s).

If more than one PRS periodicities are configured in positioning frequency layer *i*, the least common multiple of PRS periodicities among all DL PRS resource sets in the positioning frequency layer is used to derive , where,

- , is the PRS periodicity with muting per PRS resource,

- is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

- is the scaling factor considering PRS resource muting. , where

- is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and is the size of the bitmap .

- is the UE capability combination per band for RRC\_INACTIVE state where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSymbols-r17* in TS 37.355 [34], T (ms) corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms-r17* in TS 37.355 [34], [ and T-N (>0) is the time required to process duration N of DL PRS symbols already buffered in memory], for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34],

- is UE capability for number of DL PRS resources that it can process in a slot [in RRC\_INACTIVE state as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive-r17* specified in TS 37.355 [34].

The time *s*tarts from the first DRX cycle containing the DL PRS resource(s) in the assistance data after both the *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message are delivered from LMF to the UE via LPP [34].

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

If the DRX cycle is reconfigured during the RSTD measurement period, then the measurement period can be longer.

When PRS-RSRP is configured for DL-TDOA, RSTD and PRS-RSRP are performed over the same measurement period.

The measurement requirements do not apply to any PRS resource that always collides with other higher-priority DL signals/channels, as specified in clause 5.6.1.

Longer RSTD measurement period is expected when there are collisions between PRS resources and other higher-priority DL signals/channels.

If changes for any PFL during the measurement period, the measurement period could be longer.

The measurement requirements do not apply for a PRS resource, if the PRS resource is across two sampling duration of N within duration .

The measurement requirements do not apply for a PRS resource, if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

The requirements in clause 4.x1.5 do not apply if the PRS configuration given by higher layer paramters *NR-DL-PRS-AssistanceData* exceeds any of the UE measurement capabilities given by *NR-DL-PRS-ResourcesCapability* in *NR-DL-TDOA-ProvideCapabilities*, and it is up to UE implementation which PRS resources are measured, subject to UE measurement capabilities*.*

If cell re-selection occurs while RSTD and DL RSCPD measurements are being performed, then the UE shall continue and complete the on-going RSTD and DL RSCPD measurements after the cell selection is completed. The RSTD and DL RSCPD measurement period can be longer.

If the RRC state transition occurs from RRC\_IDLE to RRC\_CONNECTED state during the measurement period then the UE shall continue the RSTD and DL RSCPD measurement in the RRC\_CONNECTED state. The RSTD and DL RSCPD measurement period can be longer.

The UE shall meet the RSTD measurement accuracy requirements in clause 10.1.23.2.

The UE shall meet the DL-RSCPD measurement accuracy requirements in clause 10.x.x.x.

<End of Change 1>