**3GPP TSG-RAN WG4 Meeting # 111 *R4-2409804***

**Fukuoka, JP, May.20 - May.24, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.106** | **CR** | **0069** | **rev** | **1** | **Current version:** | **18.4.0** |  |
|  |
| *For* ***HE******LP*** *on using this form: comprehensive instructions can be found at http://www.3gpp.org/Change-Requests.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for TS 38.106, Correction on conducted receiver general requirement |
|  |  |
| ***Source to WG:*** | CATT |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_netcon\_repeater-Core |  | ***Date:*** | 2024-04-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP TR 21.900. | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | To correct conducted receiver general requirement for NCR |
|  |  |
| ***Summary of change:*** | To modify the title of conducted receiver general requirement in Clause 6.14. |
|  |  |
| ***Consequences if not approved:*** | The conducted receiver general requirement of NCR would be confusing. |
|  |  |
| ***Clauses affected:*** | 6.1, 6.14 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revised from R4-2407506 |

<Start of Change 1>

## 6.1 General

Clause 6 includes the conducted characteristics for both transmitter and receiver.

For conducted transmitter characteristics:

Unless otherwise stated, the conducted transmitter characteristics are specified at the *antenna connector* for *repeater type 1-C* configuration in normal operating conditions.

Requirements apply in both DL and UL unless otherwise stated or declared.

For the DL the *antenna connector* on the BS side is the input and the *antenna connector* on the UE side is the output.

For the UL the *antenna connector* on the UE side is the input and the *antenna connector* on the BS side is the output.

For conducted receiver characteristics:

Conducted receiver characteristics are specified at *antenna connector* for *NCR type 1-C* and TAB connector for *NCR type 1-H*, with full complement of transceivers for the configuration in normal operating condition.

Unless otherwise stated, the following arrangements apply for conducted receiver characteristics requirements in clause 9:

- Requirements apply during the receive period.

- Requirements shall be met for any transmitter setting.

- Throughput requirements defined for the conducted receiver characteristics do not assume HARQ retransmissions.

- For ACS, blocking and intermodulation characteristics, the negative offsets of the interfering signal apply relative to the lower *passband* edge or *inter-passband gap*, and the positive offsets of the interfering signal apply relative to the upper *passband* edge or *inter-passband gap*.

NOTE 1: In normal operating condition the NCR-MT in TDD operation is configured to TX OFF power during *receive period*.

<End of Change 1>

<Start of Change 2>

## . 6.14 Void

<End of Change 2>