**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_perf\_enh-Perf) Editorial CR change to combine tables for requirements applicability for optional UE features |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** |

|  |
| --- |
| The Tables 6.1.1.3-1 and 6.1.1.3-2 are both for optional UE features but are in two separate tables. There is no reason to have two separate tables.  |
|  |
|  |

 |
|  |  |
| ***Summary of change:*** | Combine tables for requirements applicability for optional UE features |
|  |  |
| ***Consequences if not approved:*** | It will be confusing to have 2 separate tables for the same applicability |
|  |  |
| ***Clauses affected:*** | 6.1.1.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-4 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revised from R4-2407238 |

<Start of Change 1>

6.1.1.3 Applicability of requirements for optional UE features

The performance requirements in Table 6.1.1.3-1 shall apply for UEs which support optional UE features with capability signalling only.

**Table 6.1.1.3-1: Requirements applicability for optional UE features**

|  |  |  |  |
| --- | --- | --- | --- |
| **UE feature/capability [14]** | **Test type** | **Test list** | **Applicability notes** |
| CQI table with target BLER of 10^-5New CQI table (cqi-TableAlt) | FR1 FDD | CQI | Clause 6.2.2.1.1.2Clause 6.2.3.1.1.2 |  |
| FR1 TDD | CQI | Clause 6.2.2.2.1.2Clause 6.2.3.2.1.2 |
| Alternative 64QAM MCS table for PDSCH New 64QAM MCS table for PDSCH (*dl-64QAM-MCS-TableAlt*) | FR1 FDD | CQI | Clause 6.2.2.1.1.2Clause 6.2.3.1.1.2 |  |
| FR1 TDD | CQI | Clause 6.2.2.2.1.2Clause 6.2.3.2.1.2 |  |
| Validating P/SP-CSI-RS reception (*periodicAndSemi-PersistentCSI-RS-r16*) | FR1 TDD | CQI | Clause 6.2.2.2.1.3Clause 6.2.3.2.1.3Clause 6.2A.3.1.2Clause 6.2A.4.1.1 | The requirements apply only in case tested UE supporting operations in shared spectrum access and validation of P/SP-CSI-RS reception based on DCI |
| Supported UL channels for dynamic channel access mode (*ul-DynamicChAccess-r16* ) or UL channel access for semi-static channel access mode (*ul-Semi-StaticChAccess-r16*) or both | FR1 TDD | CQI | Clause 6.2.2.2.1.3Clause 6.2.3.2.1.3 | The requirements apply only in case tested UE supports one of UL channels for dynamic channel access mode and UL channel access for semi-static channel access mode |
| 1024QAM modulation for PDSCH for FR1 (pdsch-1024QAM-FR1-r17) | FR1 FDD | CQI | Clause 6.2.2.1.1.3 (Test 1)Clause 6.2.3.1.1.3 (Test 1) |  |
|  | FR1 TDD | CQI | Clause 6.2.2.2.1.4 (Test 1)Clause 6.2.3.2.1.4 (Test 1) |  |
| Support of Type II codebook(*CodebookParameters contains type2, supportedCSI-RS-ResourceList, parameterLx, amplitudeScalingType, amplitudeSubsetRestriction*) | FR1 FDD | PMI | Clause 6.3.2.1.5Clause 6.3.3.1.5 |  |
| FR1 TDD | PMI | Clause 6.3.2.2.5Clause 6.3.3.2.5 |  |
| Support of Enhanced Type II codebook with at least 16 ports per CSI-RS resource(*codebookParametersAddition-r16 contains etype2R1-r16, supportedCSI-RS-ResourceListAdd-r16, maxNumberTxPortsPerResource*) | FR1 FDD | PMI | Clause 6.3.2.1.6Clause 6.3.3.1.6 |  |
| FR1 TDD | PMI | Clause 6.3.2.2.6Clause 6.3.3.2.6 |  |

**Table 6.1.1.3-2: Void**

<End of Change 1>