**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The PDSCH requirements for MU-MIMO advanced receiver agreed to be defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add new tests  • Modify Chapter 5.2.3.2.17 to add new tests | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The performance requirements for MU-MIMO advanced receiver will be incomplete. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS38.521-4 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**START OF CHANGE 1**

##### 5.2.3.2.17 Minimum requirements for PDSCH with intra-cell inter-user interference

The performance requirements are specified in Table 5.2.3.2.17-3 and and Table 5.2.3.2.17-4, with the addition of test parameters in Table 5.2.3.2.17-2 and the downlink physical channel setup according to Annex C.3.1.

The performance requirements for UE supporting Enhanced Receiver Type 2 are specified in Table 5.2.3.2.17-6 and Table 5.2.3.2.17-7, with the addition of test parameters in Tables 5.2.3.2.17-2, 5.2.3.2.17-5 and the downlink physical channel setup according to Annex C.3.1.

The test purposes are specified in Table 5.2.3.2.17-1.

Table 5.2.3.2.17-1: Tests purpose

|  |  |
| --- | --- |
| Purpose | Test index |
| Verify PDSCH performance under 4 receive antenna conditions, when the PDSCH transmission of target UE is interfered by co-scheduled UE. | 1-1, 2-1 |
| Verify PDSCH performance under 4 receive antenna conditions, when the PDSCH transmission of target UE is interfered by co-scheduled UE with Enhanced Receiver Type 2 when modulation order for co-scheduled UE is explicitly signaled by DCI. | 3-1, 4-1 |
| Verify PDSCH performance under 4 receive antenna conditions, when the PDSCH transmission of target UE is interfered by co-scheduled UE with Enhanced Receiver Type 2 when modulation order for co-scheduled UE is detected. | 3-2, 4-2 |

Table 5.2.3.2.17-2: Test parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Unit | Target UE | Co-scheduled UE |
| Duplex mode | |  | TDD | |
| Active DL BWP index | |  | 1 | |
| PDSCH configuration | Mapping type |  | Type A | |
| k0 |  | 0 | |
| Starting symbol (S) |  | 2 | |
| Length (L) |  | 12 | |
| PDSCH aggregation factor |  | 1 | |
| PRB bundling type |  | Static | |
| PRB bundling size |  | 2 | |
| Resource allocation type |  | Type 0 | |
| RBG size |  | Config2 | |
| VRB-to-PRB mapping type |  | Non-interleaved | |
| VRB-to-PRB mapping interleaver bundle size |  | N/A | |
| PDSCH DMRS configuration (Note 1) | DMRS Type |  | Type 1 | |
| Number of additional DMRS |  | 1 | |
| Maximum number of OFDM symbols for DL front loaded DMRS |  | 1 | |
| Antenna ports indexes |  | {1000} for tests 1-1, 3-1, 3-2  {1000, 1001} for tests 2-1, 4-1, 4-2 | {1001} for tests 1-1, 3-1, 3-2  {1002, 1003} for tests 2-1, 4-1, 4-2 |
| Number of PDSCH DMRS CDM group(s) without data |  | 1 for tests 1-1, 3-1, 3-2  2 for tests 2-1, 4-1, 4-2 | 1 for tests 1-1, 3-1, 3-2  2 for tests 2-1, 4-1, 4-2 |
| PDSCH & PDSCH DMRS Precoding configuration | |  | Single Panel Type I, Randomized precoder selection for every PRB bundle and updated per slot, with equal probability of each applicable i1/i2 combination or codebook  Index, chosen from section 5.2.2.2.1 of TS 38.214 [12]. | Single Panel Type I, Randomized precoder selection for every PRB bundle and updated per slot, with equal probability of each applicable i1/i2 combination or codebook  Index, chosen from section 5.2.2.2.1 of TS 38.214 [12].  Any column of precoder matrix is not equal to any column of precoder matrix of Target UE for test 1-1  Select the precoder to ensure any column of precoder is orthogonal to any column of precoder for the target PDSCH for test 2-1, 3-1, 3-2, 4-1, 4-2 |
| MU-MIMO Beamforming Model | |  | As specified in B.4.2 | |
| Number of HARQ Processes | |  | 8 | N/A |
| The number of slots between PDSCH and corresponding HARQ-ACK information | |  | Specific to each TDD UL-DL pattern and as defined in Annex A.1.2 | N/A |
| Note 1: DMRS scrambling ID is the same for both target and co-shceduled UEs. | | | | |

Table5.2.3.1.17-3: Minimum performance for target UE with Rank 1

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test num. | Reference channel | Bandwidth (MHz) / Subcarrier spacing (kHz) | Modulation format and code rate | | TDD UL-DL pattern | Propagation condition | Correlation matrix and antenna configuration | Reference value | |
| Target UE | Co-scheduled UE | Fraction of  maximum  throughput  (%) | SNR (dB) |
| 1-1 | R.PDSCH.7-1.1 TDD | 40 / 30 | 16QAM, 0.48 | Random 16QAM symbols | FR1.30-1 | TDLC300-100 | 2x4, ULA Low | 70 | 11.8 |

Table 5.2.3.2.17-4: Minimum performance for target UE with Rank 2

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test num. | Reference channel | Bandwidth (MHz) / Subcarrier spacing (kHz) | Modulation format and code rate | | TDD UL-DL pattern | Propagation condition | Correlation matrix and antenna configuration | Reference value | |
| Target UE | Co-scheduled UE | Fraction of  maximum  throughput  (%) | SNR (dB) |
| 2-1 | R.PDSCH.7-1.2 TDD | 40 / 30 | 16QAM, 0.48 | Random 16QAM symbols | FR1.30-1 | TDLA30-10 | 4x4, ULA Low | 70 | 15.5 |

The parameters in Table 5.2.3.2.17-5 are configured for requirements with Enhanced Receiver Type 2.

Table 5.2.3.2.17-5: Assistance Information parameters for requirements with Enhanced Receiver Type 2

|  |  |  |
| --- | --- | --- |
| Parameter | | Value |
| AdvancedReceiver-MU-MIMO-r18 | precodingAndResourceAllocation | True |
| pdsch-TimeDomainAllocation | True |
| mcs-Table | qam256 |
| advReceiver-MU-MIMO-DCI-1-1 | Enabled |
| Co-scheduled UE information in DCI (Table 7.3.1.2.2-12 of TS38.212) | | 1 for Test 3-1  2 for Test 4-1  6 for Test 3-2, 4-2 |

Table 5.2.3.2.17-6: Minimum performance for target UE with Rank 1 with Enhanced Receiver Type 2

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test num. | Reference channel | Bandwidth (MHz) / Subcarrier spacing (kHz) | Modulation format and code rate | | TDD UL-DL pattern | Propagation condition | Correlation matrix and antenna configuration | Reference value | |
| Target UE | Co-scheduled UE | Fraction of  maximum  throughput  (%) | SNR (dB) |
| 3-1 | R.PDSCH.7-1.1 TDD | 40 / 30 | 16QAM, 0.48 | Random QPSK symbols | FR1.30-1 | TDLC300-100 | 2x4, ULA Medium | 70 | [15.5] |
| 3-2 | R.PDSCH.7-1.3 TDD | 40 / 30 | 64QAM, 0.43 | Random 16-QAM symbols | FR1.30-1 | TDLC300-100 | 2x4, ULA Medium | 70 | [19.5] |

Table 5.2.3.2.17-7: Minimum performance for target UE with Rank 2 with Enhanced Receiver Type 2

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test num. | Reference channel | Bandwidth (MHz) / Subcarrier spacing (kHz) | Modulation format and code rate | | TDD UL-DL pattern | Propagation condition | Correlation matrix and antenna configuration | Reference value | |
| Target UE | Co-scheduled UE | Fraction of  maximum  throughput  (%) | SNR (dB) |
| 4-1 | R.PDSCH.7-1.4 TDD | 40 / 30 | 64QAM, 0.43 | Random 16QAM symbols | FR1.30-1 | TDLA30-10 | 4x4, ULA Low | 70 | [25.3] |
| 4-2 | R.PDSCH.7-1.2 TDD | 40 / 30 | 16QAM, 0.48 | Random QPSK symbols | FR1.30-1 | TDLA30-10 | 4x4, ULA Low | 70 | [14.9] |

**END OF CHANGE 1**