**3GPP TSG-RAN4 Meeting#111 *R4-2409900***

**Fukuoka City, Fukuoka, Japan, 20th – 24th May, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.104** | **CR** |  | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | ❌ | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on 38.104 Test preambles for multiple PRACH with repetition 2 |
|  |  |
| ***Source to WG:*** | ZTE Corporation, Sanechips |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_cov\_enh2-Perf |  | ***Date:*** | 2024-05-21 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Multiple PRACH for FR2-1 and FR1 are introduced in Rel-18, the test preambles for both FR2-1 and FR1 need to be defined for demodulation requirement. |
| ***,***  |  |
| ***Summary of change:*** | Defining Test preambles of multiple PRACH with repetition 2 for FR1;Defining Test preambles of multiple PRACH with repetition 2 for FR2-1. |
|  |  |
| ***Consequences if not approved:*** | Incomplete demodulation requirements if the corresponding Test preambles are not defined. |
|  |  |
| ***Clauses affected:*** | A.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS/TR 38.141-1,38.141-2 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**<Start of change>**

# A.6 PRACH Test preambles

Table A.6-1: Test preambles for Normal Mode in FR1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| 0 | 1.25 | 13 | 22 | 32 |
| A1, A2, A3, | 15 | 23 | 0 | 0 |
| B4, C0, C2 | 30 | 46 | 0 | 0 |

Table A.6-2: Test preambles for Normal Mode in FR2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| A1, A2, A3, | 60 | 69 | 0 | 0 |
| B4, C0, C2 | 120 | 69 | 0 | 0 |

Table A.6-3: Test preambles for high speed train restricted set type A

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| 0 | 1.25 | 15 | 384 | 0 |

Table A.6-4: Test preambles for high speed train restricted set type B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| 0 | 1.25 | 15 | 30 | 30 |

Table A.6-5: Test preambles for high speed train short formats in FR1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| A2, B4, C2 | 15 | 23 | 0 | 0 |
|  | 30 | 46 | 0 | 0 |

Table A.6-6: Test preambles for PRACH with LRA=1151 and LRA=571

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| A2, B4, C2 | 15 | 164 | 0 | 0 |
|  | 30 | 190 | 0 | 0 |

Table A.6-7: Test preambles for high speed train short formats in FR2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | Logical sequence index | v |
| C2 | 120 | 0 | 0 | 0 |

Table A.6-8: Test preambles for PRACH with LRA=139, LRA=571 and LRA=1151 for 120 kHZ and 480 kHz SCS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | LRA | Ncs | Logical sequence index | v |
| A2B4, C2 | 120 | 571 | 285 | 0 | 0 |
| 120 | 1151 | 575 | 0 | 0 |
| 480 | 139 | 69 | 0 | 0 |
| 480 | 571 | 285 | 0 | 0 |

Table A.6-9: Test preambles for normal mode PRACH with repetitions, LRA=139 in FR2-1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Burst format | SCS (kHz) | Ncs | No. Repetitions | Logical sequence index | v |
|  A2, B4, C2 | 120 | 69 | 2 | 0 | 0 |

**<End of change>**