**3GPP SA WG2 Meeting #164 *S2-240xxxx***

**Maastricht, NL, 19-23 August 2024 *(was S2-240xxxx)***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **23.501** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **19.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps | **x** | ME | **x** | Radio Access Network | **x** | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Configuration of Mobile Wireless Access Backhaul in 5GS | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Incorporated, Sony?, Huawei?, Ericsson?, Nokia?, LGE?, ZTE?, Samsung? | | | | | | | | | |
| ***Source to TSG:*** | SA2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | VMR\_Ph2 | | | | |  | ***Date:*** | | | 2024-08-19 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The approved VMR\_Ph2 work item (SP-240632) is set to specify the architecture enhancements, functionalities and procedures to support MWAB based on conclusions of TR 23.700-06 (clause 8).  This contribution added the configuration control for the MWAB to operate in 5GS. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add the configuration control for MWAB new clause 5.x.2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No proper support of VMR\_Ph2 feature in Rel-19. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | (new) 5.x.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*FIRST CHANGE*

### 5.x.2 Configuration of the MWAB

The two components of MWAB, i.e. MWAB-UE and MWAB-gNB, are configured independently. The MWAB-UE is configured by its HPLMN and/or the BH PLMN (if roaming) for the operations. The MWAB-gNB is configured by the MWAB Broadcasted PLMN. The MWAB-UE and MWAB-gNB may be also pre-configured with some operation parameters.

In order to support MWAB operation, the MWAB-UE should be configured with the following information, besides the normal configurations for a UE:

- (optional) UE Local Configurations of the BH PDU session(s) parameters;

- (optional) dedicated BH PDU session parameters for Emergency Service support (as described in clause 5.x.8).

In order to support MWAB operation, the MWAB-gNB should be configured with the following information:

- Address of the OAM server (e.g. IP address, FQDN) of the MWAB Broadcasted PLMN;

- (optional) configurations on when/where to turn on/off the MWAB-gNB operation;

- AS layer operation parameters for the NG-RAN as defined in TS 38.300 [27].

*End of CHANGEs*