**3GPP TSG-SA5 Meeting #156 S5-244521**

**Maastricht, Netherlands, 19 - 23 August 2024**

**Source: Ericsson LM**

**Title: Solution for PS Data Off**

**Document for: Approval**

**Agenda Item: 7.5.3**

1 Decision/action requested

***The group is asked to discuss and agree on the proposal.***

2 References

[1] 3GPP TS 28.851 Study on charging aspects of next generation real time communication services phase 2

3 Rationale

Addition of solution for using the current PS Data Off information element..

4 Detailed proposal

This document proposes the following changes in TR 28.851 [1].

|  |
| --- |
| **First change** |

7.x Solution #X: Reuse of 3GPP PS Data Off Status

7.X.1 General

This solution #X resolves the key issues 1a and 1b. The solution is based on the current 3GPP PS Data Off Status information element define in TS 32.255 [x], received from the SMF the PS Data Off status can be determined, together with the Change of 3GPP PS Data off Status trigger defined in TS 32.255 [x].

7.X.1 Description

If any charging information is received in the CHF with the 3GPP PS Data Off Status set to Activated, all data usage reported should be rated this information considered.

|  |
| --- |
| **End of change** |