**3GPP TSG-SA5 Meeting #156 *S5-244445***

**Maastricht, Netherlands, 19 - 23 August 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **32.291** | **CR** | **0575** | **rev** | **1** | **Current version:** | **17.10.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Rel-17 CR 32.291 Correction of SMSChargingInformation | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson LM | | | | | | | | | |
| ***Source to TSG:*** | SA5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI16, 5GS\_Ph1-SMSCH | | | | |  | ***Date:*** | | | 2024-08-22 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The referenced to TS 23.040 in table 6.1.6.2.2.3-2 is missing in the references for sMUserDataHeader and is should be stated that it excludes any padding or filler. The sMDataCodingScheme is missing a refence. Both should have the clause as well included in the reference. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding reference to TS 23.040 for sMDataCodingScheme, sMUserDataHeader, and sMStatus.  Updating pattern for sMUserDataHeader and sMStatus. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Undefined representation of attributes may lead till interoperability issues. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, and 6.1.2.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Revision of S5-244141 | | | | | | | | |

|  |
| --- |
| **First change** |

2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] - [13] Void.

[14] 3GPP TS 32.254: "Telecommunication management; Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging ".

[15] - [28] Void.

[29] 3GPP TS 32.274: "Telecommunication management; Charging management;Short Message Service (SMS) charging".

[30] 3GPP TS 32.255: "Telecommunication management; Charging management; 5G Data connectivity domain charging; stage 2".

[31] 3GPP TS 32.256: "Telecommunication management; Charging management; 5G connection and mobility domain charging; stage 2".

[32] 3GPP TS 32.260: "Telecommunication management; Charging management; IP Multimedia Subsystem (IMS) charging".

[33] 3GPP TS 32.275: "Telecommunication management; Charging management; MultiMedia Telephony (MMTel) charging".

[34] 3GPP TS 32.281: " Telecommunication management; Charging management; Announcement

[35] 3GPP TS 32.277: "Telecommunication management; Charging management; Proximity-based Services (ProSe) charging".

[36] 3GPP TS 32.257: "Telecommunication management; Charging management; Edge computing domain charging; stage 2".

[37] - [49] Void.

[50] - [57] Void.

[58] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI).

[59] - [69] Void.[70] 3GPP TS 28.201: "Charging management; Network slice performance and analytics charging in the 5G System (5GS); Stage 2".

[71] 3GPP TS 28.202: "Charging management; Network slice management charging in the 5G System (5GS); Stage 2".

[72] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TR 21.900: "Technical Specification Group working methods".

[102] 3GPP TS 24.605: "Conference (CONF) using IP Multimedia (IM) Core Network (CN) subsystem; Protocol specification".

[103] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS) "

[104] - [199] Void

[200] - [252] Void

[253] 3GPP TS 28.532: "Management and orchestration; Management services".

[254] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM); Stage 2 and stage 3".

[255] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects".

[256] 3GPP TS 28.554: "Management and orchestration;5G end to end Key Performance Indicators (KPI)".

[257] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[258] 3GPP TS 24.229: "IP Multimedia Call Control Protocol based on SIP and SDP; Stage 3".

[259] 3GPP TS 29.078: "Customised Applications for Mobile network Enhanced Logic (CAMEL); CAMEL Application Part (CAP) specification".".

[260] 3GPP TS 29.228: "IP Multimedia (IM) Subsystem Cx and Dx interface; signalling flows and message contents".

[261] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[262] 3GPP TS 28.550: "Management and orchestration; Performance assurance ".

[263] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements ".

[264] - [298] Void

[299] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[300] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[301] 3GPP TS 29.594: "5G System; Spending Limit Control Service; Stage 3".

[302] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[303] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[304] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[305] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[306] 3GPP TS 29.520: "5G System; Network Data Analytics Services;Stage 3".

[307] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification".

[308] 3GPP TS 24.334: " Proximity-services (ProSe) User Equipment (UE) to ProSe function protocol aspects; Stage 3".

[309] 3GPP TS 29.558: "Enabling Edge Applications; Application Programming Interface (API) specification; stage 3".

[310] 3GPP TS 28.538: "Management and orchestration; Edge Computing Management".

[311] 3GPP TS 24.558: "Enabling Edge Applications; Protocol specification".

[312] - [370] Void

[371] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[372] - [389] Void

[390] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[391] - [399] Void

[400] Void.

[401] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2) ".

[402] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format ".

[403] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[404] IETF RFC 3986: "Uniform Resource Identifiers (URI): Generic Syntax".

[405] IETF RFC 7315: "Private Extensions to the Session Initiation Protocol (SIP) for the 3rd Generation Partnership Projects (3GPP)".

[406] IETF RFC 3261: "SIP: Session Initiation Protocol".

[407] IETF RFC 8866: "SDP: Session Description Protocol".

[408] IETF RFC 5646: "Tags for Identifying Languages".

[409] - [499] Void.

[500] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[501] - [599] Void.

|  |
| --- |
| **Second change** |

6.1.6.2.3.2 Type SMSChargingInformation

**Table  6.1.6.2.2.3-2: Definition of type SMSChargingInformation**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| originatorInfo | OriginatorInfo | OM | 0..1 | originator of the SM |  |
| recipientInfo | Array(RecipientInfo) | OC | 0..N | recipient information for the SM |  |
| userEquipment Info | Pei | OC | 0..1 | the identification of the terminal |  |
| roamerInOut | RoamerInOut | OC | 0..1 | In-bound or Out-bound roamer |  |
| userLocationInfo | UserLocation | OC | 0..1 | provides information on the location |  |
| uetimeZone | TimeZone | OC | 0..1 | the UE Time Zone the UE is currently located |  |
| rATType | RatType | OC | 0..1 | the identification of the RAT type. |  |
| sMSCAddress | string | OM | 0..1 | the address (e.g. E.164) of the SMS-service centre sending the Charging Data Request used for producing the record. (SMSC Address) |  |
| sMDataCodingScheme | integer | OM | 0..1 | the information from the TP-Data-Coding-Scheme (TP DCS) field in the TPDU specified in TS 23.040 [103] clause 9.2.3.10. |  |
| sMMessageType | SMmessageType | OM | 0..1 | identifies the message that triggered the generation of charging information. |  |
| sMReplyPathRequested | ReplyPathRequested | OC | 0..1 | an indication of whether a reply SM to an original SM was requested to follow the same path as identified by the TP-Reply-Path (TP-RP) flag. |  |
| sMUserDataHeader | string | OC | 0..1 | the user data header (TP-UDH) extracted from the TP-User-Data (TP-UD) specified in TS 23.040 [103] clause 9.2.3.24, excluding any padding and filler. |  |
| sMStatus | string | OC | 0..1 | the information from the TP-Status (TP-ST) field in the TPDU specified in TS 23.040 [103] clause 9.2.3.15.  It carries the value in hexadecimal representation.  Pattern: '^[0-7]?[0-9a-fA-F] $' |  |
| sMDischargeTime | DateTime | OC | 0..1 | the time associated with the event being reported in the SM Status field. This information is only applicable to delivery report charging procedures. |  |
| numberofMessagesSent | Uint32 | OC | 0..1 | the number of SMSs sent by the IMS application or the total number of short messages when this SM is part of concatenated short message, if applicable. |  |
| sMServiceType | SMServiceType | OC | 0..1 | the type of SM service that caused the charging interaction. It is only applicable for SM supplementary service procedures. |  |
| sMSequenceNumber | Uint32 | OC | 0..1 | the sequence number of this SM within the concatenated short message |  |
| sMSresult | Uint32 | C | 0..1 | the result of the attempted SM transaction, if unsuccessful.  This field is only for offline charging. |  |
| submissionTime | DateTime | OC | 0..1 | the timestamp of when the submitted SM arrived at the originating SMS Node |  |
| sMpriority | SMPriority | OC | 0..1 | any priority information associated with an SM |  |
| messageReference | string | OM | 0..1 | the identity used to identify an SM in the SMS node associated with entity that submitted it |  |
| messageSize | Uint32 | OM | 0..1 | the total number of short messages when this SM is part of concatenated short message |  |
| messageClass | MessageClass | OM | 0..1 | implementation dependent the value selected for a specific transaction. |  |
| deliveryReportRequested | DeliveryReportRequested | OC | 0..1 | indicates whether a delivery report is requested by the SM originator |  |



|  |
| --- |
| **End of changes** |