**3GPP TSG-SA5 Meeting #156 *S5-245048***

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0441** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Rel18 CR TS 28.622 Removing unnecessary statement on MnsAgent usage in SBMA |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | 16 |  | ***Date:*** | 2024-08-08 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The statement in clause 4.3.2a of TS 28.622 is misleading since it implies that the other IOCs defined in the specification are not based on SBMA.. |
|  |  |
| ***Summary of change:*** | Deleting the redundant statement on MnsAgent usage |
|  |  |
| ***Consequences if not approved:*** | The statement is misleading and can lead to misinterpratation of the standard |
|  |  |
| ***Clauses affected:*** | 4.3.2a |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | S5-245048 is the revision of S5-244317.  |

|  |
| --- |
| **Begin Change** |

### 4.3.2a MnsAgent

#### 4.3.2a.1 Definition

The MnsAgent represents the MnS producers, incl. the supporting hardware and software, available for a certain management scope that is related to the object name-containing the MnS Agent.

The MnSAgent can be name-contained under an IOC as follows:

1) ManagementNode;

2) SubNetwork, if the SubNetwork does not contain a ManagementNode;

3) ManagedElement, if it is the root element.

In case the MnsAgent is name-contained under a ManagementNode, the management scope is the complete management scope of the ManagementNode or a subset thereof.

In case the MnsAgent is name-contained under a SubNetwork, the management scope is the complete SubNetwork or a subset thereof.

In case the MnsAgent is name-contained under a ManagedElement, the management scope is the complete ManagedElement or a subset thereof.

#### 4.3.2a.2 Attributes

The MnSAgent IOC includes the attributes inherited from Top\_ IOC (defined in TS 28.620 [9]), attributes inherited from Top IOC (defined in clause 4.3.8) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute Name | S | isReadable  | isWritable | isInvariant | isNotifyable |
| systemDN | M | T | F | F | T |

#### 4.3.2a.3 Attribute constraints

None.

#### 4.3.2a.4 Notifications

The common notifications defined in clause 4.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **End Change** |