**3GPP TSG RAN WG1 #100bis R1-200xxxx**

**e-Meeting, April 20th – 30th, 2020**

Source: moderator (vivo)

Title: Feature lead summary on ULFPTx-01

Agenda Item: 7.2.6.4

Document for: Discussion and Decision

1. Introduction

Following email thread is assigned for discussion:

[100b-e-NR-eMIMO-ULFPTx-01] Email discussion on Issue #2 in R1-2002746: For 4Tx and partial-coherent UE in Mode 2, when the SRS resource set is configured with 2 ports SRS and 4 ports SRS, and the codebook subset associated with 2 port SRS resource. By 4/24 and corresponding TP (if any) by 4/30 – Rakesh (vivo)

1. Discussion on issue 2[1]
	1. Issue 2: For 4Tx and partial-coherent UE in Mode 2, when the SRS resource set is configured with 2 ports SRS and 4 ports SRS, and the codebook subset associated with 2 port SRS resource:
* Alt1: introduce a new UE capability, UE indicates whether it is *fullyAndPartialAndNonCoherent or nonCoherent*
* Alt2: the codebook subset is *nonCoherent*
* Alt3: the codebook subset is *fullyAndPartialAndNonCoherent*

Please provide your views/comments in the table below

|  |  |
| --- | --- |
| Company/organization | Comments |
| OPPO | Support Alt.21. According to the LS R1-2001513, some new RRC parameter is needed for Alt.1. Introducing non-essential new RRC parameter at a so-late stage is not a wise design, and may lead to further workload and more risk for ASN.1 frozen
2. As explained several times, it cannot be guaranteed that the 2 ports are coherent. Thus Alt.3 does not work for many UE implementations.
 |
| CMCC | We support Alt2, since we think the motivation of Alt1 or Alt3 is not clear. In our understanding, the 2 ports can be considered as coherent only when the 2 ports are virtualized from the first and third port (i.e., using [1 0 1 0]) or from the second and fourth port (i.e., using [0 1 0 1]) of the 4 ports. Let’s take the former case as an example, we can assume both the first and the third port can support 20dBm in order to support full power transmission. However, in that case, the 2-port is equivalent to the 4-port using reported TPMIs (e.g., using G4, ; ) which can support full power transmission.  |
| LG | Support Alt 2. Similar view with OPPO, in order to avoid new RRC parameter, Alt 2 or Alt 3 can be considered. Between Alt 2 and Alt 3, we think Alt 2 is more preferable, since Alt 3. may require higher UE implementation complexity/cost compared to Alt 2.  |
| Huawei, HiSilicon | Support Alt.2. Here the condition is 2-port SRS and 4 port SRS resources are both configured. For the following all three cases:If each antenna port is virtualized from a group of two coherent antennas, then after virtualization, it will be non-coherent between the two ports. If each antenna port is virtualized from a group of two non-coherent antennas, the after virtualization, the phase in each port is difficult to be guaranteed. So, it results to non-coherent between two ports.If each antenna port is virtualized from a group of two non-coherent antennas with [1 0] or [0 1], yes, the two ports will be coherent. However, the case is equivalent to non-virtualized case with [1 0 1 0] or [0 1 0 1], without any benefits.From above, only Alt.2 makes sense. Some detailed discussion also can be find in R1-2001565.  |
| Samsung | We prefer Alt 1 due to the following reason:* The virtualization of 2 ports (from 4 ports) is up to UE implementations, and the UE should have the freedom/flexibility to implement any virtualization of 2 ports. This freedom is completely lost in Alt2 since it restricts 2 ports to be non-coherent. Alt3 is also restrictive, but it is better than Alt 2, at least in the sense that TPMI can be non-coherent or full-coherent.
* Re the comment “If each antenna port is virtualized from a group of two non-coherent antennas with [1 0] or [0 1], yes, the two ports will be coherent. However, the case is equivalent to non-virtualized case with [1 0 1 0] or [0 1 0 1],” we also need to look at TPMI payload, which is certainly not the same. In particular, the TPMI payload is more in case of 4 ports than in case of 2 ports. Hence, the two cases are not equivalent operationally.

Re CMCC comment, in our view, mode 2 has two solutions: (1) based on TPMI group signaling and (2) based on multiple SRS resources with different number of SRS ports. This email discussion pertains to (2), not (1). |
| CATT | OK with alt-2 and alt-3, with slight preference on alt-2. Alt-1 is not preferred due to RRC impact. In our view this is not a critical issue to warrant RRC changes at this late stage. Last but now least, there has been no thorough evaluation on the performance gain over the other simpler alternatives.  |

Observation:

Proposal:

# References

[1] R1-2002746, Summary of prep email discussion on ULFPTx, RAN1#100b-e