**3GPP TSG-RAN WG1 Meeting #101-eR1-20wxyz**

**e-Meeting, May 25 – June 5, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.212** | **CR** |  | **rev** |  | **Current version:** | **14.12.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction to define the values of SPS activation/release in DCI format 5A |
|  |  |
| ***Source to WG:*** | FUTUREWEI |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | LTE\_V2X-Core |  | ***Date:*** | 2020-6-11 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-14 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | DCI 5A contains a SPS activation/release field. However, it is not defined which field value corresponds to activation, and which field value correspond to release. |
|  |  |
| ***Summary of change:*** | The change is to add the meaning of 0 and 1 for this field.The TP was endorsed in R1-2004955 as part of [101-e-NR-5G\_V2X\_NRSL-NRUuSchedulingLTESL-01]. |
|  |  |
| ***Consequences if not approved:*** | The UE does not know how to interpret this field. |
|  |  |
| ***Clauses affected:*** | 5.3.3.1.9A |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.211, TS 36.213 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

##### 5.3.3.1.9A Format 5A

-- text is omitted ----

When the format 5A CRC is scrambled with SL-SPS-V-RNTI, the following fields are present:

- SL SPS configuration index – 3 bits as defined in clause 14.2.1 of [3].

- Activation/release indication – 1 bit, where value 0 indicates release and value 1 indicates activation.