**3GPP TSG-RAN WG1 Meeting #101-eR1-20wxyz**

**e-Meeting, May 25 – June 5, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.212** | **CR** |  | **rev** |  | **Current version:** | **13.10.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction to remove the term ‘compact’ for DCI format 6-1A |
|  |  |
| ***Source to WG:*** | FUTUREWEI |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | LTE\_MTCe2\_L1 |  | ***Date:*** | 2020-6-11 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-13 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The initial draft of eMTC DL CE mode A functionality was included within DCI format 1A, which is a “compact” DCI format. The term was not removed when the functionality was copied into a standalone DCI format. The term “compact” in 6-1A may be misleading, as there is no corresponding “non-compact” format. |
|  |  |
| ***Summary of change:*** | Delete the term “compact” from the preamble of DCI format 6-1A |
|  |  |
| ***Consequences if not approved:*** | Possible confusion when reading the DCI format 6-1A |
|  |  |
| ***Clauses affected:*** | 5.3.3.1.12 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.211, TS 36.213 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Isolated impact analysis: There is no impact to any UE or eNB implementation |
|  |  |
| ***This CR's revision history:*** |  |

##### 5.3.3.1.12 Format 6-1A

DCI format 6-1A is used for the scheduling of one PDSCH codeword in one cell and random access procedure initiated by a PDCCH order. The DCI corresponding to a PDCCH order can be carried by MPDCCH.