**3GPP TSG RAN WG1 Meeting #101-e R1-200xxxx**

**E-meeting, May 25 – June 5, 2020**

**Title:** [DRAFT] Reply LS on transmit power of CSI-RS across different occasions

**Response to:** **R1-2003273 (R4-2005377)**

**Release:** Rel-16

**Work Item:** NR\_unlic-core,

**Source:** RAN WG1

**To:** RAN WG4

**Cc:**

**Contact Person:**

#### Name: Jiayin Zhang

**Tel. Number:**

E-mail Address: zhangjiayin@huawei.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:**

RAN1 received the RAN4 LSon the transmit power of CSI-RS across different occasions and is requested to confirm whether a UE can assume that CSI-RS (for L1-RSRP, RLM, BFD and CBD) is transmitted with the same transmit power across different occasions during the measurement period, and whether this also applies to SSB-based RRM measurements.

RAN1 confirms that UE can assume same transmit power of NZP CSI-RS or SSB (for L1-RSRP, RLM, BFD CBD and RRM) across different occasions and can average the measurement during the measurement period.

**2. Actions:**

**To RAN4.**

**ACTION:** RAN1 kindly requests RAN4 to take the above information into account when considering the design of L1-RSRP, RLM, BFD, CBD and SSB-based RRM measurements for NR-U

**3. Date of Next TSG-RAN1 Meetings:**

TSG RAN WG1 Meeting #102-e Aug 2020 e-Meeting

TSG RAN WG1 Meeting #102-bis 12 – 16 Oct 2020 China