**3GPP TSG RAN WG1 Meeting #101-e                     R1-200xxxx**

**e-Meeting, May 25th – June 5th, 2020**

**Agenda Item: 7.2.2.2.3**

**Source: Moderator (Huawei)**

**Title: Feature lead summary#1 on 101-e-NR-unlic-NRU-HARQ-03 (NNK1 value)**

**Document for: Discussion and Decision**

# Introduction

This document provides updated proposals on issues C1, C2 and C3 that are prioritized for RAN1#101e among the issues identified for the **corrections related to NNK1 value** [1].

[101-e-NR-unlic-NRU-HARQ-03] Email discussion/approval on issues C1, C2 and C3 from R1-2004692 until 5/28; if necessary, endorse associated TPs by 6/3 – David (Huawei)

* Issue C1 (leftover):
	+ FFS: DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate Scell dormancy
	+ FFS: DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate SPS release (note: some dependency on B6)
* Issue C2: DCI format 1\_2 usage with PUCCH priority in case of NNK1 value signaled in PDSCH-to-HARQ\_feedback timing indicator
* Issue C3: Out-of-Order issue for NNK1

Each sub-section per issue includes an initial FL proposal based on the summary of the submitted Tdocs, and provides a table for collecting companies’ views on the FL’s proposal.

# Issue C1

|  |  |
| --- | --- |
| C1 | - FFS: DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate Scell dormancy- FFS: DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate SPS release |

Summary of companies’ views:

DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate Scell dormancy

* Support: ZTE, Sanechips, Huawei, HiSilicon, LGE
* Do not support: Nokia, Nokia Shanghai Bell

DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate SPS release

* Support: ZTE, Sanechips, Huawei, HiSilicon, LGE, Qualcomm
* Do not support: Nokia, Nokia Shanghai Bell

|  |  |
| --- | --- |
| **Company** | **Comments on issue C1** |
|  |  |

|  |  |
| --- | --- |
| **Company** | **Summary of proposals** |
| ZTE(R1-2003452) | DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate SPS release.DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate Scell dormancy. |
| Huawei(R1-2003514) | DCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate Scell dormancyDCI format 1\_1 should not simultaneously indicate a NNK1 value and indicate SPS release**TP#2 for TS 38.213 Clause 10.2(on top of R1-2003180)**=== Unchanged part omitted ===A UE validates, for scheduling activation or scheduling release, a DL SPS assignment PDCCH or a configured UL grant Type 2 PDCCH if- the CRC of a corresponding DCI format is scrambled with a CS-RNTI provided by *cs-RNTI*, and- the new data indicator field in the DCI format for the enabled transport block is set to '0', and- the DFI flag field, if present, in the DCI format is set to '0', and- if the PDSCH-to-HARQ\_feedback timing indicator field in the DCI format is present, the PDSCH-to-HARQ\_feedback timing indicator field does not provide an inapplicable value from *dl-DataToUL-ACK*. === Unchanged part omitted ===**TP#3 for TS 38.213 Clause 10.3(on top of R1-2003180)**=== Unchanged part omitted ===If a UE is provided search space sets to monitor PDCCH for detection of DCI format 1\_1, and if- the CRC of DCI format 1\_1 is scrambled by a C-RNTI or a MCS-C-RNTI, and if - *resourceAllocation* = *resourceAllocationType0* and all bits of the frequency domain resource assignment field in DCI format 1\_1 are equal to 0, or- *resourceAllocation* = *resourceAllocationType1* and all bits of the frequency domain resource assignment field in DCI format 1\_1 are equal to 1- *resourceAllocation = dynamicSwitch* and all bits of the frequency domain resource assignment field in DCI format 1\_1 are equal to 0 or 1- if the PDSCH-to-HARQ\_feedback timing indicator field in the DCI format is present, the PDSCH-to-HARQ\_feedback timing indicator field does not provide an inapplicable value from *dl-DataToUL-ACK*.the UE considers the DCI format 1\_1 as indicating SCell dormancy, not scheduling a PDSCH reception or indicating a SPS PDSCH release, and for transport block 1 interprets the sequence of fields of=== Unchanged part omitted === |
| LG(R1-2004015) | Proposal #7: DCI format 1\_1 indicating Scell dormancy operation or DL SPS release is not allowed to indicate NNK1 value (simultaneously) |
| Nokia(R1-2004257) | For both DL SPS release and Scell dormancy indication, precluding NNK1 value in DCI would imply a scheduling restriction, since DL SPS release nor Scell dormancy indication could be transmitted in the end of gNB COT. On the other hand, there is no specification impact from supporting these cases. **Proposal 10: *Inapplicable value of K1 in DL SPS release and Scell dormancy DCI is not precluded*** |
| Qualcomm(R1-2004445) | Proposal 1. If UE is configured with a SPS configuration, one bit is appended to the end of Type-3 HARQ-Ack codebook. If UE detects a DCI format releasing an SPS configuration and indicates the slot in which the Type-3 HARQ-Ack is reported, the bit is set to Ack; otherwise, the bit is set to Nack.* UE does not expect NN-K1 in a SPS release DCI.

===TP for 38.213 Section 10.2==A UE validates, for scheduling activation or scheduling release, a DL SPS assignment PDCCH or a configured UL grant Type 2 PDCCH if- the CRC of a corresponding DCI format is scrambled with a CS-RNTI provided by *cs-RNTI*, and- the new data indicator field in the DCI format for the enabled transport block is set to '0', and- the DFI flag field, if present, in the DCI format is set to '0', and- the PDSCH-to-HARQ\_feedback timing indicator field,if present, does not provide an inapplicable value from *dl-DataToUL-ACK*. If a UE is provided a single configuration for UL grant Type 2 PUSCH or for SPS PDSCH, validation of the DCI format is achieved if all fields for the DCI format are set according to Table 10.2-1 or Table 10.2-2. --Unchanged part omitted------------------------ |

# Issue C2

|  |  |
| --- | --- |
| C2 | DCI format 1\_2 usage with PUCCH priority in case of NNK1 value signaled in PDSCH-to-HARQ\_feedback timing indicator |

Companies are invited to provide their views using the table below, considering the following cases. Type 3 HARQ-ACK codebook is not mentioned since there is no field in DCI Format 1\_2 for triggering a request for Type 2 HARQ-ACK codebook.

* When two HARQ-ACK codebooks are configured for the same serving cell, if the UE detects a DCI format 1\_2 scheduling a PDSCH and indicating Priority indicator value, please provide your views on whether providing an inapplicable value for PDSCH-to-HARQ\_feedback timing indicator field is supported and if so in which conditions using the table below:

|  |  |  |
| --- | --- | --- |
|  | NNK1 value is not expected to be signaled in DCI format 1\_2 | NNK1 value can be signaled in DCI format 1\_2 |
| Case1: UE is configured with Type1 HARQ-ACK codebook |  |  |
| Case2: UE is configured with Type2 HARQ-ACK codebook |  |  |
| Case3: UE is configured with enhanced Type2 HARQ-ACK codebook |  |  |

Companies are invited to provide more detailed (lengthy) comments using the table below:

|  |  |
| --- | --- |
| **Company** | **Summary of proposals and further companies’ views** |
| MediaTek(R1-2003658) | Proposal 1: When enhanced dynamic HARQ-ACK codebook is configured, reuse the mechanism specified for handling DCI format 1\_0 to handle DCI format 1\_2On handling of DCI format with inapplicable K1 value, UE may multiplex the HARQ-ACK information corresponding to a first DCI format indicating an inapplicable K1 value in a PUCCH that is indicated by an applicable value in a second DCI format. According to current specification, UE only multiplexes UCIs with the same priority index in a PUCCH or PUSCH, and multiplexing procedure is behaved independently for each HARQ-ACK codebook that is associated with a PUCCH with one of the priority indexes. Thus, it is pretty clear that UE multiplexes the HARQ-ACK information corresponding to the first DCI format only when the second DCI format indicates a PUCCH with the same priority index. Observation 2: If a UE receives a first DCI providing an inapplicable K1 value, and the UE detects a second DCI indicates a slot of PUCCH or PUSCH transmission by an applicable K1 value, it is clear in current specification that UE only multiplexes the corresponding HARQ-ACK information in the PUCCH or PUSCH transmission of a same priority index indicated by the first DCI, if applicable. |
| Ericsson(R1-2003845) | Proposal 6: When two HARQ-ACK codebooks are configured for the same serving cell, if the UE detects a DCI scheduling a PDSCH and indicating Priority indicator value and inapplicable value for PDSCH-to-HARQ\_feedback timing indicator field, the HARQ-ACK information corresponding to the PDSCH is multiplexed in PUCCH occasion indicated by the immediate next DCI scheduling another PDSCH and indicating the same Priority indicator value and applicable value for PDSCH-to-HARQ\_feedback timing indicator.Proposal 7: The presence of (PDSCH group index, New feedback indicator, Number of requested PDSCH group(s), total DAI for non-scheduled group) in DCI 1\_2 and (total DAI for non-scheduled group) in DCI 0\_2 can be disabled even when enhanced dynamic codebook is configured. Proposal 8: The presence of One-shot HARQ-ACK request field in DCI 1\_2 can be disabled even if higher layer parameter pdsch-HARQ-ACK-OneShotFeedback-r16 is configured. |
| Nokia, NSB (from prioritization discussion) | NN-K1 should be supported with 1\_2 (spec clarification is essential) |
| ZTE (from prioritization discussion) | At least the enhanced type2/type3 CB for DCI format 1\_2 should not be discussed in Rel-16 |
|  |  |
|  |  |
|  |  |

# Issue C3

|  |  |
| --- | --- |
| C3 | Out-of-Order issue for NNK1 |

Companies are invited to provide detailed comments on the issue and on the TP proposed in R1-2004445 using the table below.

|  |  |
| --- | --- |
| **Company** | **Summary of proposals and further companies’ views** |
| Qualcomm(R1-2004445) | Non-numeric K1 may result in out-of-order operation. This can happen when a first DCI that indicates non-numeric K1 is detected but a second DCI that indicates a numeric K1 (and was supposed to indicate the timing for HARQ-Ack for the PDSCH scheduled by the first DCI) is missed.**Proposal 2. HARQ-Ack for a PDSCH that is scheduled with a non-numeric K1 is multiplexed in the next PUCCH that carries HARQ-Ack and satisfies the UE PDSCH processing timeline for the PDSCH if UE has not detected the second DCI with numeric-K1 that points to an slot earlier than the PUCCH slot**.==TP for 38.213 Section 9.1.3===--Unchanged part omitted------------------------If a UE receives a first PDSCH scheduled by a first DCI format that the UE detects in a first PDCCH monitoring occasion and includes a PDSCH-to-HARQ\_feedback timing indicator field providing an inapplicable value from *dl-DataToUL-ACK*, - if the UE detects a second DCI format, the UE multiplexes the corresponding HARQ-ACK information in a PUCCH or PUSCH transmission in a slot that is indicated by a value of a PDSCH-to-HARQ\_feedback timing indicator field in the second DCI format, where- if the UE is not provided *pdsch-HARQ-ACK-Codebook = enhancedDynamic-r16*, the UE detects the second DCI format in any PDCCH monitoring occasion after the first one- if the UE is provided *pdsch-HARQ-ACK-Codebook = enhancedDynamic-r16*, the UE detects the second DCI format in any PDCCH monitoring occasion after the first one, and the second DCI format indicates a HARQ-ACK information report for a same PDSCH group index as indicated by the first DCI format as described in Clause 9.1.3.3 - if the UE is provided *pdsch-HARQ-ACK-OneShotFeedback-r16*, the UE detects the second DCI format in any PDCCH monitoring occasion after the first one, and the second DCI format includes a One-shot HARQ-ACK request field with value 1, the UE includes the HARQ-ACK information in a Type-3 HARQ-ACK codebook, as described in Clause 9.1.4.- if there is a PUCCH or PUSCH transmission in a slot that carries HARQ-Ack and satisfies timing conditions in Clause 9.2.5, and the second DCI has not been detected that points to an earlier slot for HARQ-Ack transmission, the UE multiplexes the HARQ-ACK information for the first PDSCH in the PUCCH or PUSCH transmission in the slot. --Unchanged part omitted------------------------ |
|  |  |
|  |  |
|  |  |

# Conclusions

TBD

# References

1. R1-2004692 FL summary\_1 for 72223 NRU HARQ moderator (Huawei), RAN1#101-e
2. R1-2003372 Remaining issues on HARQ operation for NR-U vivo
3. R1-2003452 Remaining issues on the HARQ for NR-U ZTE, Sanechips
4. R1-2003514 Maintenance on HARQ-ACK enhancement Huawei, HiSilicon
5. R1-2003658 Remaining issues on HARQ operation for NR-U MediaTek Inc.
6. R1-2003730 Enhancements to HARQ for NR-unlicensed Intel Corporation
7. R1-2003823 Text proposals for HARQ enhancement for NR-U Lenovo, Motorola Mobility
8. R1-2003845 HARQ enhancement Ericsson
9. R1-2003862 HARQ enhancement for NR-U Samsung
10. R1-2004015 Remaining issues of HARQ procedure for NR-U LG Electronics
11. R1-2004087 Discussion on the remaining issues of HARQ enhancements OPPO
12. R1-2004257 Remaining issues on NR-U HARQ scheduling and feedback Nokia, Nokia Shanghai Bell
13. R1-2004325 Remaining issues and corrections on HARQ enhancement for NR-U Sharp
14. R1-2004445 TP for Enhancements to Scheduling and HARQ Operation for NR-U Qualcomm Incorporated
15. R1-2004529 Text proposal for enhanced dynamic HARQ procedures Google Inc.