**3GPP TSG RAN WG1 #101 R1-200xxxx**

**e-Meeting, May 25th– June 5th, 2020**

Agenda Item: 7.2.6.3

Source: Moderator (Apple)

Title: Feature Lead Summary on L1-SINR and SCell BFR email thread #3

Document for: Discussion/Decision

# Introduction

In this contribution, we provide a summary of issues on L1-SINR and SCell BFR email thread #3

# SRS beam after BFR

Reason for change

After the SCell BFR response have been received by UE for the step 2 MAC-CE, it has been agreed that all CORESET and PUCCH beams in the failed SCell will be reset to the new beam reported in step 2 MAC-CE. It would be also beneficial to reset the beams for SRS resources with the usages of ‘codebook’ and ‘non-codebook’ and hence the beams for PUSCH to quickly recover the UL data transmission as well.

Summary of changes

For SRS for CB and nCB usages with spatial relation configured, after 28 symbols from receiving response to step 2 MAC-CE, UE applies the new beam indicated in step 2 MAC-CE for SRS on the failed SCell if a new beam is identified.

Consequences if not approved

UE has to keep previous beam after receiving response to MAC CE.

***TP for 38.213***

|  |
| --- |
| 38.213->6 Link recovery procedures  […]  A UE can be provided, by *schedulingRequestIDForBFR*, a configuration for PUCCH transmission with a link recovery request (LRR) as described in Clause 9.2.4. The UE can transmit in a first PUSCH at least one MAC CE providing one index for at least one corresponding SCell with radio link quality worse than Qout,LR, an index for a periodic CSI-RS configuration or for a SS/PBCH block provided by higher layers, as described in [11, TS 38.321], if any, for a corresponding SCell. After 28 symbols from a last symbol of a PDCCH reception with a DCI format scheduling a PUSCH transmission with a same HARQ process number as for the transmission of the first PUSCH and having a toggled NDI field value, the UE  - monitors PDCCH in all CORESETs on the SCell(s) indicated by the MAC CE using the same antenna port quasi co-location parameters as the ones associated with the corresponding index(es) , if any  - transmits PUCCH on a PUCCH-SCell using a same spatial domain filter as the one corresponding to for periodic CSI-RS or SS/PBCH block reception, as described in Clause 9.2.2, and using a power determined as described in Clause 7.2.1 with , , and , if  - the UE is provided *PUCCH-SpatialRelationInfo* for the PUCCH,  - a PUCCH with the LRR was either not transmitted or was transmitted on the PCell or the PSCell, and  - the PUCCH-SCell is included in the SCell(s) indicated by the MAC-CE  - transmits SRS resource with higher layer parameter usage in SRS-ResourceSet set to 'codebook' and 'nonCodebook' using a same spatial domain filter as the one corresponding to for periodic CSI-RS or SS/PBCH block reception, as described in Clause 9.2.2, and using a power determined as described in Clause 7.3.1 with , and , if  - the UE is provided *spatialRelationInfo* for the SRS resource  where the SCS configuration for the 28 symbols is the smallest of the SCS configurations of the active DL BWP for the PDCCH reception and of the active DL BWP(s) of the at least one SCell.  […] |

**Companies view and comments**

|  |  |
| --- | --- |
| Company | View |
| Apple | Agree with this in principle, but the condition “if the UE is provided *spatialRelationInfo* for the SRS resource” should be removed. |
| Ericsson | Agree with Apple: the TP is fine in principle, but the condition on *spatialRelationInfo* is unnecessary, the UE would apply the defaults in any case. |
| Sony | Agree in principle. |