**3GPP TSG RAN WG1 Meeting #106-e R1-21xxxxx**

**E-Meeting, August 16th – August 27th, 2021**

**Agenda Item: 6**

**Source: Moderator (Huawei)**

**Title: Feature lead summary on 106-e-LTE-6CRs-02**

**Document for: Discussion and Decision**

# Introduction

This documents provides the summary of discussions on the corresponding email discussion, regarding the proposed CR in [1].

[106-e-LTE-6CRs-02] Email discussion/approval on Correction on cyclic shift for eMTC PUR ([R1-2107688](file:///C:\Users\Docs\R1-2107688.zip)) – Yubo (Huawei)

* Issue 3: Correction on cyclic shift for eMTC PUR
* Discussion and decision by August 18, CR by August 20, final check by August 24

# Discussion

In [1], a correction on cyclic shift for eMTC PUR is proposed due to the following reason:

|  |  |
| --- | --- |
| ***Reason for change:*** | The parameter *pusch-CyclicShift* in higher layer parameter *PUR-PUSCH-Config* is intended to be used in PUSCH corresponding to preconfigured uplink resource. However, in the current spec, it is not limited to PUR PUSCH. |
|  |  |
| ***Summary of change:*** | It is clarified that the parameter *pusch-CyclicShift* in higher layer parameter *PUR-PUSCH-Config* is for PUSCH corresponding to preconfigured uplink resource. |
|  |  |
| ***Consequences if not approved:*** | The parameter *pusch-CyclicShift* in higher layer parameter *PUR-PUSCH-Config* will also be used in non-PUR PUSCH mistakenly, such as msg3 etc. |

The proposed change is as following:

=======================Change to TS 36.211=====================================

**<Unchanged parts are omitted>**

5.5.2.1.1 Reference signal sequence

**<Unchanged parts are omitted>**

The cyclic shift  in a slot  is given as if the ul-V-SPS-RNTI-r14 was used to transmit the most recent uplink-related DCI for the transport block associated with the corresponding PUSCH transmission. For PUSCH transmissions not using sub-PRB allocations, if *pusch-CyclicShift* in higher layer parameter *PUR-PUSCH-Config* is configured it provides the value of and the cyclic shift  in a slot  is given as for PUSCH (re)transmission corresponding to preconfigured uplink resource.

**<Unchanged parts are omitted>**

======================End of change to TS 36.211=================================

Please input your comment on the motivation and CR above:

|  |  |
| --- | --- |
| Companies | Comments |
| Ericsson | If this CR is to be agreed for clarification purposes, we suggest using the same wording order we agreed for a similar issue (i.e., R1-2106196) in RAN1# 105-e, that is:   |  | | --- | | **<Unchanged parts are omitted>**  5.5.2.1.1 Reference signal sequence  **<Unchanged parts are omitted>**  The cyclic shift  in a slot  is given as if the ul-V-SPS-RNTI-r14 was used to transmit the most recent uplink-related DCI for the transport block associated with the corresponding PUSCH transmission. For PUSCH transmissions not using sub-PRB allocations, if *pusch-CyclicShift* in higher layer parameter *PUR-PUSCH-Config* is configured for PUSCH (re)transmission corresponding to preconfigured uplink resource it provides the value of , and the cyclic shift  in a slot  is given as .  **<Unchanged parts are omitted>** |   Moreover, in the revision above a “comma” was added after “”. Otherwise, it seems to say that the higher layer parameter provides both “” and “”, however in my understanding it only provides “” as to calculate “”. |
|  |  |
|  |  |

# Summary

# References

1. R1-2107688 Correction on cyclic shift for eMTC PUR Huawei, HiSilicon