3GPP TSG-RAN WG1 Meeting #106-e R1-21xxxxx

e-Meeting, August 16th – 27th, 2021

Agenda Item: 6

Source: Moderator (Ericsson)

Title: Moderator Summary [106-e-LTE-6CRs-03]

Document for: Discussion and Decision

# 1 Introduction

In [1], it was mentioned that “the higher layer parameter “*operationModeInfo*” has been solely used in some clauses of TS 36.213 [2], letting aside the non-anchor carrier” case.

In relation with the above, the following e-mail discussion has been granted:

|  |
| --- |
| [106-e-LTE-6CRs-03] Email discussion/approval on Deployment Mode Indicator for anchor and non-anchor carriers ([R1-2108120](file:///D%3A%5CDocuments%5C3GPP%20documents%5CRAN1%5CTSGR1_106-e%5CDocs%5CR1-2108120.zip)) – Gerardo (Ericsson)Issue 4: Deployment Mode Indicator for anchor and non-anchor carriersDiscussion and decision by 8/18, CR by 8/20, final check by 8/24 |

# 2 Background

In [1], the following was mentioned:

“In Release-13, the higher layer parameter “*operationModeInfo*” was introduced [TS 36.331]:

|  |
| --- |
| ***operationModeInfo***Deployment scenario (in-band/guard-band/standalone) and related information. See TS 36.211 [21] and TS 36.213 [23].*Inband-SamePCI* indicates an in-band deployment and that the NB-IoT and LTE cell share the same physical cell id and have the same number of NRS and CRS ports.*Inband-DifferentPCI* indicates an in-band deployment and that the NB-IoT and LTE cell have different physical cell id.*guardband* indicatesa guard-band deployment.*standalone* indicates a standalone deployment. |

On the other hand, in Release-13 the higher layer parameter “*inbandCarrierInfo*” was also introduced [TS 36.331]:

|  |
| --- |
| ***inbandCarrierInfo***Provides the configuration of a non-anchor inband carrier. |

One issue that has been recently identified is that the higher layer parameter “*operationModeInfo*” has been solely used in some clauses of TS 36.213, letting aside the non-anchor carrier.”

The document in [1] identifies “clauses of TS 36.213 where the non-anchor carrier case covered by the higher layer parameter “*inbandCarrierInfo*” has been missed”.

The sections below contain the following information based on [1].

* Section 2.1: Lists four Rel-13 clauses missing the higher layer parameter “*inbandCarrierInfo*”. The fix on the identified clauses will require a Rel-13 CR, and their corresponding Rel-14, Rel-15, and Rel-16 mirror CRs.
* Section 2.2: Lists two clauses that only refer to the higher parameter “*operationModeInfo*”, for which the higher layer parameter “*inbandCarrierInfo*” does not need to be added.

## 2.1 Listing of clauses missing the higher layer parameter “*inbandCarrierInfo*”

### 2.1.1 Rel-13: TS 36.213, clause 16.2.2: Downlink Power Allocation

|  |
| --- |
| ------------------------------------------------------- Text Start -----------------------------------------------------------16.2.2 Downlink power allocationThe eNodeB determines the downlink transmit energy per resource element.For an NB-IoT cell, the UE may assume NRS EPRE is constant across the downlink NB-IoT system bandwidth and constant across all subframes that contain NRS, until different NRS power information is received. The downlink NRS EPRE can be derived from the downlink narrowband reference-signal transmit power given by *nrs-Power* + *nrs-PowerOffsetNonAnchor,* where the parameter *nrs-Power* is provided by higher layers and *nrs-powerOffsetNonAnchor* is zero if it is not provided by higher layers. The downlink narrowband reference-signal transmit power is defined as the linear average over the power contributions (in [W]) of all resource elements that carry narrowband reference signals within the operating NB-IoT system bandwidth.A UE may assume the ratio of NPDSCH EPRE to NRS EPRE among NPDSCH REs (not applicable to NPDSCH REs with zero EPRE) is 0 dB for an NB-IoT cell with one NRS antenna port and -3 dB for an NB-IoT cell with two NRS antenna ports.A UE may assume the ratio of NPBCH EPRE to NRS EPRE among NPBCH REs (not applicable to NPBCH REs with zero EPRE) is 0 dB for an NB-IoT cell with one NRS antenna port and -3 dB for an NB-IoT cell with two NRS antenna ports.A UE may assume the ratio of NPDCCH EPRE to NRS EPRE among NPDCCH REs (not applicable to NPDCCH REs with zero EPRE) is 0 dB for an NB-IoT cell with one NRS antenna port and -3 dB for an NB-IoT cell with two NRS antenna ports.If higher layer parameter *operationModeInfo* indicates '00', and when the higher layer parameter *inbandCarrierInfo* is present for a cell, the ratio of NRS EPRE to CRS EPRE is given by the parameter *nrs-CRS-PowerOffset* if the parameter *nrs-CRS-PowerOffset* is provided by higher layers, and the ratio of NRS EPRE to CRS EPRE may be assumed to be 0 dB if the parameter *nrs-CRS-PowerOffset* is not provided by higher layers. If *nrs-CRS-PowerOffset* is provided by higher layers and is a non-integer value, the value of *nrs-Power* is 0.23 dBm higher than indicated.------------------------------------------------------- Text End ------------------------------------------------------------ |

|  |  |  |
| --- | --- | --- |
| **Company** | **OK with incorporating *inbandCarrierInfo* in TS 36.213 clause 16.2.2?** | **Comments** |
|  |  |  |

### 2.1.2 Rel-13: TS 36.213, clause 16.4.1.4 NPDSCH starting position

|  |
| --- |
| -------------------------------------------------- Text Start -----------------------------------------------------16.4.1.4 NPDSCH starting positionThe starting OFDM symbol for NPDSCH is given by index  in the first slot in a subframe  and is determined as follows- if subframe  is a subframe used for receiving SIB1-NB- if the value of the higher layer parameter *operationModeInfo* is set to '00' or '01', and when the higher layer parameter *inbandCarrierInfo* is present- otherwise- else- is given by the higher layer parameter *eutraControlRegionSize* if the value of the higher layer parameter *eutraControlRegionSize* is present- otherwise------------------------------------------------------- Text End ------------------------------------------------------------ |

|  |  |  |
| --- | --- | --- |
| **Company** | **OK with incorporating *inbandCarrierInfo* in TS 36.213 clause 16.4.1.4?** | **Comments** |
|  |  |  |

### 2.1.3 Rel-13: TS 36.213, clause 16.4.1.5.1 Transport blocks not mapped for *SystemInformationBlockType1-NB*

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| -------------------------------------------------- Text Start -----------------------------------------------------16.4.1.5.1 Transport blocks not mapped for *SystemInformationBlockType1-NB*The TBS is given by the (,) entry of Table 16.4.1.5.1-1. For the value of the higher layer parameter *operationModeInfo* set to '00' or '01', and when the higher layer parameter *inbandCarrierInfo* is present, .**Table 16.4.1.5.1-1: Transport block size (TBS) table.**

|  |  |
| --- | --- |
|  |  |
| **0** | **1** | **2** | **3** | **4** | **5** | **6** | **7** |
| 0 | 16 | 32 | 56 | 88 | 120 | 152 | 208 | 256 |
| 1 | 24 | 56 | 88 | 144 | 176 | 208 | 256 | 344 |
| 2 | 32 | 72 | 144 | 176 | 208 | 256 | 328 | 424 |
| 3 | 40 | 104 | 176 | 208 | 256 | 328 | 440 | 568 |
| 4 | 56 | 120 | 208 | 256 | 328 | 408 | 552 | 680 |
| 5 | 72 | 144 | 224 | 328 | 424 | 504 | 680 |  |
| 6 | 88 | 176 | 256 | 392 | 504 | 600 |  |  |
| 7 | 104 | 224 | 328 | 472 | 584 | 680 |  |  |
| 8 | 120 | 256 | 392 | 536 | 680 |  |  |  |
| 9 | 136 | 296 | 456 | 616 |  |  |  |  |
| 10 | 144 | 328 | 504 | 680 |  |  |  |  |
| 11 | 176 | 376 | 584 |  |  |  |  |  |
| 12 | 208 | 440 | 680 |  |  |  |  |  |

-------------------------------------------------------- Text end ----------------------------------------------------------- |

|  |  |  |
| --- | --- | --- |
| **Company** | **OK with incorporating *inbandCarrierInfo* in TS 36.213 clause 16.4.1.5.1?** | **Comments** |
|  |  |  |

### 2.1.4 Rel-13: TS 36.213, clause 16.8 UE procedure for acquiring cell-specific reference signal sequence and raster offset

|  |
| --- |
| -------------------------------------------------- Text Start -----------------------------------------------------16.8 UE procedure for acquiring cell-specific reference signal sequence and raster offsetIf the higher layer parameter *operationModeInfo* indicates *inband-SamePCI*, and when the higher layer parameter *inbandCarrierInfo* is present for a cell, the UE may derive cell-specific reference signal sequence and raster offset from the higher layer parameter *eutra-CRS-SequenceInfo* according to Table 16.8-1, where E-UTRA PRB index  is defined as .-------------------------------------------------------- Text end ----------------------------------------------------------- |

|  |  |  |
| --- | --- | --- |
| **Company** | **OK with incorporating *inbandCarrierInfo* in TS 36.213 clause 16.8?** | **Comments** |
|  |  |  |

## 2.2 Listing of unaffected clauses by not including the higher layer parameter “*inbandCarrierInfo*”

### 2.2.1 Rel-13: TS 36.213, clause 16.1.1: Cell search

According with [1], for clause 16.1.1, the cell search does not need a change to include the higher layer parameter “*inbandCarrierInfo*” as the cell search is only used on the anchor carrier. Thus, the use of the higher layer parameter “*operationModeInfo*” in clause 16.1.1 is sufficient.

|  |
| --- |
| 16.1.1 Cell searchCell search is the procedure by which a UE acquires time and frequency synchronization with a cell and detects the narrowband physical layer Cell ID. If the higher layer parameter *operationModeInfo* indicates '*inband-SamePCI*' or *samePCI-Indicator* indicates '*samePCI*'' for a cell, the UE may assume that the physical layer cell ID is same as the narrowband physical layer cell ID for the cell.The following signals are transmitted in the downlink to facilitate cell search for Narrowband IoT: the narrowband primary and narrowband secondary synchronization signals. A UE may assume the antenna ports 2000 – 2001 and the antenna port for the narrowband primary/secondary synchronization signals of a serving cell are quasi co-located (as defined in [3]) with respect to Doppler shift and average delay. |

|  |  |  |
| --- | --- | --- |
| **Company** | **OK with no incorporating *inbandCarrierInfo* in TS 36.213 clause 16.1.1?** | **Comments** |
|  |  |  |

### 2.2.1 Rel-14: TS 36.213, clause 16.4: Narrowband physical downlink shared channel related procedures

According with [1], for clause 16.4 introduced in Rel-14 [3], the higher layer parameter “*inbandCarrierInfo*” would need to be added if the third bullet in clause 16.4 were not present. Nonetheless, the higher layer parameter “*downlinkBitmapNonAnchor*” is not an optional field (i.e., it will always be present) which covers the non-anchor carrier case making the inclusion of the higher layer parameter “*inbandCarrierInfo*” in the second bullet of clause 16.4 unnecessary.

|  |
| --- |
| 16.4 Narrowband physical downlink shared channel related proceduresA NB-IoT UE shall assume a subframe as a NB-IoT DL subframe if- the UE determines that the subframe does not contain NPSS/NSSS/NPBCH/ *SystemInformationBlockType1-NB* transmission, and- for a NB-IoT carrier that a UE receives higher layer parameter *operationModeInfo,* the subframe is configured as NB-IoT DL subframe after the UE has obtained *SystemInformationBlockType1-NB*. - the subframe is configured as NB-IoT DL subframe by the higher layer parameter *downlinkBitmapNonAnchor*.For a NB-IoT UE that supports *twoHARQ-Processes-r14*, there shall be a maximum of 2 downlink HARQ processes. |

|  |  |  |
| --- | --- | --- |
| **Company** | **OK with no incorporating *inbandCarrierInfo* in TS 36.213 clause 16.4?** | **Comments** |
|  |  |  |

# 5 References

1. [R1-2108120](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_106-e/Docs/R1-2108120.zip), “Deployment Mode Indicator for anchor and non-anchor carriers,” Ericsson, e-Meeting, August 16th – 27th, 2021.
2. [TS 36.213](https://www.3gpp.org/ftp/Specs/archive/36_series/36.213/36213-eg0.zip), Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures, v13.16.0.
3. [TS 36.213](https://www.3gpp.org/ftp/Specs/archive/36_series/36.213/36213-eg0.zip), Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures, v14.16.0.