**3GPP TSG RAN WG1 Meeting #106-e R1-210xxxx**

**e-Meeting, August 16th – 27th, 2021**

**Source: Moderator (ZTE)**

**Title: Email Discussion Summary of [106-e-NR-7.1CRs-03]**

**Agenda item: 7.1**

**Document for:** **Discussion/Decision**

# Introduction

During RAN1#106-e, three contributions were submitted to discuss and clarify the ambiguity issue for accumulated closed loop power control for BWP switching [1-3]. During the preparation phase, companies agreed to discuss this issue in RAN1#106-e meeting.

|  |
| --- |
| [106-e-NR-7.1CRs-03] Issue#5: Draft CR on accumulated closed loop power control for BWP switching by August 20 – Bo (ZTE)[R1-2106536](file:///D%3A%5CDocuments%5C3GPP%20documents%5CRAN1%5CTSGR1_106-e%5CDocs%5CR1-2106536.zip) Discussion on accumulated closed loop power control for BWP switching ZTE[R1-2106537](file:///D%3A%5CDocuments%5C3GPP%20documents%5CRAN1%5CTSGR1_106-e%5CDocs%5CR1-2106537.zip) Draft CR on accumulated closed loop power control for BWP switching ZTE[R1-2107503](file:///D%3A%5CDocuments%5C3GPP%20documents%5CRAN1%5CTSGR1_106-e%5CDocs%5CR1-2107503.zip) Draft 38.213 CR on PUSCH/PUCCH power control adjustment state during UL BWP change MediaTek Inc. |

This summary is trying to collect/summarize companies’ input and draw potential TP based on companies’ input.

# Discussion

## Background introduction

In current NR spec [4], power control parameters, such as parameters for open loop power control (e.g. P0, alpha), for closed loop power control (e.g. number of closed loop power control loops), and for path loss (e.g. PL-RS, i.e. DL RS for path-loss measurement), are configured per BWP *b* per carrier *f* per cell *c*. However, it is not clear for the UE behavior on how to handle accumulated closed loop value in the new active BWP in the case of UL BWP change.

***Observation****: From spec perspective, there is no clear UE behavior on handling accumulated closed loop value in the case of UL BWP change.*

Furthermore, when reviewing the already RAN1 agreement, it can be observed that in RAN1 #90-bis, it is agreed that up to 2 closed-loop power control processes is maintained for PUSCH:

Agreement: For N closed-loop power control processes, i.e., fc(i,l), for NR PUSCH power control for serving cell c, the following working assumption is confirmed:

* **N is up to 2**

In RAN1 #90-bis, it is also agreed as a working assumption that up to 2 closed-loop power control processes is maintained for PUCCH:

Working Assumption:

* Support *P*cmax,c(*i*), *P*0\_PUCCH(*F*), *PL*c(*k*), g(*i*) for NR PUCCH power control in slot *i* for serving cell *c*.
* **Support up to 2 closed-loop power control processes, i.e., *l***

It means that configuring each UL BWP with up to two independent power control adjustment states is NOT aligned with the agreements in RAN1#90-bis (i.e., up to 2 for PUSCH, and up to 2 for PUCCH, per serving cell).

For sake of presentation, in both [1] and [3], some examples are raised for clarifying the difference between “per BWP power state control” and “per cell power state control”. One example in [3] is copied as follows. It can be observed that “per cell power state control” offers benefits for Tx power continuity over “per BWP power state control” when UL BWP changes. Some more details can be found in companion contributions [1], [2] and [3].



**Figure 1** Illustrative example of “per BWP power state control” v.s. “per cell power state control”

## Companies’ input

According to the input from contributions [1-3], clarifying the UE behavior on how to handle accumulated closed loop power control value in the new active BWP when active BWP changes becomes essential and necessary. In such case, the ‘per cell power state control’ is aligned with already agreement, and is beneficial for transmit power continuity.

* Specifically, for each closed loop *l*, when BWP changes, the accumulated closed loop value for the new BWP should be reset or re-determined according to the accumulated closed loop value from the previous BWP.

For moving forward this issue, we will try to reach consensus/agreement between companies firstly; after that, the draft TP based on the consensus/agreement will be discussed accordingly.

Based on above, the following proposal is provided.

***Proposal:*** *For each accumulated closed loop l in a serving cell/uplink, UE shall use the same PUSCH/PUCCH/SRS power control adjustment state (i.e.,*//*) before and after UL BWP changes.*

* *Note that the UE is not expected to maintain more than two PUSCH/PUCCH power control adjustment states and more than one independent SRS power control adjustment state (i.e., not tied to PUSCH closed loop) per serving cell/uplink.*

Please provide company’s view in the table below.

|  |  |
| --- | --- |
| Company | Comment |
| Futurewei | We do not support this. Our view is that the power control state should be reset to zero after BWP switch since other power control parameters and PL-RS can be all different now. Note that by resetting to zero, the UE only maintains up to 2 close loop power control states for the active BWP. |
| Apple | Support the proposal. There was no agreement that BWP switching would have any impact on CL-PC state. So UE should still maintain the CL-PC state.  |

If supporting the above proposal, please provide company’s views on two candidate CRs in [2] (R1-2106537) and [3] (R1-2107503) as in the appendix (e.g., which one is preferred, or suggestions on drafting CR); otherwise, please provide the recommended spec change.

|  |  |
| --- | --- |
| Company | Comment |
| Futurewei | This can be discussed later after the first issue is concluded.  |
| Apple | Support R1-2106537 |

# Summary

The following potential TP is updated based on the companies’ input.

**Draft TP**

# Reference

[1] R1-2106536, Discussion on accumulated closed loop power control for BWP switching, ZTE

[2] R1-2106537, Draft CR on accumulated closed loop power control for BWP switching, ZTE

[3] R1-2107503, Draft 38.213 CR on PUSCH/PUCCH power control adjustment state during UL BWP change, MediaTek Inc.

[4] 3GPP TS 38.213-fe0, NR Physical layer procedures for control

# Appendix

## Candidate TP#1 in R1-2106537

In [2] (R1-2106537), the following candidate TP is provided for PUSCH/PUCCH/SRS:

|  |
| --- |
| 7.1.1 UE behaviour<Unchanged part omitted>-  is the PUSCH power control adjustment state  for active UL BWP  of carrier  of serving cell  and PUSCH transmission occasion  if the UE is not provided *tpc-Accumulation*, where - The  values are given in Table 7.1.1-1-  is a sum of TPC command values in a set  of TPC command values with cardinality  that the UE receives between  symbols before PUSCH transmission occasion  and  symbols before PUSCH transmission occasion  on active UL BWP  of carrier  of serving cell  for PUSCH power control adjustment state , where  is the smallest integer for which  symbols before PUSCH transmission occasion  is earlier than  symbols before PUSCH transmission occasion - If a PUSCH transmission is scheduled by a DCI format 0\_0 or DCI format 0\_1,  is a number of symbols for active UL BWP  of carrier  of serving cell  after a last symbol of a corresponding PDCCH reception and before a first symbol of the PUSCH transmission - If a PUSCH transmission is configured by *ConfiguredGrantConfig*,  is a number of  symbols equal to the product of a number of symbols per slot, , and the minimum of the values provided by *k2* in *PUSCH-ConfigCommon* for active UL BWP  of carrier  of serving cell  - If the UE has reached maximum power for active UL BWP of carrier  of serving cell  at PUSCH transmission occasion  and , then - If UE has reached minimum power for active UL BWP of carrier  of serving cell  at PUSCH transmission occasion  and , then - For the first PUSCH transmission occasion after an active UL BWP changes, a power control adjustment state is determined by a latest PUSCH power control adjustment state from the previous BWP.- A UE resets accumulation of a PUSCH power control adjustment state  for active UL BWP  of carrier  of serving cell  to - If a configuration for a corresponding  value is provided by higher layers- If a configuration for a corresponding  value is provided by higher layerswhere  is determined from the value of  as - If  and the UE is provided higher *SRI-PUSCH-PowerControl*,  is the *sri-PUSCH-ClosedLoopIndex* value(s) configured in any *SRI-PUSCH-PowerControl* with the *sri-P0-PUSCH-AlphaSetId* value corresponding to  - If  and the UE is not provided *SRI-PUSCH-PowerControl* or , - If ,  is provided by the value of *powerControlLoopToUse*<Unchanged part omitted>7.2.1 UE behaviour<Unchanged part omitted>-  is the current PUCCH power control adjustment state  for active UL BWP  of carrier  of serving cell  and PUCCH transmission occasion , where - The  values are given in Table 7.1.2-1-  is a sum of TPC command values in a set  of TPC command values with cardinality  that the UE receives between  symbols before PUCCH transmission occasion  and  symbols before PUCCH transmission occasion  on active UL BWP  of carrier  of serving cell  for PUCCH power control adjustment state, where  is the smallest integer for which  symbols before PUCCH transmission occasion  is earlier than  symbols before PUCCH transmission occasion - If the PUCCH transmission is in response to a detection by the UE of a DCI format 1\_0 or DCI format 1\_1,  is a number of symbols for active UL BWP  of carrier  of serving cell  after a last symbol of a corresponding PDCCH reception and before a first symbol of the PUCCH transmission- If the PUCCH transmission is not in response to a detection by the UE of a DCI format 1\_0 or DCI format 1\_1,  is a number of  symbols equal to the product of a number of symbols per slot, , and the minimum of the values provided by *k2* in *PUSCH-ConfigCommon* for active UL BWP  of carrier  of serving cell - If the UE has reached maximum power for active UL BWP  of carrier  of primary cell  at PUCCH transmission occasion  and , then - If UE has reached minimum power for active UL BWP  of carrier  of primary cell  at PUCCH transmission occasion  and , then  - For the first PUCCH transmission occasion after an active UL BWP changes, a power control adjustment state is determined by a latest PUCCH power control adjustment state from the previous BWP.- If a configuration of a  value for a corresponding PUCCH power control adjustment state  for active UL BWP  of carrier  of serving cell  is provided by higher layers, -  If the UE is provided *PUCCH-SpatialRelationInfo*, the UE determines the value of  from the value of  based on a *pucch-SpatialRelationInfoId* value associated with the *p0-PUCCH-Id* value corresponding to  and with the *closedLoopIndex* value corresponding to ; otherwise, - Else, - , where , and  is the TPC command value indicated in a random access response grant corresponding to a PRACH transmission or is the TPC command value in a DCI format with CRC scrambled by C-RNTI or MCS-C-RNTI that the UE detects in a first PDCCH reception in a search space set provided by *recoverySearchSpaceId* if the PUCCH transmission is a first PUCCH transmission after 28 symbols from a last symbol of the first PDCCH reception, and, if the UE transmits PUCCH on active UL BWP  of carrier  of serving cell , ; otherwise,  where  is provided by higher layers and corresponds to the total power ramp-up requested by higher layers from the first to the last preamble for active UL BWP  of carrier  of primary cell , and  corresponds to PUCCH format 0 or PUCCH format 1<Unchanged part omitted>7.3.1 UE behaviour<Unchanged part omitted>-  if the UE is not configured for PUSCH transmissions on active UL BWP  of carrier  of serving cell , or if *srs-PowerControlAdjustmentStates* indicates separate power control adjustment states between SRS transmissions and PUSCH transmissions, and if *tpc-Accumulation* is not provided, where - The  values are given in Table 7.1.1-1-  is jointly coded with other TPC commands in a PDCCH with DCI format 2\_3, as described in Clause 11.4-  is a sum of TPC command values in a set  of TPC command values with cardinality  that the UE receives between  symbols before SRS transmission occasion  and  symbols before SRS transmission occasion  on active UL BWP  of carrier  of serving cell  for SRS power control adjustment state, where  is the smallest integer for which  symbols before SRS transmission occasion  is earlier than  symbols before SRS transmission occasion - if the SRS transmission is aperiodic,  is a number of symbols for active UL BWP  of carrier  of serving cell  after a last symbol of a corresponding PDCCH triggering the SRS transmission and before a first symbol of the SRS transmission - if the SRS transmission is semi-persistent or periodic,  is a number of  symbols equal to the product of a number of symbols per slot, , and the minimum of the values provided by *k2* in *PUSCH-ConfigCommon* for active UL BWP  of carrier  of serving cell  - If the UE has reached maximum power for active UL BWP  of carrier  of serving cell  at SRS transmission occasion  and , then - If UE has reached minimum power for active UL BWP  of carrier  of serving cell  at SRS transmission occasion  and , then - For the first SRS transmission occasion after an active UL BWP changes, a power control adjustment state is determined by a latest SRS power control adjustment state from the previous BWP.- If a configuration for a  value or for a  value for a corresponding SRS power control adjustment state  for active UL BWP  of carrier  of serving cell  is provided by higher layers-  - Else-  where is the TPC command value indicated in the random access response grant corresponding to the random access preamble that the UE transmitted on active UL BWP  of carrier  of the serving cell , and ; where  is provided by higher layers and corresponds to the total power ramp-up requested by higher layers from the first to the last preamble for active UL BWP  of carrier  of serving cell .<Unchanged part omitted> |

## Candidate TP#2 in R1-2107503

In [3] (R1-2107503), the following candidate TP is provided for PUSCH/PUCCH:

|  |
| --- |
| 7.1.1 UE behaviour<Unchanged parts are omitted>For the PUSCH power control adjustment state  for active UL BWP  of carrier  of serving cell  in PUSCH transmission occasion -  is a TPC command value included in a DCI format 0\_0 or DCI format 0\_1 that schedules the PUSCH transmission occasion  on active UL BWP  of carrier  of serving cell  or jointly coded with other TPC commands in a DCI format 2\_2 with CRC scrambled by TPC-PUSCH-RNTI, as described in Clause 11.3-  if the UE is configured with *twoPUSCH-PC-AdjustmentStates* and  if the UE is not configured with *twoPUSCH-PC-AdjustmentStates* or if the PUSCH transmission is scheduled by a RAR UL grant as described in Clause 8.3- For each, UE uses the same PUSCH power control adjustment state  before and after UL BWP change. A UE is not expected to maintain more than two PUSCH power control adjustment states per serving cell<Unchanged parts are omitted>7.2.1 UE behaviour<Unchanged parts are omitted>For the PUCCH power control adjustment state  for active UL BWP  of carrier  of primary cell  and PUCCH transmission occasion -  is a TPC command value and is included in a DCI format 1\_0 or DCI format 1\_1 for active UL BWP  of carrier  of the primary cell  that the UE detects for PUCCH transmission occasion  or is jointly coded with other TPC commands in a DCI format 2\_2 with CRC scrambled by TPC-PUCCH-RNTI [5, TS 38.212], as described in Clause 11.3-  if the UE is provided *twoPUCCH-PC-AdjustmentStates* and *PUCCH-SpatialRelationInfo* and  if the UE is not provided *twoPUCCH-PC-AdjustmentStates* or *PUCCH-SpatialRelationInfo*- For each, UE uses the same PUCCH power control adjustment state  before and after UL BWP change. A UE is not expected to maintain more than two PUCCH power control adjustment states per serving cell<Unchanged parts are omitted> |