**3GPP TSG RAN WG1 #106-e R1- 210xxxxx**

**e-Meeting, August 16th – 27th, 2021**

**Source: Moderator (vivo)**

**Title: Summary of [106-e-NR-5G\_V2X-05] Discussion on R1-2107979: Clarification on PUCCH Power control when the number of SL HARQ-ACK bits larger than 11**

**Agenda Item: 7.2.4**

**Document for: Discussion and Decision**

**Introduction**

The document is to collect companies’ inputs and provide a summary for the email discussion thread [106-e-NR-5G\_V2X-05] Discussion on [R1-2107979](../../Docs/R1-2107979.zip): Clarification on PUCCH Power control when the number of SL HARQ-ACK bits larger than 11 by August 20 – Siqi (vivo)

The 1st point is planned as following, companies are highly appreciated to provide their inputs before this check point:

* **1st check point: August 17, UTC 23:59 pm**

The 2nd check point: [TBD]

**Discussion**

## Issue#1 PUCCH power when there are more than 11 SL HARQ-ACK bits

The transmission power of PUCCH on active UL BWP  of carrier  of primary cell  is determined based on the following formula, where  is a PUCCH transmission power adjustment component which is depended on the PUCCH format as well as the number of UCI bits to be transmitted:

 [dBm]

|  |
| --- |
| 7.2.1 UE behaviour- For a PUCCH transmission using PUCCH format 2 or PUCCH format 3 or PUCCH format 4 and for a number of UCI bits larger than 11, , where - - -  is a number of HARQ-ACK information bits that the UE determines as described in clause 9.1.2.1 for Type-1 HARQ-ACK codebook and as described in clause 9.1.3.1 or 9.1.3.3 for Type-2 HARQ-ACK codebook, or as described in clause 9.1.4 for Type-3 HARQ-ACK codebook. If the UE is not provided any of *pdsch-HARQ-ACK-Codebook*, *pdsch-HARQ-ACK-Codebook-r16*, or *pdsch-HARQ-ACK-OneShotFeedback*,  if the UE includes a HARQ-ACK information bit in the PUCCH transmission; otherwise, -  is a number of SR information bits that the UE determines as described in clause 9.2.5.1-  is a number of CSI information bits that the UE determines as described in clause 9.2.5.2  |

If a PUCCH format2/3/4 is used for SL HARQ-ACK reporting and the number of SL HARQ-ACK bits is larger than 11, the current spec is not clear on how to determine the  for PUCCH power control **as in the current spec the  is defined as the number of HARQ-ACK bits generated for PDSCH** as described in clause 9.1.2.1 for Type-1 HARQ-ACK codebook or as described in clause 9.1.3.1 or 9.1.3.3 for Type-2 HARQ-ACK codebook, or as described in clause 9.1.4 for Type-3 HARQ-ACK codebook. It also seems to imply that SR, CSI should be considered for .

Thus, the UE behavior in the case of reporting more than 11 SL HARQ-ACK bits should be clarified, i.e.,  and  should be set to 0 since multiplexing between SL HARQ-ACK and CSI/SR in a PUCCH is not allowed, and  should be set to the number of the SL HARQ-ACK bits determined in Clause 16.5.1 for type1 codebook or Clause 16.5.2 for type2 codebook.

In [1], following changes are proposed:

***================proposed changes in [1] ===================***

|  |
| --- |
| 16.5.1.1 Type-1 HARQ-ACK codebook in physical uplink control channel====omitted====If , the UE determines a number of HARQ-ACK information bits for obtaining a transmission power for a PUCCH, as described in clause 7.2.1, as where is a number of HARQ-ACK information bits determined for corresponding PSSCH transmissions with corresponding PSFCH reception occasions in PSFCH reception occasion .If , and if the PUCCH transmission uses PUCCH format 2 or PUCCH format 3 or PUCCH format 4, the UE determines a transmission power for the PUCCH, as described in Clause 7.2.1, except that -  =.- =0- =0====omitted==== |

|  |
| --- |
| 16.5.2.1 Type-2 HARQ-ACK codebook in physical uplink control channel====omitted====If , the UE determines a number of HARQ-ACK information bits for obtaining a transmission power for a PUCCH, as described in clause 7.2.1, as where - is a value of a counter SAI field in a last DCI format 3\_0 scheduling PSSCH transmissions associated with PSFCH reception occasions that the UE detects within the PDCCH monitoring occasions- if the UE does not detect any DCI format 3\_0 scheduling PSSCH transmissions associated with PSFCH reception occasions in any of the PDCCH monitoring occasions- is a total number of DCI format 3\_0, scheduling PSSCH transmissions associated with PSFCH reception occasions, that the UE detects within the PDCCH monitoring occasions. if the UE does not detect any DCI format 3\_0 scheduling PSSCH transmissions with associated PSFCH reception occasions in any of the PDCCH monitoring occasions- is a number of DCI format 3\_0 scheduling PSSCH transmissions with associated PSFCH reception occasions that the UE detects in PDCCH monitoring occasion - is a number of SL configured grants for which the UE transmits corresponding HARQ-ACK information in a same PUCCH as for HARQ-ACK information corresponding to PSFCH reception occasions within the PDCCH monitoring occasionsIf , and if the PUCCH transmission uses PUCCH format 2 or PUCCH format 3 or PUCCH format 4, the UE determines a transmission power for the PUCCH, as described in Clause 7.2.1, except that -  =.- =0- =0====omitted==== |

## Company views

Please kindly provide your views in the table below.

**Question 1: Do you agree that issue#1 should be addressed(i.e., power control for PUCCH with more than 11 SL HARQ-ACK bits should be specified)?**

* **If no, please provide the reasons and your suggestions, if any.**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not |  Comment |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2: Do you agree with the proposed changes for issue#1?**

* **If no, please provide the reasons and your suggestions, if any.**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not |  Comment |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary**

[Based on the discussion, we conclude that ……TBD]

**Reference**

1. R1-2107979, Clarification on PUCCH Power control when the number of SL HARQ-ACK bits larger than 11, vivo