**3GPP TSG RAN WG1 #106-e R1-210xxxxx**

**e-Meeting, August 16th – 27th, 2021**

**Source: Moderator (Ericsson)**

**Title: Summary of Discussion on R1-2108140:** **[Draft] Correction on synchronization procedure for sidelink transmission**

**Agenda Item: 7.2.4**

**Document for: Discussion and Decision**

# Introduction

This document provides a summary of the discussion on a draft CR [1] regarding corrections on the synchronization procedure for sidelink transmissions and collects the companies’ views on whether the draft CR should be included in the specification.

The discussion for this CR can be found in the following email thread: [106-e-NR-5G\_V2X-07] Discussion on R1-2108140: [Draft] Correction on synchronization procedure for sidelink transmission by August 18 - Jose (Ericsson)

# Summary of the discussion on R1-2108140

The following CR is proposed in [1] to correct the synchronization procedure for sidelink in order to also include the scenario when no serving cell is available. The reason for this change is that without this correction the synchronization procedure will not work when there is no serving cell. The proposed text change is the following:

## 16.1 Synchronization procedures

A UE receives the following SL synchronization signals in order to perform synchronization procedures based on S-SS/PSBCH blocks: SL primary synchronization signals (S-PSS) and SL secondary synchronization signals (S-SSS) [4, TS 38.211].

A UE assumes that reception occasions of a physical sidelink broadcast channel (PSBCH), S-PSS, and S-SSS are in consecutive symbols [4, TS 38.211] and form a S-SS/PSBCH block.

For reception of a S-SS/PSBCH block, a UE assumes a frequency location corresponding to the subcarrier with index 66 in the S-SS/PSBCH block [4, TS 38.211], is provided by *sl-AbsoluteFrequencySSB*. The UE assumes that a S-PSS symbol, a S-SSS symbol, and a PSBCH symbol have a same transmission power. The UE assumes a same numerology of the S-SS/PSBCH as for a SL BWP of the S-SS/PSBCH block reception, and that a bandwidth of the S-SS/PSBCH is within a bandwidth of the SL BWP. The UE assumes the subcarrier with index 0 in the S-SS/PSBCH block is aligned with a subcarrier with index 0 in an RB of the SL BWP.

A UE is provided, by *sl-NumSSB-WithinPeriod*, a number of S-SS/PSBCH blocks in a period of 16 frames. The UE assumes that a transmission of the S-SS/PSBCH blocks in the period is with a periodicity of 16 frames. The UE determines indexes of slots that include S-SS/PSBCH block as +, where

- index 0 corresponds to a first slot in a frame with SFN of the serving cell satisfying or DFN satisfying (DFN mod 16) = 0

- is a S-SS/PSBCH block index within the number of S-SS/PSBCH blocks in the period, with

- is a slot offset from a start of the period to the first slot including S-SS/PSBCH block, provided by *sl-TimeOffsetSSB*

- is a slot interval between S-SS/PSBCH blocks, provided by *sl-timeInterval*

**<Unchanged parts omitted>**

## 2.1 Company views

**Q1: Do you agree with the issue identified in R1-2108140?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Reply (Yes/No)** | **Comments** |
| OPPO | Yes |  |
|  |  |  |

**Q2: Do you agree to adopt the text proposal from R1-2108140 (also captured in Section 2)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Reply (Yes/No)** | **Comments** |
| OPPO | Yes in principle | One clarification/comment on “of the serving cell”:  SFN can imply that it is the case of “serving cell available”, while DFN implies “serving cell is not available”. Maybe we can just say as follows:  \*\*\*\*\*\*\*\*\*\*\*  - index 0 corresponds to a first slot in a frame with SFN ~~of the serving cell~~ satisfying or DFN satisfying (DFN mod 16) = 0  \*\*\*\*\*\*\*\*\*\*\* |
|  |  |  |

# References

1. R1-2108140 [Draft] Correction on synchronization procedure for sidelink transmission,” Ericsson, RAN1 #106-e.