**3GPP TSG-RAN WG1 Meeting #106-eR1-210xxxx**

**e-meeting, 16 - 27 August, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **[DRAFT] CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.212** | **CR** |  | **rev** | **-** | **Current version:** | **16.6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | [Draft] Correction on SPS resource set configuration for DCI format 0\_2 in TS 38.212 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Moderator (Qualcomm), Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_L1enh-URLLC-Core | | | | |  | ***Date:*** | | | 2021-08-23 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To capture the correction on the configuration of SRS resource set(s) assocaited with *srs-ResourceSetToAddModListDCI-0-2* based on the outcome of email discussion [106-e-NR-L1enh-URLLC-01] | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify that, the higher layer parameters *‘srs-ResourceSetId’* and *‘srs-ResourceIdList’* associated with SRS resource set with usage='*codeBook*' or '*nonCodeBook*' configured by *srs-ResourceSetToAddModListDCI-0-2* can be configured differently from these higher layer parameters associated with the SRS resource set configured by *srs-ResourceSetToAddModList* with the same usage. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The network will not be able to configure different number of SRS resources in the SRS resource set associated with DCI format 0\_1 and 0\_2, and hence the bit width of SRI in DCI format 0\_1 and 0\_2 can not be configured differently. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.3.1.1.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

7.3.1.1.3 Format 0\_2

< Unchanged parts are omitted >

- SRS resource indicator –or bits, where is the number of configured SRS resources in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModListDCI-0-2*, and associated with the higher layer parameter *usage* of value '*codeBook*' or '*nonCodeBook*', where the SRS resource set is composed of the first SRS resources together with other configurations in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModList*, if any, and associated with the higher layer parameter *usage* of value '*codeBook*' or '*nonCodeBook*', respectively, except for the higher layer parameters *‘srs-ResourceSetId’ and ‘srs-ResourceIdList’*

- bits according to Tables 7.3.1.1.2-28/29/30/31 if the higher layer parameter *txConfig = nonCodebook*, where is the number of configured SRS resources in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModListDCI-0-2*, and associated with the higher layer parameter *usage* of value '*nonCodeBook*', where the SRS resource set is composed of the first SRS resources together with other configurations in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModList*, if any, and associated with the higher layer parameter *usage* of value '*nonCodeBook*', except for the higher layer parameters *‘srs-ResourceSetId’ and ‘srs-ResourceIdList’,* and

- if UE supports operation with *maxMIMO-LayersDCI-0-2* and the higher layer parameter *maxMIMO-LayersDCI-0-2* of *PUSCH-ServingCellConfig* of the serving cell is configured, *Lmax* is given by that parameter

- otherwise, *Lmax* is given by the maximum number of layers for PUSCH supported by the UE for the serving cell for non-codebook based operation.

- bits according to Tables 7.3.1.1.2-32 if the higher layer parameter *txConfig = codebook*, where is the number of configured SRS resources in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModListDCI-0-2*, and associated with the higher layer parameter *usage* of value '*codeBook*', where the SRS resource set is composed of the first SRS resources together with other configurations in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModList*, if any, and associated with the higher layer parameter *usage* of value '*codeBook*', except for the higher layer parameters *‘srs-ResourceSetId’ and ‘srs-ResourceIdList’*.

< Unchanged parts are omitted >