**3GPP TSG RAN WG1 #106-e R1-210XXXX**

**e-Meeting, August 16th – 27th, 2021**

**Agenda item:** 7.2.5

**Source:** Moderator (Qualcomm)

**Title:** Summary of [106-e-NR-L1enh-URLLC-01]

**Document for:** Discussion and Decision

# Introduction

This document is created to facilitate the email discussion of “[106-e-NR-L1enh-URLLC-01] Issue#3: Correction on SRS resource configuration. This email thread is triggered by the following draft CR.

R1-2107318 Remaining issues on PDCCH enhancements for URLLC Qualcomm Incorporated

# Explanation of the problem

In the RAN1 #105\_e meeting, an agreement was made to restrict the RRCs parameters associated with the SRS resource set in *srs-ResourceSetToAddModListDCI-0-2* with usage equal to “*codebook*” or “*noncodebook*” to be the same as the RRC parameters associated with the SRS resource set configured in *srs-ResourceSetToAddModList* with the same usage. The purpose is to make sure that the SRS resource set configured by *srs-ResourceSetToAddModListDCI-0-2* only contain a subset of SRS resources that are configured by the SRS resources set in *srs-ResourceSetToAddModList*.

However, [1] argues that it is neither necessary nor correct to make all RRC parameters associated with the two SRS resource sets to be the same. For example, [1] suggests to remove the restrictions of same RRC configuration for the following parameters associated with an SRS resource set configuration.

* *srs-ResourceSetId*
* *srs-ResourceIdList*
* *aperiodicSRS-ResourceTrigger*
* *aperiodicSRS-ResourceTriggerList*

Furthermore, the following CR on TS 38.212 was proposed.

7.3.1.1.3 Format 0\_2

< Unchanged parts are omitted >

- SRS resource indicator –$ \left⌈log\_{2}\left(\sum\_{k=1}^{min\left\{L\_{max}, N\_{SRS,0\\_2}\right\}}\left(\begin{matrix}N\_{SRS,0\\_2}\\k\end{matrix}\right)\right)\right⌉ $or $\left⌈log\_{2}N\_{SRS, 0\\_2}\right⌉ $bits, where $N\_{SRS, 0\\_2}$ is the number of configured SRS resources in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModListDCI-0-2*, and associated with the higher layer parameter *usage* of value '*codeBook*' or '*nonCodeBook*', where the SRS resource set is composed of the first $N\_{SRS, 0\\_2}$ SRS resources together with other configurations in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModList*, if any, and associated with the higher layer parameter *usage* of value '*codeBook*' or '*nonCodeBook*', respectively, except for the higher layer parameters *‘srs-ResourceSetId’, ‘srs-ResourceIdList’, ‘aperiodicSRS-ResourceTrigger’,* and *‘aperiodicSRS-ResourceTriggerList’*

- $\left⌈log\_{2}\left(\sum\_{k=1}^{min\left\{L\_{max}, N\_{SRS,0\\_2}\right\}}\left(\begin{matrix}N\_{SRS,0\\_2}\\k\end{matrix}\right)\right)\right⌉$ bits according to Tables 7.3.1.1.2-28/29/30/31 if the higher layer parameter *txConfig = nonCodebook*, where $N\_{SRS, 0\\_2}$ is the number of configured SRS resources in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModListDCI-0-2*, and associated with the higher layer parameter *usage* of value '*nonCodeBook*', where the SRS resource set is composed of the first $N\_{SRS, 0\\_2}$ SRS resources together with other configurations in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModList*, if any, and associated with the higher layer parameter *usage* of value '*nonCodeBook*', except for the higher layer parameters *‘srs-ResourceSetId’, ‘srs-ResourceIdList’, ‘aperiodicSRS-ResourceTrigger’,* and *‘aperiodicSRS-ResourceTriggerList’,* and

- if UE supports operation with *maxMIMO-LayersDCI-0-2* and the higher layer parameter *maxMIMO-LayersDCI-0-2* of *PUSCH-ServingCellConfig* of the serving cell is configured, *Lmax* is given by that parameter

- otherwise, *Lmax* is given by the maximum number of layers for PUSCH supported by the UE for the serving cell for non-codebook based operation.

- $\left⌈log\_{2}N\_{SRS, 0\\_2}\right⌉ $bits according to Tables 7.3.1.1.2-32 if the higher layer parameter *txConfig = codebook*, where $N\_{SRS, 0\\_2}$ is the number of configured SRS resources in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModListDCI-0-2*, and associated with the higher layer parameter *usage* of value '*codeBook*', where the SRS resource set is composed of the first $N\_{SRS, 0\\_2}$ SRS resources together with other configurations in the SRS resource set configured by higher layer parameter *srs-ResourceSetToAddModList*, if any, and associated with the higher layer parameter *usage* of value '*codeBook*', except for the higher layer parameters *‘srs-ResourceSetId’, ‘srs-ResourceIdList’, ‘aperiodicSRS-ResourceTrigger’,* and *‘aperiodicSRS-ResourceTriggerList’*.

< Unchanged parts are omitted >

For your reference, the RRC configuration for SRS resource set in Rel-16 is provided below.



# Company views

Companies are encouraged to provide comments on the following questions.

**Q1: Do you agree with the intention of the CR described in Section 2 that the RRC parameters associated with the SRS resource set configured in *srs-ResourceSetToAddModListDCI-0-2* and *srs-ResourceSetToAddModList* with the same usage can not all be configured the same? If not, any justifications?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comment** |
| HW/HiSi | [No] | Tentative no support. In our view it does not seem needed to configure the parameters separately since the SRS resource set of 0\_2 is intended to be a sub-set of 0\_1. The specification is not broken, and this CR would be an optimization in our view. But we would like to hear the views from others. |
| Apple | [No] | We have a similar understanding as Huawei.  |
| Nokia, NSB | No | We agree with Huawei/HiSi assessment there, this is regarded as some unnecessary optimization.  |
| Ericsson | No | Our understanding of the CRs made in RAN1#105e is similar to HW/HiSi/Apple/Nokia/NSB. The intention was that SRS resource set of DCI format 0\_2 is the subset of that of 0\_1, including the configurations. Before the CRs was made, it was stipulated that only a single SRS resource set can be configured for ‘codebook’, which was more restrictive. The same for ‘nonCodebook’.[1] argues that something is incorrect in current spec. But we fail to see the error case at the moment. If it is true that there is an error, we are open to correct. Maybe QC can explain better. |
|  |  |  |

**Q2: If you answer to Q1 is yes, what are the RRC parameters that you think may or must be configured differently?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comment** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2: If you answer to Q1 is yes, any additional comments on the CR in Section 2?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or No** | **Comment** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

To be added after the discussion.

# References

1. R1-2107318, Remaining issues on PDCCH enhancements for URLLC, Qualcomm, 3GPP WG1 106-e, Aug 16-27, 2021.