**3GPP TSG-RAN WG1 Meeting #106-e R1-210xxxx**

**e-Meeting, August 16th – 27th, 2021**

**Agenda Item: 7.2.8**

**Source: Moderator (Huawei)**

**Title: Summary of [106-e-NR-Pos-01] Replacement of cell terminology**

**Document for: Discussion and decision**

# Introduction

This document provides the summary for [106-e-NR-Pos-01] on the replacement of cell terminology.

[106-e-NR-Pos-01] Email discussion/approval on replacement of cell terminology (Aspect #1) until August 20 – Su (Huawei)

The related submission of contributions includes

1. R1-2106448 Draft CR on terminology correction to cell for positioning Huawei, HiSilicon
2. R1-2107991 Maintenance on Rel-16 NR positioning vivo

The email discussion is divided into two rounds, with the intermediate summary at 23:59 UTC, Aug. 18.

# General information

In [1], it is proposed to change the terminology “cell” in the descriptions of the higher layer parameters *NR-DL-PRS-SFN0-Offset* and *dl-PRS-QCL-Info* as shown below:

* In *NR-DL-PRS-SFN0-Offset*, the “transmitting cell” is changed to “DL PRS resource set”, and the “reference cell” is changed to “reference indicated by *nr-DL-PRS-ReferenceInfo*”.
* In *dl-PRS-QCL-Info*, “a non-serving cell” is changed to “not from any serving cell”.

The corresponding TP is provided below:

|  |
| --- |
| **TS 38.214** 5.1.6.5 PRS reception procedure========================= Unchanged parts =========================A DL PRS resource set is configured by *NR-DL-PRS-ResourceSet*, consists of one or more DL PRS resources and it is defined by:========================= Unchanged parts =========================*- NR-DL-PRS-SFN0-Offset* defines the time offset of the SFN0 slot 0 for the DL PRS resource set with respect to SFN0 slot 0 of reference provided by *nr-DL-PRS-ReferenceInfo*. ========================= Unchanged parts =========================A DL PRS resource is defined by:========================= Unchanged parts =========================*- dl-PRS-QCL-Info* defines any quasi co-location information of the DL PRS resource with other reference signals. The DL PRS may be configured with QCL 'typeD' with a DL PRS either from a serving cell or not from any serving cell, or with *rs-Type* set to 'typeC', 'typeD', or 'typeC-plus-typeD' with a SS/PBCH Block from a serving or non-serving cell.========================= Unchanged parts ========================= |

In [2], the similar change was proposed, for the description of ‘cell’ in section 5.1.6.5 in TS38.214, it is suggested to use the unified description just like ‘TRP’ in the specification, e.g., ‘*dl-PRS-ID*’ as provided in TP below:

|  |
| --- |
| **TS 38.214 (clause 5.1.6.5)**< Unchanged parts are omitted >*NR-DL-PRS-SFN0-Offset* defines the time offset of the SFN0 slot 0 for ~~the transmitting cell~~ each *dl-PRS-ID* with respect to SFN0 slot 0 of the reference indicated by *dl-PRS-ID* in higher layer parameter *nr-DL-PRS-ReferenceInfo*~~reference cell~~. < Unchanged parts are omitted > |

# Discussion

## *NR-DL-PRS-SFN0-Offset*

The reason for the change was believed to be removing “cell” terminology, since from UE reception of PRS perspective, TRP and cell should be differentiated. [1] also argued that PRS could be transmitted from a TRP-only TP where there is no cell associated with it.

### Proposal: Select one alternative to fix the cell terminology in *NR-DL-PRS-SFN0-Offset*

* **Alt.1**

|  |
| --- |
| *- NR-DL-PRS-SFN0-Offset* defines the time offset of the SFN0 slot 0 for the DL PRS resource set with respect to SFN0 slot 0 of reference provided by *nr-DL-PRS-ReferenceInfo*.  |

* **Alt.2**

|  |
| --- |
| *NR-DL-PRS-SFN0-Offset* defines the time offset of the SFN0 slot 0 for ~~the transmitting cell~~ each *dl-PRS-ID* with respect to SFN0 slot 0 of the reference indicated by *dl-PRS-ID* in higher layer parameter *nr-DL-PRS-ReferenceInfo*~~reference cell~~.  |

* **Alt.3 Others**

|  |  |  |
| --- | --- | --- |
| **Company** | **Alternative** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

## *dl-PRS-QCL-Info*

The reason for the change was that PRS/PRS QCL could refer to the PRS resource from the same PRS-only TP, which does not necessarily need to be a cell.

### Proposal: Decide whether to adopt the following change.

|  |
| --- |
| *- dl-PRS-QCL-Info* defines any quasi co-location information of the DL PRS resource with other reference signals. The DL PRS may be configured with QCL 'typeD' with a DL PRS either from a serving cell or not from any serving cell, or with *rs-Type* set to 'typeC', 'typeD', or 'typeC-plus-typeD' with a SS/PBCH Block from a serving or non-serving cell. |

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

TBD