**3GPP TSG-RAN WG1 Meeting #106-e R1-21xxxxx**

**e-Meeting, August 16th – 27th, 2021**

**Agenda Item: 7.2.8**

**Source: Moderator (vivo)**

**Title: Summary of [106-e-NR-Pos-05]**

**Document for: Discussion and decision**

# Introduction

This document provides the summary for [106-e-NR-Pos-05] on alignment with RAN4 on DL PRS Processing.

[106-e-NR-Pos-05] Email discussion/approval on alignment with RAN on DL PRS processing (Aspect #6) until August 20 – Huaming (vivo)

# General information

In [1], it is noticed that based on current TS 38.133, in RSTD/RSRP/Rx-Tx time difference measurement period requirements, it is described that if more than one PRS periodicities are configured in PRS frequency layer *i*, the least common multiple of PRS periodicities among all DL PRS resource sets is used to represent the periodicity of DL PRS resource on frequency layer *i* and further derive the measurement period of that PRS frequency layer *i*.

It is proposed to adopt one of the following options and related text proposals into TS38.214 regarding PRS processing capability.

***Option 1:*** ***change the descriptions related to ‘P msec window’ to align with RAN4 specification***.

|  |
| --- |
| < Unchanged parts are omitted >  For the case when measurement gap is configured, the UE DL PRS processing capability is defined in [TS 37.355]. For the purpose of DL PRS processing capability, the duration *K* msec of DL PRS symbols within *P* msec window ~~corresponding to the maximum PRS periodicity in a positioning frequency layer~~ described in Clause 9.9.2.5 [11, TS 38.133], is calculated by…  < Unchanged parts are omitted > |

***Option 2:*** ***delete the descriptions related to ‘P msec window’.***

|  |
| --- |
| < Unchanged parts are omitted >  For the case when measurement gap is configured, the UE DL PRS processing capability is defined in [TS 37.355]. For the purpose of DL PRS processing capability, the duration *K* msec of DL PRS symbols within *P* msec window ~~corresponding to the maximum PRS periodicity in a positioning frequency layer~~, is calculated by…  < Unchanged parts are omitted > |

In [2], the following changes were proposed to align with RAN4 specification on DL PRS processing:

* Evaluation window of P should no longer be corresponding to the maximum PRS periodicity, and the simplest way is to cite the RAN4 terminology .
* Duration calculation equation, the counted PRS slot/symbol should be mapping to those PRS that are neither muted nor outside the MG. From RAN1 perspective, those PRS could be referred to as “PRS to process”, as UE is not expected to process those PRS outside the MG or muted.
* Change the wording “For the purpose of DL PRS processing capability” since it may sometimes be interpreted inaccurately. The suggested wording can be “For the purpose of DL PRS processing”.

|  |
| --- |
| =========================== Unchanged parts ===========================  For the case when measurement gap is configured, the UE DL PRS processing capability is defined in [TS 37.355]. For the purpose of DL PRS processing, the duration *K* msec of DL PRS symbols within *P* msec window corresponding to as defined in clause 9.9 of [11, TS 38.133] in positioning frequency layer , is calculated by  *-* Type 1 duration calculation with UE symbol level buffering capability  *-* Type 2 duration calculation with UE slot level buffering capability  *- S* is the set of slots based on the numerology of the DL PRS of a serving cell within the *P* msec window in the positioning frequency layer that contains potential DL PRS resources to process considering the actual *nr-DL-PRS-ExpectedRSTD*, *nr-DL-PRS-ExpectedRSTD-Uncertainty* provided for each pair of DL PRS Resource Sets.  *-* For Type 1, is the smallest interval in msec within slot corresponding to an integer number of OFDM symbols based on the numerology of the DL PRS of a serving cell that covers the union of the potential PRS symbols to process and determines the PRS symbol occupancy within slot , where the interval considers the actual *nr-DL-PRS-ExpectedRSTD*, *nr-DL-PRS-ExpectedRSTD-Uncertainty* provided for each pair of DL PRS resource sets (target and reference).  *-* For Type 2, is the numerology of the DL PRS, and is the cardinality of the set .  =========================== Unchanged parts =========================== |

# Discussion

## *P msec window*

As pointed out by [1] and [2], current description window P is not aligned with RAN4’s specification and not technical correct. Both [1] and [2] proposed to align window P to RAN4 specification. Given the proposed option 1 in [1] and the proposed TP in [2] are very similar with the same intention: to cite the RAN4 specification and given TP in [2] is more clear on the clause of TS38.133, moderator suggest to take that change.

### Proposal: Select the following text proposal to align with RAN4 on DL PRS processing with respect to P msec window.

|  |
| --- |
| < Unchanged parts are omitted >  For the case when measurement gap is configured, the UE DL PRS processing capability is defined in [TS 37.355]. For the purpose of DL PRS processing capability, the duration *K* msec of DL PRS symbols within *P* msec window corresponding to as defined in clause 9.9 of [11, TS 38.133] ~~the maximum PRS periodicity~~ in ~~a~~ positioning frequency layer *i*, is calculated by…  < Unchanged parts are omitted > |

Companies are invited to express their views and suggestions in table below:

|  |  |
| --- | --- |
| Company Name | Comments |
| OPPO | OK with the proposal |
| Huawei, HiSilicon | Support. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## *Other changes*

[2] also proposed some other changes for clarity and to avoid confusion.

- Duration calculation equation, the counted PRS slot/symbol should be mapping to those PRS that are neither muted nor outside the MG. From RAN1 perspective, those PRS could be referred to as “PRS to process”, as UE is not expected to process those PRS outside the MG or muted.

- Change the wording “For the purpose of DL PRS processing capability” since it may sometimes be interpreted inaccurately.

### Proposal: Decide whether to adopt the following changes.

|  |
| --- |
| =========================== Unchanged parts ===========================  For the case when measurement gap is configured, the UE DL PRS processing capability is defined in [TS 37.355]. For the purpose of DL PRS processing ~~capability~~,  …  *- S* is the set of slots based on the numerology of the DL PRS of a serving cell within the *P* msec window in the positioning frequency layer that contains potential DL PRS resources to process considering the actual *nr-DL-PRS-ExpectedRSTD*, *nr-DL-PRS-ExpectedRSTD-Uncertainty* provided for each pair of DL PRS Resource Sets.  *-* For Type 1, is the smallest interval in msec within slot corresponding to an integer number of OFDM symbols based on the numerology of the DL PRS of a serving cell that covers the union of the potential PRS symbols to process and determines the PRS symbol occupancy within slot , where the interval considers the actual *nr-DL-PRS-ExpectedRSTD*, *nr-DL-PRS-ExpectedRSTD-Uncertainty* provided for each pair of DL PRS resource sets (target and reference).  =========================== Unchanged parts =========================== |

Companies are invited to express their views and suggestions in table below:

|  |  |
| --- | --- |
| Company Name | Comments |
| OPPO | Ok with the proposal |
| Huawei, HiSilicon | Support. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusion

TBD

# References

1. R1-2107991 Maintenance on Rel-16 NR positioning vivo
2. R1-2108189 Aligning PRS duration calculation with RAN4 Huawei, HiSilicon