Companies are to share their inputs on the excel spreadsheet in /tsg\_ran/WG1\_RL1/TSGR1\_106-e/Inbox/drafts/8.1.1/RRC/ herein.

## Inputs on initial version

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| Apple | **For QCL-Info\_r17, we suggest we add some clarification for SRI*** **SRS ResourceId (SRS for beam management, only applicable for UL TCI)**

**We are not sure whether the following PC parameters are needed, but it seems we can reuse legacy prameters?*** **p0\_Alpha\_CLIdPUSCHSet**
* **p0\_Alpha\_CLIdPUCCHSet**
* **p0\_Alpha\_CLIdSRSSet**
* **p0\_Alpha\_CLIdSetId**

**We are not sure whether we need to introduce the following parameters. It seems legacy CSI report framework already cover the following aspects*** **InterCellBeamMetrics**
* **InterCellMeasurementRS**
* **InterCellReportType**

**Regarding the change of CORESET TCI list, we think some discussion is needed. Currently unified TCI is applied for multiple channels, and it should be selected from the TCI state pool in PDSCH-Config instead of the pool in CORESET*** **ControlResourceSet**

**Regarding the following parameters, we are not sure whether we need to create a new structure for Rel-17 or not (It seems this is a RAN2 problem?). But what we need seems to be numberOfN only. In addition, we think it is not necessary to introduce numberOfM.*** **mpe-Reporting-FR2-r17**
* **MPE-Config-FR2-r17**
* **mpe-ProhibitTimer-r17**
* **mpe-Threshold-r17**
* **numberOfN**
* **numberOfM**
 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version 01

Please share your inputs, if any, in the following table

....