**3GPP TSG RAN WG1 #106-e R1-2108399**

**e-Meeting, August 16th – 27th, 2021**

**Agenda item:** 8.1.1

**Source:** Moderator (Samsung)

**Title:** Moderator summary#4 for multi-beam enhancement: ROUND 3

**Document for:** Discussion and Decision

## Introduction

In this summary, the term “item 1” refers to the first item in the Rel.17 NR FeMIMO WID, i.e. multi-beam enhancement:

|  |
| --- |
| 1. Enhancement on multi-beam operation, mainly targeting FR2 while also applicable to FR1:    1. Identify and specify features to facilitate more efficient (lower latency and overhead) DL/UL beam management for intra-cell and inter-cell scenarios to support higher UE speed and/or a larger number of configured TCI states:       1. Common beam for data and control transmission/reception for DL and UL, especially for intra-band CA       2. Unified TCI framework for DL and UL beam indication       3. Enhancement on signaling mechanisms for the above features to improve latency and efficiency with more usage of dynamic control signaling (as opposed to RRC)       4. For inter-cell beam management, a UE can transmit to or receive from only a single cell (i.e. serving cell does not change when beam selection is done). This includes L1-only measurement/reporting (i.e. no L3 impact) and beam indication associated with cell(s) with any Physical Cell ID(s)          1. The beam indication is based on Rel-17 unified TCI framework          2. The same beam measurement/reporting mechanism will be reused for inter-cell mTRP          3. This work shall only consider intra-DU and intra-frequency cases    2. Identify and specify features to facilitate UL beam selection for UEs equipped with multiple panels, considering UL coverage loss mitigation due to MPE, based on UL beam indication with the unified TCI framework for UL fast panel selection |

This summary includes the following:

* Observation and proposal
* Summary of current companies’ positions on each of the aspects within the category

**This round targets some email endorsement after the next GTW on Monday 08/23 (12:00-15:00 UTC). Please provide your inputs. As usual I will move the discussion on prospective proposals to the email reflector as it gets close to the endorsement time.**

## Summary of companies’ inputs

The listed issues are structured primarily to facilitate some progress on pending issues identified in the agreements (see Appendix A).

### Issue 1 (Rel.17 unified TCI framework) and 2 (inter-cell beam management)

Table 1 Summary: issue 1 and 2 sticky points

|  |
| --- |
| **Proposal 1.B-3**  **Working Assumption (to be confirmed this week)**  On Rel.17 unified TCI framework, for intra-cell beam indication, the following DL RSs can share the same indicated Rel-17 TCI state as UE-dedicated reception on PDSCH and for UE-dedicated reception on all or subset of CORESETs in a CC:   * DMRS(s) associated with non-UE-dedicated reception on CORESET(s) and the associated PDSCH   + FFS: Any restriction on the SS type other than USS associated with the CORESET(s)   *Objected by Futurewei*  **Proposal 2.A.1+5**  On Rel.17 beam indication enhancements for inter-cell beam management, the supported Rel-17 MAC-CE-based and/or DCI-based beam indication (at least using DCI formats 1\_1/1\_2 with and without DL assignment including the associated MAC-CE-based TCI state activation) applies to:   * The same channels and signals as for intra-cell beam management (what has been agreed up to day 5 of RAN1#106-e). Select one from the following alternatives:   + Alt1. Additionally applicable for non-UE specific channels     - Note: Some companies have concerns that this violates RAN conclusion from RAN#92-e   + Alt3. No additional channel from non-serving cell is allowed * For the aforementioned applicable DL channels and DL signals, SSB associated with a physical cell ID different from that of the serving cell is used as an indirect QCL reference for DL TCI (in case of separate DL/UL TCI) or joint TCI   + Note: When RS X is an indirect QCL reference of a target channel, there exists at least one other source signal on the QCL chain between RS X and the target channel. Here, Rel-15/16 QCL rule is reused by replacing SSB with SSB associated with a physical cell ID different from that of the serving cell * This inter-cell beam management does not mandate a UE to support more than one active TCI state / QCL per band   *3rd bullet point was proposed by Apple, but Futurewei couldn’t accept* |

Futurewei has stated that the reason for their objection over proposal 1.B-3 is because it is related to proposal 2.A-1+5. While the two are not categorically related (one for intra-cell, the other for inter-cell), the wording “the same channels and signals ...” indeed links proposal 2.A-1+5 by reference to proposal 1.B-3.

To progress together and compromise, the moderator proposes the following combo:

|  |
| --- |
| **Combo Proposal**:  On Rel.17 unified TCI framework, for intra-cell beam indication, the following DL RSs can share the same indicated Rel-17 TCI state as UE-dedicated reception on PDSCH and for UE-dedicated reception on all or subset of CORESETs in a CC:   * DMRS(s) associated with non-UE-dedicated reception on CORESET(s) and the associated PDSCH   + FFS: Any restriction on the SS type other than USS associated with the CORESET(s)   On Rel.17 beam indication enhancements for inter-cell beam management, the supported Rel-17 MAC-CE-based and/or DCI-based beam indication (at least using DCI formats 1\_1/1\_2 with and without DL assignment including the associated MAC-CE-based TCI state activation) applies to:   * The channels and signals as for intra-cell beam management except for non-UE-specific channels * For the aforementioned applicable DL channels and DL signals, SSB associated with a physical cell ID different from that of the serving cell is used as an indirect QCL reference for DL TCI (in case of separate DL/UL TCI) or joint TCI   + Note: When RS X is an indirect QCL reference of a target channel, there exists at least one other source signal on the QCL chain between RS X and the target channel. Here, Rel-15/16 QCL rule is reused by replacing SSB with SSB associated with a physical cell ID different from that of the serving cell * This inter-cell beam management does not mandate a UE to maintain more than one active TCI state / QCL per band for a given time   + That is, beam switching across slots is used to receive or transmit along two different beams |

Table 2 Additional inputs: issue 1

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Share your inputs on the above Combo Proposal** |
|  |  |
|  |  |
|  |  |

### Issue 3 (beam indication signaling medium)

Table 5 Summary: issue 3

|  |  |
| --- | --- |
| **Proposal** | **Companies’ views** |
| 3.A BAT quantization/definition   * Alt1: X ms (hence not SCS dependent) * Alt2: Y symbols (hence SCS dependent) | **Alt1 (X ms)**: Apple, OPPO, CATT, ZTE  **Alt2 (Y symbols**): Ericsson, Samsung, Qualcomm, Intel, MTK, NTT Docomo, Spreadtrum, Lenovo/MotM, Xiaomi, LG, Sony, Nokia/NSB, IDC |
| 3.B How to determine BAT in case of CA | **Highest BAT among CCs**: Samsung, MTK, Xiaomi, Nokia/NSB,  **The BAT is determined by the scheduled carrier, and offset if added based on the relation between the SCS of PDCCH and the scheduled channel (existing)**: Ericsson  **BAT for smallest SCS among CCs**: Qualcomm, Intel, Lenovo/MotM, Sony  **One value for all CCs**: Apple, Spreadtrum, OPPO, CATT, ZTE  **BAT for CC with largest delay**: NTT Docomo |
|  |  |

**Proposal 3.A**: On Rel-17 DCI-based beam indication, regarding application time of the beam indication, the first slot that is at least Y symbols after the last symbol of the acknowledgment of the joint or separate DL/UL beam indication.

* In case of CA, the BAT is determined by the scheduled carrier, and offset is added based on the relation between the SCS of PDCCH and the scheduled channel

Table 6 Additional inputs: issue 3

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **Please share your views on the FL proposal** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 4 (MP-UE)

Table 7 Summary: issue 4

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 4.1 | Whether to support the following measurement/reporting scheme for UE-initiated panel activation/selection:   * Opt1-1: A panel entity corresponds to a reported CSI-RS and/or SSB resource index in a beam reporting instance   + The correspondence between a panel entity and a reported CSI-RS and/or SSB resource index is informed to NW   + Note: the correspondence between a CSI-RS and/or SSB resource index and a panel entity is determined by the UE (analogous to Rel-15/16) * Opt1-2: A panel entity is referring to a new panel ID within CSI/beam reports   + FFS: Detailed design of the new panel ID including the information conveyed by the new panel ID   + Note: The association between the new panel ID and the panel entity is determined by the UE   Opt1-3: No additional specification support | **Opt1-1:** Huawei/HiSi, Sony (2nd priority), MTK, Intel, Apple (if UE-initiated beam reporting and UE cap are supported), [Nokia/NSB], IDC  **Opt1-2:** Huawei/HiSi, ZTE, vivo, IDC, MotM/Lenovo, Spreadturm, Sony, Samsung, CMCC, Fraunhofer IIS/HHI, AT&T, LGE, NTT Docomo, Xiaomi   * Panel ID: Huawei/HiSi, ZTE, CMCC, Fraunhofer/HHI, AT&T, LGE, NTT Docomo, Xiaomi, IDC * Resource set: Samsung   **Opt1-3:** CATT, OPPO, FGI/APT, Ericsson, Apple (if UE-initiated beam reporting and UE cap are **not** supported) |
| 4.2 | Whether to support CB-based SRS resources with different numbers of ports | **Yes**: Huawei/HiSi, CATT, OPPO, Qualcomm, [Fraunhofer IIS/HHI], Apple (only the SRS set aligned with UE selected panel can be indicated), LGE, NTT Docomo, MTK, IDC  **No**: [vivo], Ericsson |
| 4.3 | Whether to support NCB-based SRS resource sets with different numbers of resources | **Yes**: ZTE, LGE, Apple (only the SRS set aligned with UE selected panel can be indicated), IDC, CATT  **No**: [vivo], Ericsson |
|  |  |  |

It was proposed offline that a possible compromise is to agree on Opt 1-1 of 4.1 together with the proposal below

**Proposal 4.A**: On Rel.17 enhancements to facilitate UE-initiated panel activation and selection:

* No specification enhancement on UE reporting to facilitate UE-initiated panel activation/selection
* Support codebook-based SRS resources with different maximum number of UL MIMO layers per panel entity
  + FFS (to be concluded in RAN1#106bis-e): need for dynamic reporting of SRS resource specific candidate spatial source(s)

Table 8 Additional inputs: issue 4

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Share your input on the above FL proposals** |
|  |  |
|  |  |
|  |  |

### Issue 5 (MPE mitigation)

Table 9 Summary: issue 5

|  |  |
| --- | --- |
| **Proposal** | **Companies’ views** |
| 5.A below | **Support:** Qualcomm, NTT Docomo, Spreadtrum, Lenovo/MotM, OPPO, Xiaomi, vivo, ZTE, CMCC, Sony, Nokia/NSB, Samsung  **Not support:** Ericsson, Intel, Apple, MTK, CATT, LG, |

The following observation can be made:

* 5.1: In round 0 (and since the last meeting), the proponents of 1A and 2A failed to converge. In this round we will try to start from option 1D. The proposal below is made based on the inputs from companies’ contributions and discussion. Note that this is the last attempt (i.e. we will not return to 1A and/or 2A).

**Proposal 5.A**: On Rel.17 enhancements to facilitate MPE mitigation, support the following enhancement on the Rel-16 event-triggered P-MPR-based reporting (included in the PHR report when a threshold is reached, reported via MAC-CE):

* N≥1 P-MPR values can be reported [together with N≥1 SSBRI(s)/CRI(s)]
* FFS: Whether N represents the number of selected beams or the number of panels
* FFS: Whether beam-specific and/or panel-specific PHR is also reported
* FFS: Additional reporting quantities, e.g. SSBRI/CRI, MPR+DL RSRP, UL RSRP, or modified virtual PHR
* FFS: additional signaling (e.g. CSI triggering) from the NW

Table 10 Additional inputs: issue 5

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 9**  **2) Share your inputs on the above FL proposals** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 6 (advanced beam refinement/tracking)

(Round 4)

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2106864 | Summary of offline discussion on unified TCI and inter-cell beam management | Moderator (Samsung) |
| 2 | R1-2106463 | Enhancements on multi-beam operation in Rel-17 | Huawei, HiSilicon |
| 3 | R1-2106541 | Enhancements on Multi-beam Operation | ZTE |
| 4 | R1-2106571 | Further discussion on multi beam enhancement | vivo |
| 5 | R1-2106640 | Remaining Details on Enhancements for Multi-beam Operation | IDC, Inc. |
| 6 | R1-2106666 | Enhancements on Multi-beam Operation | Lenovo, Motorola Mobility |
| 7 | R1-2106685 | Enhancements on Multi-beam Operation | Spreadtrum Communications |
| 8 | R1-2106789 | Further enhancement on multi-beam operation | Sony |
| 9 | R1-2106864 | Moderator summary for multi-beam enhancement | Moderator (Samsung) |
| 10 | R1-2106865 | Multi-Beam Enhancements | Samsung |
| 11 | R1-2106935 | Discussions on enhancements on multi-beam operation | CATT |
| 12 | R1-2107029 | Enhancements on Multi-beam Operation | Fujitsu |
| 13 | R1-2107085 | Enhancement on multi-beam operation | FUTUREWEI |
| 14 | R1-2107143 | Discussion on multi-beam operation | NEC |
| 15 | R1-2107203 | Enhancements on Multi-beam Operation | OPPO |
| 16 | R1-2107297 | Discussion of enhancements on multi-beam operation | FGI, Asia Pacific Telecom |
| 17 | R1-2107323 | Enhancements on Multi-beam Operation | Qualcomm Incorporated |
| 18 | R1-2107390 | Enhancements on multi-beam operation | CMCC |
| 19 | R1-2107464 | Enhancements on multi-beam operation | Fraunhofer IIS, Fraunhofer HHI |
| 20 | R1-2107485 | Enhancement on multi-beam operation | MTK Inc. |
| 21 | R1-2107570 | Enhancements to Multi-Beam Operations | Intel Corporation |
| 22 | R1-2107628 | Enhancements on Multi-beam Operation | Ericsson |
| 23 | R1-2107689 | Enhancements on Multi-beam operations | AT&T |
| 24 | R1-2107718 | Views on Rel-17 Beam Management enhancement | Apple |
| 25 | R1-2107814 | Enhancements on Multi-beam Operation | LG Electronics |
| 26 | R1-2107838 | Discussion on multi-beam operation | NTT DOCOMO, INC. |
| 27 | R1-2107893 | Enhancements on multi-beam operation | Xiaomi |
| 28 | R1-2108019 | Enhancements on Multi-beam Operation | Convida Wireless |
| 29 | R1-2108052 | Enhancements on Multi-beam Operation | Nokia, Nokia Shanghai Bell |
| 30 | R1-2106548 | Further details on Multi-beam and Multi-TRP operation | ZTE |
| 31 | R1-2106671 | HARQ feedback of SPS PDSCH reception in multi-DCI based multiple TRPs | Lenovo, Motorola Mobility |
| 32 | R1-2106872 | Additional enhancements for multi-beam | Samsung |
| 33 | R1-2107210 | Discussion on further enhancements for multi-beam operation | OPPO |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |