Companies are to share their inputs on the excel spreadsheet in [/tsg\_ran/WG1\_RL1/TSGR1\_106-e/Inbox/drafts/8.1.2.1/PUCCH&PUSCH/RRC/](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_106-e/Inbox/drafts/8.1.2.1/PUCCH%20%26%20PUSCH/RRC) herein.

## Inputs on initial version

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| Apple | * **MappingPattern: It seems we have not agreed this is configured by RRC** * **FFS: PUCCH-SpatialRelationInfo (without referenceSignal) or PUCCH-PowerControlSetInfo (new IE): I am not sure whether we have agreed that “from RAN1 point of view, one possible example is to reuse PUCCH-SpatialRelationInfo except for the referenceSignal”. In our view, it can be as follows:**   + **PUCCH-PowerControlSetInfo; whether to reuse legacy structure or create new structure is up to RAN2; candidate value: similar to PUCCH-spatialRelationInfo without referenceSignal** * **SecondTPCFieldDCI-x-y: In our view, one RRC parameter per UL channel seems to be enough.** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version 01

Please share your inputs, if any, in the following table

....