3GPP TSG RAN WG1 Meeting #106-e R1-210xxxx

16th August – 27th August 2021

Agenda Item: 8.10

Source: Moderator (Qualcomm Incorporated)

Title: Summary of initial assessment on Rel-17 upper layer parameters to support eIAB physical layer operation [Post-106-e-Rel17-RRC-10]

Document for: Information

This document provides a summary of the following email discussion on upper layer parameters to support eIAB physical layer operation:

[Post-106-e-Rel17-RRC-10] eIAB – to be moderated by Luca (Qualcomm)

An initial assessment of the required upper layer parameters for Rel-17 eIAB has been made with input from the FLs of the applicable agenda items 8.10.1 and 8.10.2 and it is summarized in the following table.

Companies are encouraged to provide feedback in the comments section at the end of the document.

| **Param. ID** | **Sub-feature group** | **New or existing parameter** | **Parameter name in specification** | **Description** | **Value range** | **Default value** | **IAB node specific/IAB nodes common** | **Specification** | **Signaling** | **Comment** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| P01 | Resource multiplexing | New | Rel-17 IAB-DU-Resource-Configuration-H/S/NA-Config (final name in specification to be determined by RAN2/3) | Per-cell H/S/NA attributes per-resource type | {Hard, Soft, Not Available} per RB set, per resource type in a slot [TBD relative to IAB-DU-Resource-Configuration-TDD-Config] |  | IAB node specific |  | **F1AP** | **RAN1 #105-e**  Agreement  For frequency domain multiplexing, H/S/NA configurations for an IAB-node are provided separately in addition to the Rel-16 H/S/NA  **Agreement**  If an IAB node is configured with a frequency-domain H/S/NA configuration down select between the following options:   * Alt. 1 Either the Rel-16 H/S/NA configuration or frequency domain configuration is applied for a given resource   + FFS: Whether configurations are switched with per-slot, per-resource type within a slot, or per-symbol granularity * Alt. 2 The Rel-16 H/S/NA configuration and frequency domain configuration are jointly applied   **RAN1 #106-e**  **Agreement**  The semi-static configuration of H/S/NA resource type in frequency domain is provided per RB set, per D/U/F resource type within a slot. |
| P02 | Resource multiplexing | New | RB Set Configuration | Indicates the RB set size in number of PRBs used for frequency domain multiplexing between given IAB-DU and IAB-MT cells | • List of values {2, 4, 8, 16, 32, 64}  • FFS: Value(s) in case of multiple configured BWPs at the IAB-MT |  | IAB node specific |  | **F1AP** | **RAN1 #106-e**  **Agreement**  N is a configured number of PRBs, where the CU configures N   * N = {2, 4, 8, 16, 32, 64} * FFS: Value(s) of N in case of multiple configured BWPs at the IAB-MT * This agreement does not revert any existing RAN1 agreement   **Requires intra/inter CU coordination:** No |
| P03 | Resource multiplexing | New | Frequency Domain H/S/NA Configuration Reference SCS | Indicates reference SCS to be applied to Rel-17 IAB-DU-Resource-Configuration-H/S/NA-Config at the IAB-DU | FR1: {15kHz, 30kHz, 60kHz}  FR2: {60kHz, 120kHz} |  | IAB node specific |  | **F1AP** | **RAN1 #106-e**  **Agreement**  A Reference SCS is configured for frequency domain H/S/NA configuration.  **Requires intra/inter CU coordination:** No |
| P04 | Resource multiplexing | New | Peer Parent DU Resource Configuration | Indicates the DU resource configuration (UL/DL/FL, H/S/NA) of the other peer parent node that connects to the same IAB-node | IAB-DU-Resource-Configuration-TDD-Config + Frequency Domain H/S/NA Configuration Reference SCS |  | IAB node specific |  | **F1AP and Xn** | **RAN1 #106-e**  **Agreement**  For intra-donor and inter-donor DC scenarios, in addition to coordination at the donor CU(s), a parent-node can be made aware of the DU resource configuration (UL/DL/FL, H/S/NA) of the other peer parent node that connects to the same IAB-node. |
| P05 | Resource multiplexing | New | Peer Parent Common Resource Configuration | Indicates the semi-static and/or cell-common higher layer configuration (e.g. SSB, CORESET 0, and RACH and configurations) from/for different parent nodes. | TBD (at least cell-common higher layer configuration (e.g. SSB, CORESET 0, and RACH and configurations) |  | IAB node specific |  | **F1AP and Xn** | **RAN1 #106-e**  **Agreement**  For intra-donor and inter-donor DC scenarios, coordinating the semi-static and/or cell-common higher layer configuration (e.g. SSB, CORESET 0, and RACH and configurations) from/for different parent nodes. |
| P06 | Resource multiplexing | New | Rel-17 IAB-DU-Resource-Configuration-H/S/NA-Config (final name in specification to be determined by RAN2/3) | Per-cell H/S/NA attributes per-resource type | {Hard, Soft, Not Available} per RB set, per resource type in a slot [TBD relative to IAB-DU-Resource-Configuration-TDD-Config] |  | IAB node specific |  | **F1AP** | **RAN1 #105-e**  **Agreement**  For frequency domain multiplexing, H/S/NA configurations for an IAB-node are provided separately in addition to the Rel-16 H/S/NA  **Agreement**  If an IAB node is configured with a frequency-domain H/S/NA configuration down select between the following options:   * Alt. 1 Either the Rel-16 H/S/NA configuration or frequency domain configuration is applied for a given resource   + FFS: Whether configurations are switched with per-slot, per-resource type within a slot, or per-symbol granularity * Alt. 2 The Rel-16 H/S/NA configuration and frequency domain configuration are jointly applied   **RAN1 #106-e**  **Agreement**  The semi-static configuration of H/S/NA resource type in frequency domain is provided per RB set, per D/U/F resource type within a slot. |
| P07 | Resource multiplexing | New | RB Set Configuration | Indicates the RB set size in number of PRBs used for frequency domain multiplexing between given IAB-DU and IAB-MT cells | • List of values {2, 4, 8, 16, 32, 64}  • FFS: Value(s) in case of multiple configured BWPs at the IAB-MT |  | IAB node specific |  | **F1AP** | **RAN1 #106-e**  **Agreement**  N is a configured number of PRBs, where the CU configures N   * N = {2, 4, 8, 16, 32, 64} * FFS: Value(s) of N in case of multiple configured BWPs at the IAB-MT * This agreement does not revert any existing RAN1 agreement   **Requires intra/inter CU coordination:** No |
| P08 | Resource multiplexing | New | Frequency Domain H/S/NA Configuration Reference SCS | Indicates reference SCS to be applied to Rel-17 IAB-DU-Resource-Configuration-H/S/NA-Config at the IAB-DU | FR1: {15kHz, 30kHz, 60kHz}  FR2: {60kHz, 120kHz} |  | IAB node specific |  | **F1AP** | **RAN1 #106-e**  **Agreement**  A Reference SCS is configured for frequency domain H/S/NA configuration.  **Requires intra/inter CU coordination:** No |
| P09 | Resource multiplexing | New | Peer Parent DU Resource Configuration | Indicates the DU resource configuration (UL/DL/FL, H/S/NA) of the other peer parent node that connects to the same IAB-node | IAB-DU-Resource-Configuration-TDD-Config + Frequency Domain H/S/NA Configuration Reference SCS |  | IAB node specific |  | **F1AP** | **RAN1 #106-e**  **Agreement**  For intra-donor and inter-donor DC scenarios, in addition to coordination at the donor CU(s), a parent-node can be made aware of the DU resource configuration (UL/DL/FL, H/S/NA) of the other peer parent node that connects to the same IAB-node. |
| P10 | Resource multiplexing | New | Rel-17 Desired Guard Symbols | Number of symbols the IAB node would like the parent IAB node not to use at the edge (beginning or end) of a slot for Case #6 and Case #7 timing cases when there is a transition between the IAB node MT and DU per cell | FFS |  | IAB node specific | Resource multiplexing | **MAC-CE** | **RAN1 #106-e**  **Agreement**  MAC-CE signaling of Desired/Provided Guard Symbols is enhanced (e.g. using the same Rel-16 MAC-CE design) to support indication of guard symbols additionally required for Case #6 and Case #7 timing cases.   * FFS: Number of guard symbols associated with Case #6 and Case #7 timing modes * FFS: Need for explicit indication of guard symbols switching between timing cases |
| P11 | Resource multiplexing | New | Rel-17 Provided Guard Symbols | Number of symbols the IAB node uses at the edge (beginning or end) of a slot for Case #6 and Case #7 timing cases when there is a transition between the IAB node MT and DU at the child node per cell | FFS |  | IAB node specific | Resource multiplexing | **MAC-CE** |
| P12 | Resource multiplexing | New | Simultaneous Operation Beam Indication | Signaling from a parent node to a child node indicating beams of an IAB-DU in the direction of which simultaneous operation is restricted | FFS |  | IAB node specific | Resource multiplexing | **MAC-CE** | **RAN1 #106-e**  **Agreement**  MAC-CE signaling from a parent node is supported for indication of beams of an IAB-DU in the direction of which simultaneous operation is restricted   * FFS: Details of beam indication (e.g. TCI state ID, Spatial relation information ID, RS ID (including CSI-RS, SRS, SSB, etc.)) * FFS: Applicability to other beams   **Agreement**  **Spatial domain restrictions from a parent node or recommendations from a child node is limited to a subset of time resources in which simultaneous operation is applied.**   * **FFS: Handling of frequency resources in case of FDM operation** * **FFS: Support for implicit/explicit indication of the simultaneous operation mode** |
| P13 | Interference management | Existing parameter | *Intended TDD DL-UL Configuration* | Rel-16 *Intended TDD DL-UL Configuration* is extended to support IAB-specific UFD patterns. | Permutation: ENUMERATED (DFU, UFD, …) | DFU | IAB node specific |  | **F1AP and Xn** | **RAN1#105-e**  Agreement  Rel-16 CLI coordination signalling (Intended TDD DL-UL Configuration) is extended to support IAB specific UFD patterns.  FFS: Support the exchange of IAB-DU H/S/NA resource configuration information among neighbouring IAB-nodes/IAB-donors for CLI management purposes. |
| P14 | Resource multiplexing | New | Peer DU Resource Configuration | Indicates the DU resource configuration (UL/DL/FL, H/S/NA) of the peer IAB-node or donor DU that can be used for interference management or resource coordination in case of DC. | IAB-DU-Resource-Configuration-TDD-Config + Frequency Domain H/S/NA Configuration Reference SCS |  | IAB node specific |  | **F1AP and Xn** | **RAN1#106-e**  **Agreement**  Support the exchange of semi-static Rel-16 IAB-DU H/S/NA resource configuration information and Rel-17 frequency domain IAB-DU H/S/NA resource configuration information among neighbouring IAB-nodes/IAB-donors  Also related to parameter “Peer Parent DU Resource Configuration” as common signaling may be desirable. |
| P15 | Timing control | New | Timing Case Indication | The parent-node indicates to an IAB-node when (over which time resources) a timing case is performed, including:   * When Case 6 timing is performed at the IAB-node. * When Case 7 timing is performed at the parent-node. * [FFS] when Case 7 timing is performed at the IAB-node. | FFS |  | IAB node specific |  | **FFS** | **RAN1#104-e**  **Agreement**  Switching between Case 1, Case 6, and Case 7 timing is supported.   * FFS whether Case 6 and Case 7 timing shall be restricted to certain resources, e.g. excluding resources used for access or TDM backhaul * FFS details on switching including the switching conditions * FFS relationship between switching timing modes with the usage/indication of different resource multiplexing modes * FFS whether Rel-16 OTA synchronization shall be enhanced to support switching timing modes   **RAN1#105-e**  **Agreement**  An IAB-node is indicated when Case 6 timing is performed at the IAB-node.   * FFS details of the indication (e.g. semi-static and/or dynamic, implicit and/or explicit, linkage to multiplexing capability, etc.).   FFS whether an IAB-node is also indicated when Case 7 timing is performed at the IAB-node.  **RAN1#106-e**  **Agreement**  An IAB-node is explicitly indicated by the parent node when Case 6 timing is performed at the IAB-node at least for specific time resources.   * FFS: whether the indication should be associated with another dimensions, e.g. multiplexing cases * FFS whether an IAB-node is explicitly indicated by the parent node when Case 7 timing is performed at the IAB-node.   **RAN1#106-e**  **Agreement**  An IAB-node is explicitly indicated by the parent node when Case 7 timing is performed at the parent node.  FFS for signalling details |
| P16 | Timing control | New | Case7 Timing Offset | The parent-node indicates to an IAB-node an offset to be used by the IAB-MT to set its UL TX timing based on the legacy TA loop and the indicated offset. | FFS |  | IAB node specific |  | **FFS** | **RAN1#106-e**  **Agreement**  For Case 7 timing at a parent node, the IAB-MT Tx timing of the node is obtained via the legacy TA loop plus an offset from the parent node.  FFS range, granularity, and signaling details of the offset. |
| P17 | Power control | New | Desired DL TX Power Adjustment | The IAB-MT indicates to its parent-node, its desired DL TX power adjustment to assist with the parent-node’s DL TX power allocation. This indication is provided at least for specific time resources and can further be associated with spatial configuration. | FFS |  | IAB node specific |  | **FFS** | **RAN1#104-e**  **Agreement**  Support an IAB-node indicating information to assist with the DL power control of its parent-node towards the IAB-node without mandating an expected behavior at the parent node.   * Note: At least the assistance information is for supporting the simultaneous operation within the IAB-node to avoid power imbalance * FFS: type of assistance information (e.g., desired received power, power adjustment, preferred CSI-RS resource) * FFS: whether this information is provided to the parent-node, the CU, or both. * FFS: applicability of the assistance information (e.g. relation to beams or multiplexing modes)   FFS: the channel carrying this assistance information  **RAN1#105-e**  **Agreement**  The information to assist DL power allocation of the parent-node is indicated by the IAB-MT to the parent node DU in terms of desired power adjustment.   * FFS applicability of assistance information, e.g. per multiplexing scenario, per resource, etc.   **RAN1#106-e**  **Agreement**  The desired DL TX power adjustment, indicated by the IAB-MT to its parent-node to assist with the parent-node’s DL TX power allocation, is provided at least for specific time resources.  The desired DL TX power adjustment can further be associated with spatial configuration. (e.g., MT’s DL RX beams).   * FFS: signalling details, e.g. indication via MAC-CE, PUCCH, or legacy CSI framework. |
| P18 | Power control | New | DL TX Power Adjustment | The parent-node indicates to the IAB-node an adjustment to the parent-node’s DL TX power (e.g., in response to receiving Desired DL TX Power Adjustment from the IAB-node). This indication is provided at least for specific time resources and can further be associated with spatial configuration. | FFS |  | IAB node specific |  | **FFS** | **RAN1#106-e**  **Agreement**  Support an IAB-node indicating adjustment to its DL TX power to a child node (e.g., in response to receiving the DL TX power assistance information from the child node) at least for specific time resources.  The DL TX power adjustment indication can further be associated with spatial configuration. (e.g., MT’s DL RX beams).  FFS: signalling details. |
| P19 | Power control | New | Desired IAB-MT PSD range | The IAB-node indicates to its parent-node, its desired PSD range to help with its MT’s UL TX power control. | FFS |  | IAB node specific |  | **FFS** | **RAN1#106-e**  **Agreement**  Support an IAB-node indicating its desired IAB-MT PSD range to help with its MT’s UL TX power control. This information is provided to the parent node.  FFS: applicability of assistance information, e.g., per multiplexing scenario, per resource, etc.  FFS: signaling details, including the possibility to extend PHR. |

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |

NOTE: the Parameter ID field is an arbitrary field that was added to facilitate referencing a particular row in the parameters table when commenting.