**3GPP TSG RAN WG1 Meeting #107-e R1-211xxxx**

**e-Meeting, November 11– November 19, 2021**

|  |
| --- |
| *CR-Form-v12.0* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **36.213** | **CR** |  | **rev** | **-** | **Current version:** | **V16.7.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Clarification on HARQ bundling for LTE-M MTB scheduling in FDD |
|  |  |
| ***Source to WG:*** | Moderator(ZTE), Sanechips, Ericsson |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | LTE\_eMTC5-Core |  | ***Date:*** | 2021-11-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | For FDD, if the UE is configured with higher layer parameter harq-AckBundling in ce-PDSCH-MultiTB-Config and multiple TB are scheduled in the corresponding DCI, the number of TBs in a bundle and the number of bundles determined by is not aligned with that in Table 7.3-1 defined in TS36.213 clause 7.3. |
|  |  |
| ***Summary of change:*** | Modify the bundling rule in TS36.213 clause 10.2 for multiple TB scheduling in FDD1. Replace the formula as
2. Add the explanation for M as ‘ is determined according to clause 7.3’
3. Remove the redundant description for NTB and bundling size *M*.
 |
|  |  |
| ***Consequences if not approved:*** | Uplink timing determined by the bundling rule in FDD for multiple TBs scheduling is not correct according to the agreement and the current spec in TS36.213 clause 7.3. |
|  |  |
| ***Clauses affected:*** | 10.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |   |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |   |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 10.2 Uplink HARQ-ACK timing

**<Unchanged parts are omitted>**

For FDD, if a BL/CE UE is configured with CEModeA, and if the UE is configured with higher layer parameter *harq-AckBundling* in *ce-PDSCH-MultiTB-Config* and multiple TB are scheduled in the corresponding DCI, the BL/CE UE shall upon detection of a PDSCH intended for the UE and for which an HARQ-ACK shall be provided, transmit the HARQ-ACK response using the same  derived according to Clause 10.1.2.1 in subframe(s) with , *i =0,1, …, N-1*, where

-  is the number of TB bundles, and is determined according to clause 7.3;

- if the UE is not configured with higher layer parameter *interleaving* in *ce-PDSCH-MultiTB-Config* and the UE is not in half-duplex FDD operation

- ,

- otherwise

- subframe **,**

- subframe is the last subframe in which the PDSCH containing TB bundle is transmitted;

- subframe is the last subframe in which the PDSCH is transmitted;

- denotes the number of consecutive subframes including non-BL/CE subframes where the PUCCH with HARQ ACK for TB bundle with repetition number of *N* is transmitted;

and

**<Unchanged parts are omitted>**