**Possible compromise for 3.B**

**Proposal 3.B**: Refine the following agreement as follows:

Agreement

On Rel-17 DCI-based beam indication, regarding application time of the beam indication, the UE is configured with at least one beam application time (BAT) ~~[~~per BWP per CC~~]~~

* Note: It was agreed that the BAT associated with the carrier(s) (hence BWP(s)/CC(s)) on which the beam indication applies is determined based on the carrier with the smallest SCS among the carrier(s) (hence BWP(s)/CC(s)) applying the beam indication
* TBD (maintenance): whether a second configured BAT is also supported, e.g. for MPUE or inter-cell BM
* ~~TBD (RAN1#107-e): Whether or not the UE may assume that BWPs configured with same SCS [in a same CC group] share a same value of BAT~~
* For CCs/BWPs configured with common TCI state ID update, the UE may assume the CCs/BWPs have the same BAT value