Companies are to share their inputs on the excel spreadsheet in /tsg\_ran/WG1\_RL1/TSGR1\_107-e/Inbox/drafts/8.1.3/RRC/ herein.

## Inputs on version 01

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| *FL* | The list is updated from the version endorsed in last meeting on the following aspects (marked in blue)* Two FFS points are cleaned up as we are already in the last meeting.
* The spec clause number is updated based on endorsed RAN1 Rel-17 specs.
* The only unstable parameter was TriggerSRSOnly. My recommendation is to remove this one. From technical perspective, as the Rel-15/16 behavior is gNB will not send a DCI triggering SRS without data and without CSI request. It still works without this parameter. A Rel-17 UE that supports this feature can just transmit SRS when it receives a DCI triggering SRS without data and without CSI request, as this DCI can only be send by a Rel-17 gNB which implements this feature.
 |
| Intel | Ok with FL’s suggestion to remove TriggerSRSOnly. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version xx

Please share your inputs, if any, in the following table

....