**3GPP TSG RAN WG1 #108-e R1-2nnnnn**

**e-Meeting, February 21st – March 3rd, 2022**

**Source: Ad-Hoc Chair (AT&T)**

**Title: Session Notes of AI 8.16.1**

**Agenda Item:** **8.16.1**

**Document for:** **Endorsement**

1.

#### 8.16.1 UE features for further enhancements on NR-MIMO

[108-e-R17-UE-features-MIMO-01] Email discussion on UE features for further enhancements on NR-MIMO – Ralf (AT&T)

* 1st check point: February 25
* Final check point: March 3

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  23. NR\_FeMIMO | 23-1-1 | Unified TCI ~~[~~with joint DL/UL TCI update~~]~~ for intra- [and inter-cell] beam management | 1. Joint DL/UL TCI update with their components: (configuration mechanism, QCL rules, applicable source and target signals)
2. WA: The maximum number of configured joint TCI states [per BWP per CC] [in a band] [in a band combination]
3. ~~a) The maximum number of~~ One MAC-CE activated joint TCI state~~s~~ per CC [in a band] [in a band combination]
4. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication [for one active TCI state]

FFS: whether to include the following components ~~2-14~~ into this FG or one or more separate FGsFFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-1 must also support said basic FGs~~FFS: basic FGs for UEs supporting CA~~FFS: separate FGs for inter/intra/joint/separate 1. For PUCCH, PUSCH, and SRS, association between TCI state and UL PC settings except for PL RS
2. The maximum number of MAC-CE activated joint TCI states across all CCs [in a band] [in a band combination]
3. Common multi-CC TCI state ID update and activation
4. ~~[The minimum beam application time between PUCCH of ACK and the first slot in Y symbols per SCS]~~
5. Beam misalignment between the DL source RS in the TCI state to provide spatial relation indication and the PL-RS
6. ~~TCI state indication [mode]: update and activation [in case of updates]~~~~b) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 with DL assignment)c) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 without DL assignment)~~
7. Reference BWP/CC configured with reference TCI state pool shared by a set of BWP/CCNote: agree component, final wording may change (e.g., when this is merged with other components/FGs)
8. Maximum number of CCs configured with BFR FFS whether this is a component or just a note in the FG to reuse R16 signaling
9. Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH, and SRS reusing the Rel-15/16 signaling/configuration design(s)Note: This has no impact on detail signaling design for SRS TCI indication
10. The maximum number of configured joint TCI state pools across all BWPs and all CCs in a band [in a band combination] ~~FFS: Whether to make component 9 a prerequisite or merge with 9~~
11. [Alt. 1: [The maximum number of PDSCH-Configs containing TCI states that can referred to from a PDSCH-Config without TCI statesAlt. 2: Support PDSCH-Config which contains a reference to another CC/BWP, in which the PDSCH-Config contains the TCI state list]

[16. The minimum time gap between the beam indication PDCCH and first slot where beam is applied] |  |  |  |  |  |  |  |  |  | Optional with capability signalling |
|  23. NR\_FeMIMO | 23-1-1b | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management with more than one MAC-CE activated joint TCI state | 1. TCI state indication [mode]: update and activation [in case of updates]b) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 with DL assignment)c) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 without DL assignment)
2. [The minimum beam application time between PUCCH of ACK and the first slot in Y symbols per SCS]
3. The maximum number of MAC-CE activated joint TCI states per CC [in a band] [in a band combination]
 | 23-1-1 |  |  |  |  |  |  |  | Component 3 candidate values: {2, …} | Optional with capability signalling |
|  23. NR\_FeMIMO | 23-1-1c | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management with carrier aggregation | Per CC configuration of TCI state pools | 23-1-1 |  |  |  |  |  |  |  |  | Optional with capability signalling |

* Note: There will not be a component to signal the maximum number of configured joint TCI states across all BWPs and all CCs

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-2-1 | PDCCH repetition | 1. Support of intra-slot PDCCH repetition based on two linked SS sets associated with corresponding CORESETs [with [non-SFN scheme] TDM and FDM [(except FDM based PDCCH repetition for FR2)] ~~[~~including PDCCH repetition for Type 3 CSS~~]~~2. ~~Support of reporting one number as~~ Required number of BDs for the two PDCCH candidates~~FFS:~~ 3. Support max number of overlaps when one of the linked PDCCH candidates uses the same set of CCEs as an individual (unlinked) PDCCH candidate per scheduled component carrier per slot |   |  |  |  |  |  |  |  | Component 2 candidate values: ~~details~~ 2 or 3Component 3~~4~~ candidate values: ~~[~~{~~0,~~1,2,3, FFS more}~~]~~~~[~~Note: UE supports PDCCH repetition for the following (basic) PDCCH monitoring capability: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, the monitoring occasion is within the first 3 OFDM symbols of a slot~~]~~~~[~~Note: for component 3, ~~if N PDCCH candidates are overlapped, the number of overlaps~~ each unique pair of overlaps is counted as one.~~]~~ | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-3-1 | Multi-TRP PUSCH repetition (type A) ~~[~~-~~CB]~~ codebook based | 1. Support of multi-TRP PUSCH repetition (based on PUSCH repetition type A) ~~[for CB]~~- sequential mapping for repetitions equal to or larger than 2~~[~~- cyclic mapping for 2 repetitions~~]~~~~[2. The maximum number of PHR reporting across all CCs (including those related to M-TRP PUSCH repetition and the legacy Rel-15/16 PUSCH transmission)]~~~~[3. Support dynamic switching between multi-TRP PUSCH scheme and single-TRP PUSCH transmission]~~3. Support of two SRS resource sets with usage set to 'codebook'4. Supported number of SRS resources in one SRS resource set~~FFS: Support PUSCH operations: CB based and NCB based and corresponding parameters including number of SRS resources~~ |  |  |  |  | FFS |  |  |  | ~~[Candidate component values: {CB, non-CB, both}]~~Component 4 candidate values: {1,2 [,4]}  | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-3-1-2 | Multi-TRP PUSCH repetition (type A) - non-codebook based | 1. Support of multi-TRP PUSCH repetition for non-codebook based PUSCH (based on PUSCH repetition type A)2. Support of two SRS resource sets with usage set to 'nonCodebook'3. Supported number of SRS resources in one SRS resource set | 2-15 |  |  |  | FFS |  |  |  | Component 3: {1,2,3,4} | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-3-1-2a | Two associated CSI-RS resources | Support of up to two NZP CSI-RS resources associated with the two SRS resource sets for non-codebook-based mTRP PUSCH | 2-15a, 23-3-1-2 |  |  |  | Per Band |  |  |  |  | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-3-1-2b | CSI-RS processing framework for SRS with two associated CSI-RS resources | 1. Maximum number of periodic SRS resources associated with first and second CSI-RS per BWP2. Maximum number of aperiodic SRS resources associated with first and second CSI-RS per BWP3. Maximum number of semi-persistent SRS resources associated with first and second CSI-RS per BWP4. UE can process Y SRS resources associated with first and second CSI-RS resources simultaneously in a CC. Includes P/SP/A SRS[5. UE can process up to X CSI-RS resources associated with SRS for non-codebook based transmission simultaneously] | 23-3-1-2a |  |  |  | Per Band |  |  |  | [Component 1: {1 to 8}Component 2: {1 to 8}Component 3: {1 to 8}Component 4: {1 to 16}Component 5: {1,2}] | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-7-1 | Basic Features of CSI Enhancement for Multi-TRP | 1. Support of NZP CSI-RS resource pairs used as CMR (channel measurement resource) pairs for NCJT measurement hypothesis: Support of N=1
2. Maximum number of NZP CSI-RS resources in one CSI-RS resource set: Ks,max
3. CSI report mode ~~[~~selection~~]~~ of mode 1 with X=0 ~~[~~and/or~~]~~ mode 2
4. A list of ~~[~~supported combinations, up to 16, across all CCs simultaneously, where each combination is~~]~~
5. ~~[Maximum number of Tx ports in one NZP CSI-RS resource associated with a single-TRP measurement hypothesis]~~
6. Maximum number of Tx ports in one NZP CSI-RS resource associated with an NCJT measurement hypothesis
7. ~~[Maximum total number of CMRs for single-TRP measurement] [per CC/across all CCs]~~
8. Maximum total number of CMRs for NCJT measurement ~~[per CC/across all CCs]~~
9. ~~[Maximum total number of Tx ports of NZP CSI-RS resources associated with single-TRP measurement hypotheses] [per CC/across all CCs]~~
10. Maximum total number of Tx ports of NZP CSI-RS resources associated with NCJT measurement hypotheses ~~[per CC/across all CCs]~~
11. ~~[Maximum total number of Tx ports of NZP CSI-RS resources associated with one NCJT measurement]~~
12. [A list of (Y1,Y2): UE can process Y1 NCJT CSI and Y2 sTRP CSI measurement hypothesis simultaneously in a CC]
13. [A list of (X1,X2): UE can process X1 NCJT CSI and X2 sTRP CSI measurement hypothesis simultaneously across all CCs]
 | ~~FFS~~ |  |  |  | ~~[~~Per band and per BC~~]~~ |  |  |  | ~~[~~Component 2 candidate value set: {~~[0~~, 2, 3,~~]~~ 4, 5, 6, 7, 8}~~]~~~~[~~Component 3 candidate value set: { mode 1 with X=0, mode 2, both}~~]~~Component ~~5~~ 4 candidate values:1. ~~[{2, 4, 8, 12, 16, 24, 32}]~~
2. {2, 4, 8, 12, 16~~[~~, 24, 32~~]~~}
3. ~~[{1,2,3,4 … 64}]~~
4. {2,3,4 … 64}
5. ~~[{4,5,6, …, 256}]~~
6. {2,3,4, …, 256}

[Component 6 5: The list can have maximum of 16 pairs.- Y1: {1 to 4}- Y2: {1 to 8}][Component 7 6: The list can have maximum of 16 pairs.- X1: {1 to 16}- X2: {1 to 32}]Note: ‘NCJT’ is not used in RAN1 specifications and will be aligned with 38.214 | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-7-1b | Active CSI-RS resources and ports in the presence of multi-TRP CSI | 1. List of codebook combinations
2. List of {max number of ports per resource, max number of resources, max number of total ports} for each codebook combination
 | 23-7-1 |  |  |  | Per band and per BC |  |  |  | Component 1 candidate values:Codebook 1 = {[‘NCJT’,] NCJT+Type 1 SP (for sTRP)}{Codebook 2, Codebook 3} = {(NULL, NULL}), {“Rel 16 combinations in FG 16-8”}, {“New Rel17 combinations in FG 23-9-5”}}Component 2 candidate values: - Maximum 16 triplets for each codebook combination - Max # of Tx ports in one resource: {2, 4,8,12,16,24,32} - Max # resources: {1 to 64} - Max # total ports: {4 to 256}Note 1: A CMR pair configured for NCJT will be counted as two activated resources, a CMR configured for sTRP will be counted as one activated resource for a triplet.Note2: This capability is relevant only when UE is configured with NCJT CSI in at least one CSI report setting in at least one CC in the band and/or band combination. | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  23. NR\_FeMIMO | 23-1-1 | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management | 1. Joint DL/UL TCI update with their components: (configuration mechanism, QCL rules, applicable source and target signals)
2. WA: The maximum number of configured joint TCI states [per BWP per CC] [in a band] [in a band combination]
3. One MAC-CE activated joint TCI state per CC [in a band] [in a band combination]
4. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication [for one active TCI state]
5. The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band

FFS: whether to include the following components into this FG or one or more separate FGsFFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-1 must also support said basic FGsFFS: separate FGs for inter/intra/joint/separate 1. For PUCCH, PUSCH, and SRS, association between TCI state and UL PC settings except for PL RS
2. ~~The maximum number of MAC-CE activated joint TCI states across all CCs [in a band] [in a band combination]~~
3. Common multi-CC TCI state ID update and activation
4. Beam misalignment between the DL source RS in the TCI state to provide spatial relation indication and the PL-RS
5. ~~Reference BWP/CC configured with reference TCI state pool shared by a set of BWP/CCNote: agree component, final wording may change (e.g., when this is merged with other components/FGs)~~
6. Maximum number of CCs configured with BFR FFS whether this is a component or just a note in the FG to reuse R16 signaling
7. Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH, and SRS reusing the Rel-15/16 signaling/configuration design(s)Note: This has no impact on detail signaling design for SRS TCI indication
8. ~~The maximum number of configured joint TCI state pools across all BWPs and all CCs in a band [in a band combination]~~
9. ~~[Alt. 1: [The maximum number of PDSCH-Configs containing TCI states that can referred to from a PDSCH-Config without TCI statesAlt. 2: Support PDSCH-Config which contains a reference to another CC/BWP, in which the PDSCH-Config contains the TCI state list]~~

[16. The minimum time gap between the beam indication PDCCH and first slot where beam is applied] |  |  |  |  | FFS | FFS | FFS | FSS | FFS: how to count the MAC-CE activated joint TCI | Optional with capability signalling |
|  23. NR\_FeMIMO | 23-1-1b | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management with more than one MAC-CE activated joint TCI state per CC | 1. TCI state indication [mode]: update and activation [in case of updates]b) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 with DL assignment)c) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 without DL assignment)
2. [The minimum beam application time between PUCCH of ACK and the first slot in Y symbols per SCS]
3. The maximum number of MAC-CE activated joint TCI states per CC [in a band] [in a band combination]
 | 23-1-1 |  |  |  | FFS | FFS | FFS | FSS | Component 3 candidate values: [{2, …}]Note: The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band for more than one MAC-CE activated joint TCI state is signaled in 23-1-1, component 5 | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1d | Per BWP TCI state pool configuration for CA mode | 1. Support of TCI state pool configuration per BWP for CA mode | 23-1-1 |  |  |  | FFS | FFS | FFS | FSS | FFS: A UE that supports 23-1-1 together with CA must indicate this FG is supported] | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1e | TCI state pool configuration with TCI pool sharing for CA mode | 1. Support of reference BWP/CC configured with reference TCI state pool shared by a set of BWP/CC2. The maximum number of configured joint TCI state pools across all BWPs and all CCs in a band  | 23-1-1 |  |  |  | FFS | FFS | FFS | FSS | Component 2 candidate values: FFSFFS: A UE that supports 23-1-1 together with CA must support this FG] | Optional with capability signaling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  23. NR\_FeMIMO | 23-1-2 | Inter-cell beam measurement and reporting [(for inter-cell BM [and mTRP])] | 1. Support of L1-RSRP measurement and reporting on SSB(s) with PCI(s) different from serving cell PCI2. Support of up to K[=4] SSBRI-RSRP [pairs/beams] in one report [where at least one [pair/beam] associated with a PCI different from serving cell PCI can be reported] (FFS: if K is a component candidate value)3. The maximum number of [RRC-configured] PCI(s) different from serving cell PCI for L1-RSRP measurement] (FFS: whether to split this for FR1 and FR2) (FFS: whether/how to capture different values/behaviors for periodic/aperiodic/semi-persistent L1-RSRP measurement)FFS: whether to include the following components ~~2-13~~ into this FG or one or more separate FGsFFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-2 must also support said basic FGs~~2. Support of up to K[=4] SSBRI-RSRP [pairs/beams] in one report [where at least one [pair/beam] associated with a PCI different from serving cell PCI can be reported] (FFS: if K is a component candidate value)~~~~3. The maximum number of [RRC-configured] PCI(s) different from serving cell PCI for L1-RSRP measurement] (FFS: whether to split this for FR1 and FR2) (FFS: whether/how to capture different values/behaviors for periodic/aperiodic/semi-persistent L1-RSRP measurement)~~[4. The max number of SSB resources configured to measure L1-RSRP within a slot with PCI(s) same as or different from serving cell PCI [across all CC]][5. The max number of SSB resources configured to measure L1-RSRP with PCI(s) same as or different from serving cell PCI [across all CC]][6. Support on that SSB(s) with PCI(s) different from serving cell PCI configured for L1 beam measurement and report are not included in SSBs with PCIs configured for L3 mobility measurement][7. The maximum number of configured additional PCIs is X1 when time domain positions and periodicity of configured SSBs with additional PCIs are the same as time domain positions and periodicity of the serving cell SSBs][8. The maximum number of configured additional PCIs is X2 when time domain positions and periodicity of configured SSBs with additional PCIs are different with time domain positions and periodicity of the serving cell SSBs][9. Supported mode inter-cell measurement: {inside SMTC, both inside and outside SMTC}][10. Supported mode of measurement over overlapped SSBs: {overlapped, both overlapped and non-overlapped}][11. Maximum number of overlapped SSBs in one SSB resource for L1-RSRP measurement][12. The maximum total number of SSB/CSI-RS/CSI-IM resources configured to measure within a slot across all CCs in one frequency range for any of L1-RSRP measurement, L1-SINR measurement, pathloss measurement, BFD, RLM and new beam identification for both intra-cell and inter-cell measurement (Similar to FG 16-1g)][13.[The maximum total number of SSB/CSI-RS/CSI-IM resources configured across all CCs in one frequency range for any of L1-RSRP measurement, L1-SINR measurement, pathloss measurement, BFD, RLM and new beam identification for both intra-cell and inter-cell measurement (Similar to FG 16-1g)] | [2-24, 2-29] |  |  |  | [per band] |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-5-1 | Group based L1-RSRP reporting enhancements | 1. Max number N of beam groups (M=2 beams per beam group) in a single L1-RSRP reporting instance based on measurement on two CMR resource sets ~~[2. Maximum number of SSB and CSI-RS resources for measurement in both CMR sets within a slot across all CCs]~~~~[3. Maximum number of configured SSB and CSI-RS resources for measurement in both CMR sets across all CCs]~~ |  |  |  |  |  |  |  |  | Component 1 candidate values: {1,2,3,4}~~Component 2 candidate values: FFS~~~~Component 3 candidate values: FFS~~~~FFS: If FG 23-5-1a is not introduced, the relationship of this FG with FG 16-1g/16-1g-1 needs to be further clarified~~ | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-5-1 | Group based L1-RSRP reporting enhancements | 1. Max number N of beam groups (M=2 beams per beam group) in a single L1-RSRP reporting instance based on measurement on two CMR resource sets ~~[~~2. Maximum number of SSB and CSI-RS resources for measurement in both CMR sets within a slot across all CCs~~]~~~~[~~3. Maximum number of configured SSB and CSI-RS resources for measurement in both CMR sets across all CCs~~]~~ |  | Yes |  | Group based L1-RSRP reporting enhancements are not supported | Per band | n/a | n/a | n/a | Component 1 candidate values: {1,2,3,4}Component 2 candidate values: FFS Component 3 candidate values: FFS Note: component 2 and 3 are also counted in FG 16-1g and 16-1g-1~~FFS: If FG 23-5-1a is not introduced, the relationship of this FG with FG 16-1g/16-1g-1 needs to be further clarified~~ | Optional with capability signalling |
| ~~23. NR\_FeMIMO~~ | ~~23-5-1a~~ | ~~Resources for [for beam management , PL measurement, BFD, RLM, and new beam identification]~~  | ~~1. Maximum number of SSB and CSI-RS resources for measurement in both CMR sets within a slot across all CCs~~~~2. Maximum number of configured SSB and CSI-RS resources for measurement in both CMR sets across all CCs~~~~Note: Strive to align the final implementation of FG 23-5-1a with related R15/16 implementations~~ ~~If 23-5-1a ends up being identical to one or more of Rel.15/ 16 FGs this row will be deleted~~ |  |  |  |  |  |  |  |  | ~~Component 1 candidate values: FFS~~  | ~~Optional with capability signalling~~ |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-5-2 | MTRP BFR ~~enhancement~~ based on two BFD-RS sets | 1. ~~Support of the~~ Maximum number of supported BFD-RS resources per set per BWP~~2. [Support of Rel-17 M-TRP BFR based on two BFD-RS sets]~~ ~~[3. Support one PUCCH-SR resource for MTRP BFRQ]~~3. Supported maximum number of BFD-RS resources across two BFD-RS sets per BWP  |  | Yes |  | MTRP BFR based on two BFD-RS sets is not supported | Per band | n/a | n/a | n/a | ~~[~~Component 1 candidate values: {1, 2~~,…~~}~~]~~Component 3 candidate values: {2,3,4} | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-5-2a | PUCCH-SR resources for MTRP BFRQ | 1. Max number of PUCCH-SR resources for MTRP BFRQ per cell group~~[2. association between a BFD-RS resource set on SpCell and a PUCCH SR resource (if component candidate value equals 2)]~~ |  | Yes |  | PUCCH-SR resources for MTRP BFRQ is not supported | Per UE | No | Yes | No | Component candidate values: {~~[0,~~1~~]~~, 2}[Note: A UE that supports FG 23-5-2 must indicate this FG is supported with at least component candidate value 1] | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-5-2b | Association between a BFD-RS resource set on SpCell and a PUCCH SR resource | Support of association between a BFD-RS resource set on SpCell and a PUCCH SR resource  | 23-5-2a | Yes |  | Association between a BFD-RS resource set on SpCell and a PUCCH SR resource is not supported | Per UE | No | Yes | No | [Note: A UE that supports FG 23-5-2a with candidate value 2 must indicate this FG is supported with at least component candidate value 1] | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-6-1 | SFN scheme A (scheme 1) for PDSCH and PDCCH | 1. Support of SFN scheme A for PDCCH scheduling ~~[single TRP/]~~ SFN Scheme A PDSCH ~~[and default QCL assumption with one or two TCI states for PDCCH]~~ |  | SFN scheme A (scheme 1) for PDSCH and PDCCH is not supported | Yes |  | ~~[Per band or~~ per FS ~~or per FSPC]~~ |  |  |  |  | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-6-1-1 | SFN scheme A (scheme 1) for PDCCH only | Support of SFN scheme A for PDCCH scheduling single TRP PDSCH |  | SFN scheme A (scheme 1) for PDCCH only is not supported  | Yes |  | Per FS |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-6-1a | Dynamic switching - scheme A | Support of dynamic switching between single-TRP and PDSCH SFN scheme A by TCI state field in DCI formats 1\_1, 1\_2 | ~~23-6-2[b]~~  | Dynamic switching - scheme A is not supported | Yes |  | ~~[Per band or~~ per FS ~~or per FSPC]~~ |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-6-1b | SFN scheme A (scheme 1) for PDSCH only | 1. Support of SFN scheme A for PDSCH ~~[only~~ scheduled by ~~[~~single TRP/ ~~Scheme A]~~ PDCCH~~] [and default QCL assumption with one or two TCI states for PDSCH]~~ |  | SFN scheme A (scheme 1) for PDSCH only is not supported | Yes |  | ~~[Per band or~~ per FS ~~or per FSPC]~~ |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-6-2 | SFN scheme B (TRP based pre-compensation) for PDSCH and PDCCH | 1. Support of SFN scheme B for PDCCH scheduling SFN Scheme B PDSCH ~~[and default QCL assumption with one or two TCI states for PDCCH]~~ | ~~[23-6-1]~~ | SFN scheme B (TRP based pre-compensation) for PDSCH and PDCCH is not supported | Yes |  | ~~[Per band or~~ per FS ~~or per FSPC]~~ |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-6-2a | Dynamic switching – scheme B | Support of dynamic switching between single-TRP and PDSCH SFN scheme B by TCI state field in DCI formats 1\_1, 1\_2 | ~~[23-6-2[b]]~~ | Dynamic switching – scheme B is not supported | Yes |  | ~~[Per band or~~ per FS ~~or per FSPC]~~ |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-6-2b | SFN scheme B (TRP based pre-compensation) for PDSCH only | 1. Support of SFN scheme B for PDSCH ~~[only and default QCL assumption with two TCI states for PDSCH] [~~scheduled by ~~[~~single TRP~~/Scheme B]~~ PDCCH~~]~~ | ~~[23-6-1]~~ | SFN scheme B (TRP based pre-compensation) for PDSCH only is not supported  | Yes |  | ~~[Per band or~~ per FS ~~or per FSPC]~~ |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-1-1 | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management | 1. Joint DL/UL TCI update with their components: (configuration mechanism, QCL rules, applicable source and target signals)
2. WA: The maximum number of configured joint TCI states [per BWP per CC] [in a band] [in a band combination]
3. One MAC-CE activated joint TCI state per CC [in a band] [in a band combination]
4. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication [for one active TCI state]
5. The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band

FFS: whether to include the following components into this FG or one or more separate FGsFFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-1 must also support said basic FGsFFS: separate FGs for inter/intra/joint/separate 1. ~~For PUCCH, PUSCH, and SRS, association between TCI state and UL PC settings except for PL RS~~
2. ~~Common multi-CC TCI state ID update and activation~~
3. ~~Beam misalignment between the DL source RS in the TCI state to provide spatial relation indication and the PL-RS~~
4. Maximum number of CCs configured with BFR FFS whether this is a component or just a note in the FG to reuse R16 signaling
5. Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH, and SRS reusing the Rel-15/16 signaling/configuration design(s)Note: This has no impact on detail signaling design for SRS TCI indication
6. [The minimum time gap between the beam indication PDCCH and first slot where beam is applied]
 |  |  |  |  | FFS | FFS | FFS | FSS | FFS: how to count the MAC-CE activated joint TCI | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1f | Common multi-CC TCI state ID update and activation | Common multi-CC TCI state ID update and activation  | 23-1-1 |  |  |  | FFS | FFS | FFS | FSS |  | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1g | Beam misalignment between the DL source RS in the TCI state  | Beam misalignment between the DL source RS in the TCI state to provide spatial relation indication and the PL-RS | 23-1-1 |  |  |  | FFS | FFS | FFS | FSS |  | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1h | Association between TCI state and UL PC settings for PUCCH, PUSCH, and SRS | For PUCCH, PUSCH, and SRS, association between TCI state and UL PC settings except for PL RS | 23-1-1 |  |  |  | FFS | FFS | FFS | FSS | [Note: A UE that supports FG 23-1-1 must indicate this FG is supported] | Optional with capability signaling |

**Agreement: Remove FG 23-1-1c**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ~~23. NR\_FeMIMO~~ | ~~23-1-1c~~ | ~~Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management with carrier aggregation~~ | ~~Per CC configuration of TCI state pools~~ | ~~23-1-1~~ |  |  |  |  |  |  |  |  | ~~Optional with capability signalling~~ |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-1-1 | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management | 1. Joint DL/UL TCI update with their components: (configuration mechanism, QCL rules, applicable source and target signals)
2. WA: The maximum number of configured joint TCI states [per BWP per CC] [in a band] [in a band combination]
3. One MAC-CE activated joint TCI state per CC [in a band] [in a band combination]
4. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication [for one active TCI state]
5. The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band

FFS: whether to include the following components into this FG or one or more separate FGsFFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-1 must also support said basic FGsFFS: separate FGs for inter/intra/joint/separate 1. ~~Maximum number of CCs configured with BFR FFS whether this is a component or just a note in the FG to reuse R16 signaling~~
2. Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH, and SRS reusing the Rel-15/16 signaling/configuration design(s)Note: This has no impact on detail signaling design for SRS TCI indication
3. [The minimum time gap between the beam indication PDCCH and first slot where beam is applied]
 |  |  |  |  | FFS | FFS | FFS | FSS | FFS: how to count the MAC-CE activated joint TCI | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1c | SCell BFR with unified TCI framework | 1. Support of SCell BFR with unified TCI framework [2. Maximum number of CCs configured with SCell BFR with unified TCI framework [in a band with SpCell BFR] |  |  |  |  |  |  |  |  |  | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-1-1 | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management | 1. Joint DL/UL TCI update with their components: (configuration mechanism, QCL rules, applicable source and target signals)
2. WA: The maximum number of configured joint TCI states [per BWP per CC] [in a band] [in a band combination]
3. One MAC-CE activated joint TCI state per CC [in a band] [in a band combination]
4. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication [for one active TCI state]
5. The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band
6. [The minimum time gap between the beam indication PDCCH and first slot where beam is applied]

~~FFS: whether to include the following components into this FG or one or more separate FGs~~~~FFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-1 must also support said basic FGs~~~~FFS: separate FGs for inter/intra/joint/separate~~ 1. ~~Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH, and SRS reusing the Rel-15/16 signaling/configuration design(s)Note: This has no impact on detail signaling design for SRS TCI indication~~
2. ~~[The minimum time gap between the beam indication PDCCH and first slot where beam is applied]~~
 |  | Yes |  | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management is not supported | FFS | FFS | FFS | FSS | FFS: how to count the MAC-CE activated joint TCI | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1i | Indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH [, and SRS] | Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH [, and SRS] (except for TRS and for CORESET #0 and the respective PDSCH reception) reusing the Rel-15/16 signaling/configuration design(s)  | 23-1-1 | Yes  |  | Indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH [, and SRS] reusing the Rel-15/16 signaling/configuration design(s) is not supported | FFS | FFS | FFS | FSS | Note: This has no impact on detail signaling design for SRS TCI indication[A UE that supports 23-1-1 must indicate this FG is supported] | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1j | Indication/configuration of R17 TCI states for CORESET #0 | Support of indication/configuration of R17 TCI states for CORESET #0 and the respective PDSCH reception reusing the Rel-15/16 signaling/configuration design(s) | 23-1-1 | Yes  |  | Support of indication/configuration of R17 TCI states for CORESET #0 and the respective PDSCH reception reusing the Rel-15/16 signaling/configuration design(s) is not supported  | FFS | FFS | FFS | FSS | [A UE that supports 23-1-1 must indicate this FG is supported] | Optional with capability signalling |

* FFS: Whether basic FGs are defined, and if so, which FGs are basic FGs, i.e., a UE that supports FG 23-1-1 must also support said basic FGs
* FFS: separate FGs for inter/intra/joint/separate

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-1-1 | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management | 1. Joint DL/UL TCI update with their components: (configuration mechanism, QCL rules, applicable source and target signals)
2. WA: The maximum number of configured joint TCI states [per BWP per CC] [in a band] [in a band combination]
3. One MAC-CE activated joint TCI state per CC [in a band] [in a band combination]
4. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication [for one active TCI state]
5. The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band
6. ~~[The minimum time gap between the beam indication PDCCH and first slot where beam is applied]~~
 |  | Yes |  | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management is not supported | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | FFS: how to count the MAC-CE activated joint TCI | Optional with capability signalling |
|  23. NR\_FeMIMO | 23-1-1b | Unified TCI with joint DL/UL TCI update for intra- [and inter-cell] beam management with more than one MAC-CE activated joint TCI state per CC | 1. TCI state indication [mode]: update and activation [in case of updates]b) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 with DL assignment)c) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 without DL assignment)
2. [The minimum beam application time between PUCCH of ACK and the first slot in Y symbols per SCS]
3. The maximum number of MAC-CE activated joint TCI states per CC [in a band] [in a band combination]
4. [The minimum time gap between the beam indication PDCCH and first slot where beam is applied]
 | 23-1-1 | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | Component 3 candidate values: {2, …}Note: The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band for more than one MAC-CE activated joint TCI state is signaled in 23-1-1, component 5 | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1c | SCell BFR with unified TCI framework | 1. Support of SCell BFR with unified TCI framework [2. Maximum number of CCs configured with SCell BFR with unified TCI framework [in a band with SpCell BFR] |  | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a |  | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1d | Per BWP TCI state pool configuration for CA mode | 1. Support of TCI state pool configuration per BWP for CA mode | 23-1-1 | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | FFS: A UE that supports 23-1-1 together with CA must indicate this FG is supported] | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1e | TCI state pool configuration with TCI pool sharing for CA mode | 1. Support of reference BWP/CC configured with reference TCI state pool shared by a set of BWP/CC2. The maximum number of configured joint TCI state pools across all BWPs and all CCs in a band  | 23-1-1 | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | Component 2 candidate values: FFSFFS: A UE that supports 23-1-1 together with CA must support this FG] | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1f | Common multi-CC TCI state ID update and activation | Common multi-CC TCI state ID update and activation  | 23-1-1 | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a |  | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1g | Beam misalignment between the DL source RS in the TCI state  | Beam misalignment between the DL source RS in the TCI state to provide spatial relation indication and the PL-RS | 23-1-1 | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | FFS: FR2 only | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1h | Association between TCI state and UL PC settings for PUCCH, PUSCH, and SRS | For PUCCH, PUSCH, and SRS, association between TCI state and UL PC settings except for PL RS | 23-1-1 | Yes |  |  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | [Note: A UE that supports FG 23-1-1 must indicate this FG is supported] | Optional with capability signaling |
| 23. NR\_FeMIMO | 23-1-1i | Indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH [, and SRS] | Support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH [, and SRS] (except for TRS and for CORESET #0 and the respective PDSCH reception) reusing the Rel-15/16 signaling/configuration design(s)  | 23-1-1 | Yes  |  | Indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH [, and SRS] reusing the Rel-15/16 signaling/configuration design(s) is not supported | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | Note: This has no impact on detail signaling design for SRS TCI indication[A UE that supports 23-1-1 must indicate this FG is supported] | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-1-1j | Indication/configuration of R17 TCI states for CORESET #0 | Support of indication/configuration of R17 TCI states for CORESET #0 and the respective PDSCH reception reusing the Rel-15/16 signaling/configuration design(s) | 23-1-1 | Yes  |  | Support of indication/configuration of R17 TCI states for CORESET #0 and the respective PDSCH reception reusing the Rel-15/16 signaling/configuration design(s) is not supported  | ~~FFS~~ per band | ~~FFS~~ n/a | ~~FFS~~ n/a | ~~FFS~~ n/a | [A UE that supports 23-1-1 must indicate this FG is supported] | Optional with capability signalling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-1-2 | Inter-cell beam measurement and reporting [(for inter-cell BM [and mTRP])] | 1. Support of L1-RSRP measurement and reporting on SSB(s) with PCI(s) different from serving cell PCI2. Support of up to K[=4] SSBRI-RSRP [pairs/beams] in one report [where at least one [pair/beam] associated with a PCI different from serving cell PCI can be reported] (FFS: if K is a component candidate value)3. The maximum number of [RRC-configured] PCI(s) different from serving cell PCI for L1-RSRP measurement] (FFS: whether to split this for FR1 and FR2) (FFS: whether/how to capture different values/behaviors for periodic/aperiodic/semi-persistent L1-RSRP measurement)4. The max number of SSB resources configured to measure L1-RSRP within a slot with PCI(s) same as or different from serving cell PCI [across all CC][5. The max number of SSB resources configured to measure L1-RSRP with PCI(s) same as or different from serving cell PCI [across all CC]][6. Support on that SSB(s) with PCI(s) different from serving cell PCI configured for L1 beam measurement and report are not included in SSBs with PCIs configured for L3 mobility measurement][7. Supported mode inter-cell measurement: {inside SMTC, both inside and outside SMTC}][8. Supported mode of measurement over overlapped SSBs: {overlapped, both overlapped and non-overlapped}][9. Maximum number of overlapped SSBs in one SSB resource for L1-RSRP measurement]~~FFS: whether to include the following components into this FG or one or more separate FGs~~~~FFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-2 must also support said basic FGs~~~~[4. The max number of SSB resources configured to measure L1-RSRP within a slot with PCI(s) same as or different from serving cell PCI [across all CC]]~~~~[5. The max number of SSB resources configured to measure L1-RSRP with PCI(s) same as or different from serving cell PCI [across all CC]]~~~~[6. Support on that SSB(s) with PCI(s) different from serving cell PCI configured for L1 beam measurement and report are not included in SSBs with PCIs configured for L3 mobility measurement]~~~~[7. The maximum number of configured additional PCIs is X1 when time domain positions and periodicity of configured SSBs with additional PCIs are the same as time domain positions and periodicity of the serving cell SSBs]~~~~[8. The maximum number of configured additional PCIs is X2 when time domain positions and periodicity of configured SSBs with additional PCIs are different with time domain positions and periodicity of the serving cell SSBs]~~~~[9. Supported mode inter-cell measurement: {inside SMTC, both inside and outside SMTC}]~~~~[10. Supported mode of measurement over overlapped SSBs: {overlapped, both overlapped and non-overlapped}]~~~~[11. Maximum number of overlapped SSBs in one SSB resource for L1-RSRP measurement]~~~~[12. The maximum total number of SSB/CSI-RS/CSI-IM resources configured to measure within a slot across all CCs in one frequency range for any of L1-RSRP measurement, L1-SINR measurement, pathloss measurement, BFD, RLM and new beam identification for both intra-cell and inter-cell measurement (Similar to FG 16-1g)]~~~~[13.[The maximum total number of SSB/CSI-RS/CSI-IM resources configured across all CCs in one frequency range for any of L1-RSRP measurement, L1-SINR measurement, pathloss measurement, BFD, RLM and new beam identification for both intra-cell and inter-cell measurement (Similar to FG 16-1g)]~~ | [2-24, 2-29] | Yes |  | Inter-cell beam measurement and reporting [(for inter-cell BM [and mTRP])] is not supported | ~~[~~per band~~]~~ | n/a | n/a | n/a | [Note: Whether component 4 and/or 5 are also counted in FG16-1g/16-1g-1] | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-4 | IntCell-mTRP | 1. Support of RRC configuration of additional PCI different from serving cell associated with the TCI state and/or QCL-info~~[~~2. The maximum number of configured additional PCIs per CC is X1 (case 1) when each configuration of SSB time domain positions and periodicity of the additional PCIs is the same as SSB time domain positions and periodicity of the serving cell PCI~~]~~~~[~~3. The maximum number of configured additional PCIs per CC is X2 (Case 2) when the configurations of SSB time domain positions and periodicity of the additional PCIs is not according to Case 1~~]~~ | FFS | Yes |  | IntCell-mTRP is not supported | Per band | n/a | n/a | n/a | ~~[~~Component 2 candidate values: {[0,]1,2,3,[ 4, 5, 6,] 7}~~]~~~~[~~Component 3 candidate values: {0,1,2,3, [ 4, 5, 6,]7}~~]~~Note: UE indicates a non-zero value for at least one of component 2 or component 3FFS: how to count X1 and X2[Note: case1 and case2 cannot be enabled simultaneously] | Optional with capability signalling |

* FFS: Whether basic FGs are defined, and if so, which components are basic FGs, i.e., a UE that supports FG 23-1-2 must also support said basic FGs

**Proposal: Introduce the following new FG**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-1-1k | Unified TCI with separate DL/UL TCI update for intra- [and inter-] cell beam management | 1. Support of unified TCI with separate DL/UL TCI update for intra- [and inter-] cell beam management
2. WA: The maximum number of configured DL TCI states [per BWP per CC] [in a band] [in a band combination]
3. WA: The maximum number of configured UL TCI states [per BWP per CC] [in a band] [in a band combination]
4. One MAC-CE activated separate TCI state per CC [in a band] [in a band combination]
5. TCI state indication [mode]: update and activation [in case of updates]a) MAC CE based TCI state indication respectively [for one active TCI state]
6. [The maximum number of MAC-CE activated separate TCI states for DL across all CC(s) in a band]
7. The maximum number of MAC-CE activated separate TCI states for UL across all CC(s) in a band
 | 23-1-1 | Yes |  | Unified TCI with separate DL/UL TCI update for intra- [and inter-] cell beam management | Per band | n/a | n/a | n/a |  | Optional with capability signalling |

**Proposed Agreement: Adopt the following new feature group**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-2-4 | Simultaneous configuration of PDCCH repetition and multi-TRP multi-DCI | Support of simultaneous configuration of PDCCH repetition and multi-TRP multi-DCI | 23-2-1, 16-2a |  Yes |   | Simultaneous configuration of PDCCH repetition and multi-TRP multi-DCI is not supported | FFS | FFS | FFS | FFS |   | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-9-5 | Active CSI-RS resources and ports for mixed codebook types in any slot | 1. List of codebook combinations
2. List of {max number of ports per resource, max number of resources, max number of total ports} for each codebook combination
 | 23-9-1, 16-3a, 16-3b, 16-3a-1, 16-3b-1, 2-36, 2-40, 2-41, 2-43 |  |  |  | Per band and per BC |  |  |  | Component 1 candidate values:Codebook 1 = {Type I SP, Type I MP}{Codebook 2, Codebook 3} = {{FeType II PS M=1, NULL},{FeType II PS M=2 R=1, NULL}[, {FeType II PS M=2 R=2, NULL}], {Type II, FeType II PS M=1}, {Type II, FeType II PS M=2 R=1} ,{eType II R=1, FeType II PS M=1},{eType II R=1, FeType II PS M=2 R=1}}FFS: The list of {Codebook 2, Codebook 3} may be refined depending on outcome of discussion for FG 23-9-2 Component 1 and FG 23-9-4 Component 2Component 2 candidate values: - Maximum 16 triplets for each codebook combination - Max # of Tx ports in one resource: {4,8,12,16,24,32} - Max # resources: {1 to 64} - Max # total ports: {4 to 256}Note 1：if a UE reports one or more codebook combinations in 23-9-5, then usage of active CSI-RS resources and ports for multiple codebooks in any slot is allowed only within those combinations Note 2: For coexisting of mixed codebooks in any slot, gNB need to honor 16-8, 23-9-5 and per-codebook capability 2-36/40/41/43, 16-3a/b and 16-3a-1/16-3b-1, and 23-9-1/23-9-2/23-9-4[Note: If the list of triplets for a codebook combination is empty then the list of triplets is reused from the codebook combination indicated previously] | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-3-3 | Multi-TRP PUCCH repetition-intra-slot | Support of PUCCH repetition scheme 3 (intra-slot repetition)- sequential mapping for repetitions larger than 2[- cyclic mapping for 2 repetitions]  | FFS | Yes |  | PUCCH repetition scheme 3 (intra-slot repetition) is not supported | FFS | FFS | FFS | FFS |  | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-3-2 | Multi-TRP PUCCH repetition | 1. Support of PUCCH repetition scheme 1 (inter-slot repetition)- sequential mapping for repetitions larger than 2~~[~~- cyclic mapping for 2 repetitions~~]~~[2. Support of up to two PUCCH spatial relation per PUCCH resource] | FFS | Yes |  | PUCCH repetition scheme 1 (inter-slot repetition) is not supported | FFS | FFS | FFS | FFS |  | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-3-1 | Multi-TRP PUSCH repetition (type A) -codebook based  | 1. Support of multi-TRP PUSCH repetition (based on PUSCH repetition type A)- sequential mapping for repetitions ~~equal to or~~ larger than 2- cyclic mapping for 2 repetitions3. Support of two SRS resource sets with usage set to 'codebook'4. Supported number of SRS resources in one SRS resource set | FFS | Yes |  | Multi-TRP PUSCH repetition (type A) is not supported for codebook based | FFS | FFS | FFS | FFS | Component 4 candidate values: {1,2 [,4]} | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-3-1-2 | Multi-TRP PUSCH repetition (type A) - non-codebook based | 1. Support of multi-TRP PUSCH repetition for non-codebook based PUSCH (based on PUSCH repetition type A)- sequential mapping for repetitions larger than 2- cyclic mapping for 2 repetitions2. Support of two SRS resource sets with usage set to 'nonCodebook'3. Supported number of SRS resources in one SRS resource set | 2-15 | Yes |  | Multi-TRP PUSCH repetition (type A) is not supported for non-codebook based | FFS | FFS | FFS | FFS | Component 3: {1,2,3,4} | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-3-1-2a | Two associated CSI-RS resources | Support of up to two NZP CSI-RS resources associated with the two SRS resource sets for non-codebook-based mTRP PUSCH | 2-15a, 23-3-1-2 | Yes |  | Two associated CSI-RS resources are not supported | Per Band | n/a | n/a | n/a |  | Optional with capability signalling |
| 23. NR\_FeMIMO | 23-3-1-2b | CSI-RS processing framework for SRS with two associated CSI-RS resources | 1. Maximum number of periodic SRS resources associated with first and second CSI-RS per BWP2. Maximum number of aperiodic SRS resources associated with first and second CSI-RS per BWP3. Maximum number of semi-persistent SRS resources associated with first and second CSI-RS per BWP4. UE can process Y SRS resources associated with first and second CSI-RS resources simultaneously in a CC. Includes P/SP/A SRS[5. UE can process up to X CSI-RS resources associated with SRS for non-codebook based transmission simultaneously] | 23-3-1-2a | Yes |  | CSI-RS processing framework for SRS with two associated CSI-RS resources is not supported | Per Band | n/a | n/a | n/a | [Component 1: {1 to 8}Component 2: {1 to 8}Component 3: {1 to 8}Component 4: {1 to 16}Component 5: {1,2}] | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  23. NR\_FeMIMO | 23-1-3 | MPE mitigation | 1. Support of enhanced [PHR] reporting which includes pairs of (P-MPR, SSBRI/CRI)2. Maximum number of reported P-MPR and SSBRI/CRI pairs 3. Maximum number of candidate RS(s) configured in a RRC pool for MPE mitigation |  | Yes |  | [MPE mitigation is not supported] | FFS | FFS | FFS | FFS | 2. Candidate value of {1,2,3, 4}3. Candidate value ~~FFS~~ [{8, 12, 16, 28, 32, 48, 64}] | Optional with capability signalling |

**Proposed Agreement: Adopt Companies to submit their views on the highlighted issues below**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-2-1 | PDCCH repetition | 1. Support of intra-slot PDCCH repetition based on two linked SS sets associated with corresponding CORESETs [with [non-SFN scheme] TDM and FDM [(except FDM based PDCCH repetition for FR2)] including PDCCH repetition for Type 3 CSS2. Required number of BDs for the two PDCCH candidates3. Support max number of overlaps when one of the linked PDCCH candidates uses the same set of CCEs as an individual (unlinked) PDCCH candidate per scheduled component carrier per slot |   | Yes |  | PDCCH repetition is not supported | FFS | FFS | FFS | FFS | Component 2 candidate values: 2 or 3Component 3 candidate values: {1,2,3, FFS more}Note: UE supports PDCCH repetition for the following (basic) PDCCH monitoring capability: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, the monitoring occasion is within the first 3 OFDM symbols of a slotNote: for component 3, each unique pair of overlaps is counted as one. | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-8-1 | SRS triggering offset enhancement | 1. ~~[Support of/~~The maximum number of configured available slots offsets for~~]~~ determining aperiodic SRS location based on available slot [2. Maximum actual slots offset] | 2-52 | Yes |  | SRS triggering offset enhancement is not supported | Per band | n/a | n/a | n/a | Candidate 1 component values: {1, 2, [3,] 4}[Candidate 2 component values: FFS] | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-7-1 | Basic Features of CSI Enhancement for Multi-TRP | 1. Support of NZP CSI-RS resource pairs used as CMR (channel measurement resource) pairs for NCJT measurement hypothesis: Support of N=1
2. Maximum number of NZP CSI-RS resources in one CSI-RS resource set: Ks,max
3. CSI report mode selection of mode 1 with X=0 and/or mode 2
4. A list of supported combinations, up to 16, across all CCs simultaneously, where each combination is
5. Maximum number of Tx ports in one NZP CSI-RS resource associated with an NCJT measurement hypothesis
6. Maximum total number of CMRs for NCJT measurement
7. Maximum total number of Tx ports of NZP CSI-RS resources associated with NCJT measurement hypotheses
8. [A list of (Y1,Y2): UE can process Y1 NCJT CSI and Y2 sTRP CSI measurement hypothesis simultaneously in a CC]
9. [A list of (X1,X2): UE can process X1 NCJT CSI and X2 sTRP CSI measurement hypothesis simultaneously across all CCs]
 |  | Yes |  | CSI Enhancement for Multi-TRP is not supported | Per band and per BC | n/a | n/a | n/a | Component 2 candidate value set: {2, 3, 4, 5, 6, 7, 8}Component 3 candidate value set: { mode 1 with X=0, mode 2, both}Component 4 candidate values:1. {2, 4, 8, 12, 16~~[~~, 24, 32~~]~~}
2. {2,3,4 … 64}
3. {2,3,4, …, 256}

[Component 5: The list can have maximum of 16 pairs.- Y1: {1 to 4}- Y2: {1 to 8}][Component 6: The list can have maximum of 16 pairs.- X1: {1 to 16}- X2: {1 to 32}]Note: ‘NCJT’ is not used in RAN1 specifications and will be aligned with 38.214 | Optional with capability signalling |

**Proposed Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23. NR\_FeMIMO | 23-3-1-2b | CSI-RS processing framework for SRS with two associated CSI-RS resources | 1. Maximum number of periodic SRS resources associated with first and second CSI-RS per BWP2. Maximum number of aperiodic SRS resources associated with first and second CSI-RS per BWP3. Maximum number of semi-persistent SRS resources associated with first and second CSI-RS per BWP4. UE can process Y SRS resources associated with first and second CSI-RS resources simultaneously in a CC. Includes P/SP/A SRS[5. UE can process up to X CSI-RS resources associated with SRS for non-codebook based transmission simultaneously] | 23-3-1-2a | Yes |  | CSI-RS processing framework for SRS with two associated CSI-RS resources is not supported | Per Band | n/a | n/a | n/a | [Component 1: {1 to 8}Component 2: {1 to 8}Component 3: {1 to 8}Component 4: {1 to 16}Component 5: {1,2}] | Optional with capability signalling |

[R1-2200936](../../Docs/R1-2200936.zip) Rel-17 UE features for further NR MIMO enhancements Huawei, HiSilicon

[R1-2201120](../../Docs/R1-2201120.zip) Discussion on remaining issues of FeMIMO features vivo

[R1-2201199](../../Docs/R1-2201199.zip) UE features for feMIMO ZTE

[R1-2201230](../../Docs/R1-2201230.zip) UE features for further enhancements on NR-MIMO OPPO

[R1-2201344](../../Docs/R1-2201344.zip) On UE features for Rel-17 feMIMO CATT

[R1-2201408](../../Docs/R1-2201408.zip) On UE features for further enhancements on NR-MIMO Nokia, Nokia Shanghai Bell

[R1-2201501](../../Docs/R1-2201501.zip) Discussion on Rel.17 FeMIMO UE features NTT DOCOMO, INC.

[R1-2201562](../../Docs/R1-2201562.zip) Discussion on UE features for FeMIMO Spreadtrum Communications

[R1-2201574](../../Docs/R1-2201574.zip) Discussion on Rel-17 UE feature for NR FeMIMO LG Electronics

[R1-2201723](../../Docs/R1-2201723.zip) On UE features for feMIMO Intel Corporation

[R1-2201791](../../Docs/R1-2201791.zip) Views on Rel-17 FeMIMO UE features Apple

[R1-2201882](../../Docs/R1-2201882.zip) Discussion on UE features for FeMIMO CMCC

[R1-2201952](../../Docs/R1-2201952.zip) Discussion on UE features for FeMIMO Xiaomi

[R1-2202038](../../Docs/R1-2202038.zip) Views on UE features for Rel-17 NR FeMIMO Samsung

[R1-2202058](../../Docs/R1-2202058.zip) UE Features for further enhancements on NR MIMO MediaTek Inc.

[R1-2202092](../../Docs/R1-2202092.zip) Discussion on UE features for FeMIMO Lenovo

[R1-2202165](../../Docs/R1-2202165.zip) Discussion on FeMIMO UE features Qualcomm Incorporated

[R1-2202282](../../Docs/R1-2202282.zip) Discussion on UE features for FeMIMO Ericsson