**3GPP TSG RAN WG1 Meeting #108-e  R1-** **22xxxxx**

**e-Meeting, February 21 – March 3, 2022**

**Agenda Item: 7.2.10**

**Source: Moderator (Huawei)**

**Title: Discussion on correction for Rel-16 UE dormancy adaptation**

**Document for: Discussion and Decision**

# Introduction

This document aims to discuss the correction on Rel1-6 dormancy indication raised in [1] per the following.

[108-e-R16-MRDC-CA-01] Email discussion/approval on the proposals in the draft CR in [R1-2202427](file:///D%3A%5CUsers%5Ct00496347%5CDocuments%5C3GPP%5Cdownload%5CRAN1%23108%5CDocs%5CR1-2202427.zip) by February 25 – Xiaolei (Huawei)

It is suggested to have companies’ initial round of input by the following

* check point: 23:59 UTC, February 22, 2022

# Summary of the issues

In R1-2202427, draft CR was proposed and the changes are summarized as following:

|  |
| --- |
| ***Reason for change:***1. RAN2 changed the configuration structure regarding dormancy cell groups from *DormancySCellGroups,* which explicitly includes a list of dormancy groups*,* in v16.0.0 to *dormancyGroupWithinActiveTime* in v16.7.0. TS 38.331 v16.7.0 specifies *dormancyGroupWithinActiveTime* as dormancy group ID for each configured SCell. Under this new configuration structure of *dormancyGroupWithinActiveTime*, it is not clear how to determine the number of bits for PDCCH dormancy indication field by the description of “according to higher layer parameter *dormancyGroupWithinActiveTime*”.
2. Similar issues exists for the determination of the number of bits for PDCCH dormancy indication field by the description of “according to higher layer parameter *dormancyGroupOutsideActiveTime*”.
3. The description of “with MSB to LSB of the bitmap corresponding to the first to last configured SCell group” is also not clear considering *dormancyGroupWithinActiveTime* is configured per configured SCell in TS 38.331 v16.7.0.

***Summary of change:***1. Update the description for dormancy indication field to capture that the field size is according to “the highest group index provided by higher layer parameter *dormancyGroupWithinActiveTime*”.
2. Update the description of “with MSB to LSB of the bitmap corresponding to the first to last configured SCell group” to “with MSB to LSB of the bitmap corresponding to the configured SCell group with lowest to highest group index”.
3. Similar changes are applied for the case when *dormancyGroupOutsideActiveTime* is configured.
 |

# Discussion

During the preparation phase [2], 9 companies provided comments, and there is clear support to resolve the issues in the draft CR in R1-2202427 in RAN1#108.

## First round

**Discussion Point 1: the number of bits for SCell dormancy indication field**

The Change#1 and Change#3 are similar changes applied respectively for the cases where *dormancyGroupWithinActiveTime* and *dormancyGroupOutsideActiveTime* are configured. Therefore, the two changes can be discussed together.

According to the comments collected during preparation phase, companies have different understanding regarding the number of bits for SCell dormancy indication field. The reason seems that RAN2 changed the configuration structure regarding dormancy cell groups from *DormancySCellGroups*, which explicitly includes a list of dormancy groups, in v16.0.0 to *dormancyGroupWithinActiveTime*/ *dormancyGroupOutsideActiveTime* in v16.7.0. TS 38.331 v16.7.0 specifies *dormancyGroupWithinActiveTime* as dormancy group ID for each configured SCell. Under this signaling method in RAN2, it is unclear on how to figure out the number of bits of the field by the description of “according to higher layer parameter *dormancyGroupWithinActiveTime* or *dormancyGroupOutsideActiveTime*”.

**To align companies’ understanding, please provide your understanding between following Alt.1 and Alt.2. Your comments on the related TPs are also appreciated:**

* **Alt.1: the number of bits for SCell dormancy indication field is according to the highest group index provided by higher layer parameter *dormancyGroupWithinActiveTime* or dormancyGroupOutsideActiveTime for SCells.**

|  |
| --- |
| 7.3.1.1.2 Format 0\_1========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupWithinActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to the highest group index provided by higher layer parameter *dormancyGroupWithinActiveTime* for SCells*,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupWithinActiveTime,* with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.========================= Unchanged parts =========================7.3.1.2.2 Format 1\_1========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupWithinActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to the highest group index provided by higher layer parameter *dormancyGroupWithinActiveTime* for SCells*,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupWithinActiveTime,* with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.========================= Unchanged parts =========================7.3.1.3.7 Format 2\_6========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupOutsideActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to the highest group index provided by higher layer parameter *dormancyGroupOutsideActiveTime* for SCells*,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupOutsideActiveTime,* with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. |

* **Alt.2: the number of bits for SCell dormancy indication field is according to the number of configured group indexes provided by higher layer parameter *dormancyGroupWithinActiveTime* or dormancyGroupOutsideActiveTime for SCells.**

|  |
| --- |
| 7.3.1.1.2 Format 0\_1========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupWithinActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to the number of configured group indexes provided by higher layer parameter *dormancyGroupWithinActiveTime* for SCells*,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupWithinActiveTime,* with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.========================= Unchanged parts =========================7.3.1.2.2 Format 1\_1========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupWithinActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to the number of configured group indexes provided by higher layer parameter *dormancyGroupWithinActiveTime* for SCells*,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupWithinActiveTime,* with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.========================= Unchanged parts =========================7.3.1.3.7 Format 2\_6========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter dormancyGroupOutsideActiveTime is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to the number of configured group indexes provided by higher layer parameter dormancyGroupOutsideActiveTime for SCells, where each bit corresponds to one of the SCell group(s) configured by higher layers parameter dormancyGroupOutsideActiveTime, with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. |

|  |  |  |
| --- | --- | --- |
| Company | Alternatives | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Discussion point 2**

**Please provide your comments on Change#2 in the table.**

|  |
| --- |
| 7.3.1.1.2 Format 0\_1========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupWithinActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to higher layer parameter *dormancyGroupWithinActiveTime,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupWithinActiveTime,* with MSB to LSB of the bitmap corresponding to the ~~first to last~~ configured SCell group with lowest to highest group index. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.========================= Unchanged parts =========================7.3.1.2.2 Format 1\_1========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupWithinActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to higher layer parameter *dormancyGroupWithinActiveTime,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupWithinActiveTime,* with MSB to LSB of the bitmap corresponding to the ~~first to last~~ configured SCell group with lowest to highest group index. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.========================= Unchanged parts =========================7.3.1.3.7 Format 2\_6========================= Unchanged parts =========================- SCell dormancy indication – 0 bit if higher layer parameter *dormancyGroupOutsideActiveTime* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to higher layer parameter *dormancyGroupOutsideActiveTime,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *dormancyGroupOutsideActiveTime,* with MSB to LSB of the bitmap corresponding to the ~~first to last~~ configured SCell group with lowest to highest group index. |

|  |  |  |
| --- | --- | --- |
| Company | Alternatives | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Second round

# Conclusion

# References

1. [R1-2202427](file:///C%3A%5CUsers%5Ct00496347%5CAppData%5CLocal%5CDocs%5CR1-2202427.zip), Correction on Rel-16 UE Power Saving Huawei, HiSilicon.

[2] [R1-2202509](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_108-e/Inbox/R1-2202509.zip), [108-e-Prep-AI7.2.10] Preparation phase summary for Rel-16 NR MR-DC & CA maintenance, Moderator (Nokia)