**3GPP TSG-RAN WG1 Meeting #108-e R1-22xxxxx**

**e-Meeting, February 21st – March 3rd , 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **37.213** | **CR** | **xxx** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  Rel-16 editorial corrections for TS 37.213 |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_unlic-Core |  | ***Date:*** | 2022-03-08 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Misalignment of higher-layer parameter name between TS 37.213 and TS 38.331. |
|  |  |
| ***Summary of change:*** | Alignment of higher-layer parameter name, as follows:Change “*channelAccessMode* = *semistatic*” to “*channelAccessMode* = *semiStatic*” |
|  |  |
| ***Consequences if not approved:*** | Inconsistent specifications |
|  |  |
| ***Clauses affected:*** | 4.1, 4.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 4.1 Downlink channel access procedures

An eNB operating LAA Scell(s) on channel(s) and a gNB performing transmission(s) on channel(s) shall perform the channel access procedures described in this clause for accessing the channel(s) on which the transmission(s) are performed.

In this clause, $X\_{Thresh} $ for sensing is adjusted as described in clause 4.1.5 when applicable.

A gNB performs channel access procedures in this clause unless the higher layer parameter *ChannelAccessMode-r16* is provided and *ChannelAccessMode-r16 =' semiStatic'.*

< Unchanged parts are omitted >

## 4.2 Uplink channel access procedures

A UE performing transmission(s) on LAA Scell(s), an eNB scheduling or configuring UL transmission(s) for a UE performing transmission(s) on LAA Scell(s), and a UE performing transmission(s) on channel(s) and a gNB scheduling or configuring UL transmission(s) for a UE performing transmissions on channel(s) shall perform the procedures described in this clause for the UE to access the channel(s) on which the transmission(s) are performed.

In this clause, transmissions from a UE are considered as separate UL transmissions, irrespective of having a gap between transmissions or not, and $X\_{Thresh}$ for sensing is adjusted as described in clause 4.2.3 when applicable.

A UE performs channel access procedures in this clause unless the higher layer parameter *ChannelAccessMode-r16* is provided and *ChannelAccessMode-r16 =' semiStatic'*.

If a UE fails to access the channel(s) prior to an intended UL transmission to a gNB, Layer 1 notifies higher layers about the channel access failure.