**3GPP TSG RAN WG1 #110 R1-22xxxxx**

**Toulouse, France, August 22nd – 26th, 2022**

**Source: vivo**

**Title: Summary of issues of SL power control in R1-2206715**

**Agenda item: 7.2.4**

**Document for:** **Discussion and Decision**

Introduction

In RAN1#110 meeting, one contribution [1, vivo] is submitted to clarify the SL power control. According to the chairman’s guidance, this document is to collect companies’ views on the issue of SL power control raised in R1-2206715.

Discussion

## Round 1

In [1], the following issue was identified:

In the power control formula in Uu, the transmission power of PUCCH or PUSCH is related to **two components**: P0 and P0nominal, whereas the value range of P0 for PUCCH or PUSCH is **[-16,15]**, and the value range of P0nominal for PUCCH or PUSCH is **[-202..24]**. While the value range for P0 used for power control of PSCCH/PSSCH/PSFCH/S-SSB is [-16,15], the same as that for Uu, but the **P0nominal is missing and the corresponding RRC parameter has even not been defined in R16 SL**. This results in inappropriate transmission power for SL, e.g., the controllable Tx power range of SL is much smaller than UL, and consequently, the minimum SL power would be much larger than that of UL, which causes strong interference to UL in the same frequency. This defeats the purpose of DL pathloss-based SL power control, which is to mitigate interference to the UL reception of the gNB. The relevant NR spec text is copied in appendix A for convenience.

Moreover, it was agreed that the baseline for R16 SL open-loop power control is R14 LTE V2X open-loop power control, in which case only P0 is considered. But it should be noted that the lower limit for *P0-SL* for LTE V2X is the same as the lower limit for *p0-NominalPUSCH* for LTE UL(i.e., -126).

* LTE UL

UplinkPowerControlCommon ::= SEQUENCE {

p0-NominalPUSCH INTEGER (-126..24),

alpha Alpha-r12,

p0-NominalPUCCH INTEGER (-127..-96),

deltaFList-PUCCH DeltaFList-PUCCH,

deltaPreambleMsg3 INTEGER (-1..6)

}

UplinkPowerControlDedicated ::= SEQUENCE {

p0-UE-PUSCH INTEGER (-8..7),

deltaMCS-Enabled ENUMERATED {en0, en1},

accumulationEnabled BOOLEAN,

p0-UE-PUCCH INTEGER (-8..7),

pSRS-Offset INTEGER (0..15),

filterCoefficient FilterCoefficient DEFAULT fc4

}

* LTE V2X

SL-TxParameters-r12 ::= SEQUENCE {

alpha-r12 Alpha-r12,

p0-r12 P0-SL-r12

}

P0-SL-r12 ::= INTEGER (-126..31)

-- ASN1STOP

| *SL-TxParameters* field descriptions |
| --- |
| ***alpha***  Parameter(s): ,,,,,,, See TS 36.213 [23], clauses 14.1.1.5, 14.2.1.3, 14.3.1 and 14.4, where al0 corresponds to 0, al04 corresponds to value 0.4, al05 to 0.5, al06 to 0.6, al07 to 0.7, al08 to 0.8, al09 to 0.9 and al1 corresponds to 1. This field applies for sidelink power control. |
| ***p0***  Parameter: ,,,,,,, see TS 36.213 [23], clauses 14.1.1.5, 14.2.1.3, 14.3.1 and 14.4, unit dBm. |

|  |
| --- |
| Agreements:   * SL open-loop power control is supported.   + For unicast, groupcast, broadcast, it is supported that the open-loop power control is based on the pathloss between TX UE and gNB (if TX UE is in-coverage).     - This is at least to mitigate interference to UL reception at gNB.     - Rel-14 LTE sidelink open-loop power control is the baseline.     - gNB should be able to enable/disable this power control.   + At least for unicast, it is supported that the open-loop power control is also based on the pathloss between TX UE and RX UE.     - (Pre-)configuration should be able to enable/disable this power control.     - FFS whether this is applicable to groupcast     - FFS whether this requires information signaling in the sidelink.   + Further study its potential impact, e.g., on resource allocation. * FFS whether closed-loop power control is additionally needed |

Observation 1: NR PUCCH or PUSCH transmission power is determined based on two components: P0 and P0nominal. However, in NR SL, P0nominal is not defined, which results in inappropriate or incorrect TX power for SL transmission and also defeats the purpose of mitigating interference to UL reception at gNB.

To address this issue, the following options are proposed:

* Option 1. Introduce new RRC parameters (e.g., *dl-P0-nominal-PSSCH-PSCCH, sl-P0-nominal-PSSCH-PSCCH, dl-P0-nominal-PSBCH, dl-P0-nominal-PSFCH*) indicating the nominal power for PSSCH/PSCCH/S-SSB/PSFCH, and modify the power formula by adding the value of the nominal power for sidelink transmission.
* Option 2. Reuse the nominal power of UL transmission (e.g., the value indicated by p0-NominalWithGrant) for SL power control.
* Option 3. Change the value range of the existing RRC parameter P0, e.g., to [-218, 39], or other value ranges.

Option 1 and option 3 are much more flexible and aligned with the Uu, however, both of them require RRC specification changes. Option 2 requires PHY spec change only. However, it is only applicable to in-coverage UE (e.g., connected UE or idle UE), but not applicable to OoC UE (e.g., OoC UE performing SL pathloss-based power control).

**Q1: Do you agree that the issue of SL power control as discussed in** [1] **should be addressed?**

|  |  |  |
| --- | --- | --- |
| **Company** | **agree or not** | **Comment** |
| vivo | yes | If this issue is not addressed, the SL TX power would be forced to be Pcmax or Pmax,CBR even if DL PL or SL PL is used for SL power control, which would lead to large interference to UL reception at gNB side or to SL reception of other SL UEs. |
| Intel | Comments | We acknowledge that the resulting power control is different due to the different parameter ranges, but at this stage to us it is unclear what the parameter range of UL would be and whether the range for SL needs to be the same, considering that the UL has closed loop power control, but the SL only has open loop power control. |
|  |  |  |

**Q2: If the answer to Q1 is yes, which option do you prefer? If you have concerns about the options, please further elaborate on your concerns or a different option to address this issue.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comment** |
| vivo | Option2 or option1 | Option2 avoids changes to ASN.1, thus it is our first preference. However, option 2 has a disadvantage that it does not solve the problem of power control of the OoC UE, in other words, SL TX power control based on SL PL for unicast transmission of OoC UE is still broken. Option1 is also supported to fix this issue for both IC UE and OoC UE. If option1 is agreed, we need to send a LS to RAN2 for ASN.1 change. |
|  |  |  |
|  |  |  |

Summary

TBD

Reference

1. R1-2206715,‘Correction on P0 of SL power control’, vivo

Appendix A: copy of NR spec

* **PUCCH**

|  |
| --- |
| If a UE transmits a PUCCH on active UL BWP  of carrier  in the primary cell  using PUCCH power control adjustment state with index , the UE determines the PUCCH transmission power  in PUCCH transmission occasion  as  [dBm]  where  -  is the UE configured maximum output power defined in [8-1, TS 38.101-1], [8-2, TS 38.101-2] and [8-3, TS 38.101-3] for carrier  of primary cell  in PUCCH transmission occasion  -  is a parameter composed of the sum of a component , provided by *p0-nominal*, or  dBm if *p0-nominal* is not provided, for carrier  of primary cell  and, if provided, a component  provided by *p0-PUCCH-Value* in *P0-PUCCH* for active UL BWP  of carrier  of primary cell , where .  is a size for a set of  values provided by *maxNrofPUCCH-P0-PerSet*. The set of  values is provided by *p0-Set*. If *p0-Set* is not provided to the UE, , |

PUCCH related P0 and P0nominal

PUCCH-PowerControl ::= SEQUENCE {

p0-Set SEQUENCE (SIZE (1..maxNrofPUCCH-P0-PerSet)) OF P0-PUCCH OPTIONAL, -- Need M

pathlossReferenceRSs SEQUENCE (SIZE (1..maxNrofPUCCH-PathlossReferenceRSs)) OF PUCCH-PathlossReferenceRS

OPTIONAL, -- Need M

twoPUCCH-PC-AdjustmentStates ENUMERATED {twoStates} OPTIONAL, -- Need S

...,

[[

pathlossReferenceRSs-v1610 SetupRelease { PathlossReferenceRSs-v1610 } OPTIONAL -- Need M

]]

}

P0-PUCCH ::= SEQUENCE {

p0-PUCCH-Id P0-PUCCH-Id,

p0-PUCCH-Value INTEGER (-16..15)

}

PUCCH-ConfigCommon ::= SEQUENCE {

pucch-ResourceCommon INTEGER (0..15) OPTIONAL, -- Cond InitialBWP-Only

pucch-GroupHopping ENUMERATED { neither, enable, disable },

hoppingId INTEGER (0..1023) OPTIONAL, -- Need R

p0-nominal INTEGER (-202..24) OPTIONAL, -- Need R

...

}

* **PUSCH**

|  |
| --- |
| If a UE transmits a PUSCH on active UL BWP  of carrier  of serving cell  using parameter set configuration with index  and PUSCH power control adjustment state with index , the UE determines the PUSCH transmission power  in PUSCH transmission occasion  as  [dBm]  where,  - is the UE configured maximum output power defined in [8-1, TS 38.101-1], [8-2, TS 38.101-2] and [8-3, TS 38.101-3] for carrier  of serving cell  in PUSCH transmission occasion .  -  is a parameter composed of the sum of a component  and a component  where .  If a UE established dedicated RRC connection using a Type-1 random access procedure, as described in clause 8, and is not provided *P0-PUSCH-AlphaSet* or for a PUSCH (re)transmission corresponding to a RAR UL grant as described in clause 8.3,  , , and ,  where is provided by *preambleReceivedTargetPower* [11, TS 38.321] and is provided by *msg3-DeltaPreamble*, or  dB if *msg3-DeltaPreamble* is not provided, for carrier  of serving cell  - If a UE established dedicated RRC connection using a Type-2 random access procedure, as described in clause 8, and is not provided *P0-PUSCH-AlphaSet*,or for a PUSCH transmission for Type-2 random access procedure as described in clause 8.1A,  , , and ,  where is provided by *msgA-preambleReceivedTargetPower*, or by *preambleReceivedTargetPower* if *msgA-preambleReceivedTargetPower* isnot provided and is provided by *msgA-DeltaPreamble*, or dB if *msgA-DeltaPreamble* is not provided, for carrier of serving cell  - For a PUSCH (re)transmission configured by *ConfiguredGrantConfig*, ,  is provided by *p0-NominalWithoutGrant*, or  if *p0-NominalWithoutGrant* is not provided, and  is provided by *p0* obtained from *p0-PUSCH-Alpha* in *ConfiguredGrantConfig* that provides an index *P0-PUSCH-AlphaSetId* to a set of *P0-PUSCH-AlphaSet* for active UL BWP  of carrier  of serving cell  - For , a  value, applicable for all , is provided by *p0-NominalWithGrant,* or  if *p0-NominalWithGrant* is not provided, for each carrier  of serving cell  and a set of values are provided by a set of *p0* in *P0-PUSCH-AlphaSet* indicated by a respective set of *p0-PUSCH-AlphaSetId* for active UL BWP  of carrier  of serving cell  - If the UE is provided by *SRI-PUSCH-PowerControl* more than one values of *p0-PUSCH-AlphaSetId* and if a DCI format scheduling the PUSCH transmission includes an SRI field, the UE obtains a mapping from *sri-PUSCH-PowerControlId* in *SRI-PUSCH-PowerControl* between a set of values for the SRI field in the DCI format [5, TS 38.212] and a set of indexes provided by *p0-PUSCH-AlphaSetId* that map to a set of *P0-PUSCH-AlphaSet* values and determines the value of  from the *p0-PUSCH-AlphaSetId* value that is mapped to the SRI field value. If the DCI format also includes an open-loop power control parameter set indication field and a value of the open-loop power control parameter set indication field is '1', the UE determines a value of  from a first value in *P0-PUSCH-Set* with a *p0-PUSCH-SetId* value mapped to the SRI field value.  - If the PUSCH transmission except for the PUSCH retransmission corresponding to a RAR UL grant is scheduled by a DCI format that does not include an SRI field, or if *SRI-PUSCH-PowerControl* is not provided to the UE, ,  - If *P0-PUSCH-Set* is provided to the UE and the DCI format includes an open-loop power control parameter set indication field, the UE determines a value of  from  - a first *P0-PUSCH-AlphaSet* in *p0-AlphaSets* if a value of the open-loop power control parameter set indication field is '0' or '00'  - a first value in *P0-PUSCH-Set* with the lowest *p0-PUSCH-SetID* value if a value of the open-loop power control parameter set indication field is '1' or '01'  - a second value in *P0-PUSCH-Set* with the lowest *p0-PUSCH-SetID* value if a value of the open-loop power control parameter set indication field is '10'  - else, the UE determines  from the value of the first *P0-PUSCH-AlphaSet* in *p0-AlphaSets* |

PUSCH related P0 and P0nominal

PUSCH-ConfigCommon ::= SEQUENCE {

groupHoppingEnabledTransformPrecoding ENUMERATED {enabled} OPTIONAL, -- Need R

pusch-TimeDomainAllocationList PUSCH-TimeDomainResourceAllocationList OPTIONAL, -- Need R

msg3-DeltaPreamble INTEGER (-1..6) OPTIONAL, -- Need R

p0-NominalWithGrant INTEGER (-202..24) OPTIONAL, -- Need R

...

}

***p0-NominalWithGrant***

P0 value for PUSCH with grant (except msg3). Value in dBm. Only even values (step size 2) allowed (see TS 38.213 [13], clause 7.1) This field is cell specific

PUSCH-PowerControl ::= SEQUENCE {

tpc-Accumulation ENUMERATED { disabled } OPTIONAL, -- Need S

msg3-Alpha Alpha OPTIONAL, -- Need S

p0-NominalWithoutGrant INTEGER (-202..24) OPTIONAL, -- Need M

p0-AlphaSets SEQUENCE (SIZE (1..maxNrofP0-PUSCH-AlphaSets)) OF P0-PUSCH-AlphaSet OPTIONAL, -- Need M

pathlossReferenceRSToAddModList SEQUENCE (SIZE (1..maxNrofPUSCH-PathlossReferenceRSs)) OF PUSCH-PathlossReferenceRS

OPTIONAL, -- Need N

pathlossReferenceRSToReleaseList SEQUENCE (SIZE (1..maxNrofPUSCH-PathlossReferenceRSs)) OF PUSCH-PathlossReferenceRS-Id

OPTIONAL, -- Need N

twoPUSCH-PC-AdjustmentStates ENUMERATED {twoStates} OPTIONAL, -- Need S

deltaMCS ENUMERATED {enabled} OPTIONAL, -- Need S

sri-PUSCH-MappingToAddModList SEQUENCE (SIZE (1..maxNrofSRI-PUSCH-Mappings)) OF SRI-PUSCH-PowerControl

OPTIONAL, -- Need N

sri-PUSCH-MappingToReleaseList SEQUENCE (SIZE (1..maxNrofSRI-PUSCH-Mappings)) OF SRI-PUSCH-PowerControlId

OPTIONAL -- Need N

}

P0-PUSCH-AlphaSet ::= SEQUENCE {

p0-PUSCH-AlphaSetId P0-PUSCH-AlphaSetId,

p0 INTEGER (-16..15) OPTIONAL, -- Need S

alpha Alpha OPTIONAL -- Need S

}

P0-PUSCH-AlphaSetId ::= INTEGER (0..maxNrofP0-PUSCH-AlphaSets-1)

***p0-NominalWithoutGrant***

P0 value for UL grant-free/SPS based PUSCH. Value in dBm. Only even values (step size 2) allowed (see TS 38.213 [13], clause 7.1).

* **SL**

|  |
| --- |
| A UE determines a power for an S-SS/PSBCH block transmission occasion in slot on active SL BWP of carrier as  [dBm]  where  - is defined in [8-1, TS 38.101-1]  - is a value of *dl-P0-PSBCH* if provided; else,  - is a value of *dl-Alpha-PSBCH*, if provided; else,  - when the active SL BWP is on a serving cell , as described in clause 7.1.1 except that  - the RS resource is the one the UE uses for determining a power of a PUSCH transmission scheduled by a DCI format 0\_0 in serving cell when the UE is configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell  - the RS resource is the one corresponding to the SS/PBCH block the UE uses to obtain MIB when the UE is not configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell  - is a number of resource blocks for a S-SS/PSBCH block transmission with SCS configuration |
| A UE determines a power for a PSSCH transmission on a resource pool in symbols where a corresponding PSCCH is not transmitted in PSCCH-PSSCH transmission occasion on active SL BWP of carrier as:  [dBm]  where  - is defined in [8-1, TS 38.101-1]  - is determined by a value of *sl-MaxTxPower* based on a priority level of the PSSCH transmission and a CBR range that includes a CBR measured in slot [6, TS 38.214]; if *sl-MaxTxPower* is not provided, then ;  - if *dl-P0-PSSCH-PSCCH* is provided  - [dBm]  - else  - [dBm]  where  - is a value of *dl-P0-PSSCH-PSCCH* if provided  - is a value of *dl-Alpha-PSSCH-PSCCH*, if provided; else,  - when the active SL BWP is on a serving cell , as described in clause 7.1.1 except that  - the RS resource is the one the UE uses for determining a power of a PUSCH transmission scheduled by a DCI format 0\_0 in serving cell when the UE is configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell  - the RS resource is the one corresponding to the SS/PBCH block the UE uses to obtain MIB when the UE is not configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell  - is a number of resource blocks for the PSSCH transmission occasion and is a SCS configuration  - if *sl-P0-PSSCH-PSCCH* is provided and if a SCI format scheduling the PSSCH transmission includes a cast type indicator field indicating unicast  - [dBm]  - else  - [dBm]  where  - is a value of *sl-P0-PSSCH-PSCCH*, if provided  - is a value of *sl-Alpha-PSSCH-PSCCH*, if provided; else,  - , where  - is obtained from a PSSCH transmit power per RE summed over the antenna ports of the UE, higher layer filtered across PSSCH transmission occasions using a filter configuration provided by *sl-FilterCoefficient*, and  - is a RSRP, as defined in [7, TS 38.215], that is reported to the UE from a UE receiving the PSCCH-PSSCH transmission and is obtained from a PSSCH DM-RS using a filter configuration provided by *sl-FilterCoefficient*  - is a number of resource blocks for PSCCH-PSSCH transmission occasion and is a SCS configuration  ===omitted=== |
| A UE with scheduled PSFCH transmissions, and capable of transmitting a maximum of PSFCHs, determines a number of simultaneous PSFCH transmissions and a power for a PSFCH transmission , , on a resource pool in PSFCH transmission occasion on active SL BWP of carrier as  - if *dl-P0-PSFCH* is provided,  [dBm]  where  - is a value of *dl-P0-PSFCH*  - is a value of *dl-Alpha-PSFCH*, if provided; else,  ===omitted===  - else  [dBm]  where the UE autonomously determines PSFCH transmissions with ascending order of corresponding priority field values as described in clause 16.2.4.2 such that and where is determined for the PSFCH transmissions according to [8-1, TS 38.101-1]. |

SL related P0 and P0nominal

SL-PSBCH-Config-r16 ::= SEQUENCE {

dl-P0-PSBCH-r16 INTEGER (-16..15) OPTIONAL, -- Need M

dl-Alpha-PSBCH-r16 ENUMERATED {alpha0, alpha04, alpha05, alpha06, alpha07, alpha08, alpha09, alpha1} OPTIONAL, -- Need M

...

}

SL-PowerControl-r16 ::= SEQUENCE {

sl-MaxTransPower-r16 INTEGER (-30..33),

sl-Alpha-PSSCH-PSCCH-r16 ENUMERATED {alpha0, alpha04, alpha05, alpha06, alpha07, alpha08, alpha09, alpha1} OPTIONAL, -- Need M

dl-Alpha-PSSCH-PSCCH-r16 ENUMERATED {alpha0, alpha04, alpha05, alpha06, alpha07, alpha08, alpha09, alpha1} OPTIONAL, -- Need S

sl-P0-PSSCH-PSCCH-r16 INTEGER (-16..15) OPTIONAL, -- Need S

dl-P0-PSSCH-PSCCH-r16 INTEGER (-16..15) OPTIONAL, -- Need M

dl-Alpha-PSFCH-r16 ENUMERATED {alpha0, alpha04, alpha05, alpha06, alpha07, alpha08, alpha09, alpha1} OPTIONAL, -- Need S

dl-P0-PSFCH-r16 INTEGER (-16..15) OPTIONAL, -- Need M

...

}

Appendix B: TP based on option2

### 16.2.0 S-SS/PSBCH blocks

A UE determines a power for an S-SS/PSBCH block transmission occasion in slot on active SL BWP of carrier as

[dBm]

where

- is defined in [8-1, TS 38.101-1]

- is a value of *dl-P0-PSBCH* if provided; else,

- is a value of *p0-NominalWithGrant* if provided for a serving cell when the active SL BWP is on the serving cell ; else,

- is a value of *dl-Alpha-PSBCH*, if provided; else,

- when the active SL BWP is on a serving cell , as described in clause 7.1.1 except that

- the RS resource is the one the UE uses for determining a power of a PUSCH transmission scheduled by a DCI format 0\_0 in serving cell when the UE is configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell

- the RS resource is the one corresponding to the SS/PBCH block the UE uses to obtain MIB when the UE is not configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell

- is a number of resource blocks for a S-SS/PSBCH block transmission with SCS configuration

### 16.2.1 PSSCH

A UE determines a power for a PSSCH transmission on a resource pool in symbols where a corresponding PSCCH is not transmitted in PSCCH-PSSCH transmission occasion on active SL BWP of carrier as:

[dBm]

where

- is defined in [8-1, TS 38.101-1]

- is determined by a value of *sl-MaxTxPower* based on a priority level of the PSSCH transmission and a CBR range that includes a CBR measured in slot [6, TS 38.214]; if *sl-MaxTxPower* is not provided, then ;

- if *dl-P0-PSSCH-PSCCH* is provided

- [dBm]

- else

- [dBm]

where

- is a value of *dl-P0-PSSCH-PSCCH* if provided

- is a value of *p0-NominalWithGrant* if provided for a serving cell when the active SL BWP is on the serving cell ; else,

- is a value of *dl-Alpha-PSSCH-PSCCH*, if provided; else,

- when the active SL BWP is on a serving cell , as described in clause 7.1.1 except that

- the RS resource is the one the UE uses for determining a power of a PUSCH transmission scheduled by a DCI format 0\_0 in serving cell when the UE is configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell

- the RS resource is the one corresponding to the SS/PBCH block the UE uses to obtain MIB when the UE is not configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell

- is a number of resource blocks for the PSSCH transmission occasion and is a SCS configuration

- if *sl-P0-PSSCH-PSCCH* is provided and if a SCI format scheduling the PSSCH transmission includes a cast type indicator field indicating unicast

- [dBm]

- else

- [dBm]

where

- is a value of *sl-P0-PSSCH-PSCCH*, if provided

- is a value of *p0-NominalWithGrant* if provided for a serving cell when the active SL BWP is on the serving cell ; else,

- is a value of *sl-Alpha-PSSCH-PSCCH*, if provided; else,

- , where

- is obtained from a PSSCH transmit power per RE summed over the antenna ports of the UE, higher layer filtered across PSSCH transmission occasions using a filter configuration provided by *sl-FilterCoefficient*, and

- is a RSRP, as defined in [7, TS 38.215], that is reported to the UE from a UE receiving the PSCCH-PSSCH transmission and is obtained from a PSSCH DM-RS using a filter configuration provided by *sl-FilterCoefficient*

- is a number of resource blocks for PSCCH-PSSCH transmission occasion and is a SCS configuration

The UE splits the power equally across the antenna ports on which the UE transmits the PSSCH with non-zero power.

A UE determines a power for a PSSCH transmission on a resource pool in the symbols where a corresponding PSCCH is transmitted in PSCCH-PSSCH transmission occasion on active SL BWP of carrier as

[dBm]

where is a number of resource blocks for the corresponding PSCCH transmission in PSCCH-PSSCH transmission occasion .

The UE splits the power equally across the antenna ports on which the UE transmits the PSSCH with non-zero power.

### 16.2.3 PSFCH

A UE with scheduled PSFCH transmissions, and capable of transmitting a maximum of PSFCHs, determines a number of simultaneous PSFCH transmissions and a power for a PSFCH transmission , , on a resource pool in PSFCH transmission occasion on active SL BWP of carrier as

- if *dl-P0-PSFCH* is provided,

[dBm]

where

- is a value of *dl-P0-PSFCH*

- a value of *p0-NominalWithGrant* if provided for a serving cell when the active SL BWP is on the serving cell ; else,

- is a value of *dl-Alpha-PSFCH*, if provided; else,

- when the active SL BWP is on a serving cell , as described in clause 7.1.1 except that

- the RS resource is the one the UE uses for determining a power of a PUSCH transmission scheduled by a DCI format 0\_0 in serving cell when the UE is configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell

- the RS resource is the one corresponding to the SS/PBCH block the UE uses to obtain MIB when the UE is not configured to monitor PDCCH for detection of DCI format 0\_0 in serving cell

- if

- if , where is determined for PSFCH transmissions according to [8-1, TS 38.101-1]

- and [dBm]

- else

- UE autonomously determines PSFCH transmissions with ascending order of corresponding priority field values as described in clause 16.2.4.2 such that where  is a number of PSFCHs with priority value and is defined as

- the largest value satisfying where is determined according to [8-1, TS 38.101-1] for transmission of all PSFCHs assigned with priority values 1, 2, …, , if any

- zero, otherwise

and

[dBm]

where is defined in [8-1, TS 38.101-1] and is determined for the PSFCH transmissions

- else

- the UE autonomously selects PSFCH transmissions with ascending order of corresponding priority field values as described in clause 16.2.4.2

- if , where is determined for the PSFCH transmissions according to [8-1, TS 38.101-1]

- and [dBm]

- else

- the UE autonomously selects PSFCH transmissions in ascending order of corresponding priority field values as described in clause 16.2.4.2 such that where is a number of PSFCHs with priority value and is defined as

- the largest value satisfying where is determined according to [8-1, TS 38.101-1] for transmission of all PSFCHs assigned with priority values 1, 2, …, , if any

- zero, otherwise

and

[dBm]

where is determined for the simultaneous PSFCH transmissions according to [8-1, TS 38.101-1]

- else

[dBm]

where the UE autonomously determines PSFCH transmissions with ascending order of corresponding priority field values as described in clause 16.2.4.2 such that and where is determined for the PSFCH transmissions according to [8-1, TS 38.101-1].